(module "SOP65P400X130-8N" (layer F.Cu)
  (descr "DCT0008A")
  (tags "Integrated Circuit")
  (attr smd)
  (fp_text reference IC** (at 0 0) (layer F.SilkS)
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_text value "SOP65P400X130-8N" (at 0 0) (layer F.SilkS) hide
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_line (start -2.75 -1.825) (end 2.75 -1.825) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.75 -1.825) (end 2.75 1.825) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.75 1.825) (end -2.75 1.825) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.75 1.825) (end -2.75 -1.825) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.4 -1.475) (end 1.4 -1.475) (layer F.Fab) (width 0.1))
  (fp_line (start 1.4 -1.475) (end 1.4 1.475) (layer F.Fab) (width 0.1))
  (fp_line (start 1.4 1.475) (end -1.4 1.475) (layer F.Fab) (width 0.1))
  (fp_line (start -1.4 1.475) (end -1.4 -1.475) (layer F.Fab) (width 0.1))
  (fp_line (start -1.4 -0.825) (end -0.75 -1.475) (layer F.Fab) (width 0.1))
  (fp_line (start -1.05 -1.475) (end 1.05 -1.475) (layer F.SilkS) (width 0.2))
  (fp_line (start 1.05 -1.475) (end 1.05 1.475) (layer F.SilkS) (width 0.2))
  (fp_line (start 1.05 1.475) (end -1.05 1.475) (layer F.SilkS) (width 0.2))
  (fp_line (start -1.05 1.475) (end -1.05 -1.475) (layer F.SilkS) (width 0.2))
  (fp_line (start -2.5 -1.55) (end -1.4 -1.55) (layer F.SilkS) (width 0.2))
  (pad 1 smd rect (at -1.95 -0.975 90) (size 0.45 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.95 -0.325 90) (size 0.45 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.95 0.325 90) (size 0.45 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.95 0.975 90) (size 0.45 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.95 0.975 90) (size 0.45 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.95 0.325 90) (size 0.45 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 1.95 -0.325 90) (size 0.45 1.1) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 1.95 -0.975 90) (size 0.45 1.1) (layers F.Cu F.Paste F.Mask))
  (model SN74AUC2G08DCTR.stp
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
