ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 1


   1              		.cpu cortex-m7
   2              		.arch armv7e-m
   3              		.fpu fpv5-d16
   4              		.eabi_attribute 28, 1
   5              		.eabi_attribute 20, 1
   6              		.eabi_attribute 21, 1
   7              		.eabi_attribute 23, 3
   8              		.eabi_attribute 24, 1
   9              		.eabi_attribute 25, 1
  10              		.eabi_attribute 26, 1
  11              		.eabi_attribute 30, 1
  12              		.eabi_attribute 34, 1
  13              		.eabi_attribute 18, 4
  14              		.file	"stm32h7xx_hal_mdma.c"
  15              		.text
  16              	.Ltext0:
  17              		.cfi_sections	.debug_frame
  18              		.file 1 "Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c"
  19              		.section	.text.MDMA_SetConfig,"ax",%progbits
  20              		.align	1
  21              		.syntax unified
  22              		.thumb
  23              		.thumb_func
  25              	MDMA_SetConfig:
  26              	.LVL0:
  27              	.LFB354:
   1:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
   2:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   ******************************************************************************
   3:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @file    stm32h7xx_hal_mdma.c
   4:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @author  MCD Application Team
   5:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief  This file provides firmware functions to manage the following
   6:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *         functionalities of the Master Direct Memory Access (MDMA) peripheral:
   7:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *           + Initialization/de-initialization functions
   8:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *           + I/O operation functions
   9:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *           + Peripheral State and errors functions
  10:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   ******************************************************************************
  11:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @attention
  12:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *
  13:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * Copyright (c) 2017 STMicroelectronics.
  14:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * All rights reserved.
  15:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *
  16:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * This software is licensed under terms that can be found in the LICENSE file
  17:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * in the root directory of this software component.
  18:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * If no LICENSE file comes with this software, it is provided AS-IS.
  19:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *
  20:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   ******************************************************************************
  21:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   @verbatim
  22:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   ==============================================================================
  23:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                         ##### How to use this driver #####
  24:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   ==============================================================================
  25:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   [..]
  26:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****    (#) Enable and configure the peripheral to be connected to the MDMA Channel
  27:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****        (except for internal SRAM/FLASH memories: no initialization is
  28:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****        necessary) please refer to Reference manual for connection between peripherals
  29:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****        and MDMA requests.
  30:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
  31:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****    (#)
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 2


  32:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****        For a given Channel use HAL_MDMA_Init function to program the required configuration through
  33:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****        transfer request , channel priority, data endianness, Source increment, destination incremen
  34:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****        source data size, destination data size, data alignment, source Burst, destination Burst ,
  35:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****        buffer Transfer Length, Transfer Trigger Mode (buffer transfer, block transfer, repeated blo
  36:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****        or full transfer) source and destination block address offset, mask address and data.
  37:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
  38:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****        If using the MDMA in linked list mode then use function HAL_MDMA_LinkedList_CreateNode to fi
  39:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****        Note that parameters given to the function HAL_MDMA_Init corresponds always to the node zero
  40:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****        Use function HAL_MDMA_LinkedList_AddNode to connect the created node to the linked list at a
  41:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****        User can make a linked list circular using function HAL_MDMA_LinkedList_EnableCircularMode ,
  42:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****        last node of the list to the first one in order to make the list circular.
  43:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****        In this case the linked list will loop on node 1 : first node connected after the initial tr
  44:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
  45:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       -@-   The initial transfer itself (node 0 corresponding to the Init).
  46:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             User can disable the circular mode using function HAL_MDMA_LinkedList_DisableCircularMo
  47:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             the connection between last node and first one.
  48:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
  49:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****        Function HAL_MDMA_LinkedList_RemoveNode can be used to remove (disconnect) a node from the t
  50:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****        When a linked list is circular (last node connected to first one), if removing node1  (node 
  51:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****        the linked list remains circular and node 2 becomes the first one.
  52:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****        Note that if the linked list is made circular the transfer will loop infinitely (or until ab
  53:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
  54:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     [..]
  55:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****        (+) User can select the transfer trigger mode (parameter TransferTriggerMode) to define the 
  56:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****            transfer upon a request :
  57:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****              (++) MDMA_BUFFER_TRANSFER : each request triggers a transfer of BufferTransferLength d
  58:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                with BufferTransferLength defined within the HAL_MDMA_Init.
  59:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****              (++) MDMA_BLOCK_TRANSFER : each request triggers a transfer of a block
  60:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                with block size defined within the function HAL_MDMA_Start/HAL_MDMA_Start_IT
  61:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                or within the current linked list node parameters.
  62:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****              (++) MDMA_REPEAT_BLOCK_TRANSFER : each request triggers a transfer of a number of bloc
  63:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                with block size and number of blocks defined within the function HAL_MDMA_Start/HAL_
  64:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                or within the current linked list node parameters.
  65:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****              (++) MDMA_FULL_TRANSFER : each request triggers a full transfer
  66:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               all blocks and all nodes(if a linked list has been created using HAL_MDMA_LinkedList_
  67:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
  68:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****      *** Polling mode IO operation ***
  69:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****      =================================
  70:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     [..]
  71:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           (+) Use HAL_MDMA_Start() to start MDMA transfer after the configuration of Source
  72:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               address and destination address and the Length of data to be transferred.
  73:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           (+) Use HAL_MDMA_PollForTransfer() to poll for the end of current transfer or a transfer 
  74:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****              In this case a fixed Timeout can be configured by User depending from his application.
  75:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           (+) Use HAL_MDMA_Abort() function to abort the current transfer : blocking method this AP
  76:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               when the abort ends or timeout (should not be called from an interrupt service routin
  77:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
  78:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****      *** Interrupt mode IO operation ***
  79:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****      ===================================
  80:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     [..]
  81:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           (+) Configure the MDMA interrupt priority using HAL_NVIC_SetPriority()
  82:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           (+) Enable the MDMA IRQ handler using HAL_NVIC_EnableIRQ()
  83:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           (+) Use HAL_MDMA_Start_IT() to start MDMA transfer after the configuration of
  84:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               Source address and destination address and the Length of data to be transferred. In t
  85:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               case the MDMA interrupt is configured.
  86:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           (+) Use HAL_MDMA_IRQHandler() called under MDMA_IRQHandler() Interrupt subroutine
  87:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           (+) At the end of data transfer HAL_MDMA_IRQHandler() function is executed and user can
  88:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               add his own function by customization of function pointer XferCpltCallback and
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 3


  89:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               XferErrorCallback (i.e a member of MDMA handle structure).
  90:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
  91:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           (+) Use HAL_MDMA_Abort_IT() function to abort the current transfer : non-blocking method.
  92:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               then the callback XferAbortCallback (if specified  by the user) is asserted once the 
  93:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               (could be called from an interrupt service routine).
  94:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
  95:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           (+) Use functions HAL_MDMA_RegisterCallback and HAL_MDMA_UnRegisterCallback respectevely 
  96:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               from the following list :
  97:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               (++) XferCpltCallback            : transfer complete callback.
  98:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               (++) XferBufferCpltCallback      : buffer transfer complete callback.
  99:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               (++) XferBlockCpltCallback       : block transfer complete callback.
 100:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               (++) XferRepeatBlockCpltCallback : repeated block transfer complete callback.
 101:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               (++) XferErrorCallback           : transfer error callback.
 102:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               (++) XferAbortCallback           : transfer abort complete callback.
 103:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 104:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     [..]
 105:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****          (+)  If the transfer Request corresponds to SW request (MDMA_REQUEST_SW) User can use func
 106:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               trigger requests manually. Function HAL_MDMA_GenerateSWRequest must be used with the 
 107:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               (++) This function returns an error if used while the Transfer has ended or not start
 108:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               (++) If used while the current request has not been served yet (current request trans
 109:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                 this function returns an error and the new request is ignored.
 110:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 111:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               Generally this function should be used in conjunctions with the MDMA callbacks:
 112:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               (++) example 1:
 113:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                  (+++) Configure a transfer with request set to MDMA_REQUEST_SW and trigger mode se
 114:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                  (+++) Register a callback for buffer transfer complete (using callback ID set to H
 115:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                  (+++) After calling HAL_MDMA_Start_IT the MDMA will issue the transfer of a first 
 116:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                  (+++) When the buffer transfer complete callback is asserted first buffer has been
 117:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                    request using HAL_MDMA_GenerateSWRequest.
 118:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 119:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               (++) example 2:
 120:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                  (+++) Configure a transfer with request set to MDMA_REQUEST_SW and trigger mode se
 121:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                  (+++) Register a callback for block transfer complete (using callback ID HAL_MDMA_
 122:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                  (+++) After calling HAL_MDMA_Start_IT the MDMA will issue the transfer of a first 
 123:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                  (+++) When the block transfer complete callback is asserted the first block has be
 124:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                    for a new block transfer request using HAL_MDMA_GenerateSWRequest.
 125:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 126:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     [..]  Use HAL_MDMA_GetState() function to return the MDMA state and HAL_MDMA_GetError() in case
 127:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 128:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****      *** MDMA HAL driver macros list ***
 129:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****      =============================================
 130:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****      [..]
 131:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****        Below the list of most used macros in MDMA HAL driver.
 132:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 133:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       (+) __HAL_MDMA_ENABLE: Enable the specified MDMA Channel.
 134:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       (+) __HAL_MDMA_DISABLE: Disable the specified MDMA Channel.
 135:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       (+) __HAL_MDMA_GET_FLAG: Get the MDMA Channel pending flags.
 136:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       (+) __HAL_MDMA_CLEAR_FLAG: Clear the MDMA Channel pending flags.
 137:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       (+) __HAL_MDMA_ENABLE_IT: Enable the specified MDMA Channel interrupts.
 138:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       (+) __HAL_MDMA_DISABLE_IT: Disable the specified MDMA Channel interrupts.
 139:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       (+) __HAL_MDMA_GET_IT_SOURCE: Check whether the specified MDMA Channel interrupt has occurred
 140:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 141:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****      [..]
 142:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       (@) You can refer to the header file of the MDMA HAL driver for more useful macros.
 143:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 144:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     [..]
 145:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 4


 146:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   @endverbatim
 147:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
 148:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 149:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /* Includes ------------------------------------------------------------------*/
 150:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** #include "stm32h7xx_hal.h"
 151:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 152:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /** @addtogroup STM32H7xx_HAL_Driver
 153:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @{
 154:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
 155:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 156:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /** @defgroup MDMA  MDMA
 157:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief MDMA HAL module driver
 158:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @{
 159:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
 160:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 161:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** #ifdef HAL_MDMA_MODULE_ENABLED
 162:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 163:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /* Private typedef -----------------------------------------------------------*/
 164:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /* Private constants ---------------------------------------------------------*/
 165:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /** @addtogroup MDMA_Private_Constants
 166:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****  * @{
 167:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****  */
 168:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** #define HAL_TIMEOUT_MDMA_ABORT    5U    /* 5 ms */
 169:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** #define HAL_MDMA_CHANNEL_SIZE     0x40U /* an MDMA instance channel size is 64 byte  */
 170:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
 171:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @}
 172:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
 173:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /* Private macro -------------------------------------------------------------*/
 174:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /* Private variables ---------------------------------------------------------*/
 175:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /* Private function prototypes -----------------------------------------------*/
 176:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /** @addtogroup MDMA_Private_Functions_Prototypes
 177:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @{
 178:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
 179:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** static void MDMA_SetConfig(MDMA_HandleTypeDef *hmdma, uint32_t SrcAddress, uint32_t DstAddress, uin
 180:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** static void MDMA_Init(MDMA_HandleTypeDef *hmdma);
 181:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 182:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
 183:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @}
 184:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
 185:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 186:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /** @addtogroup MDMA_Exported_Functions MDMA Exported Functions
 187:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @{
 188:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
 189:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 190:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /** @addtogroup MDMA_Exported_Functions_Group1
 191:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *
 192:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** @verbatim
 193:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****  ===============================================================================
 194:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****              ##### Initialization and de-initialization functions  #####
 195:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****  ===============================================================================
 196:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     [..]
 197:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     This section provides functions allowing to :
 198:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       Initialize and de-initialize the MDMA channel.
 199:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       Register and Unregister MDMA callbacks
 200:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     [..]
 201:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     The HAL_MDMA_Init() function follows the MDMA channel configuration procedures as described in
 202:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     reference manual.
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 5


 203:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     The HAL_MDMA_DeInit function allows to deinitialize the MDMA channel.
 204:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     HAL_MDMA_RegisterCallback and  HAL_MDMA_UnRegisterCallback functions allows
 205:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     respectevely to register/unregister an MDMA callback function.
 206:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 207:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** @endverbatim
 208:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @{
 209:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
 210:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 211:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
 212:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief  Initializes the MDMA according to the specified
 213:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *         parameters in the MDMA_InitTypeDef and create the associated handle.
 214:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  hmdma: Pointer to a MDMA_HandleTypeDef structure that contains
 215:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *               the configuration information for the specified MDMA Channel.
 216:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @retval HAL status
 217:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
 218:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** HAL_StatusTypeDef HAL_MDMA_Init(MDMA_HandleTypeDef *hmdma)
 219:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** {
 220:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t tickstart = HAL_GetTick();
 221:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 222:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the MDMA peripheral handle */
 223:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(hmdma == NULL)
 224:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 225:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_ERROR;
 226:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 227:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 228:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the parameters */
 229:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_STREAM_ALL_INSTANCE(hmdma->Instance));
 230:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_PRIORITY(hmdma->Init.Priority));
 231:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_ENDIANNESS_MODE(hmdma->Init.Endianness));
 232:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_REQUEST(hmdma->Init.Request));
 233:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_SOURCE_INC(hmdma->Init.SourceInc));
 234:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_DESTINATION_INC(hmdma->Init.DestinationInc));
 235:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_SOURCE_DATASIZE(hmdma->Init.SourceDataSize));
 236:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_DESTINATION_DATASIZE(hmdma->Init.DestDataSize));
 237:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_DATA_ALIGNMENT(hmdma->Init.DataAlignment));
 238:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_SOURCE_BURST(hmdma->Init.SourceBurst));
 239:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_DESTINATION_BURST(hmdma->Init.DestBurst));
 240:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_BUFFER_TRANSFER_LENGTH(hmdma->Init.BufferTransferLength));
 241:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_TRANSFER_TRIGGER_MODE(hmdma->Init.TransferTriggerMode));
 242:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_BLOCK_ADDR_OFFSET(hmdma->Init.SourceBlockAddressOffset));
 243:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_BLOCK_ADDR_OFFSET(hmdma->Init.DestBlockAddressOffset));
 244:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 245:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 246:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Allocate lock resource */
 247:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __HAL_UNLOCK(hmdma);
 248:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 249:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Change MDMA peripheral state */
 250:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->State = HAL_MDMA_STATE_BUSY;
 251:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 252:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Disable the MDMA channel */
 253:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __HAL_MDMA_DISABLE(hmdma);
 254:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 255:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check if the MDMA channel is effectively disabled */
 256:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   while((hmdma->Instance->CCR & MDMA_CCR_EN) != 0U)
 257:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 258:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Check for the Timeout */
 259:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     if((HAL_GetTick() - tickstart ) > HAL_TIMEOUT_MDMA_ABORT)
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 6


 260:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 261:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* Update error code */
 262:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->ErrorCode = HAL_MDMA_ERROR_TIMEOUT;
 263:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 264:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* Change the MDMA state */
 265:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->State = HAL_MDMA_STATE_ERROR;
 266:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 267:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       return HAL_ERROR;
 268:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 269:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 270:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 271:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Initialize the MDMA channel registers */
 272:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   MDMA_Init(hmdma);
 273:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 274:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Reset the MDMA first/last linkedlist node addresses and node counter */
 275:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->FirstLinkedListNodeAddress  = 0;
 276:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->LastLinkedListNodeAddress   = 0;
 277:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->LinkedListNodeCounter  = 0;
 278:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 279:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Initialize the error code */
 280:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->ErrorCode = HAL_MDMA_ERROR_NONE;
 281:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 282:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Initialize the MDMA state */
 283:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->State = HAL_MDMA_STATE_READY;
 284:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 285:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   return HAL_OK;
 286:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 287:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 288:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
 289:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief  DeInitializes the MDMA peripheral
 290:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  hmdma: pointer to a MDMA_HandleTypeDef structure that contains
 291:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *               the configuration information for the specified MDMA Channel.
 292:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @retval HAL status
 293:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
 294:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** HAL_StatusTypeDef HAL_MDMA_DeInit(MDMA_HandleTypeDef *hmdma)
 295:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** {
 296:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 297:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the MDMA peripheral handle */
 298:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(hmdma == NULL)
 299:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 300:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_ERROR;
 301:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 302:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 303:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Disable the selected MDMA Channelx */
 304:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __HAL_MDMA_DISABLE(hmdma);
 305:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 306:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Reset MDMA Channel control register */
 307:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CCR  = 0;
 308:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CTCR = 0;
 309:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CBNDTR = 0;
 310:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CSAR = 0;
 311:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CDAR = 0;
 312:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CBRUR = 0;
 313:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CLAR = 0;
 314:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CTBR = 0;
 315:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CMAR = 0;
 316:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CMDR = 0;
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 7


 317:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 318:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Clear all flags */
 319:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __HAL_MDMA_CLEAR_FLAG(hmdma,(MDMA_FLAG_TE | MDMA_FLAG_CTC | MDMA_FLAG_BRT | MDMA_FLAG_BT | MDMA_F
 320:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 321:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Reset the  MDMA first/last linkedlist node addresses and node counter */
 322:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->FirstLinkedListNodeAddress  = 0;
 323:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->LastLinkedListNodeAddress   = 0;
 324:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->LinkedListNodeCounter  = 0;
 325:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 326:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Initialize the error code */
 327:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->ErrorCode = HAL_MDMA_ERROR_NONE;
 328:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 329:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Initialize the MDMA state */
 330:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->State = HAL_MDMA_STATE_RESET;
 331:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 332:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Release Lock */
 333:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __HAL_UNLOCK(hmdma);
 334:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 335:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   return HAL_OK;
 336:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 337:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 338:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
 339:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief  Config the Post request Mask address and Mask data
 340:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  hmdma      : pointer to a MDMA_HandleTypeDef structure that contains
 341:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *                               the configuration information for the specified MDMA Channel.
 342:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  MaskAddress: specifies the address to be updated (written) with MaskData after a reques
 343:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  MaskData:    specifies the value to be written to MaskAddress after a request is served
 344:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *                      MaskAddress and MaskData could be used to automatically clear a peripheral
 345:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @retval HAL status
 346:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
 347:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** HAL_StatusTypeDef HAL_MDMA_ConfigPostRequestMask(MDMA_HandleTypeDef *hmdma, uint32_t MaskAddress, u
 348:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** {
 349:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   HAL_StatusTypeDef  status = HAL_OK;
 350:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 351:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the MDMA peripheral handle */
 352:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(hmdma == NULL)
 353:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 354:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_ERROR;
 355:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 356:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 357:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Process locked */
 358:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __HAL_LOCK(hmdma);
 359:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 360:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(HAL_MDMA_STATE_READY == hmdma->State)
 361:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 362:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* if HW request set Post Request MaskAddress and MaskData,  */
 363:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     if((hmdma->Instance->CTCR & MDMA_CTCR_SWRM) == 0U)
 364:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 365:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* Set the HW request clear Mask and Data */
 366:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->Instance->CMAR = MaskAddress;
 367:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->Instance->CMDR = MaskData;
 368:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 369:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /*
 370:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       -If the request is done by SW : BWM could be set to 1 or 0.
 371:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       -If the request is done by a peripheral :
 372:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****          If mask address not set (0) => BWM must be set to 0
 373:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****          If mask address set (different than 0) => BWM could be set to 1 or 0
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 8


 374:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       */
 375:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if(MaskAddress == 0U)
 376:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 377:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->Instance->CTCR &=  ~MDMA_CTCR_BWM;
 378:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 379:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       else
 380:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 381:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->Instance->CTCR |=  MDMA_CTCR_BWM;
 382:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 383:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 384:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     else
 385:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 386:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* Return error status */
 387:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       status =  HAL_ERROR;
 388:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 389:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 390:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   else
 391:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 392:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Return error status */
 393:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     status =  HAL_ERROR;
 394:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 395:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Release Lock */
 396:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __HAL_UNLOCK(hmdma);
 397:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 398:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   return status;
 399:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 400:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 401:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
 402:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief  Register callbacks
 403:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  hmdma:                pointer to a MDMA_HandleTypeDef structure that contains
 404:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *                               the configuration information for the specified MDMA Channel.
 405:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  CallbackID:           User Callback identifier
 406:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  pCallback:            pointer to callbacsk function.
 407:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @retval HAL status
 408:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
 409:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** HAL_StatusTypeDef HAL_MDMA_RegisterCallback(MDMA_HandleTypeDef *hmdma, HAL_MDMA_CallbackIDTypeDef C
 410:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** {
 411:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   HAL_StatusTypeDef status = HAL_OK;
 412:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 413:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the MDMA peripheral handle */
 414:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(hmdma == NULL)
 415:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 416:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_ERROR;
 417:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 418:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 419:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Process locked */
 420:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __HAL_LOCK(hmdma);
 421:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 422:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(HAL_MDMA_STATE_READY == hmdma->State)
 423:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 424:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     switch (CallbackID)
 425:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 426:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     case  HAL_MDMA_XFER_CPLT_CB_ID:
 427:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferCpltCallback = pCallback;
 428:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 429:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 430:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     case  HAL_MDMA_XFER_BUFFERCPLT_CB_ID:
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 9


 431:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferBufferCpltCallback = pCallback;
 432:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 433:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 434:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     case  HAL_MDMA_XFER_BLOCKCPLT_CB_ID:
 435:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferBlockCpltCallback = pCallback;
 436:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 437:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 438:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     case  HAL_MDMA_XFER_REPBLOCKCPLT_CB_ID:
 439:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferRepeatBlockCpltCallback = pCallback;
 440:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 441:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 442:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     case  HAL_MDMA_XFER_ERROR_CB_ID:
 443:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferErrorCallback = pCallback;
 444:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 445:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 446:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     case  HAL_MDMA_XFER_ABORT_CB_ID:
 447:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferAbortCallback = pCallback;
 448:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 449:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 450:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     default:
 451:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 452:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 453:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 454:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   else
 455:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 456:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Return error status */
 457:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     status =  HAL_ERROR;
 458:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 459:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 460:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Release Lock */
 461:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __HAL_UNLOCK(hmdma);
 462:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 463:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   return status;
 464:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 465:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 466:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
 467:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief  UnRegister callbacks
 468:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  hmdma:                 pointer to a MDMA_HandleTypeDef structure that contains
 469:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *                               the configuration information for the specified MDMA Channel.
 470:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  CallbackID:           User Callback identifier
 471:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *                               a HAL_MDMA_CallbackIDTypeDef ENUM as parameter.
 472:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @retval HAL status
 473:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
 474:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** HAL_StatusTypeDef HAL_MDMA_UnRegisterCallback(MDMA_HandleTypeDef *hmdma, HAL_MDMA_CallbackIDTypeDef
 475:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** {
 476:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   HAL_StatusTypeDef status = HAL_OK;
 477:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 478:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the MDMA peripheral handle */
 479:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(hmdma == NULL)
 480:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 481:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_ERROR;
 482:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 483:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 484:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Process locked */
 485:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __HAL_LOCK(hmdma);
 486:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 487:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(HAL_MDMA_STATE_READY == hmdma->State)
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 10


 488:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 489:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     switch (CallbackID)
 490:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 491:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     case  HAL_MDMA_XFER_CPLT_CB_ID:
 492:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferCpltCallback = NULL;
 493:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 494:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 495:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     case  HAL_MDMA_XFER_BUFFERCPLT_CB_ID:
 496:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferBufferCpltCallback = NULL;
 497:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 498:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 499:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     case  HAL_MDMA_XFER_BLOCKCPLT_CB_ID:
 500:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferBlockCpltCallback = NULL;
 501:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 502:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 503:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     case  HAL_MDMA_XFER_REPBLOCKCPLT_CB_ID:
 504:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferRepeatBlockCpltCallback = NULL;
 505:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 506:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 507:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     case  HAL_MDMA_XFER_ERROR_CB_ID:
 508:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferErrorCallback = NULL;
 509:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 510:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 511:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     case  HAL_MDMA_XFER_ABORT_CB_ID:
 512:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferAbortCallback = NULL;
 513:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 514:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 515:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     case   HAL_MDMA_XFER_ALL_CB_ID:
 516:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferCpltCallback = NULL;
 517:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferBufferCpltCallback = NULL;
 518:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferBlockCpltCallback = NULL;
 519:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferRepeatBlockCpltCallback = NULL;
 520:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferErrorCallback = NULL;
 521:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferAbortCallback = NULL;
 522:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 523:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 524:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     default:
 525:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       status = HAL_ERROR;
 526:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 527:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 528:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 529:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   else
 530:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 531:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     status = HAL_ERROR;
 532:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 533:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 534:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Release Lock */
 535:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __HAL_UNLOCK(hmdma);
 536:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 537:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   return status;
 538:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 539:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 540:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
 541:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @}
 542:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
 543:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 544:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /** @addtogroup MDMA_Exported_Functions_Group2
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 11


 545:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****  *
 546:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** @verbatim
 547:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****  ===============================================================================
 548:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                       #####  Linked list operation functions  #####
 549:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****  ===============================================================================
 550:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     [..]  This section provides functions allowing to:
 551:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       (+) Create a linked list node
 552:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       (+) Add a node to the MDMA linked list
 553:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       (+) Remove a node from the MDMA linked list
 554:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       (+) Enable/Disable linked list circular mode
 555:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** @endverbatim
 556:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @{
 557:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
 558:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 559:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
 560:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief  Initializes an MDMA Link Node according to the specified
 561:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *         parameters in the pMDMA_LinkedListNodeConfig .
 562:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  pNode: Pointer to a MDMA_LinkNodeTypeDef structure that contains Linked list node
 563:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *         registers configurations.
 564:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  pNodeConfig: Pointer to a MDMA_LinkNodeConfTypeDef structure that contains
 565:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *               the configuration information for the specified MDMA Linked List Node.
 566:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @retval HAL status
 567:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
 568:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** HAL_StatusTypeDef HAL_MDMA_LinkedList_CreateNode(MDMA_LinkNodeTypeDef *pNode, MDMA_LinkNodeConfType
 569:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** {
 570:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t addressMask;
 571:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t blockoffset;
 572:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 573:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the MDMA peripheral state */
 574:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((pNode == NULL) || (pNodeConfig == NULL))
 575:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 576:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_ERROR;
 577:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 578:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 579:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the parameters */
 580:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_PRIORITY(pNodeConfig->Init.Priority));
 581:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_ENDIANNESS_MODE(pNodeConfig->Init.Endianness));
 582:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_REQUEST(pNodeConfig->Init.Request));
 583:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_SOURCE_INC(pNodeConfig->Init.SourceInc));
 584:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_DESTINATION_INC(pNodeConfig->Init.DestinationInc));
 585:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_SOURCE_DATASIZE(pNodeConfig->Init.SourceDataSize));
 586:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_DESTINATION_DATASIZE(pNodeConfig->Init.DestDataSize));
 587:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_DATA_ALIGNMENT(pNodeConfig->Init.DataAlignment));
 588:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_SOURCE_BURST(pNodeConfig->Init.SourceBurst));
 589:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_DESTINATION_BURST(pNodeConfig->Init.DestBurst));
 590:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_BUFFER_TRANSFER_LENGTH(pNodeConfig->Init.BufferTransferLength));
 591:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_TRANSFER_TRIGGER_MODE(pNodeConfig->Init.TransferTriggerMode));
 592:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_BLOCK_ADDR_OFFSET(pNodeConfig->Init.SourceBlockAddressOffset));
 593:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_BLOCK_ADDR_OFFSET(pNodeConfig->Init.DestBlockAddressOffset));
 594:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 595:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_TRANSFER_LENGTH(pNodeConfig->BlockDataLength));
 596:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_BLOCK_COUNT(pNodeConfig->BlockCount));
 597:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 598:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 599:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Configure next Link node Address Register to zero */
 600:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   pNode->CLAR =  0;
 601:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 12


 602:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Configure the Link Node registers*/
 603:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   pNode->CTBR   = 0;
 604:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   pNode->CMAR   = 0;
 605:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   pNode->CMDR   = 0;
 606:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   pNode->Reserved = 0;
 607:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 608:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Write new CTCR Register value */
 609:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   pNode->CTCR =  pNodeConfig->Init.SourceInc | pNodeConfig->Init.DestinationInc | \
 610:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNodeConfig->Init.SourceDataSize | pNodeConfig->Init.DestDataSize           | \
 611:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       pNodeConfig->Init.DataAlignment| pNodeConfig->Init.SourceBurst            | \
 612:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         pNodeConfig->Init.DestBurst                                             | \
 613:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           ((pNodeConfig->Init.BufferTransferLength - 1U) << MDMA_CTCR_TLEN_Pos) | \
 614:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             pNodeConfig->Init.TransferTriggerMode;
 615:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 616:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* If SW request set the CTCR register to SW Request Mode*/
 617:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(pNodeConfig->Init.Request == MDMA_REQUEST_SW)
 618:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 619:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNode->CTCR |= MDMA_CTCR_SWRM;
 620:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 621:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 622:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /*
 623:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   -If the request is done by SW : BWM could be set to 1 or 0.
 624:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   -If the request is done by a peripheral :
 625:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****      If mask address not set (0) => BWM must be set to 0
 626:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****      If mask address set (different than 0) => BWM could be set to 1 or 0
 627:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
 628:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((pNodeConfig->Init.Request == MDMA_REQUEST_SW) || (pNodeConfig->PostRequestMaskAddress != 0U))
 629:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 630:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNode->CTCR |=  MDMA_CTCR_BWM;
 631:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 632:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 633:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Set the new CBNDTR Register value */
 634:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   pNode->CBNDTR = ((pNodeConfig->BlockCount - 1U) << MDMA_CBNDTR_BRC_Pos) & MDMA_CBNDTR_BRC;
 635:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 636:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* if block source address offset is negative set the Block Repeat Source address Update Mode to 
 637:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(pNodeConfig->Init.SourceBlockAddressOffset < 0)
 638:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 639:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNode->CBNDTR |= MDMA_CBNDTR_BRSUM;
 640:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /*write new CBRUR Register value : source repeat block offset */
 641:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     blockoffset = (uint32_t)(- pNodeConfig->Init.SourceBlockAddressOffset);
 642:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNode->CBRUR = blockoffset & 0x0000FFFFU;
 643:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 644:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   else
 645:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 646:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /*write new CBRUR Register value : source repeat block offset */
 647:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNode->CBRUR = (((uint32_t) pNodeConfig->Init.SourceBlockAddressOffset) & 0x0000FFFFU);
 648:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 649:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 650:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* if block destination address offset is negative set the Block Repeat destination address Updat
 651:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(pNodeConfig->Init.DestBlockAddressOffset < 0)
 652:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 653:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNode->CBNDTR |= MDMA_CBNDTR_BRDUM;
 654:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /*write new CBRUR Register value : destination repeat block offset */
 655:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     blockoffset = (uint32_t)(- pNodeConfig->Init.DestBlockAddressOffset);
 656:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNode->CBRUR |= ((blockoffset & 0x0000FFFFU) << MDMA_CBRUR_DUV_Pos);
 657:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 658:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   else
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 13


 659:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 660:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /*write new CBRUR Register value : destination repeat block offset */
 661:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNode->CBRUR |= ((((uint32_t)pNodeConfig->Init.DestBlockAddressOffset) & 0x0000FFFFU) << MDMA_C
 662:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 663:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 664:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Configure MDMA Link Node data length */
 665:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   pNode->CBNDTR |=  pNodeConfig->BlockDataLength;
 666:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 667:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Configure MDMA Link Node destination address */
 668:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   pNode->CDAR = pNodeConfig->DstAddress;
 669:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 670:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Configure MDMA Link Node Source address */
 671:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   pNode->CSAR = pNodeConfig->SrcAddress;
 672:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 673:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* if HW request set the HW request and the requet CleraMask and ClearData MaskData,  */
 674:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(pNodeConfig->Init.Request != MDMA_REQUEST_SW)
 675:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 676:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Set the HW request in CTBR register  */
 677:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNode->CTBR = pNodeConfig->Init.Request & MDMA_CTBR_TSEL;
 678:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Set the HW request clear Mask and Data */
 679:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNode->CMAR = pNodeConfig->PostRequestMaskAddress;
 680:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNode->CMDR = pNodeConfig->PostRequestMaskData;
 681:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 682:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 683:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   addressMask = pNodeConfig->SrcAddress & 0xFF000000U;
 684:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((addressMask == 0x20000000U) || (addressMask == 0x00000000U))
 685:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 686:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /*The AHBSbus is used as source (read operation) on channel x */
 687:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNode->CTBR |= MDMA_CTBR_SBUS;
 688:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 689:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 690:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   addressMask = pNodeConfig->DstAddress & 0xFF000000U;
 691:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((addressMask == 0x20000000U) || (addressMask == 0x00000000U))
 692:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 693:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /*The AHB bus is used as destination (write operation) on channel x */
 694:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNode->CTBR |= MDMA_CTBR_DBUS;
 695:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 696:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 697:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   return HAL_OK;
 698:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 699:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 700:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
 701:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief  Connect a node to the linked list.
 702:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  hmdma    : Pointer to a MDMA_HandleTypeDef structure that contains
 703:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *                    the configuration information for the specified MDMA Channel.
 704:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  pNewNode : Pointer to a MDMA_LinkNodeTypeDef structure that contains Linked list node
 705:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *                    to be add to the list.
 706:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param pPrevNode : Pointer to the new node position in the linked list or zero to insert the ne
 707:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *                    at the end of the list
 708:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *
 709:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @retval HAL status
 710:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
 711:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** HAL_StatusTypeDef HAL_MDMA_LinkedList_AddNode(MDMA_HandleTypeDef *hmdma, MDMA_LinkNodeTypeDef *pNew
 712:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** {
 713:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   MDMA_LinkNodeTypeDef *pNode;
 714:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t counter = 0, nodeInserted = 0;
 715:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   HAL_StatusTypeDef hal_status = HAL_OK;
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 14


 716:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 717:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the MDMA peripheral handle */
 718:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((hmdma == NULL) || (pNewNode == NULL))
 719:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 720:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_ERROR;
 721:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 722:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 723:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Process locked */
 724:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __HAL_LOCK(hmdma);
 725:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 726:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(HAL_MDMA_STATE_READY == hmdma->State)
 727:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 728:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Change MDMA peripheral state */
 729:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->State = HAL_MDMA_STATE_BUSY;
 730:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 731:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Check if this is the first node (after the Inititlization node) */
 732:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     if((uint32_t)hmdma->FirstLinkedListNodeAddress == 0U)
 733:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 734:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if(pPrevNode == NULL)
 735:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 736:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* if this is the first node after the initialization
 737:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         connect this node to the node 0 by updating
 738:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         the MDMA channel CLAR register to this node address */
 739:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->Instance->CLAR = (uint32_t)pNewNode;
 740:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Set the MDMA handle First linked List node*/
 741:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->FirstLinkedListNodeAddress = pNewNode;
 742:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 743:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /*reset New node link */
 744:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         pNewNode->CLAR = 0;
 745:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 746:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Update the Handle last node address */
 747:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->LastLinkedListNodeAddress = pNewNode;
 748:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 749:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->LinkedListNodeCounter = 1;
 750:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 751:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       else
 752:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 753:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hal_status = HAL_ERROR;
 754:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 755:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 756:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     else if(hmdma->FirstLinkedListNodeAddress != pNewNode)
 757:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 758:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* Check if the node to insert already exists*/
 759:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       pNode = hmdma->FirstLinkedListNodeAddress;
 760:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       while((counter < hmdma->LinkedListNodeCounter) && (hal_status == HAL_OK))
 761:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 762:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         if(pNode->CLAR == (uint32_t)pNewNode)
 763:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
 764:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           hal_status = HAL_ERROR; /* error this node already exist in the linked list and it is not
 765:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         }
 766:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         pNode = (MDMA_LinkNodeTypeDef *)pNode->CLAR;
 767:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         counter++;
 768:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 769:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 770:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if(hal_status == HAL_OK)
 771:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 772:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Check if the previous node is the last one in the current list or zero */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 15


 773:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         if((pPrevNode == hmdma->LastLinkedListNodeAddress) || (pPrevNode == NULL))
 774:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
 775:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           /* insert the new node at the end of the list */
 776:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           pNewNode->CLAR = hmdma->LastLinkedListNodeAddress->CLAR;
 777:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           hmdma->LastLinkedListNodeAddress->CLAR = (uint32_t)pNewNode;
 778:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           /* Update the Handle last node address */
 779:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           hmdma->LastLinkedListNodeAddress = pNewNode;
 780:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           /* Increment the linked list node counter */
 781:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           hmdma->LinkedListNodeCounter++;
 782:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         }
 783:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         else
 784:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
 785:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           /*insert the new node after the pPreviousNode node */
 786:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           pNode = hmdma->FirstLinkedListNodeAddress;
 787:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           counter = 0;
 788:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           while((counter < hmdma->LinkedListNodeCounter) && (nodeInserted == 0U))
 789:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           {
 790:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             counter++;
 791:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             if(pNode == pPrevNode)
 792:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             {
 793:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               /*Insert the new node after the previous one */
 794:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               pNewNode->CLAR = pNode->CLAR;
 795:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               pNode->CLAR = (uint32_t)pNewNode;
 796:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               /* Increment the linked list node counter */
 797:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               hmdma->LinkedListNodeCounter++;
 798:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               nodeInserted = 1;
 799:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             }
 800:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             else
 801:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             {
 802:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               pNode = (MDMA_LinkNodeTypeDef *)pNode->CLAR;
 803:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             }
 804:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           }
 805:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 806:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           if(nodeInserted == 0U)
 807:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           {
 808:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             hal_status = HAL_ERROR;
 809:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           }
 810:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         }
 811:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 812:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 813:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     else
 814:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 815:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hal_status = HAL_ERROR;
 816:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 817:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 818:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Process unlocked */
 819:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_UNLOCK(hmdma);
 820:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 821:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->State = HAL_MDMA_STATE_READY;
 822:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 823:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return hal_status;
 824:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 825:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   else
 826:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 827:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Process unlocked */
 828:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_UNLOCK(hmdma);
 829:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 16


 830:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Return error status */
 831:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_BUSY;
 832:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 833:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 834:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 835:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
 836:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief  Disconnect/Remove a node from the transfer linked list.
 837:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  hmdma : Pointer to a MDMA_HandleTypeDef structure that contains
 838:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *                 the configuration information for the specified MDMA Channel.
 839:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  pNode : Pointer to a MDMA_LinkNodeTypeDef structure that contains Linked list node
 840:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *                 to be removed from the list.
 841:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *
 842:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @retval HAL status
 843:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
 844:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** HAL_StatusTypeDef HAL_MDMA_LinkedList_RemoveNode(MDMA_HandleTypeDef *hmdma, MDMA_LinkNodeTypeDef *p
 845:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** {
 846:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   MDMA_LinkNodeTypeDef *ptmpNode;
 847:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t counter = 0, nodeDeleted = 0;
 848:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   HAL_StatusTypeDef hal_status = HAL_OK;
 849:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 850:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the MDMA peripheral handle */
 851:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((hmdma == NULL) || (pNode == NULL))
 852:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 853:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_ERROR;
 854:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 855:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 856:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Process locked */
 857:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __HAL_LOCK(hmdma);
 858:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 859:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(HAL_MDMA_STATE_READY == hmdma->State)
 860:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 861:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Change MDMA peripheral state */
 862:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->State = HAL_MDMA_STATE_BUSY;
 863:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 864:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* If first and last node are null (no nodes in the list) : return error*/
 865:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     if(((uint32_t)hmdma->FirstLinkedListNodeAddress == 0U) || ((uint32_t)hmdma->LastLinkedListNodeA
 866:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 867:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hal_status = HAL_ERROR;
 868:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 869:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     else if(hmdma->FirstLinkedListNodeAddress == pNode) /* Deleting first node */
 870:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 871:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* Delete 1st node */
 872:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if(hmdma->LastLinkedListNodeAddress == pNode)
 873:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 874:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /*if the last node is at the same time the first one (1 single node after the init node 0)
 875:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         then update the last node too */
 876:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 877:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->FirstLinkedListNodeAddress = 0;
 878:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->LastLinkedListNodeAddress  = 0;
 879:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->LinkedListNodeCounter = 0;
 880:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 881:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->Instance->CLAR = 0;
 882:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 883:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       else
 884:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 885:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         if((uint32_t)hmdma->FirstLinkedListNodeAddress == hmdma->LastLinkedListNodeAddress->CLAR)
 886:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 17


 887:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           /* if last node is looping to first (circular list) one update the last node connection *
 888:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           hmdma->LastLinkedListNodeAddress->CLAR = pNode->CLAR;
 889:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         }
 890:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 891:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* if deleting the first node after the initialization
 892:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         connect the next node to the node 0 by updating
 893:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         the MDMA channel CLAR register to this node address */
 894:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->Instance->CLAR = pNode->CLAR;
 895:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->FirstLinkedListNodeAddress = (MDMA_LinkNodeTypeDef *)hmdma->Instance->CLAR;
 896:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Update the Handle node counter */
 897:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->LinkedListNodeCounter--;
 898:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 899:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 900:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     else /* Deleting any other node */
 901:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 902:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /*Deleted node is not the first one : find it  */
 903:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       ptmpNode = hmdma->FirstLinkedListNodeAddress;
 904:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       while((counter < hmdma->LinkedListNodeCounter) && (nodeDeleted == 0U))
 905:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 906:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         counter++;
 907:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         if(ptmpNode->CLAR == ((uint32_t)pNode))
 908:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
 909:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           /* if deleting the last node */
 910:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           if(pNode == hmdma->LastLinkedListNodeAddress)
 911:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           {
 912:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             /*Update the linked list last node address in the handle*/
 913:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             hmdma->LastLinkedListNodeAddress = ptmpNode;
 914:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           }
 915:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           /* update the next node link after deleting pMDMA_LinkedListNode */
 916:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           ptmpNode->CLAR = pNode->CLAR;
 917:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           nodeDeleted = 1;
 918:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           /* Update the Handle node counter */
 919:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           hmdma->LinkedListNodeCounter--;
 920:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         }
 921:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         else
 922:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
 923:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           ptmpNode = (MDMA_LinkNodeTypeDef *)ptmpNode->CLAR;
 924:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         }
 925:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 926:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 927:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if(nodeDeleted == 0U)
 928:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 929:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* last node reashed without finding the node to delete : return error */
 930:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hal_status = HAL_ERROR;
 931:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 932:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 933:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 934:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Process unlocked */
 935:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_UNLOCK(hmdma);
 936:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 937:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->State = HAL_MDMA_STATE_READY;
 938:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 939:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return hal_status;
 940:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 941:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   else
 942:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 943:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Process unlocked */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 18


 944:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_UNLOCK(hmdma);
 945:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 946:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Return error status */
 947:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_BUSY;
 948:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 949:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 950:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 951:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
 952:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief  Make the linked list circular by connecting the last node to the first.
 953:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  hmdma : Pointer to a MDMA_HandleTypeDef structure that contains
 954:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *                 the configuration information for the specified MDMA Channel.
 955:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @retval HAL status
 956:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
 957:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** HAL_StatusTypeDef HAL_MDMA_LinkedList_EnableCircularMode(MDMA_HandleTypeDef *hmdma)
 958:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** {
 959:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   HAL_StatusTypeDef hal_status = HAL_OK;
 960:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 961:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the MDMA peripheral handle */
 962:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(hmdma == NULL)
 963:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 964:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_ERROR;
 965:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 966:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 967:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Process locked */
 968:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __HAL_LOCK(hmdma);
 969:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 970:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(HAL_MDMA_STATE_READY == hmdma->State)
 971:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 972:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Change MDMA peripheral state */
 973:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->State = HAL_MDMA_STATE_BUSY;
 974:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 975:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* If first and last node are null (no nodes in the list) : return error*/
 976:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     if(((uint32_t)hmdma->FirstLinkedListNodeAddress == 0U) || ((uint32_t)hmdma->LastLinkedListNodeA
 977:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 978:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hal_status = HAL_ERROR;
 979:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 980:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     else
 981:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 982:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* to enable circular mode Last Node should be connected to first node */
 983:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->LastLinkedListNodeAddress->CLAR = (uint32_t)hmdma->FirstLinkedListNodeAddress;
 984:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 985:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 986:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 987:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Process unlocked */
 988:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __HAL_UNLOCK(hmdma);
 989:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 990:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->State = HAL_MDMA_STATE_READY;
 991:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 992:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   return hal_status;
 993:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 994:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 995:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
 996:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief  Disable the linked list circular mode by setting the last node connection to null
 997:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  hmdma : Pointer to a MDMA_HandleTypeDef structure that contains
 998:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *                 the configuration information for the specified MDMA Channel.
 999:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @retval HAL status
1000:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 19


1001:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** HAL_StatusTypeDef HAL_MDMA_LinkedList_DisableCircularMode(MDMA_HandleTypeDef *hmdma)
1002:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** {
1003:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   HAL_StatusTypeDef hal_status = HAL_OK;
1004:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1005:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the MDMA peripheral handle */
1006:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(hmdma == NULL)
1007:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1008:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_ERROR;
1009:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1010:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1011:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Process locked */
1012:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __HAL_LOCK(hmdma);
1013:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1014:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(HAL_MDMA_STATE_READY == hmdma->State)
1015:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1016:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Change MDMA peripheral state */
1017:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->State = HAL_MDMA_STATE_BUSY;
1018:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1019:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* If first and last node are null (no nodes in the list) : return error*/
1020:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     if(((uint32_t)hmdma->FirstLinkedListNodeAddress == 0U) || ((uint32_t)hmdma->LastLinkedListNodeA
1021:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
1022:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hal_status = HAL_ERROR;
1023:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
1024:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     else
1025:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
1026:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* to disable circular mode Last Node should be connected to NULL */
1027:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->LastLinkedListNodeAddress->CLAR = 0;
1028:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
1029:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1030:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1031:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Process unlocked */
1032:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __HAL_UNLOCK(hmdma);
1033:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1034:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->State = HAL_MDMA_STATE_READY;
1035:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1036:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   return hal_status;
1037:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
1038:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1039:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
1040:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @}
1041:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
1042:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1043:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /** @addtogroup MDMA_Exported_Functions_Group3
1044:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****  *
1045:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** @verbatim
1046:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****  ===============================================================================
1047:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                       #####  IO operation functions  #####
1048:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****  ===============================================================================
1049:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     [..]  This section provides functions allowing to:
1050:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       (+) Configure the source, destination address and data length and Start MDMA transfer
1051:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       (+) Configure the source, destination address and data length and
1052:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           Start MDMA transfer with interrupt
1053:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       (+) Abort MDMA transfer
1054:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       (+) Poll for transfer complete
1055:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       (+) Generate a SW request (when Request is set to MDMA_REQUEST_SW)
1056:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       (+) Handle MDMA interrupt request
1057:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 20


1058:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** @endverbatim
1059:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @{
1060:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
1061:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1062:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
1063:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief  Starts the MDMA Transfer.
1064:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  hmdma           : pointer to a MDMA_HandleTypeDef structure that contains
1065:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *                           the configuration information for the specified MDMA Channel.
1066:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  SrcAddress      : The source memory Buffer address
1067:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  DstAddress      : The destination memory Buffer address
1068:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  BlockDataLength : The length of a block transfer in bytes
1069:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  BlockCount      : The number of a blocks to be transfer
1070:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @retval HAL status
1071:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
1072:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** HAL_StatusTypeDef HAL_MDMA_Start(MDMA_HandleTypeDef *hmdma, uint32_t SrcAddress, uint32_t DstAddres
1073:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** {
1074:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the parameters */
1075:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_TRANSFER_LENGTH(BlockDataLength));
1076:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_BLOCK_COUNT(BlockCount));
1077:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1078:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the MDMA peripheral handle */
1079:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(hmdma == NULL)
1080:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1081:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_ERROR;
1082:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1083:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1084:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Process locked */
1085:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __HAL_LOCK(hmdma);
1086:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1087:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(HAL_MDMA_STATE_READY == hmdma->State)
1088:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1089:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Change MDMA peripheral state */
1090:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->State = HAL_MDMA_STATE_BUSY;
1091:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1092:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Initialize the error code */
1093:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->ErrorCode = HAL_MDMA_ERROR_NONE;
1094:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1095:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Disable the peripheral */
1096:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_MDMA_DISABLE(hmdma);
1097:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1098:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Configure the source, destination address and the data length */
1099:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     MDMA_SetConfig(hmdma, SrcAddress, DstAddress, BlockDataLength, BlockCount);
1100:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1101:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Enable the Peripheral */
1102:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_MDMA_ENABLE(hmdma);
1103:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1104:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     if(hmdma->Init.Request == MDMA_REQUEST_SW)
1105:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
1106:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* activate If SW request mode*/
1107:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->Instance->CCR |=  MDMA_CCR_SWRQ;
1108:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
1109:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1110:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   else
1111:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1112:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Process unlocked */
1113:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_UNLOCK(hmdma);
1114:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 21


1115:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Return error status */
1116:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_BUSY;
1117:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1118:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1119:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   return HAL_OK;
1120:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
1121:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1122:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
1123:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief  Starts the MDMA Transfer with interrupts enabled.
1124:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  hmdma           : pointer to a MDMA_HandleTypeDef structure that contains
1125:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *                           the configuration information for the specified MDMA Channel.
1126:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  SrcAddress      : The source memory Buffer address
1127:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  DstAddress      : The destination memory Buffer address
1128:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  BlockDataLength : The length of a block transfer in bytes
1129:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  BlockCount      : The number of a blocks to be transfer
1130:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @retval HAL status
1131:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
1132:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** HAL_StatusTypeDef HAL_MDMA_Start_IT(MDMA_HandleTypeDef *hmdma, uint32_t SrcAddress, uint32_t DstAdd
1133:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** {
1134:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the parameters */
1135:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_TRANSFER_LENGTH(BlockDataLength));
1136:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_BLOCK_COUNT(BlockCount));
1137:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1138:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the MDMA peripheral handle */
1139:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(hmdma == NULL)
1140:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1141:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_ERROR;
1142:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1143:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1144:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Process locked */
1145:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __HAL_LOCK(hmdma);
1146:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1147:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(HAL_MDMA_STATE_READY == hmdma->State)
1148:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1149:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Change MDMA peripheral state */
1150:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->State = HAL_MDMA_STATE_BUSY;
1151:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1152:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Initialize the error code */
1153:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->ErrorCode = HAL_MDMA_ERROR_NONE;
1154:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1155:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Disable the peripheral */
1156:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_MDMA_DISABLE(hmdma);
1157:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1158:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Configure the source, destination address and the data length */
1159:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     MDMA_SetConfig(hmdma, SrcAddress, DstAddress, BlockDataLength, BlockCount);
1160:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1161:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Enable Common interrupts i.e Transfer Error IT and Channel Transfer Complete IT*/
1162:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_MDMA_ENABLE_IT(hmdma, (MDMA_IT_TE | MDMA_IT_CTC));
1163:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1164:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     if(hmdma->XferBlockCpltCallback != NULL)
1165:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
1166:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* if Block transfer complete Callback is set enable the corresponding IT*/
1167:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       __HAL_MDMA_ENABLE_IT(hmdma, MDMA_IT_BT);
1168:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
1169:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1170:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     if(hmdma->XferRepeatBlockCpltCallback != NULL)
1171:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 22


1172:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* if Repeated Block transfer complete Callback is set enable the corresponding IT*/
1173:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       __HAL_MDMA_ENABLE_IT(hmdma, MDMA_IT_BRT);
1174:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
1175:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1176:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     if(hmdma->XferBufferCpltCallback != NULL)
1177:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
1178:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* if buffer transfer complete Callback is set enable the corresponding IT*/
1179:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       __HAL_MDMA_ENABLE_IT(hmdma, MDMA_IT_BFTC);
1180:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
1181:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1182:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Enable the Peripheral */
1183:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_MDMA_ENABLE(hmdma);
1184:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1185:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     if(hmdma->Init.Request == MDMA_REQUEST_SW)
1186:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
1187:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* activate If SW request mode*/
1188:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->Instance->CCR |=  MDMA_CCR_SWRQ;
1189:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
1190:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1191:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   else
1192:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1193:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Process unlocked */
1194:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_UNLOCK(hmdma);
1195:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1196:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Return error status */
1197:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_BUSY;
1198:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1199:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1200:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   return HAL_OK;
1201:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
1202:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1203:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
1204:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief  Aborts the MDMA Transfer.
1205:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  hmdma  : pointer to a MDMA_HandleTypeDef structure that contains
1206:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *                 the configuration information for the specified MDMA Channel.
1207:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *
1208:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @note  After disabling a MDMA Channel, a check for wait until the MDMA Channel is
1209:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *        effectively disabled is added. If a Channel is disabled
1210:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *        while a data transfer is ongoing, the current data will be transferred
1211:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *        and the Channel will be effectively disabled only after the transfer of
1212:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *        this single data is finished.
1213:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @retval HAL status
1214:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
1215:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** HAL_StatusTypeDef HAL_MDMA_Abort(MDMA_HandleTypeDef *hmdma)
1216:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** {
1217:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t tickstart =  HAL_GetTick();
1218:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1219:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the MDMA peripheral handle */
1220:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(hmdma == NULL)
1221:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1222:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_ERROR;
1223:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1224:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1225:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(HAL_MDMA_STATE_BUSY != hmdma->State)
1226:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1227:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->ErrorCode = HAL_MDMA_ERROR_NO_XFER;
1228:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 23


1229:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Process Unlocked */
1230:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_UNLOCK(hmdma);
1231:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1232:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_ERROR;
1233:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1234:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   else
1235:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1236:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Disable all the transfer interrupts */
1237:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_MDMA_DISABLE_IT(hmdma, (MDMA_IT_TE | MDMA_IT_CTC | MDMA_IT_BT | MDMA_IT_BRT | MDMA_IT_BFT
1238:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1239:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Disable the channel */
1240:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_MDMA_DISABLE(hmdma);
1241:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1242:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Check if the MDMA Channel is effectively disabled */
1243:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     while((hmdma->Instance->CCR & MDMA_CCR_EN) != 0U)
1244:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
1245:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* Check for the Timeout */
1246:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if( (HAL_GetTick()  - tickstart ) > HAL_TIMEOUT_MDMA_ABORT)
1247:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
1248:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Update error code */
1249:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->ErrorCode |= HAL_MDMA_ERROR_TIMEOUT;
1250:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1251:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Process Unlocked */
1252:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         __HAL_UNLOCK(hmdma);
1253:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1254:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Change the MDMA state */
1255:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->State = HAL_MDMA_STATE_ERROR;
1256:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1257:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         return HAL_ERROR;
1258:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
1259:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
1260:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1261:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Clear all interrupt flags */
1262:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_MDMA_CLEAR_FLAG(hmdma, (MDMA_FLAG_TE | MDMA_FLAG_CTC | MDMA_FLAG_BT | MDMA_FLAG_BRT | MDM
1263:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1264:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Process Unlocked */
1265:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_UNLOCK(hmdma);
1266:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1267:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Change the MDMA state*/
1268:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->State = HAL_MDMA_STATE_READY;
1269:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1270:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1271:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   return HAL_OK;
1272:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
1273:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1274:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
1275:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief  Aborts the MDMA Transfer in Interrupt mode.
1276:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  hmdma  : pointer to a MDMA_HandleTypeDef structure that contains
1277:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *                 the configuration information for the specified MDMA Channel.
1278:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @retval HAL status
1279:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
1280:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** HAL_StatusTypeDef HAL_MDMA_Abort_IT(MDMA_HandleTypeDef *hmdma)
1281:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** {
1282:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the MDMA peripheral handle */
1283:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(hmdma == NULL)
1284:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1285:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_ERROR;
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 24


1286:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1287:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1288:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(HAL_MDMA_STATE_BUSY != hmdma->State)
1289:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1290:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* No transfer ongoing */
1291:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->ErrorCode = HAL_MDMA_ERROR_NO_XFER;
1292:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1293:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_ERROR;
1294:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1295:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   else
1296:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1297:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Set Abort State  */
1298:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->State = HAL_MDMA_STATE_ABORT;
1299:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1300:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Disable the stream */
1301:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_MDMA_DISABLE(hmdma);
1302:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1303:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1304:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   return HAL_OK;
1305:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
1306:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1307:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
1308:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief  Polling for transfer complete.
1309:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  hmdma:          pointer to a MDMA_HandleTypeDef structure that contains
1310:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *                        the configuration information for the specified MDMA Channel.
1311:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  CompleteLevel: Specifies the MDMA level complete.
1312:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  Timeout:       Timeout duration.
1313:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @retval HAL status
1314:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
1315:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** HAL_StatusTypeDef HAL_MDMA_PollForTransfer(MDMA_HandleTypeDef *hmdma, HAL_MDMA_LevelCompleteTypeDef
1316:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** {
1317:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t levelFlag, errorFlag;
1318:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t tickstart;
1319:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1320:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the parameters */
1321:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_LEVEL_COMPLETE(CompleteLevel));
1322:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1323:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the MDMA peripheral handle */
1324:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(hmdma == NULL)
1325:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1326:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_ERROR;
1327:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1328:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1329:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(HAL_MDMA_STATE_BUSY != hmdma->State)
1330:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1331:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* No transfer ongoing */
1332:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->ErrorCode = HAL_MDMA_ERROR_NO_XFER;
1333:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1334:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_ERROR;
1335:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1336:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1337:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Get the level transfer complete flag */
1338:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   levelFlag = ((CompleteLevel == HAL_MDMA_FULL_TRANSFER)  ? MDMA_FLAG_CTC  : \
1339:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                (CompleteLevel == HAL_MDMA_BUFFER_TRANSFER)? MDMA_FLAG_BFTC : \
1340:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                (CompleteLevel == HAL_MDMA_BLOCK_TRANSFER) ? MDMA_FLAG_BT   : \
1341:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                MDMA_FLAG_BRT);
1342:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 25


1343:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1344:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Get timeout */
1345:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   tickstart = HAL_GetTick();
1346:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1347:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   while(__HAL_MDMA_GET_FLAG(hmdma, levelFlag) == 0U)
1348:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1349:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     if((__HAL_MDMA_GET_FLAG(hmdma, MDMA_FLAG_TE) != 0U))
1350:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
1351:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* Get the transfer error source flag */
1352:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       errorFlag = hmdma->Instance->CESR;
1353:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1354:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if((errorFlag & MDMA_CESR_TED) == 0U)
1355:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
1356:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Update error code : Read Transfer error  */
1357:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->ErrorCode |= HAL_MDMA_ERROR_READ_XFER;
1358:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
1359:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       else
1360:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
1361:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Update error code : Write Transfer error */
1362:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->ErrorCode |= HAL_MDMA_ERROR_WRITE_XFER;
1363:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
1364:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1365:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if((errorFlag & MDMA_CESR_TEMD) != 0U)
1366:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
1367:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Update error code : Error Mask Data */
1368:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->ErrorCode |= HAL_MDMA_ERROR_MASK_DATA;
1369:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
1370:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1371:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if((errorFlag & MDMA_CESR_TELD) != 0U)
1372:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
1373:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Update error code : Error Linked list */
1374:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->ErrorCode |= HAL_MDMA_ERROR_LINKED_LIST;
1375:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
1376:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1377:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if((errorFlag & MDMA_CESR_ASE) != 0U)
1378:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
1379:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Update error code : Address/Size alignment error */
1380:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->ErrorCode |= HAL_MDMA_ERROR_ALIGNMENT;
1381:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
1382:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1383:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if((errorFlag & MDMA_CESR_BSE) != 0U)
1384:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
1385:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Update error code : Block Size error */
1386:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->ErrorCode |= HAL_MDMA_ERROR_BLOCK_SIZE;
1387:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
1388:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1389:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       (void) HAL_MDMA_Abort(hmdma); /* if error then abort the current transfer */
1390:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1391:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /*
1392:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         Note that the Abort function will
1393:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           - Clear all transfer flags
1394:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           - Unlock
1395:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           - Set the State
1396:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       */
1397:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1398:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       return HAL_ERROR;
1399:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 26


1400:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
1401:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1402:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Check for the Timeout */
1403:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     if(Timeout != HAL_MAX_DELAY)
1404:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
1405:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if(((HAL_GetTick() - tickstart ) > Timeout) || (Timeout == 0U))
1406:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
1407:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Update error code */
1408:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->ErrorCode |= HAL_MDMA_ERROR_TIMEOUT;
1409:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1410:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         (void) HAL_MDMA_Abort(hmdma); /* if timeout then abort the current transfer */
1411:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1412:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /*
1413:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           Note that the Abort function will
1414:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             - Clear all transfer flags
1415:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             - Unlock
1416:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             - Set the State
1417:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         */
1418:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1419:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         return HAL_ERROR;
1420:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
1421:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
1422:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1423:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1424:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Clear the transfer level flag */
1425:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(CompleteLevel == HAL_MDMA_BUFFER_TRANSFER)
1426:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1427:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_MDMA_CLEAR_FLAG(hmdma, MDMA_FLAG_BFTC);
1428:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1429:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1430:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   else if(CompleteLevel == HAL_MDMA_BLOCK_TRANSFER)
1431:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1432:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_MDMA_CLEAR_FLAG(hmdma, (MDMA_FLAG_BFTC | MDMA_FLAG_BT));
1433:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1434:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1435:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   else if(CompleteLevel == HAL_MDMA_REPEAT_BLOCK_TRANSFER)
1436:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1437:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_MDMA_CLEAR_FLAG(hmdma, (MDMA_FLAG_BFTC | MDMA_FLAG_BT | MDMA_FLAG_BRT));
1438:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1439:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   else if(CompleteLevel == HAL_MDMA_FULL_TRANSFER)
1440:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1441:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_MDMA_CLEAR_FLAG(hmdma, (MDMA_FLAG_BRT | MDMA_FLAG_BT | MDMA_FLAG_BFTC | MDMA_FLAG_CTC));
1442:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1443:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Process unlocked */
1444:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_UNLOCK(hmdma);
1445:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1446:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->State = HAL_MDMA_STATE_READY;
1447:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1448:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   else
1449:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1450:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_ERROR;
1451:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1452:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1453:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   return HAL_OK;
1454:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
1455:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1456:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 27


1457:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief  Generate an MDMA SW request trigger to activate the request on the given Channel.
1458:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  hmdma:       pointer to a MDMA_HandleTypeDef structure that contains
1459:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *                     the configuration information for the specified MDMA Stream.
1460:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @retval HAL status
1461:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
1462:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** HAL_StatusTypeDef HAL_MDMA_GenerateSWRequest(MDMA_HandleTypeDef *hmdma)
1463:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** {
1464:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t request_mode;
1465:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1466:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the MDMA peripheral handle */
1467:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(hmdma == NULL)
1468:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1469:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_ERROR;
1470:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1471:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1472:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Get the softawre request mode */
1473:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   request_mode = hmdma->Instance->CTCR & MDMA_CTCR_SWRM;
1474:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1475:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((hmdma->Instance->CCR &  MDMA_CCR_EN) == 0U)
1476:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1477:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* if no Transfer on going (MDMA enable bit not set) return error */
1478:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->ErrorCode = HAL_MDMA_ERROR_NO_XFER;
1479:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1480:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_ERROR;
1481:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1482:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   else if(((hmdma->Instance->CISR &  MDMA_CISR_CRQA) != 0U) || (request_mode == 0U))
1483:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1484:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* if an MDMA ongoing request has not yet end or if request mode is not SW request return error
1485:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->ErrorCode = HAL_MDMA_ERROR_BUSY;
1486:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1487:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_ERROR;
1488:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1489:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   else
1490:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1491:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Set the SW request bit to activate the request on the Channel */
1492:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->Instance->CCR |= MDMA_CCR_SWRQ;
1493:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1494:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return HAL_OK;
1495:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1496:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
1497:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1498:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
1499:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief  Handles MDMA interrupt request.
1500:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  hmdma: pointer to a MDMA_HandleTypeDef structure that contains
1501:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *               the configuration information for the specified MDMA Channel.
1502:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @retval None
1503:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
1504:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** void HAL_MDMA_IRQHandler(MDMA_HandleTypeDef *hmdma)
1505:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** {
1506:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __IO uint32_t count = 0;
1507:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t timeout = SystemCoreClock / 9600U;
1508:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1509:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t generalIntFlag, errorFlag;
1510:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1511:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* General Interrupt Flag management ****************************************/
1512:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   generalIntFlag =  1UL << ((((uint32_t)hmdma->Instance - (uint32_t)(MDMA_Channel0))/HAL_MDMA_CHANN
1513:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((MDMA->GISR0 & generalIntFlag) == 0U)
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 28


1514:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1515:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     return; /* the  General interrupt flag for the current channel is down , nothing to do */
1516:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1517:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1518:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Transfer Error Interrupt management ***************************************/
1519:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((__HAL_MDMA_GET_FLAG(hmdma, MDMA_FLAG_TE) != 0U))
1520:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1521:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     if(__HAL_MDMA_GET_IT_SOURCE(hmdma, MDMA_IT_TE) != 0U)
1522:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
1523:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* Disable the transfer error interrupt */
1524:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       __HAL_MDMA_DISABLE_IT(hmdma, MDMA_IT_TE);
1525:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1526:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* Get the transfer error source flag */
1527:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       errorFlag = hmdma->Instance->CESR;
1528:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1529:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if((errorFlag & MDMA_CESR_TED) == 0U)
1530:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
1531:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Update error code : Read Transfer error  */
1532:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->ErrorCode |= HAL_MDMA_ERROR_READ_XFER;
1533:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
1534:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       else
1535:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
1536:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Update error code : Write Transfer error */
1537:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->ErrorCode |= HAL_MDMA_ERROR_WRITE_XFER;
1538:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
1539:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1540:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if((errorFlag & MDMA_CESR_TEMD) != 0U)
1541:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
1542:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Update error code : Error Mask Data */
1543:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->ErrorCode |= HAL_MDMA_ERROR_MASK_DATA;
1544:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
1545:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1546:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if((errorFlag & MDMA_CESR_TELD) != 0U)
1547:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
1548:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Update error code : Error Linked list */
1549:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->ErrorCode |= HAL_MDMA_ERROR_LINKED_LIST;
1550:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
1551:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1552:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if((errorFlag & MDMA_CESR_ASE) != 0U)
1553:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
1554:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Update error code : Address/Size alignment error */
1555:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->ErrorCode |= HAL_MDMA_ERROR_ALIGNMENT;
1556:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
1557:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1558:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if((errorFlag & MDMA_CESR_BSE) != 0U)
1559:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
1560:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Update error code : Block Size error error */
1561:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->ErrorCode |= HAL_MDMA_ERROR_BLOCK_SIZE;
1562:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
1563:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1564:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* Clear the transfer error flags */
1565:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       __HAL_MDMA_CLEAR_FLAG(hmdma, MDMA_FLAG_TE);
1566:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
1567:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1568:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1569:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Buffer Transfer Complete Interrupt management ******************************/
1570:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((__HAL_MDMA_GET_FLAG(hmdma, MDMA_FLAG_BFTC) != 0U))
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 29


1571:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1572:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     if(__HAL_MDMA_GET_IT_SOURCE(hmdma, MDMA_IT_BFTC) != 0U)
1573:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
1574:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* Clear the buffer transfer complete flag */
1575:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       __HAL_MDMA_CLEAR_FLAG(hmdma, MDMA_FLAG_BFTC);
1576:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1577:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if(hmdma->XferBufferCpltCallback != NULL)
1578:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
1579:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Buffer transfer callback */
1580:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->XferBufferCpltCallback(hmdma);
1581:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
1582:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
1583:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1584:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1585:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Block Transfer Complete Interrupt management ******************************/
1586:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((__HAL_MDMA_GET_FLAG(hmdma, MDMA_FLAG_BT) != 0U))
1587:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1588:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     if(__HAL_MDMA_GET_IT_SOURCE(hmdma, MDMA_IT_BT) != 0U)
1589:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
1590:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* Clear the block transfer complete flag */
1591:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       __HAL_MDMA_CLEAR_FLAG(hmdma, MDMA_FLAG_BT);
1592:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1593:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if(hmdma->XferBlockCpltCallback != NULL)
1594:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
1595:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Block transfer callback */
1596:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->XferBlockCpltCallback(hmdma);
1597:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
1598:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
1599:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1600:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1601:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Repeated Block Transfer Complete Interrupt management ******************************/
1602:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((__HAL_MDMA_GET_FLAG(hmdma, MDMA_FLAG_BRT) != 0U))
1603:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1604:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     if(__HAL_MDMA_GET_IT_SOURCE(hmdma, MDMA_IT_BRT) != 0U)
1605:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
1606:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* Clear the repeat block transfer complete flag */
1607:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       __HAL_MDMA_CLEAR_FLAG(hmdma, MDMA_FLAG_BRT);
1608:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1609:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if(hmdma->XferRepeatBlockCpltCallback != NULL)
1610:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
1611:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Repeated Block transfer callback */
1612:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->XferRepeatBlockCpltCallback(hmdma);
1613:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
1614:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
1615:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1616:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1617:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Channel Transfer Complete Interrupt management ***********************************/
1618:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((__HAL_MDMA_GET_FLAG(hmdma, MDMA_FLAG_CTC) != 0U))
1619:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1620:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     if(__HAL_MDMA_GET_IT_SOURCE(hmdma, MDMA_IT_CTC) != 0U)
1621:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
1622:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* Disable all the transfer interrupts */
1623:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       __HAL_MDMA_DISABLE_IT(hmdma, (MDMA_IT_TE | MDMA_IT_CTC | MDMA_IT_BT | MDMA_IT_BRT | MDMA_IT_B
1624:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1625:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if(HAL_MDMA_STATE_ABORT == hmdma->State)
1626:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
1627:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Process Unlocked */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 30


1628:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         __HAL_UNLOCK(hmdma);
1629:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1630:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Change the DMA state */
1631:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->State = HAL_MDMA_STATE_READY;
1632:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1633:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         if(hmdma->XferAbortCallback != NULL)
1634:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
1635:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           hmdma->XferAbortCallback(hmdma);
1636:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         }
1637:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         return;
1638:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
1639:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1640:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* Clear the Channel Transfer Complete flag */
1641:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       __HAL_MDMA_CLEAR_FLAG(hmdma, MDMA_FLAG_CTC);
1642:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1643:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* Process Unlocked */
1644:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       __HAL_UNLOCK(hmdma);
1645:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1646:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* Change MDMA peripheral state */
1647:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->State = HAL_MDMA_STATE_READY;
1648:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1649:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if(hmdma->XferCpltCallback != NULL)
1650:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
1651:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Channel Transfer Complete callback */
1652:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->XferCpltCallback(hmdma);
1653:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
1654:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
1655:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1656:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1657:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* manage error case */
1658:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(hmdma->ErrorCode != HAL_MDMA_ERROR_NONE)
1659:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1660:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->State = HAL_MDMA_STATE_ABORT;
1661:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1662:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Disable the channel */
1663:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_MDMA_DISABLE(hmdma);
1664:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1665:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     do
1666:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
1667:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       if (++count > timeout)
1668:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
1669:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         break;
1670:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
1671:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
1672:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     while((hmdma->Instance->CCR & MDMA_CCR_EN) != 0U);
1673:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1674:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Process Unlocked */
1675:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     __HAL_UNLOCK(hmdma);
1676:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1677:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     if((hmdma->Instance->CCR & MDMA_CCR_EN) != 0U)
1678:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
1679:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* Change the MDMA state to error if MDMA disable fails */
1680:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->State = HAL_MDMA_STATE_ERROR;
1681:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
1682:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     else
1683:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
1684:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* Change the MDMA state to Ready if MDMA disable success */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 31


1685:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->State = HAL_MDMA_STATE_READY;
1686:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
1687:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1688:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1689:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     if (hmdma->XferErrorCallback != NULL)
1690:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
1691:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       /* Transfer error callback */
1692:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferErrorCallback(hmdma);
1693:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
1694:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1695:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
1696:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1697:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
1698:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @}
1699:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
1700:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1701:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /** @addtogroup MDMA_Exported_Functions_Group4
1702:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****  *
1703:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** @verbatim
1704:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****  ===============================================================================
1705:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                     ##### State and Errors functions #####
1706:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****  ===============================================================================
1707:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     [..]
1708:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     This subsection provides functions allowing to
1709:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       (+) Check the MDMA state
1710:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       (+) Get error code
1711:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1712:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** @endverbatim
1713:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @{
1714:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
1715:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1716:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
1717:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief  Returns the MDMA state.
1718:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  hmdma: pointer to a MDMA_HandleTypeDef structure that contains
1719:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *               the configuration information for the specified MDMA Channel.
1720:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @retval HAL state
1721:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
1722:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** HAL_MDMA_StateTypeDef HAL_MDMA_GetState(MDMA_HandleTypeDef *hmdma)
1723:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** {
1724:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   return hmdma->State;
1725:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
1726:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1727:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
1728:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief  Return the MDMA error code
1729:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  hmdma : pointer to a MDMA_HandleTypeDef structure that contains
1730:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *              the configuration information for the specified MDMA Channel.
1731:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @retval MDMA Error Code
1732:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
1733:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** uint32_t HAL_MDMA_GetError(MDMA_HandleTypeDef *hmdma)
1734:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** {
1735:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   return hmdma->ErrorCode;
1736:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
1737:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1738:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
1739:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @}
1740:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
1741:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 32


1742:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
1743:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @}
1744:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
1745:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1746:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /** @addtogroup MDMA_Private_Functions
1747:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @{
1748:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
1749:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1750:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
1751:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief  Sets the MDMA Transfer parameter.
1752:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  hmdma:       pointer to a MDMA_HandleTypeDef structure that contains
1753:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *                     the configuration information for the specified MDMA Channel.
1754:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  SrcAddress: The source memory Buffer address
1755:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  DstAddress: The destination memory Buffer address
1756:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  BlockDataLength : The length of a block transfer in bytes
1757:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  BlockCount: The number of blocks to be transferred
1758:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @retval HAL status
1759:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
1760:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** static void MDMA_SetConfig(MDMA_HandleTypeDef *hmdma, uint32_t SrcAddress, uint32_t DstAddress, uin
1761:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** {
  28              		.loc 1 1761 1 view -0
  29              		.cfi_startproc
  30              		@ args = 4, pretend = 0, frame = 0
  31              		@ frame_needed = 0, uses_anonymous_args = 0
  32              		@ link register save eliminated.
  33              		.loc 1 1761 1 is_stmt 0 view .LVU1
  34 0000 30B4     		push	{r4, r5}
  35              		.cfi_def_cfa_offset 8
  36              		.cfi_offset 4, -8
  37              		.cfi_offset 5, -4
1762:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t addressMask;
  38              		.loc 1 1762 3 is_stmt 1 view .LVU2
1763:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1764:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Configure the MDMA Channel data length */
1765:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   MODIFY_REG(hmdma->Instance->CBNDTR ,MDMA_CBNDTR_BNDT, (BlockDataLength & MDMA_CBNDTR_BNDT));
  39              		.loc 1 1765 3 view .LVU3
  40 0002 0568     		ldr	r5, [r0]
  41 0004 6C69     		ldr	r4, [r5, #20]
  42 0006 DFF884C0 		ldr	ip, .L7
  43 000a 04EA0C0C 		and	ip, r4, ip
  44 000e C3F31003 		ubfx	r3, r3, #0, #17
  45              	.LVL1:
  46              		.loc 1 1765 3 is_stmt 0 view .LVU4
  47 0012 4CEA0303 		orr	r3, ip, r3
  48 0016 6B61     		str	r3, [r5, #20]
1766:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1767:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Configure the MDMA block repeat count */
1768:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   MODIFY_REG(hmdma->Instance->CBNDTR , MDMA_CBNDTR_BRC , ((BlockCount - 1U) << MDMA_CBNDTR_BRC_Pos)
  49              		.loc 1 1768 3 is_stmt 1 view .LVU5
  50 0018 0568     		ldr	r5, [r0]
  51 001a 6B69     		ldr	r3, [r5, #20]
  52 001c C3F31303 		ubfx	r3, r3, #0, #20
  53 0020 029C     		ldr	r4, [sp, #8]
  54 0022 013C     		subs	r4, r4, #1
  55 0024 43EA0453 		orr	r3, r3, r4, lsl #20
  56 0028 6B61     		str	r3, [r5, #20]
1769:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 33


1770:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Clear all interrupt flags */
1771:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __HAL_MDMA_CLEAR_FLAG(hmdma, MDMA_FLAG_TE | MDMA_FLAG_CTC | MDMA_CISR_BRTIF | MDMA_CISR_BTIF | MD
  57              		.loc 1 1771 3 view .LVU6
  58 002a 0368     		ldr	r3, [r0]
  59 002c 1F24     		movs	r4, #31
  60 002e 5C60     		str	r4, [r3, #4]
1772:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1773:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Configure MDMA Channel destination address */
1774:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CDAR = DstAddress;
  61              		.loc 1 1774 3 view .LVU7
  62              		.loc 1 1774 8 is_stmt 0 view .LVU8
  63 0030 0368     		ldr	r3, [r0]
  64              		.loc 1 1774 25 view .LVU9
  65 0032 DA61     		str	r2, [r3, #28]
1775:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1776:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Configure MDMA Channel Source address */
1777:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CSAR = SrcAddress;
  66              		.loc 1 1777 3 is_stmt 1 view .LVU10
  67              		.loc 1 1777 8 is_stmt 0 view .LVU11
  68 0034 0368     		ldr	r3, [r0]
  69              		.loc 1 1777 25 view .LVU12
  70 0036 9961     		str	r1, [r3, #24]
1778:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1779:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   addressMask = SrcAddress & 0xFF000000U;
  71              		.loc 1 1779 3 is_stmt 1 view .LVU13
  72              		.loc 1 1779 15 is_stmt 0 view .LVU14
  73 0038 01F07F41 		and	r1, r1, #-16777216
  74              	.LVL2:
1780:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((addressMask == 0x20000000U) || (addressMask == 0x00000000U))
  75              		.loc 1 1780 3 is_stmt 1 view .LVU15
  76              		.loc 1 1780 5 is_stmt 0 view .LVU16
  77 003c 0029     		cmp	r1, #0
  78 003e 18BF     		it	ne
  79 0040 B1F1005F 		cmpne	r1, #536870912
  80 0044 15D1     		bne	.L2
1781:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1782:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /*The AHBSbus is used as source (read operation) on channel x */
1783:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->Instance->CTBR |= MDMA_CTBR_SBUS;
  81              		.loc 1 1783 5 is_stmt 1 view .LVU17
  82              		.loc 1 1783 10 is_stmt 0 view .LVU18
  83 0046 0168     		ldr	r1, [r0]
  84              	.LVL3:
  85              		.loc 1 1783 20 view .LVU19
  86 0048 8B6A     		ldr	r3, [r1, #40]
  87              	.LVL4:
  88              		.loc 1 1783 27 view .LVU20
  89 004a 43F48033 		orr	r3, r3, #65536
  90 004e 8B62     		str	r3, [r1, #40]
  91              	.L3:
1784:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1785:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   else
1786:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1787:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /*The AXI bus is used as source (read operation) on channel x */
1788:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->Instance->CTBR &= (~MDMA_CTBR_SBUS);
1789:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1790:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1791:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   addressMask = DstAddress & 0xFF000000U;
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 34


  92              		.loc 1 1791 3 is_stmt 1 view .LVU21
  93              		.loc 1 1791 15 is_stmt 0 view .LVU22
  94 0050 02F07F42 		and	r2, r2, #-16777216
  95              	.LVL5:
1792:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((addressMask == 0x20000000U) || (addressMask == 0x00000000U))
  96              		.loc 1 1792 3 is_stmt 1 view .LVU23
  97              		.loc 1 1792 5 is_stmt 0 view .LVU24
  98 0054 002A     		cmp	r2, #0
  99 0056 18BF     		it	ne
 100 0058 B2F1005F 		cmpne	r2, #536870912
 101 005c 0FD1     		bne	.L4
1793:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1794:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /*The AHB bus is used as destination (write operation) on channel x */
1795:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->Instance->CTBR |= MDMA_CTBR_DBUS;
 102              		.loc 1 1795 5 is_stmt 1 view .LVU25
 103              		.loc 1 1795 10 is_stmt 0 view .LVU26
 104 005e 0268     		ldr	r2, [r0]
 105              	.LVL6:
 106              		.loc 1 1795 20 view .LVU27
 107 0060 936A     		ldr	r3, [r2, #40]
 108              		.loc 1 1795 27 view .LVU28
 109 0062 43F40033 		orr	r3, r3, #131072
 110 0066 9362     		str	r3, [r2, #40]
 111              	.L5:
1796:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1797:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   else
1798:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1799:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /*The AXI bus is used as destination (write operation) on channel x */
1800:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->Instance->CTBR &= (~MDMA_CTBR_DBUS);
1801:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1802:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1803:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Set the linked list register to the first node of the list */
1804:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CLAR = (uint32_t)hmdma->FirstLinkedListNodeAddress;
 112              		.loc 1 1804 3 is_stmt 1 view .LVU29
 113              		.loc 1 1804 42 is_stmt 0 view .LVU30
 114 0068 C26D     		ldr	r2, [r0, #92]
 115              		.loc 1 1804 8 view .LVU31
 116 006a 0368     		ldr	r3, [r0]
 117              		.loc 1 1804 25 view .LVU32
 118 006c 5A62     		str	r2, [r3, #36]
1805:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 119              		.loc 1 1805 1 view .LVU33
 120 006e 30BC     		pop	{r4, r5}
 121              		.cfi_remember_state
 122              		.cfi_restore 5
 123              		.cfi_restore 4
 124              		.cfi_def_cfa_offset 0
 125              	.LVL7:
 126              		.loc 1 1805 1 view .LVU34
 127 0070 7047     		bx	lr
 128              	.LVL8:
 129              	.L2:
 130              		.cfi_restore_state
1788:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 131              		.loc 1 1788 5 is_stmt 1 view .LVU35
1788:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 132              		.loc 1 1788 10 is_stmt 0 view .LVU36
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 35


 133 0072 0168     		ldr	r1, [r0]
 134              	.LVL9:
1788:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 135              		.loc 1 1788 20 view .LVU37
 136 0074 8B6A     		ldr	r3, [r1, #40]
 137              	.LVL10:
1788:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 138              		.loc 1 1788 27 view .LVU38
 139 0076 23F48033 		bic	r3, r3, #65536
 140 007a 8B62     		str	r3, [r1, #40]
1788:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 141              		.loc 1 1788 27 view .LVU39
 142 007c E8E7     		b	.L3
 143              	.LVL11:
 144              	.L4:
1800:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 145              		.loc 1 1800 5 is_stmt 1 view .LVU40
1800:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 146              		.loc 1 1800 10 is_stmt 0 view .LVU41
 147 007e 0268     		ldr	r2, [r0]
 148              	.LVL12:
1800:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 149              		.loc 1 1800 20 view .LVU42
 150 0080 936A     		ldr	r3, [r2, #40]
1800:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 151              		.loc 1 1800 27 view .LVU43
 152 0082 23F40033 		bic	r3, r3, #131072
 153 0086 9362     		str	r3, [r2, #40]
 154 0088 EEE7     		b	.L5
 155              	.L8:
 156 008a 00BF     		.align	2
 157              	.L7:
 158 008c 0000FEFF 		.word	-131072
 159              		.cfi_endproc
 160              	.LFE354:
 162              		.section	.text.MDMA_Init,"ax",%progbits
 163              		.align	1
 164              		.syntax unified
 165              		.thumb
 166              		.thumb_func
 168              	MDMA_Init:
 169              	.LVL13:
 170              	.LFB355:
1806:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1807:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** /**
1808:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @brief  Initializes the MDMA handle according to the specified
1809:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *         parameters in the MDMA_InitTypeDef
1810:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @param  hmdma:       pointer to a MDMA_HandleTypeDef structure that contains
1811:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   *                     the configuration information for the specified MDMA Channel.
1812:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   * @retval None
1813:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   */
1814:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** static void MDMA_Init(MDMA_HandleTypeDef *hmdma)
1815:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** {
 171              		.loc 1 1815 1 is_stmt 1 view -0
 172              		.cfi_startproc
 173              		@ args = 0, pretend = 0, frame = 0
 174              		@ frame_needed = 0, uses_anonymous_args = 0
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 36


 175              		@ link register save eliminated.
1816:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t blockoffset;
 176              		.loc 1 1816 3 view .LVU45
1817:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1818:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Prepare the MDMA Channel configuration */
1819:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CCR = hmdma->Init.Priority  | hmdma->Init.Endianness;
 177              		.loc 1 1819 3 view .LVU46
 178              		.loc 1 1819 37 is_stmt 0 view .LVU47
 179 0000 C368     		ldr	r3, [r0, #12]
 180              		.loc 1 1819 61 view .LVU48
 181 0002 0169     		ldr	r1, [r0, #16]
 182              		.loc 1 1819 8 view .LVU49
 183 0004 0268     		ldr	r2, [r0]
 184              		.loc 1 1819 48 view .LVU50
 185 0006 0B43     		orrs	r3, r3, r1
 186              		.loc 1 1819 24 view .LVU51
 187 0008 D360     		str	r3, [r2, #12]
1820:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1821:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Write new CTCR Register value */
1822:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CTCR =  hmdma->Init.SourceInc      | hmdma->Init.DestinationInc | \
 188              		.loc 1 1822 3 is_stmt 1 view .LVU52
 189              		.loc 1 1822 39 is_stmt 0 view .LVU53
 190 000a 4369     		ldr	r3, [r0, #20]
 191              		.loc 1 1822 68 view .LVU54
 192 000c 8269     		ldr	r2, [r0, #24]
 193              		.loc 1 1822 55 view .LVU55
 194 000e 1343     		orrs	r3, r3, r2
1823:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                            hmdma->Init.SourceDataSize | hmdma->Init.DestDataSize   | \
 195              		.loc 1 1823 39 view .LVU56
 196 0010 C269     		ldr	r2, [r0, #28]
1822:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                            hmdma->Init.SourceDataSize | hmdma->Init.DestDataSize   | \
 197              		.loc 1 1822 84 view .LVU57
 198 0012 1343     		orrs	r3, r3, r2
 199              		.loc 1 1823 68 view .LVU58
 200 0014 026A     		ldr	r2, [r0, #32]
 201              		.loc 1 1823 55 view .LVU59
 202 0016 1343     		orrs	r3, r3, r2
1824:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                            hmdma->Init.DataAlignment  | hmdma->Init.SourceBurst    | \
 203              		.loc 1 1824 39 view .LVU60
 204 0018 426A     		ldr	r2, [r0, #36]
1823:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                            hmdma->Init.SourceDataSize | hmdma->Init.DestDataSize   | \
 205              		.loc 1 1823 84 view .LVU61
 206 001a 1343     		orrs	r3, r3, r2
 207              		.loc 1 1824 68 view .LVU62
 208 001c C26A     		ldr	r2, [r0, #44]
 209              		.loc 1 1824 55 view .LVU63
 210 001e 1343     		orrs	r3, r3, r2
1825:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                            hmdma->Init.DestBurst                                   | \
 211              		.loc 1 1825 39 view .LVU64
 212 0020 026B     		ldr	r2, [r0, #48]
1824:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                            hmdma->Init.DataAlignment  | hmdma->Init.SourceBurst    | \
 213              		.loc 1 1824 84 view .LVU65
 214 0022 1343     		orrs	r3, r3, r2
1826:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                            ((hmdma->Init.BufferTransferLength - 1U) << MDMA_CTCR_TLEN_Pos) | \
 215              		.loc 1 1826 41 view .LVU66
 216 0024 826A     		ldr	r2, [r0, #40]
 217              		.loc 1 1826 63 view .LVU67
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 37


 218 0026 013A     		subs	r2, r2, #1
1825:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                            hmdma->Init.DestBurst                                   | \
 219              		.loc 1 1825 84 view .LVU68
 220 0028 43EA8243 		orr	r3, r3, r2, lsl #18
1827:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                            hmdma->Init.TransferTriggerMode;
 221              		.loc 1 1827 39 view .LVU69
 222 002c 8168     		ldr	r1, [r0, #8]
1822:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                            hmdma->Init.SourceDataSize | hmdma->Init.DestDataSize   | \
 223              		.loc 1 1822 8 view .LVU70
 224 002e 0268     		ldr	r2, [r0]
1826:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                            ((hmdma->Init.BufferTransferLength - 1U) << MDMA_CTCR_TLEN_Pos) | \
 225              		.loc 1 1826 92 view .LVU71
 226 0030 0B43     		orrs	r3, r3, r1
1822:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                            hmdma->Init.SourceDataSize | hmdma->Init.DestDataSize   | \
 227              		.loc 1 1822 25 view .LVU72
 228 0032 1361     		str	r3, [r2, #16]
1828:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1829:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* If SW request set the CTCR register to SW Request Mode */
1830:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(hmdma->Init.Request == MDMA_REQUEST_SW)
 229              		.loc 1 1830 3 is_stmt 1 view .LVU73
 230              		.loc 1 1830 17 is_stmt 0 view .LVU74
 231 0034 4368     		ldr	r3, [r0, #4]
 232              		.loc 1 1830 5 view .LVU75
 233 0036 B3F1804F 		cmp	r3, #1073741824
 234 003a 1BD0     		beq	.L17
 235              	.L10:
1831:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1832:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /*
1833:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     -If the request is done by SW : BWM could be set to 1 or 0.
1834:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     -If the request is done by a peripheral :
1835:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     If mask address not set (0) => BWM must be set to 0
1836:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     If mask address set (different than 0) => BWM could be set to 1 or 0
1837:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     */
1838:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->Instance->CTCR |= (MDMA_CTCR_SWRM | MDMA_CTCR_BWM);
1839:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1840:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1841:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Reset CBNDTR Register */
1842:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CBNDTR = 0;
 236              		.loc 1 1842 3 is_stmt 1 view .LVU76
 237              		.loc 1 1842 8 is_stmt 0 view .LVU77
 238 003c 0368     		ldr	r3, [r0]
 239              		.loc 1 1842 27 view .LVU78
 240 003e 0022     		movs	r2, #0
 241 0040 5A61     		str	r2, [r3, #20]
1843:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1844:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* if block source address offset is negative set the Block Repeat Source address Update Mode to 
1845:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(hmdma->Init.SourceBlockAddressOffset < 0)
 242              		.loc 1 1845 3 is_stmt 1 view .LVU79
 243              		.loc 1 1845 17 is_stmt 0 view .LVU80
 244 0042 436B     		ldr	r3, [r0, #52]
 245              		.loc 1 1845 5 view .LVU81
 246 0044 9342     		cmp	r3, r2
 247 0046 1BDB     		blt	.L18
1846:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1847:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->Instance->CBNDTR |= MDMA_CBNDTR_BRSUM;
1848:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Write new CBRUR Register value : source repeat block offset */
1849:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     blockoffset = (uint32_t)(- hmdma->Init.SourceBlockAddressOffset);
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 38


1850:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->Instance->CBRUR = (blockoffset & 0x0000FFFFU);
1851:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1852:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   else
1853:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1854:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Write new CBRUR Register value : source repeat block offset */
1855:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->Instance->CBRUR = (((uint32_t)hmdma->Init.SourceBlockAddressOffset) & 0x0000FFFFU);
 248              		.loc 1 1855 5 is_stmt 1 view .LVU82
 249              		.loc 1 1855 10 is_stmt 0 view .LVU83
 250 0048 0268     		ldr	r2, [r0]
 251              		.loc 1 1855 80 view .LVU84
 252 004a 9BB2     		uxth	r3, r3
 253              		.loc 1 1855 28 view .LVU85
 254 004c 1362     		str	r3, [r2, #32]
 255              	.L12:
1856:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1857:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1858:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* If block destination address offset is negative set the Block Repeat destination address Updat
1859:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(hmdma->Init.DestBlockAddressOffset < 0)
 256              		.loc 1 1859 3 is_stmt 1 view .LVU86
 257              		.loc 1 1859 17 is_stmt 0 view .LVU87
 258 004e 836B     		ldr	r3, [r0, #56]
 259              		.loc 1 1859 5 view .LVU88
 260 0050 002B     		cmp	r3, #0
 261 0052 20DB     		blt	.L19
1860:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1861:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->Instance->CBNDTR |= MDMA_CBNDTR_BRDUM;
1862:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Write new CBRUR Register value : destination repeat block offset */
1863:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     blockoffset = (uint32_t)(- hmdma->Init.DestBlockAddressOffset);
1864:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->Instance->CBRUR |= ((blockoffset & 0x0000FFFFU) << MDMA_CBRUR_DUV_Pos);
1865:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1866:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   else
1867:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1868:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /*write new CBRUR Register value : destination repeat block offset */
1869:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->Instance->CBRUR |= ((((uint32_t)hmdma->Init.DestBlockAddressOffset) & 0x0000FFFFU) << MD
 262              		.loc 1 1869 5 is_stmt 1 view .LVU89
 263              		.loc 1 1869 10 is_stmt 0 view .LVU90
 264 0054 0168     		ldr	r1, [r0]
 265              		.loc 1 1869 20 view .LVU91
 266 0056 0A6A     		ldr	r2, [r1, #32]
 267              		.loc 1 1869 28 view .LVU92
 268 0058 42EA0343 		orr	r3, r2, r3, lsl #16
 269 005c 0B62     		str	r3, [r1, #32]
 270              	.L14:
1870:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1871:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1872:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* if HW request set the HW request and the requet CleraMask and ClearData MaskData, */
1873:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if(hmdma->Init.Request != MDMA_REQUEST_SW)
 271              		.loc 1 1873 3 is_stmt 1 view .LVU93
 272              		.loc 1 1873 17 is_stmt 0 view .LVU94
 273 005e 4368     		ldr	r3, [r0, #4]
 274              		.loc 1 1873 5 view .LVU95
 275 0060 B3F1804F 		cmp	r3, #1073741824
 276 0064 24D0     		beq	.L15
1874:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1875:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Set the HW request in CTRB register  */
1876:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->Instance->CTBR = hmdma->Init.Request & MDMA_CTBR_TSEL;
 277              		.loc 1 1876 5 is_stmt 1 view .LVU96
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 39


 278              		.loc 1 1876 10 is_stmt 0 view .LVU97
 279 0066 0268     		ldr	r2, [r0]
 280              		.loc 1 1876 49 view .LVU98
 281 0068 DBB2     		uxtb	r3, r3
 282              		.loc 1 1876 27 view .LVU99
 283 006a 9362     		str	r3, [r2, #40]
 284              	.L16:
1877:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1878:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   else /* SW request : reset the CTBR register */
1879:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
1880:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->Instance->CTBR = 0;
1881:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
1882:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
1883:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Write Link Address Register */
1884:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CLAR =  0;
 285              		.loc 1 1884 3 is_stmt 1 view .LVU100
 286              		.loc 1 1884 8 is_stmt 0 view .LVU101
 287 006c 0368     		ldr	r3, [r0]
 288              		.loc 1 1884 25 view .LVU102
 289 006e 0022     		movs	r2, #0
 290 0070 5A62     		str	r2, [r3, #36]
1885:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 291              		.loc 1 1885 1 view .LVU103
 292 0072 7047     		bx	lr
 293              	.L17:
1838:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 294              		.loc 1 1838 5 is_stmt 1 view .LVU104
1838:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 295              		.loc 1 1838 10 is_stmt 0 view .LVU105
 296 0074 0268     		ldr	r2, [r0]
1838:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 297              		.loc 1 1838 20 view .LVU106
 298 0076 1369     		ldr	r3, [r2, #16]
1838:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 299              		.loc 1 1838 27 view .LVU107
 300 0078 43F04043 		orr	r3, r3, #-1073741824
 301 007c 1361     		str	r3, [r2, #16]
 302 007e DDE7     		b	.L10
 303              	.L18:
1847:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Write new CBRUR Register value : source repeat block offset */
 304              		.loc 1 1847 5 is_stmt 1 view .LVU108
1847:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Write new CBRUR Register value : source repeat block offset */
 305              		.loc 1 1847 10 is_stmt 0 view .LVU109
 306 0080 0268     		ldr	r2, [r0]
1847:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Write new CBRUR Register value : source repeat block offset */
 307              		.loc 1 1847 20 view .LVU110
 308 0082 5369     		ldr	r3, [r2, #20]
1847:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Write new CBRUR Register value : source repeat block offset */
 309              		.loc 1 1847 29 view .LVU111
 310 0084 43F48023 		orr	r3, r3, #262144
 311 0088 5361     		str	r3, [r2, #20]
1849:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->Instance->CBRUR = (blockoffset & 0x0000FFFFU);
 312              		.loc 1 1849 5 is_stmt 1 view .LVU112
1849:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->Instance->CBRUR = (blockoffset & 0x0000FFFFU);
 313              		.loc 1 1849 43 is_stmt 0 view .LVU113
 314 008a 436B     		ldr	r3, [r0, #52]
1849:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->Instance->CBRUR = (blockoffset & 0x0000FFFFU);
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 40


 315              		.loc 1 1849 30 view .LVU114
 316 008c 5B42     		rsbs	r3, r3, #0
 317              	.LVL14:
1850:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 318              		.loc 1 1850 5 is_stmt 1 view .LVU115
1850:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 319              		.loc 1 1850 10 is_stmt 0 view .LVU116
 320 008e 0268     		ldr	r2, [r0]
1850:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 321              		.loc 1 1850 43 view .LVU117
 322 0090 9BB2     		uxth	r3, r3
 323              	.LVL15:
1850:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 324              		.loc 1 1850 28 view .LVU118
 325 0092 1362     		str	r3, [r2, #32]
 326              	.LVL16:
1850:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 327              		.loc 1 1850 28 view .LVU119
 328 0094 DBE7     		b	.L12
 329              	.LVL17:
 330              	.L19:
1861:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Write new CBRUR Register value : destination repeat block offset */
 331              		.loc 1 1861 5 is_stmt 1 view .LVU120
1861:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Write new CBRUR Register value : destination repeat block offset */
 332              		.loc 1 1861 10 is_stmt 0 view .LVU121
 333 0096 0268     		ldr	r2, [r0]
1861:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Write new CBRUR Register value : destination repeat block offset */
 334              		.loc 1 1861 20 view .LVU122
 335 0098 5369     		ldr	r3, [r2, #20]
1861:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Write new CBRUR Register value : destination repeat block offset */
 336              		.loc 1 1861 29 view .LVU123
 337 009a 43F40023 		orr	r3, r3, #524288
 338 009e 5361     		str	r3, [r2, #20]
1863:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->Instance->CBRUR |= ((blockoffset & 0x0000FFFFU) << MDMA_CBRUR_DUV_Pos);
 339              		.loc 1 1863 5 is_stmt 1 view .LVU124
1863:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->Instance->CBRUR |= ((blockoffset & 0x0000FFFFU) << MDMA_CBRUR_DUV_Pos);
 340              		.loc 1 1863 43 is_stmt 0 view .LVU125
 341 00a0 836B     		ldr	r3, [r0, #56]
1863:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     hmdma->Instance->CBRUR |= ((blockoffset & 0x0000FFFFU) << MDMA_CBRUR_DUV_Pos);
 342              		.loc 1 1863 30 view .LVU126
 343 00a2 5A42     		rsbs	r2, r3, #0
 344              	.LVL18:
1864:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 345              		.loc 1 1864 5 is_stmt 1 view .LVU127
1864:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 346              		.loc 1 1864 10 is_stmt 0 view .LVU128
 347 00a4 0168     		ldr	r1, [r0]
1864:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 348              		.loc 1 1864 20 view .LVU129
 349 00a6 0B6A     		ldr	r3, [r1, #32]
1864:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 350              		.loc 1 1864 28 view .LVU130
 351 00a8 43EA0243 		orr	r3, r3, r2, lsl #16
 352 00ac 0B62     		str	r3, [r1, #32]
 353 00ae D6E7     		b	.L14
 354              	.LVL19:
 355              	.L15:
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 41


1880:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 356              		.loc 1 1880 5 is_stmt 1 view .LVU131
1880:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 357              		.loc 1 1880 10 is_stmt 0 view .LVU132
 358 00b0 0368     		ldr	r3, [r0]
1880:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 359              		.loc 1 1880 27 view .LVU133
 360 00b2 0022     		movs	r2, #0
 361 00b4 9A62     		str	r2, [r3, #40]
 362 00b6 D9E7     		b	.L16
 363              		.cfi_endproc
 364              	.LFE355:
 366              		.section	.text.HAL_MDMA_Init,"ax",%progbits
 367              		.align	1
 368              		.global	HAL_MDMA_Init
 369              		.syntax unified
 370              		.thumb
 371              		.thumb_func
 373              	HAL_MDMA_Init:
 374              	.LVL20:
 375              	.LFB335:
 219:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t tickstart = HAL_GetTick();
 376              		.loc 1 219 1 is_stmt 1 view -0
 377              		.cfi_startproc
 378              		@ args = 0, pretend = 0, frame = 0
 379              		@ frame_needed = 0, uses_anonymous_args = 0
 219:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t tickstart = HAL_GetTick();
 380              		.loc 1 219 1 is_stmt 0 view .LVU135
 381 0000 38B5     		push	{r3, r4, r5, lr}
 382              		.cfi_def_cfa_offset 16
 383              		.cfi_offset 3, -16
 384              		.cfi_offset 4, -12
 385              		.cfi_offset 5, -8
 386              		.cfi_offset 14, -4
 387 0002 0446     		mov	r4, r0
 220:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 388              		.loc 1 220 3 is_stmt 1 view .LVU136
 220:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 389              		.loc 1 220 24 is_stmt 0 view .LVU137
 390 0004 FFF7FEFF 		bl	HAL_GetTick
 391              	.LVL21:
 223:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 392              		.loc 1 223 3 is_stmt 1 view .LVU138
 223:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 393              		.loc 1 223 5 is_stmt 0 view .LVU139
 394 0008 44B3     		cbz	r4, .L24
 395 000a 0546     		mov	r5, r0
 229:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_PRIORITY(hmdma->Init.Priority));
 396              		.loc 1 229 3 is_stmt 1 view .LVU140
 230:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_ENDIANNESS_MODE(hmdma->Init.Endianness));
 397              		.loc 1 230 3 view .LVU141
 231:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_REQUEST(hmdma->Init.Request));
 398              		.loc 1 231 3 view .LVU142
 232:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_SOURCE_INC(hmdma->Init.SourceInc));
 399              		.loc 1 232 3 view .LVU143
 233:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_DESTINATION_INC(hmdma->Init.DestinationInc));
 400              		.loc 1 233 3 view .LVU144
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 42


 234:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_SOURCE_DATASIZE(hmdma->Init.SourceDataSize));
 401              		.loc 1 234 3 view .LVU145
 235:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_DESTINATION_DATASIZE(hmdma->Init.DestDataSize));
 402              		.loc 1 235 3 view .LVU146
 236:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_DATA_ALIGNMENT(hmdma->Init.DataAlignment));
 403              		.loc 1 236 3 view .LVU147
 237:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_SOURCE_BURST(hmdma->Init.SourceBurst));
 404              		.loc 1 237 3 view .LVU148
 238:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_DESTINATION_BURST(hmdma->Init.DestBurst));
 405              		.loc 1 238 3 view .LVU149
 239:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_BUFFER_TRANSFER_LENGTH(hmdma->Init.BufferTransferLength));
 406              		.loc 1 239 3 view .LVU150
 240:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_TRANSFER_TRIGGER_MODE(hmdma->Init.TransferTriggerMode));
 407              		.loc 1 240 3 view .LVU151
 241:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_BLOCK_ADDR_OFFSET(hmdma->Init.SourceBlockAddressOffset));
 408              		.loc 1 241 3 view .LVU152
 242:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_BLOCK_ADDR_OFFSET(hmdma->Init.DestBlockAddressOffset));
 409              		.loc 1 242 3 view .LVU153
 243:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 410              		.loc 1 243 3 view .LVU154
 247:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 411              		.loc 1 247 3 view .LVU155
 247:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 412              		.loc 1 247 3 view .LVU156
 413 000c 0023     		movs	r3, #0
 414 000e 84F83C30 		strb	r3, [r4, #60]
 247:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 415              		.loc 1 247 3 view .LVU157
 250:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 416              		.loc 1 250 3 view .LVU158
 250:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 417              		.loc 1 250 16 is_stmt 0 view .LVU159
 418 0012 0223     		movs	r3, #2
 419 0014 84F83D30 		strb	r3, [r4, #61]
 253:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 420              		.loc 1 253 3 is_stmt 1 view .LVU160
 421 0018 2268     		ldr	r2, [r4]
 422 001a D368     		ldr	r3, [r2, #12]
 423 001c 23F00103 		bic	r3, r3, #1
 424 0020 D360     		str	r3, [r2, #12]
 256:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 425              		.loc 1 256 3 view .LVU161
 426              	.LVL22:
 427              	.L22:
 256:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 428              		.loc 1 256 46 view .LVU162
 256:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 429              		.loc 1 256 15 is_stmt 0 view .LVU163
 430 0022 2368     		ldr	r3, [r4]
 256:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 431              		.loc 1 256 25 view .LVU164
 432 0024 DB68     		ldr	r3, [r3, #12]
 256:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 433              		.loc 1 256 46 view .LVU165
 434 0026 13F0010F 		tst	r3, #1
 435 002a 0BD0     		beq	.L26
 259:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 43


 436              		.loc 1 259 5 is_stmt 1 view .LVU166
 259:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 437              		.loc 1 259 9 is_stmt 0 view .LVU167
 438 002c FFF7FEFF 		bl	HAL_GetTick
 439              	.LVL23:
 259:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 440              		.loc 1 259 23 discriminator 1 view .LVU168
 441 0030 431B     		subs	r3, r0, r5
 259:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 442              		.loc 1 259 7 discriminator 1 view .LVU169
 443 0032 052B     		cmp	r3, #5
 444 0034 F5D9     		bls	.L22
 262:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 445              		.loc 1 262 7 is_stmt 1 view .LVU170
 262:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 446              		.loc 1 262 24 is_stmt 0 view .LVU171
 447 0036 4023     		movs	r3, #64
 448 0038 A366     		str	r3, [r4, #104]
 265:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 449              		.loc 1 265 7 is_stmt 1 view .LVU172
 265:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 450              		.loc 1 265 20 is_stmt 0 view .LVU173
 451 003a 0323     		movs	r3, #3
 452 003c 84F83D30 		strb	r3, [r4, #61]
 267:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 453              		.loc 1 267 7 is_stmt 1 view .LVU174
 267:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 454              		.loc 1 267 14 is_stmt 0 view .LVU175
 455 0040 0120     		movs	r0, #1
 456 0042 0AE0     		b	.L21
 457              	.L26:
 272:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 458              		.loc 1 272 3 is_stmt 1 view .LVU176
 459 0044 2046     		mov	r0, r4
 460 0046 FFF7FEFF 		bl	MDMA_Init
 461              	.LVL24:
 275:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->LastLinkedListNodeAddress   = 0;
 462              		.loc 1 275 3 view .LVU177
 275:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->LastLinkedListNodeAddress   = 0;
 463              		.loc 1 275 38 is_stmt 0 view .LVU178
 464 004a 0020     		movs	r0, #0
 465 004c E065     		str	r0, [r4, #92]
 276:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->LinkedListNodeCounter  = 0;
 466              		.loc 1 276 3 is_stmt 1 view .LVU179
 276:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->LinkedListNodeCounter  = 0;
 467              		.loc 1 276 38 is_stmt 0 view .LVU180
 468 004e 2066     		str	r0, [r4, #96]
 277:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 469              		.loc 1 277 3 is_stmt 1 view .LVU181
 277:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 470              		.loc 1 277 33 is_stmt 0 view .LVU182
 471 0050 6066     		str	r0, [r4, #100]
 280:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 472              		.loc 1 280 3 is_stmt 1 view .LVU183
 280:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 473              		.loc 1 280 20 is_stmt 0 view .LVU184
 474 0052 A066     		str	r0, [r4, #104]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 44


 283:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 475              		.loc 1 283 3 is_stmt 1 view .LVU185
 283:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 476              		.loc 1 283 16 is_stmt 0 view .LVU186
 477 0054 0123     		movs	r3, #1
 478 0056 84F83D30 		strb	r3, [r4, #61]
 285:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 479              		.loc 1 285 3 is_stmt 1 view .LVU187
 480              	.LVL25:
 481              	.L21:
 286:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 482              		.loc 1 286 1 is_stmt 0 view .LVU188
 483 005a 38BD     		pop	{r3, r4, r5, pc}
 484              	.LVL26:
 485              	.L24:
 225:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 486              		.loc 1 225 12 view .LVU189
 487 005c 0120     		movs	r0, #1
 488              	.LVL27:
 225:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 489              		.loc 1 225 12 view .LVU190
 490 005e FCE7     		b	.L21
 491              		.cfi_endproc
 492              	.LFE335:
 494              		.section	.text.HAL_MDMA_DeInit,"ax",%progbits
 495              		.align	1
 496              		.global	HAL_MDMA_DeInit
 497              		.syntax unified
 498              		.thumb
 499              		.thumb_func
 501              	HAL_MDMA_DeInit:
 502              	.LVL28:
 503              	.LFB336:
 295:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 504              		.loc 1 295 1 is_stmt 1 view -0
 505              		.cfi_startproc
 506              		@ args = 0, pretend = 0, frame = 0
 507              		@ frame_needed = 0, uses_anonymous_args = 0
 508              		@ link register save eliminated.
 298:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 509              		.loc 1 298 3 view .LVU192
 298:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 510              		.loc 1 298 5 is_stmt 0 view .LVU193
 511 0000 0346     		mov	r3, r0
 512 0002 0028     		cmp	r0, #0
 513 0004 25D0     		beq	.L29
 304:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 514              		.loc 1 304 3 is_stmt 1 view .LVU194
 515 0006 0168     		ldr	r1, [r0]
 516 0008 CA68     		ldr	r2, [r1, #12]
 517 000a 22F00102 		bic	r2, r2, #1
 518 000e CA60     		str	r2, [r1, #12]
 307:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CTCR = 0;
 519              		.loc 1 307 3 view .LVU195
 307:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CTCR = 0;
 520              		.loc 1 307 8 is_stmt 0 view .LVU196
 521 0010 0268     		ldr	r2, [r0]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 45


 307:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CTCR = 0;
 522              		.loc 1 307 25 view .LVU197
 523 0012 0020     		movs	r0, #0
 524              	.LVL29:
 307:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CTCR = 0;
 525              		.loc 1 307 25 view .LVU198
 526 0014 D060     		str	r0, [r2, #12]
 308:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CBNDTR = 0;
 527              		.loc 1 308 3 is_stmt 1 view .LVU199
 308:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CBNDTR = 0;
 528              		.loc 1 308 8 is_stmt 0 view .LVU200
 529 0016 1A68     		ldr	r2, [r3]
 308:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CBNDTR = 0;
 530              		.loc 1 308 25 view .LVU201
 531 0018 1061     		str	r0, [r2, #16]
 309:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CSAR = 0;
 532              		.loc 1 309 3 is_stmt 1 view .LVU202
 309:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CSAR = 0;
 533              		.loc 1 309 8 is_stmt 0 view .LVU203
 534 001a 1A68     		ldr	r2, [r3]
 309:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CSAR = 0;
 535              		.loc 1 309 27 view .LVU204
 536 001c 5061     		str	r0, [r2, #20]
 310:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CDAR = 0;
 537              		.loc 1 310 3 is_stmt 1 view .LVU205
 310:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CDAR = 0;
 538              		.loc 1 310 8 is_stmt 0 view .LVU206
 539 001e 1A68     		ldr	r2, [r3]
 310:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CDAR = 0;
 540              		.loc 1 310 25 view .LVU207
 541 0020 9061     		str	r0, [r2, #24]
 311:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CBRUR = 0;
 542              		.loc 1 311 3 is_stmt 1 view .LVU208
 311:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CBRUR = 0;
 543              		.loc 1 311 8 is_stmt 0 view .LVU209
 544 0022 1A68     		ldr	r2, [r3]
 311:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CBRUR = 0;
 545              		.loc 1 311 25 view .LVU210
 546 0024 D061     		str	r0, [r2, #28]
 312:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CLAR = 0;
 547              		.loc 1 312 3 is_stmt 1 view .LVU211
 312:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CLAR = 0;
 548              		.loc 1 312 8 is_stmt 0 view .LVU212
 549 0026 1A68     		ldr	r2, [r3]
 312:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CLAR = 0;
 550              		.loc 1 312 26 view .LVU213
 551 0028 1062     		str	r0, [r2, #32]
 313:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CTBR = 0;
 552              		.loc 1 313 3 is_stmt 1 view .LVU214
 313:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CTBR = 0;
 553              		.loc 1 313 8 is_stmt 0 view .LVU215
 554 002a 1A68     		ldr	r2, [r3]
 313:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CTBR = 0;
 555              		.loc 1 313 25 view .LVU216
 556 002c 5062     		str	r0, [r2, #36]
 314:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CMAR = 0;
 557              		.loc 1 314 3 is_stmt 1 view .LVU217
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 46


 314:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CMAR = 0;
 558              		.loc 1 314 8 is_stmt 0 view .LVU218
 559 002e 1A68     		ldr	r2, [r3]
 314:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CMAR = 0;
 560              		.loc 1 314 25 view .LVU219
 561 0030 9062     		str	r0, [r2, #40]
 315:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CMDR = 0;
 562              		.loc 1 315 3 is_stmt 1 view .LVU220
 315:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CMDR = 0;
 563              		.loc 1 315 8 is_stmt 0 view .LVU221
 564 0032 1A68     		ldr	r2, [r3]
 315:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->Instance->CMDR = 0;
 565              		.loc 1 315 25 view .LVU222
 566 0034 1063     		str	r0, [r2, #48]
 316:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 567              		.loc 1 316 3 is_stmt 1 view .LVU223
 316:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 568              		.loc 1 316 8 is_stmt 0 view .LVU224
 569 0036 1A68     		ldr	r2, [r3]
 316:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 570              		.loc 1 316 25 view .LVU225
 571 0038 5063     		str	r0, [r2, #52]
 319:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 572              		.loc 1 319 3 is_stmt 1 view .LVU226
 573 003a 1A68     		ldr	r2, [r3]
 574 003c 1F21     		movs	r1, #31
 575 003e 5160     		str	r1, [r2, #4]
 322:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->LastLinkedListNodeAddress   = 0;
 576              		.loc 1 322 3 view .LVU227
 322:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->LastLinkedListNodeAddress   = 0;
 577              		.loc 1 322 38 is_stmt 0 view .LVU228
 578 0040 D865     		str	r0, [r3, #92]
 323:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->LinkedListNodeCounter  = 0;
 579              		.loc 1 323 3 is_stmt 1 view .LVU229
 323:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   hmdma->LinkedListNodeCounter  = 0;
 580              		.loc 1 323 38 is_stmt 0 view .LVU230
 581 0042 1866     		str	r0, [r3, #96]
 324:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 582              		.loc 1 324 3 is_stmt 1 view .LVU231
 324:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 583              		.loc 1 324 33 is_stmt 0 view .LVU232
 584 0044 5866     		str	r0, [r3, #100]
 327:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 585              		.loc 1 327 3 is_stmt 1 view .LVU233
 327:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 586              		.loc 1 327 20 is_stmt 0 view .LVU234
 587 0046 9866     		str	r0, [r3, #104]
 330:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 588              		.loc 1 330 3 is_stmt 1 view .LVU235
 330:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 589              		.loc 1 330 16 is_stmt 0 view .LVU236
 590 0048 83F83D00 		strb	r0, [r3, #61]
 333:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 591              		.loc 1 333 3 is_stmt 1 view .LVU237
 333:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 592              		.loc 1 333 3 view .LVU238
 593 004c 83F83C00 		strb	r0, [r3, #60]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 47


 333:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 594              		.loc 1 333 3 view .LVU239
 335:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 595              		.loc 1 335 3 view .LVU240
 335:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 596              		.loc 1 335 10 is_stmt 0 view .LVU241
 597 0050 7047     		bx	lr
 598              	.LVL30:
 599              	.L29:
 300:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 600              		.loc 1 300 12 view .LVU242
 601 0052 0120     		movs	r0, #1
 602              	.LVL31:
 336:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 603              		.loc 1 336 1 view .LVU243
 604 0054 7047     		bx	lr
 605              		.cfi_endproc
 606              	.LFE336:
 608              		.section	.text.HAL_MDMA_ConfigPostRequestMask,"ax",%progbits
 609              		.align	1
 610              		.global	HAL_MDMA_ConfigPostRequestMask
 611              		.syntax unified
 612              		.thumb
 613              		.thumb_func
 615              	HAL_MDMA_ConfigPostRequestMask:
 616              	.LVL32:
 617              	.LFB337:
 348:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   HAL_StatusTypeDef  status = HAL_OK;
 618              		.loc 1 348 1 is_stmt 1 view -0
 619              		.cfi_startproc
 620              		@ args = 0, pretend = 0, frame = 0
 621              		@ frame_needed = 0, uses_anonymous_args = 0
 622              		@ link register save eliminated.
 349:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 623              		.loc 1 349 3 view .LVU245
 352:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 624              		.loc 1 352 3 view .LVU246
 352:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 625              		.loc 1 352 5 is_stmt 0 view .LVU247
 626 0000 78B3     		cbz	r0, .L34
 627 0002 0346     		mov	r3, r0
 358:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 628              		.loc 1 358 3 is_stmt 1 view .LVU248
 358:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 629              		.loc 1 358 3 view .LVU249
 630 0004 90F83C00 		ldrb	r0, [r0, #60]	@ zero_extendqisi2
 631              	.LVL33:
 358:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 632              		.loc 1 358 3 is_stmt 0 view .LVU250
 633 0008 0128     		cmp	r0, #1
 634 000a 2CD0     		beq	.L35
 358:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 635              		.loc 1 358 3 is_stmt 1 discriminator 2 view .LVU251
 636 000c 0120     		movs	r0, #1
 637 000e 83F83C00 		strb	r0, [r3, #60]
 358:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 638              		.loc 1 358 3 view .LVU252
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 48


 360:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 639              		.loc 1 360 3 view .LVU253
 360:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 640              		.loc 1 360 35 is_stmt 0 view .LVU254
 641 0012 93F83DC0 		ldrb	ip, [r3, #61]	@ zero_extendqisi2
 642 0016 5FFA8CF0 		uxtb	r0, ip
 360:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 643              		.loc 1 360 5 view .LVU255
 644 001a BCF1010F 		cmp	ip, #1
 645 001e 04D0     		beq	.L42
 393:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 646              		.loc 1 393 12 view .LVU256
 647 0020 0120     		movs	r0, #1
 648              	.LVL34:
 396:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 649              		.loc 1 396 3 is_stmt 1 view .LVU257
 396:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 650              		.loc 1 396 3 view .LVU258
 651 0022 0022     		movs	r2, #0
 652              	.LVL35:
 396:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 653              		.loc 1 396 3 is_stmt 0 view .LVU259
 654 0024 83F83C20 		strb	r2, [r3, #60]
 396:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 655              		.loc 1 396 3 is_stmt 1 view .LVU260
 398:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 656              		.loc 1 398 3 view .LVU261
 399:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 657              		.loc 1 399 1 is_stmt 0 view .LVU262
 658 0028 7047     		bx	lr
 659              	.LVL36:
 660              	.L42:
 348:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   HAL_StatusTypeDef  status = HAL_OK;
 661              		.loc 1 348 1 view .LVU263
 662 002a 30B4     		push	{r4, r5}
 663              		.cfi_def_cfa_offset 8
 664              		.cfi_offset 4, -8
 665              		.cfi_offset 5, -4
 363:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 666              		.loc 1 363 5 is_stmt 1 view .LVU264
 363:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 667              		.loc 1 363 14 is_stmt 0 view .LVU265
 668 002c 1C68     		ldr	r4, [r3]
 363:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 669              		.loc 1 363 24 view .LVU266
 670 002e 2569     		ldr	r5, [r4, #16]
 363:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 671              		.loc 1 363 7 view .LVU267
 672 0030 15F0804F 		tst	r5, #1073741824
 673 0034 09D1     		bne	.L32
 366:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->Instance->CMDR = MaskData;
 674              		.loc 1 366 7 is_stmt 1 view .LVU268
 366:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->Instance->CMDR = MaskData;
 675              		.loc 1 366 29 is_stmt 0 view .LVU269
 676 0036 2163     		str	r1, [r4, #48]
 367:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 677              		.loc 1 367 7 is_stmt 1 view .LVU270
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 49


 367:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 678              		.loc 1 367 12 is_stmt 0 view .LVU271
 679 0038 1868     		ldr	r0, [r3]
 367:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 680              		.loc 1 367 29 view .LVU272
 681 003a 4263     		str	r2, [r0, #52]
 375:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 682              		.loc 1 375 7 is_stmt 1 view .LVU273
 375:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 683              		.loc 1 375 9 is_stmt 0 view .LVU274
 684 003c 51B9     		cbnz	r1, .L33
 377:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 685              		.loc 1 377 9 is_stmt 1 view .LVU275
 377:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 686              		.loc 1 377 14 is_stmt 0 view .LVU276
 687 003e 1968     		ldr	r1, [r3]
 688              	.LVL37:
 377:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 689              		.loc 1 377 24 view .LVU277
 690 0040 0A69     		ldr	r2, [r1, #16]
 691              	.LVL38:
 377:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 692              		.loc 1 377 31 view .LVU278
 693 0042 22F00042 		bic	r2, r2, #-2147483648
 694 0046 0A61     		str	r2, [r1, #16]
 695              	.LVL39:
 349:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 696              		.loc 1 349 22 view .LVU279
 697 0048 0020     		movs	r0, #0
 698              	.L32:
 699              	.LVL40:
 396:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 700              		.loc 1 396 3 is_stmt 1 view .LVU280
 396:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 701              		.loc 1 396 3 view .LVU281
 702 004a 0022     		movs	r2, #0
 703 004c 83F83C20 		strb	r2, [r3, #60]
 396:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 704              		.loc 1 396 3 view .LVU282
 398:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 705              		.loc 1 398 3 view .LVU283
 399:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 706              		.loc 1 399 1 is_stmt 0 view .LVU284
 707 0050 30BC     		pop	{r4, r5}
 708              		.cfi_remember_state
 709              		.cfi_restore 5
 710              		.cfi_restore 4
 711              		.cfi_def_cfa_offset 0
 712 0052 7047     		bx	lr
 713              	.LVL41:
 714              	.L33:
 715              		.cfi_restore_state
 381:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 716              		.loc 1 381 9 is_stmt 1 view .LVU285
 381:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 717              		.loc 1 381 14 is_stmt 0 view .LVU286
 718 0054 1968     		ldr	r1, [r3]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 50


 719              	.LVL42:
 381:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 720              		.loc 1 381 24 view .LVU287
 721 0056 0A69     		ldr	r2, [r1, #16]
 722              	.LVL43:
 381:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 723              		.loc 1 381 31 view .LVU288
 724 0058 42F00042 		orr	r2, r2, #-2147483648
 725 005c 0A61     		str	r2, [r1, #16]
 726              	.LVL44:
 349:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 727              		.loc 1 349 22 view .LVU289
 728 005e 0020     		movs	r0, #0
 729 0060 F3E7     		b	.L32
 730              	.LVL45:
 731              	.L34:
 732              		.cfi_def_cfa_offset 0
 733              		.cfi_restore 4
 734              		.cfi_restore 5
 354:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 735              		.loc 1 354 12 view .LVU290
 736 0062 0120     		movs	r0, #1
 737              	.LVL46:
 354:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 738              		.loc 1 354 12 view .LVU291
 739 0064 7047     		bx	lr
 740              	.LVL47:
 741              	.L35:
 358:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 742              		.loc 1 358 3 discriminator 1 view .LVU292
 743 0066 0220     		movs	r0, #2
 744 0068 7047     		bx	lr
 745              		.cfi_endproc
 746              	.LFE337:
 748              		.section	.text.HAL_MDMA_RegisterCallback,"ax",%progbits
 749              		.align	1
 750              		.global	HAL_MDMA_RegisterCallback
 751              		.syntax unified
 752              		.thumb
 753              		.thumb_func
 755              	HAL_MDMA_RegisterCallback:
 756              	.LVL48:
 757              	.LFB338:
 410:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   HAL_StatusTypeDef status = HAL_OK;
 758              		.loc 1 410 1 is_stmt 1 view -0
 759              		.cfi_startproc
 760              		@ args = 0, pretend = 0, frame = 0
 761              		@ frame_needed = 0, uses_anonymous_args = 0
 762              		@ link register save eliminated.
 411:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 763              		.loc 1 411 3 view .LVU294
 414:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 764              		.loc 1 414 3 view .LVU295
 414:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 765              		.loc 1 414 5 is_stmt 0 view .LVU296
 766 0000 0346     		mov	r3, r0
 767 0002 50B3     		cbz	r0, .L53
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 51


 420:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 768              		.loc 1 420 3 is_stmt 1 view .LVU297
 420:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 769              		.loc 1 420 3 view .LVU298
 770 0004 90F83C00 		ldrb	r0, [r0, #60]	@ zero_extendqisi2
 771              	.LVL49:
 420:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 772              		.loc 1 420 3 is_stmt 0 view .LVU299
 773 0008 0128     		cmp	r0, #1
 774 000a 28D0     		beq	.L54
 420:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 775              		.loc 1 420 3 is_stmt 1 discriminator 2 view .LVU300
 776 000c 0120     		movs	r0, #1
 777 000e 83F83C00 		strb	r0, [r3, #60]
 420:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 778              		.loc 1 420 3 view .LVU301
 422:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 779              		.loc 1 422 3 view .LVU302
 422:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 780              		.loc 1 422 35 is_stmt 0 view .LVU303
 781 0012 93F83D00 		ldrb	r0, [r3, #61]	@ zero_extendqisi2
 422:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 782              		.loc 1 422 5 view .LVU304
 783 0016 0128     		cmp	r0, #1
 784 0018 04D0     		beq	.L57
 457:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 785              		.loc 1 457 12 view .LVU305
 786 001a 0120     		movs	r0, #1
 787              	.L45:
 788              	.LVL50:
 461:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 789              		.loc 1 461 3 is_stmt 1 view .LVU306
 461:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 790              		.loc 1 461 3 view .LVU307
 791 001c 0022     		movs	r2, #0
 792              	.LVL51:
 461:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 793              		.loc 1 461 3 is_stmt 0 view .LVU308
 794 001e 83F83C20 		strb	r2, [r3, #60]
 461:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 795              		.loc 1 461 3 is_stmt 1 view .LVU309
 463:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 796              		.loc 1 463 3 view .LVU310
 463:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 797              		.loc 1 463 10 is_stmt 0 view .LVU311
 798 0022 7047     		bx	lr
 799              	.LVL52:
 800              	.L57:
 424:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 801              		.loc 1 424 5 is_stmt 1 view .LVU312
 802 0024 0529     		cmp	r1, #5
 803 0026 16D8     		bhi	.L56
 804 0028 DFE801F0 		tbb	[pc, r1]
 805              	.L47:
 806 002c 03       		.byte	(.L52-.L47)/2
 807 002d 06       		.byte	(.L51-.L47)/2
 808 002e 09       		.byte	(.L50-.L47)/2
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 52


 809 002f 0C       		.byte	(.L49-.L47)/2
 810 0030 0F       		.byte	(.L48-.L47)/2
 811 0031 12       		.byte	(.L46-.L47)/2
 812              		.p2align 1
 813              	.L52:
 427:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 814              		.loc 1 427 7 view .LVU313
 427:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 815              		.loc 1 427 31 is_stmt 0 view .LVU314
 816 0032 5A64     		str	r2, [r3, #68]
 428:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 817              		.loc 1 428 7 is_stmt 1 view .LVU315
 411:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 818              		.loc 1 411 21 is_stmt 0 view .LVU316
 819 0034 0846     		mov	r0, r1
 428:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 820              		.loc 1 428 7 view .LVU317
 821 0036 F1E7     		b	.L45
 822              	.L51:
 431:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 823              		.loc 1 431 7 is_stmt 1 view .LVU318
 431:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 824              		.loc 1 431 37 is_stmt 0 view .LVU319
 825 0038 9A64     		str	r2, [r3, #72]
 432:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 826              		.loc 1 432 7 is_stmt 1 view .LVU320
 411:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 827              		.loc 1 411 21 is_stmt 0 view .LVU321
 828 003a 0020     		movs	r0, #0
 432:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 829              		.loc 1 432 7 view .LVU322
 830 003c EEE7     		b	.L45
 831              	.L50:
 435:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 832              		.loc 1 435 7 is_stmt 1 view .LVU323
 435:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 833              		.loc 1 435 36 is_stmt 0 view .LVU324
 834 003e DA64     		str	r2, [r3, #76]
 436:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 835              		.loc 1 436 7 is_stmt 1 view .LVU325
 411:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 836              		.loc 1 411 21 is_stmt 0 view .LVU326
 837 0040 0020     		movs	r0, #0
 436:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 838              		.loc 1 436 7 view .LVU327
 839 0042 EBE7     		b	.L45
 840              	.L49:
 439:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 841              		.loc 1 439 7 is_stmt 1 view .LVU328
 439:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 842              		.loc 1 439 42 is_stmt 0 view .LVU329
 843 0044 1A65     		str	r2, [r3, #80]
 440:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 844              		.loc 1 440 7 is_stmt 1 view .LVU330
 411:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 845              		.loc 1 411 21 is_stmt 0 view .LVU331
 846 0046 0020     		movs	r0, #0
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 53


 440:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 847              		.loc 1 440 7 view .LVU332
 848 0048 E8E7     		b	.L45
 849              	.L48:
 443:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 850              		.loc 1 443 7 is_stmt 1 view .LVU333
 443:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 851              		.loc 1 443 32 is_stmt 0 view .LVU334
 852 004a 5A65     		str	r2, [r3, #84]
 444:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 853              		.loc 1 444 7 is_stmt 1 view .LVU335
 411:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 854              		.loc 1 411 21 is_stmt 0 view .LVU336
 855 004c 0020     		movs	r0, #0
 444:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 856              		.loc 1 444 7 view .LVU337
 857 004e E5E7     		b	.L45
 858              	.L46:
 447:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 859              		.loc 1 447 7 is_stmt 1 view .LVU338
 447:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 860              		.loc 1 447 32 is_stmt 0 view .LVU339
 861 0050 9A65     		str	r2, [r3, #88]
 448:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 862              		.loc 1 448 7 is_stmt 1 view .LVU340
 411:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 863              		.loc 1 411 21 is_stmt 0 view .LVU341
 864 0052 0020     		movs	r0, #0
 448:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 865              		.loc 1 448 7 view .LVU342
 866 0054 E2E7     		b	.L45
 867              	.L56:
 424:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 868              		.loc 1 424 5 view .LVU343
 869 0056 0020     		movs	r0, #0
 870 0058 E0E7     		b	.L45
 871              	.LVL53:
 872              	.L53:
 416:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 873              		.loc 1 416 12 view .LVU344
 874 005a 0120     		movs	r0, #1
 875              	.LVL54:
 416:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 876              		.loc 1 416 12 view .LVU345
 877 005c 7047     		bx	lr
 878              	.L54:
 420:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 879              		.loc 1 420 3 discriminator 1 view .LVU346
 880 005e 0220     		movs	r0, #2
 464:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 881              		.loc 1 464 1 view .LVU347
 882 0060 7047     		bx	lr
 883              		.cfi_endproc
 884              	.LFE338:
 886              		.section	.text.HAL_MDMA_UnRegisterCallback,"ax",%progbits
 887              		.align	1
 888              		.global	HAL_MDMA_UnRegisterCallback
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 54


 889              		.syntax unified
 890              		.thumb
 891              		.thumb_func
 893              	HAL_MDMA_UnRegisterCallback:
 894              	.LVL55:
 895              	.LFB339:
 475:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   HAL_StatusTypeDef status = HAL_OK;
 896              		.loc 1 475 1 is_stmt 1 view -0
 897              		.cfi_startproc
 898              		@ args = 0, pretend = 0, frame = 0
 899              		@ frame_needed = 0, uses_anonymous_args = 0
 900              		@ link register save eliminated.
 476:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 901              		.loc 1 476 3 view .LVU349
 479:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 902              		.loc 1 479 3 view .LVU350
 479:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 903              		.loc 1 479 5 is_stmt 0 view .LVU351
 904 0000 0346     		mov	r3, r0
 905 0002 0028     		cmp	r0, #0
 906 0004 33D0     		beq	.L69
 485:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 907              		.loc 1 485 3 is_stmt 1 view .LVU352
 485:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 908              		.loc 1 485 3 view .LVU353
 909 0006 90F83C20 		ldrb	r2, [r0, #60]	@ zero_extendqisi2
 910 000a 012A     		cmp	r2, #1
 911 000c 31D0     		beq	.L70
 485:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 912              		.loc 1 485 3 discriminator 2 view .LVU354
 913 000e 0122     		movs	r2, #1
 914 0010 80F83C20 		strb	r2, [r0, #60]
 485:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 915              		.loc 1 485 3 view .LVU355
 487:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 916              		.loc 1 487 3 view .LVU356
 487:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 917              		.loc 1 487 35 is_stmt 0 view .LVU357
 918 0014 90F83D20 		ldrb	r2, [r0, #61]	@ zero_extendqisi2
 919 0018 D0B2     		uxtb	r0, r2
 920              	.LVL56:
 487:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 921              		.loc 1 487 5 view .LVU358
 922 001a 012A     		cmp	r2, #1
 923 001c 04D0     		beq	.L73
 531:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 924              		.loc 1 531 12 view .LVU359
 925 001e 0120     		movs	r0, #1
 926              	.L60:
 927              	.LVL57:
 535:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 928              		.loc 1 535 3 is_stmt 1 view .LVU360
 535:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 929              		.loc 1 535 3 view .LVU361
 930 0020 0022     		movs	r2, #0
 931 0022 83F83C20 		strb	r2, [r3, #60]
 535:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 55


 932              		.loc 1 535 3 view .LVU362
 537:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 933              		.loc 1 537 3 view .LVU363
 537:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 934              		.loc 1 537 10 is_stmt 0 view .LVU364
 935 0026 7047     		bx	lr
 936              	.LVL58:
 937              	.L73:
 489:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 938              		.loc 1 489 5 is_stmt 1 view .LVU365
 939 0028 0629     		cmp	r1, #6
 940 002a F9D8     		bhi	.L60
 941 002c DFE801F0 		tbb	[pc, r1]
 942              	.L62:
 943 0030 04       		.byte	(.L68-.L62)/2
 944 0031 08       		.byte	(.L67-.L62)/2
 945 0032 0B       		.byte	(.L66-.L62)/2
 946 0033 0E       		.byte	(.L65-.L62)/2
 947 0034 11       		.byte	(.L64-.L62)/2
 948 0035 14       		.byte	(.L63-.L62)/2
 949 0036 17       		.byte	(.L61-.L62)/2
 950 0037 00       		.p2align 1
 951              	.L68:
 492:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 952              		.loc 1 492 7 view .LVU366
 492:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 953              		.loc 1 492 31 is_stmt 0 view .LVU367
 954 0038 0022     		movs	r2, #0
 955 003a 5A64     		str	r2, [r3, #68]
 493:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 956              		.loc 1 493 7 is_stmt 1 view .LVU368
 476:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 957              		.loc 1 476 21 is_stmt 0 view .LVU369
 958 003c 0846     		mov	r0, r1
 493:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 959              		.loc 1 493 7 view .LVU370
 960 003e EFE7     		b	.L60
 961              	.L67:
 496:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 962              		.loc 1 496 7 is_stmt 1 view .LVU371
 496:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 963              		.loc 1 496 37 is_stmt 0 view .LVU372
 964 0040 0020     		movs	r0, #0
 965 0042 9864     		str	r0, [r3, #72]
 497:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 966              		.loc 1 497 7 is_stmt 1 view .LVU373
 967 0044 ECE7     		b	.L60
 968              	.L66:
 500:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 969              		.loc 1 500 7 view .LVU374
 500:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 970              		.loc 1 500 36 is_stmt 0 view .LVU375
 971 0046 0020     		movs	r0, #0
 972 0048 D864     		str	r0, [r3, #76]
 501:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 973              		.loc 1 501 7 is_stmt 1 view .LVU376
 974 004a E9E7     		b	.L60
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 56


 975              	.L65:
 504:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 976              		.loc 1 504 7 view .LVU377
 504:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 977              		.loc 1 504 42 is_stmt 0 view .LVU378
 978 004c 0020     		movs	r0, #0
 979 004e 1865     		str	r0, [r3, #80]
 505:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 980              		.loc 1 505 7 is_stmt 1 view .LVU379
 981 0050 E6E7     		b	.L60
 982              	.L64:
 508:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 983              		.loc 1 508 7 view .LVU380
 508:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 984              		.loc 1 508 32 is_stmt 0 view .LVU381
 985 0052 0020     		movs	r0, #0
 986 0054 5865     		str	r0, [r3, #84]
 509:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 987              		.loc 1 509 7 is_stmt 1 view .LVU382
 988 0056 E3E7     		b	.L60
 989              	.L63:
 512:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 990              		.loc 1 512 7 view .LVU383
 512:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 991              		.loc 1 512 32 is_stmt 0 view .LVU384
 992 0058 0020     		movs	r0, #0
 993 005a 9865     		str	r0, [r3, #88]
 513:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 994              		.loc 1 513 7 is_stmt 1 view .LVU385
 995 005c E0E7     		b	.L60
 996              	.L61:
 516:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferBufferCpltCallback = NULL;
 997              		.loc 1 516 7 view .LVU386
 516:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferBufferCpltCallback = NULL;
 998              		.loc 1 516 31 is_stmt 0 view .LVU387
 999 005e 0020     		movs	r0, #0
 1000 0060 5864     		str	r0, [r3, #68]
 517:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferBlockCpltCallback = NULL;
 1001              		.loc 1 517 7 is_stmt 1 view .LVU388
 517:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferBlockCpltCallback = NULL;
 1002              		.loc 1 517 37 is_stmt 0 view .LVU389
 1003 0062 9864     		str	r0, [r3, #72]
 518:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferRepeatBlockCpltCallback = NULL;
 1004              		.loc 1 518 7 is_stmt 1 view .LVU390
 518:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferRepeatBlockCpltCallback = NULL;
 1005              		.loc 1 518 36 is_stmt 0 view .LVU391
 1006 0064 D864     		str	r0, [r3, #76]
 519:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferErrorCallback = NULL;
 1007              		.loc 1 519 7 is_stmt 1 view .LVU392
 519:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferErrorCallback = NULL;
 1008              		.loc 1 519 42 is_stmt 0 view .LVU393
 1009 0066 1865     		str	r0, [r3, #80]
 520:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferAbortCallback = NULL;
 1010              		.loc 1 520 7 is_stmt 1 view .LVU394
 520:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       hmdma->XferAbortCallback = NULL;
 1011              		.loc 1 520 32 is_stmt 0 view .LVU395
 1012 0068 5865     		str	r0, [r3, #84]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 57


 521:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 1013              		.loc 1 521 7 is_stmt 1 view .LVU396
 521:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       break;
 1014              		.loc 1 521 32 is_stmt 0 view .LVU397
 1015 006a 9865     		str	r0, [r3, #88]
 522:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1016              		.loc 1 522 7 is_stmt 1 view .LVU398
 1017 006c D8E7     		b	.L60
 1018              	.LVL59:
 1019              	.L69:
 481:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1020              		.loc 1 481 12 is_stmt 0 view .LVU399
 1021 006e 0120     		movs	r0, #1
 1022              	.LVL60:
 481:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1023              		.loc 1 481 12 view .LVU400
 1024 0070 7047     		bx	lr
 1025              	.LVL61:
 1026              	.L70:
 485:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1027              		.loc 1 485 3 discriminator 1 view .LVU401
 1028 0072 0220     		movs	r0, #2
 1029              	.LVL62:
 538:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1030              		.loc 1 538 1 view .LVU402
 1031 0074 7047     		bx	lr
 1032              		.cfi_endproc
 1033              	.LFE339:
 1035              		.section	.text.HAL_MDMA_LinkedList_CreateNode,"ax",%progbits
 1036              		.align	1
 1037              		.global	HAL_MDMA_LinkedList_CreateNode
 1038              		.syntax unified
 1039              		.thumb
 1040              		.thumb_func
 1042              	HAL_MDMA_LinkedList_CreateNode:
 1043              	.LVL63:
 1044              	.LFB340:
 569:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t addressMask;
 1045              		.loc 1 569 1 is_stmt 1 view -0
 1046              		.cfi_startproc
 1047              		@ args = 0, pretend = 0, frame = 0
 1048              		@ frame_needed = 0, uses_anonymous_args = 0
 1049              		@ link register save eliminated.
 570:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t blockoffset;
 1050              		.loc 1 570 3 view .LVU404
 571:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1051              		.loc 1 571 3 view .LVU405
 574:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1052              		.loc 1 574 3 view .LVU406
 574:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1053              		.loc 1 574 5 is_stmt 0 view .LVU407
 1054 0000 0029     		cmp	r1, #0
 1055 0002 18BF     		it	ne
 1056 0004 0028     		cmpne	r0, #0
 1057 0006 7CD0     		beq	.L85
 580:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_ENDIANNESS_MODE(pNodeConfig->Init.Endianness));
 1058              		.loc 1 580 3 is_stmt 1 view .LVU408
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 58


 581:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_REQUEST(pNodeConfig->Init.Request));
 1059              		.loc 1 581 3 view .LVU409
 582:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_SOURCE_INC(pNodeConfig->Init.SourceInc));
 1060              		.loc 1 582 3 view .LVU410
 583:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_DESTINATION_INC(pNodeConfig->Init.DestinationInc));
 1061              		.loc 1 583 3 view .LVU411
 584:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_SOURCE_DATASIZE(pNodeConfig->Init.SourceDataSize));
 1062              		.loc 1 584 3 view .LVU412
 585:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_DESTINATION_DATASIZE(pNodeConfig->Init.DestDataSize));
 1063              		.loc 1 585 3 view .LVU413
 586:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_DATA_ALIGNMENT(pNodeConfig->Init.DataAlignment));
 1064              		.loc 1 586 3 view .LVU414
 587:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_SOURCE_BURST(pNodeConfig->Init.SourceBurst));
 1065              		.loc 1 587 3 view .LVU415
 588:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_DESTINATION_BURST(pNodeConfig->Init.DestBurst));
 1066              		.loc 1 588 3 view .LVU416
 589:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_BUFFER_TRANSFER_LENGTH(pNodeConfig->Init.BufferTransferLength));
 1067              		.loc 1 589 3 view .LVU417
 590:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_TRANSFER_TRIGGER_MODE(pNodeConfig->Init.TransferTriggerMode));
 1068              		.loc 1 590 3 view .LVU418
 591:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_BLOCK_ADDR_OFFSET(pNodeConfig->Init.SourceBlockAddressOffset));
 1069              		.loc 1 591 3 view .LVU419
 592:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_BLOCK_ADDR_OFFSET(pNodeConfig->Init.DestBlockAddressOffset));
 1070              		.loc 1 592 3 view .LVU420
 593:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1071              		.loc 1 593 3 view .LVU421
 595:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_BLOCK_COUNT(pNodeConfig->BlockCount));
 1072              		.loc 1 595 3 view .LVU422
 596:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1073              		.loc 1 596 3 view .LVU423
 600:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1074              		.loc 1 600 3 view .LVU424
 600:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1075              		.loc 1 600 15 is_stmt 0 view .LVU425
 1076 0008 0023     		movs	r3, #0
 1077 000a 4361     		str	r3, [r0, #20]
 603:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   pNode->CMAR   = 0;
 1078              		.loc 1 603 3 is_stmt 1 view .LVU426
 603:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   pNode->CMAR   = 0;
 1079              		.loc 1 603 17 is_stmt 0 view .LVU427
 1080 000c 8361     		str	r3, [r0, #24]
 604:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   pNode->CMDR   = 0;
 1081              		.loc 1 604 3 is_stmt 1 view .LVU428
 604:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   pNode->CMDR   = 0;
 1082              		.loc 1 604 17 is_stmt 0 view .LVU429
 1083 000e 0362     		str	r3, [r0, #32]
 605:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   pNode->Reserved = 0;
 1084              		.loc 1 605 3 is_stmt 1 view .LVU430
 605:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   pNode->Reserved = 0;
 1085              		.loc 1 605 17 is_stmt 0 view .LVU431
 1086 0010 4362     		str	r3, [r0, #36]
 606:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1087              		.loc 1 606 3 is_stmt 1 view .LVU432
 606:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1088              		.loc 1 606 19 is_stmt 0 view .LVU433
 1089 0012 C361     		str	r3, [r0, #28]
 609:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNodeConfig->Init.SourceDataSize | pNodeConfig->Init.DestDataSize           | \
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 59


 1090              		.loc 1 609 3 is_stmt 1 view .LVU434
 609:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNodeConfig->Init.SourceDataSize | pNodeConfig->Init.DestDataSize           | \
 1091              		.loc 1 609 35 is_stmt 0 view .LVU435
 1092 0014 0B69     		ldr	r3, [r1, #16]
 609:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNodeConfig->Init.SourceDataSize | pNodeConfig->Init.DestDataSize           | \
 1093              		.loc 1 609 65 view .LVU436
 1094 0016 4A69     		ldr	r2, [r1, #20]
 609:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNodeConfig->Init.SourceDataSize | pNodeConfig->Init.DestDataSize           | \
 1095              		.loc 1 609 46 view .LVU437
 1096 0018 1343     		orrs	r3, r3, r2
 610:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       pNodeConfig->Init.DataAlignment| pNodeConfig->Init.SourceBurst            | \
 1097              		.loc 1 610 22 view .LVU438
 1098 001a 8A69     		ldr	r2, [r1, #24]
 609:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNodeConfig->Init.SourceDataSize | pNodeConfig->Init.DestDataSize           | \
 1099              		.loc 1 609 81 view .LVU439
 1100 001c 1343     		orrs	r3, r3, r2
 610:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       pNodeConfig->Init.DataAlignment| pNodeConfig->Init.SourceBurst            | \
 1101              		.loc 1 610 57 view .LVU440
 1102 001e CA69     		ldr	r2, [r1, #28]
 610:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       pNodeConfig->Init.DataAlignment| pNodeConfig->Init.SourceBurst            | \
 1103              		.loc 1 610 38 view .LVU441
 1104 0020 1343     		orrs	r3, r3, r2
 611:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         pNodeConfig->Init.DestBurst                                             | \
 1105              		.loc 1 611 24 view .LVU442
 1106 0022 0A6A     		ldr	r2, [r1, #32]
 610:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       pNodeConfig->Init.DataAlignment| pNodeConfig->Init.SourceBurst            | \
 1107              		.loc 1 610 81 view .LVU443
 1108 0024 1343     		orrs	r3, r3, r2
 611:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         pNodeConfig->Init.DestBurst                                             | \
 1109              		.loc 1 611 57 view .LVU444
 1110 0026 8A6A     		ldr	r2, [r1, #40]
 611:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         pNodeConfig->Init.DestBurst                                             | \
 1111              		.loc 1 611 38 view .LVU445
 1112 0028 1343     		orrs	r3, r3, r2
 612:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           ((pNodeConfig->Init.BufferTransferLength - 1U) << MDMA_CTCR_TLEN_Pos) | \
 1113              		.loc 1 612 26 view .LVU446
 1114 002a CA6A     		ldr	r2, [r1, #44]
 611:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         pNodeConfig->Init.DestBurst                                             | \
 1115              		.loc 1 611 81 view .LVU447
 1116 002c 1343     		orrs	r3, r3, r2
 613:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             pNodeConfig->Init.TransferTriggerMode;
 1117              		.loc 1 613 30 view .LVU448
 1118 002e 4A6A     		ldr	r2, [r1, #36]
 613:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             pNodeConfig->Init.TransferTriggerMode;
 1119              		.loc 1 613 52 view .LVU449
 1120 0030 013A     		subs	r2, r2, #1
 612:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           ((pNodeConfig->Init.BufferTransferLength - 1U) << MDMA_CTCR_TLEN_Pos) | \
 1121              		.loc 1 612 81 view .LVU450
 1122 0032 43EA8243 		orr	r3, r3, r2, lsl #18
 614:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1123              		.loc 1 614 30 view .LVU451
 1124 0036 4A68     		ldr	r2, [r1, #4]
 613:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             pNodeConfig->Init.TransferTriggerMode;
 1125              		.loc 1 613 81 view .LVU452
 1126 0038 1343     		orrs	r3, r3, r2
 609:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNodeConfig->Init.SourceDataSize | pNodeConfig->Init.DestDataSize           | \
 1127              		.loc 1 609 15 view .LVU453
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 60


 1128 003a 0360     		str	r3, [r0]
 617:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1129              		.loc 1 617 3 is_stmt 1 view .LVU454
 617:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1130              		.loc 1 617 23 is_stmt 0 view .LVU455
 1131 003c 0B68     		ldr	r3, [r1]
 617:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1132              		.loc 1 617 5 view .LVU456
 1133 003e B3F1804F 		cmp	r3, #1073741824
 1134 0042 45D0     		beq	.L87
 1135              	.L76:
 628:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1136              		.loc 1 628 3 is_stmt 1 view .LVU457
 628:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1137              		.loc 1 628 24 is_stmt 0 view .LVU458
 1138 0044 0B68     		ldr	r3, [r1]
 628:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1139              		.loc 1 628 5 view .LVU459
 1140 0046 B3F1804F 		cmp	r3, #1073741824
 1141 004a 01D0     		beq	.L77
 628:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1142              		.loc 1 628 68 discriminator 1 view .LVU460
 1143 004c 8B6C     		ldr	r3, [r1, #72]
 628:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1144              		.loc 1 628 53 discriminator 1 view .LVU461
 1145 004e 1BB1     		cbz	r3, .L78
 1146              	.L77:
 630:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1147              		.loc 1 630 5 is_stmt 1 view .LVU462
 630:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1148              		.loc 1 630 10 is_stmt 0 view .LVU463
 1149 0050 0368     		ldr	r3, [r0]
 630:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1150              		.loc 1 630 17 view .LVU464
 1151 0052 43F00043 		orr	r3, r3, #-2147483648
 1152 0056 0360     		str	r3, [r0]
 1153              	.L78:
 634:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1154              		.loc 1 634 3 is_stmt 1 view .LVU465
 634:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1155              		.loc 1 634 32 is_stmt 0 view .LVU466
 1156 0058 4B6C     		ldr	r3, [r1, #68]
 634:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1157              		.loc 1 634 45 view .LVU467
 1158 005a 013B     		subs	r3, r3, #1
 634:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1159              		.loc 1 634 75 view .LVU468
 1160 005c 1B05     		lsls	r3, r3, #20
 634:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1161              		.loc 1 634 17 view .LVU469
 1162 005e 4360     		str	r3, [r0, #4]
 637:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1163              		.loc 1 637 3 is_stmt 1 view .LVU470
 637:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1164              		.loc 1 637 23 is_stmt 0 view .LVU471
 1165 0060 0B6B     		ldr	r3, [r1, #48]
 637:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 61


 1166              		.loc 1 637 5 view .LVU472
 1167 0062 002B     		cmp	r3, #0
 1168 0064 39DB     		blt	.L88
 647:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1169              		.loc 1 647 5 is_stmt 1 view .LVU473
 647:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1170              		.loc 1 647 77 is_stmt 0 view .LVU474
 1171 0066 9BB2     		uxth	r3, r3
 647:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1172              		.loc 1 647 18 view .LVU475
 1173 0068 0361     		str	r3, [r0, #16]
 1174              	.L80:
 651:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1175              		.loc 1 651 3 is_stmt 1 view .LVU476
 651:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1176              		.loc 1 651 23 is_stmt 0 view .LVU477
 1177 006a 4B6B     		ldr	r3, [r1, #52]
 651:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1178              		.loc 1 651 5 view .LVU478
 1179 006c 002B     		cmp	r3, #0
 1180 006e 3DDB     		blt	.L89
 661:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1181              		.loc 1 661 5 is_stmt 1 view .LVU479
 661:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1182              		.loc 1 661 10 is_stmt 0 view .LVU480
 1183 0070 0269     		ldr	r2, [r0, #16]
 661:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1184              		.loc 1 661 18 view .LVU481
 1185 0072 42EA0343 		orr	r3, r2, r3, lsl #16
 1186 0076 0361     		str	r3, [r0, #16]
 1187              	.L82:
 665:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1188              		.loc 1 665 3 is_stmt 1 view .LVU482
 665:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1189              		.loc 1 665 8 is_stmt 0 view .LVU483
 1190 0078 4368     		ldr	r3, [r0, #4]
 665:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1191              		.loc 1 665 32 view .LVU484
 1192 007a 0A6C     		ldr	r2, [r1, #64]
 665:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1193              		.loc 1 665 17 view .LVU485
 1194 007c 1343     		orrs	r3, r3, r2
 1195 007e 4360     		str	r3, [r0, #4]
 668:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1196              		.loc 1 668 3 is_stmt 1 view .LVU486
 668:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1197              		.loc 1 668 28 is_stmt 0 view .LVU487
 1198 0080 CB6B     		ldr	r3, [r1, #60]
 668:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1199              		.loc 1 668 15 view .LVU488
 1200 0082 C360     		str	r3, [r0, #12]
 671:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1201              		.loc 1 671 3 is_stmt 1 view .LVU489
 671:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1202              		.loc 1 671 28 is_stmt 0 view .LVU490
 1203 0084 8B6B     		ldr	r3, [r1, #56]
 671:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 62


 1204              		.loc 1 671 15 view .LVU491
 1205 0086 8360     		str	r3, [r0, #8]
 674:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1206              		.loc 1 674 3 is_stmt 1 view .LVU492
 674:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1207              		.loc 1 674 23 is_stmt 0 view .LVU493
 1208 0088 0B68     		ldr	r3, [r1]
 674:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1209              		.loc 1 674 5 view .LVU494
 1210 008a B3F1804F 		cmp	r3, #1073741824
 1211 008e 05D0     		beq	.L83
 677:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Set the HW request clear Mask and Data */
 1212              		.loc 1 677 5 is_stmt 1 view .LVU495
 677:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Set the HW request clear Mask and Data */
 1213              		.loc 1 677 45 is_stmt 0 view .LVU496
 1214 0090 DBB2     		uxtb	r3, r3
 677:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /* Set the HW request clear Mask and Data */
 1215              		.loc 1 677 17 view .LVU497
 1216 0092 8361     		str	r3, [r0, #24]
 679:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNode->CMDR = pNodeConfig->PostRequestMaskData;
 1217              		.loc 1 679 5 is_stmt 1 view .LVU498
 679:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNode->CMDR = pNodeConfig->PostRequestMaskData;
 1218              		.loc 1 679 30 is_stmt 0 view .LVU499
 1219 0094 8B6C     		ldr	r3, [r1, #72]
 679:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNode->CMDR = pNodeConfig->PostRequestMaskData;
 1220              		.loc 1 679 17 view .LVU500
 1221 0096 0362     		str	r3, [r0, #32]
 680:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1222              		.loc 1 680 5 is_stmt 1 view .LVU501
 680:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1223              		.loc 1 680 30 is_stmt 0 view .LVU502
 1224 0098 CB6C     		ldr	r3, [r1, #76]
 680:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1225              		.loc 1 680 17 view .LVU503
 1226 009a 4362     		str	r3, [r0, #36]
 1227              	.L83:
 683:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((addressMask == 0x20000000U) || (addressMask == 0x00000000U))
 1228              		.loc 1 683 3 is_stmt 1 view .LVU504
 683:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((addressMask == 0x20000000U) || (addressMask == 0x00000000U))
 1229              		.loc 1 683 28 is_stmt 0 view .LVU505
 1230 009c 8B6B     		ldr	r3, [r1, #56]
 683:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((addressMask == 0x20000000U) || (addressMask == 0x00000000U))
 1231              		.loc 1 683 15 view .LVU506
 1232 009e 03F07F43 		and	r3, r3, #-16777216
 1233              	.LVL64:
 684:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1234              		.loc 1 684 3 is_stmt 1 view .LVU507
 684:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1235              		.loc 1 684 5 is_stmt 0 view .LVU508
 1236 00a2 002B     		cmp	r3, #0
 1237 00a4 18BF     		it	ne
 1238 00a6 B3F1005F 		cmpne	r3, #536870912
 1239 00aa 03D1     		bne	.L84
 687:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1240              		.loc 1 687 5 is_stmt 1 view .LVU509
 687:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1241              		.loc 1 687 10 is_stmt 0 view .LVU510
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 63


 1242 00ac 8369     		ldr	r3, [r0, #24]
 1243              	.LVL65:
 687:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1244              		.loc 1 687 17 view .LVU511
 1245 00ae 43F48033 		orr	r3, r3, #65536
 1246 00b2 8361     		str	r3, [r0, #24]
 1247              	.LVL66:
 1248              	.L84:
 690:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((addressMask == 0x20000000U) || (addressMask == 0x00000000U))
 1249              		.loc 1 690 3 is_stmt 1 view .LVU512
 690:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((addressMask == 0x20000000U) || (addressMask == 0x00000000U))
 1250              		.loc 1 690 28 is_stmt 0 view .LVU513
 1251 00b4 CB6B     		ldr	r3, [r1, #60]
 690:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((addressMask == 0x20000000U) || (addressMask == 0x00000000U))
 1252              		.loc 1 690 15 view .LVU514
 1253 00b6 03F07F43 		and	r3, r3, #-16777216
 1254              	.LVL67:
 691:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1255              		.loc 1 691 3 is_stmt 1 view .LVU515
 691:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1256              		.loc 1 691 5 is_stmt 0 view .LVU516
 1257 00ba 002B     		cmp	r3, #0
 1258 00bc 18BF     		it	ne
 1259 00be B3F1005F 		cmpne	r3, #536870912
 1260 00c2 20D1     		bne	.L86
 694:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1261              		.loc 1 694 5 is_stmt 1 view .LVU517
 694:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1262              		.loc 1 694 10 is_stmt 0 view .LVU518
 1263 00c4 8369     		ldr	r3, [r0, #24]
 1264              	.LVL68:
 694:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1265              		.loc 1 694 17 view .LVU519
 1266 00c6 43F40033 		orr	r3, r3, #131072
 1267 00ca 8361     		str	r3, [r0, #24]
 1268              	.LVL69:
 697:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 1269              		.loc 1 697 10 view .LVU520
 1270 00cc 0020     		movs	r0, #0
 1271              	.LVL70:
 697:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 1272              		.loc 1 697 10 view .LVU521
 1273 00ce 7047     		bx	lr
 1274              	.LVL71:
 1275              	.L87:
 619:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1276              		.loc 1 619 5 is_stmt 1 view .LVU522
 619:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1277              		.loc 1 619 10 is_stmt 0 view .LVU523
 1278 00d0 0368     		ldr	r3, [r0]
 619:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1279              		.loc 1 619 17 view .LVU524
 1280 00d2 43F08043 		orr	r3, r3, #1073741824
 1281 00d6 0360     		str	r3, [r0]
 1282 00d8 B4E7     		b	.L76
 1283              	.L88:
 639:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /*write new CBRUR Register value : source repeat block offset */
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 64


 1284              		.loc 1 639 5 is_stmt 1 view .LVU525
 639:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /*write new CBRUR Register value : source repeat block offset */
 1285              		.loc 1 639 10 is_stmt 0 view .LVU526
 1286 00da 4368     		ldr	r3, [r0, #4]
 639:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /*write new CBRUR Register value : source repeat block offset */
 1287              		.loc 1 639 19 view .LVU527
 1288 00dc 43F48023 		orr	r3, r3, #262144
 1289 00e0 4360     		str	r3, [r0, #4]
 641:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNode->CBRUR = blockoffset & 0x0000FFFFU;
 1290              		.loc 1 641 5 is_stmt 1 view .LVU528
 641:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNode->CBRUR = blockoffset & 0x0000FFFFU;
 1291              		.loc 1 641 49 is_stmt 0 view .LVU529
 1292 00e2 0B6B     		ldr	r3, [r1, #48]
 641:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNode->CBRUR = blockoffset & 0x0000FFFFU;
 1293              		.loc 1 641 30 view .LVU530
 1294 00e4 5B42     		rsbs	r3, r3, #0
 1295              	.LVL72:
 642:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1296              		.loc 1 642 5 is_stmt 1 view .LVU531
 642:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1297              		.loc 1 642 32 is_stmt 0 view .LVU532
 1298 00e6 9BB2     		uxth	r3, r3
 1299              	.LVL73:
 642:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1300              		.loc 1 642 18 view .LVU533
 1301 00e8 0361     		str	r3, [r0, #16]
 1302              	.LVL74:
 642:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1303              		.loc 1 642 18 view .LVU534
 1304 00ea BEE7     		b	.L80
 1305              	.LVL75:
 1306              	.L89:
 653:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /*write new CBRUR Register value : destination repeat block offset */
 1307              		.loc 1 653 5 is_stmt 1 view .LVU535
 653:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /*write new CBRUR Register value : destination repeat block offset */
 1308              		.loc 1 653 10 is_stmt 0 view .LVU536
 1309 00ec 4368     		ldr	r3, [r0, #4]
 653:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     /*write new CBRUR Register value : destination repeat block offset */
 1310              		.loc 1 653 19 view .LVU537
 1311 00ee 43F40023 		orr	r3, r3, #524288
 1312 00f2 4360     		str	r3, [r0, #4]
 655:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNode->CBRUR |= ((blockoffset & 0x0000FFFFU) << MDMA_CBRUR_DUV_Pos);
 1313              		.loc 1 655 5 is_stmt 1 view .LVU538
 655:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNode->CBRUR |= ((blockoffset & 0x0000FFFFU) << MDMA_CBRUR_DUV_Pos);
 1314              		.loc 1 655 49 is_stmt 0 view .LVU539
 1315 00f4 4B6B     		ldr	r3, [r1, #52]
 655:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     pNode->CBRUR |= ((blockoffset & 0x0000FFFFU) << MDMA_CBRUR_DUV_Pos);
 1316              		.loc 1 655 30 view .LVU540
 1317 00f6 5A42     		rsbs	r2, r3, #0
 1318              	.LVL76:
 656:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1319              		.loc 1 656 5 is_stmt 1 view .LVU541
 656:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1320              		.loc 1 656 10 is_stmt 0 view .LVU542
 1321 00f8 0369     		ldr	r3, [r0, #16]
 656:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1322              		.loc 1 656 18 view .LVU543
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 65


 1323 00fa 43EA0243 		orr	r3, r3, r2, lsl #16
 1324 00fe 0361     		str	r3, [r0, #16]
 1325 0100 BAE7     		b	.L82
 1326              	.LVL77:
 1327              	.L85:
 576:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1328              		.loc 1 576 12 view .LVU544
 1329 0102 0120     		movs	r0, #1
 1330              	.LVL78:
 576:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1331              		.loc 1 576 12 view .LVU545
 1332 0104 7047     		bx	lr
 1333              	.LVL79:
 1334              	.L86:
 697:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 1335              		.loc 1 697 10 view .LVU546
 1336 0106 0020     		movs	r0, #0
 1337              	.LVL80:
 698:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1338              		.loc 1 698 1 view .LVU547
 1339 0108 7047     		bx	lr
 1340              		.cfi_endproc
 1341              	.LFE340:
 1343              		.section	.text.HAL_MDMA_LinkedList_AddNode,"ax",%progbits
 1344              		.align	1
 1345              		.global	HAL_MDMA_LinkedList_AddNode
 1346              		.syntax unified
 1347              		.thumb
 1348              		.thumb_func
 1350              	HAL_MDMA_LinkedList_AddNode:
 1351              	.LVL81:
 1352              	.LFB341:
 712:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   MDMA_LinkNodeTypeDef *pNode;
 1353              		.loc 1 712 1 is_stmt 1 view -0
 1354              		.cfi_startproc
 1355              		@ args = 0, pretend = 0, frame = 0
 1356              		@ frame_needed = 0, uses_anonymous_args = 0
 1357              		@ link register save eliminated.
 713:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t counter = 0, nodeInserted = 0;
 1358              		.loc 1 713 3 view .LVU549
 714:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   HAL_StatusTypeDef hal_status = HAL_OK;
 1359              		.loc 1 714 3 view .LVU550
 715:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1360              		.loc 1 715 3 view .LVU551
 718:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1361              		.loc 1 718 3 view .LVU552
 718:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1362              		.loc 1 718 5 is_stmt 0 view .LVU553
 1363 0000 0029     		cmp	r1, #0
 1364 0002 18BF     		it	ne
 1365 0004 0028     		cmpne	r0, #0
 1366 0006 68D0     		beq	.L105
 1367 0008 0346     		mov	r3, r0
 724:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1368              		.loc 1 724 3 is_stmt 1 view .LVU554
 724:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1369              		.loc 1 724 3 view .LVU555
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 66


 1370 000a 90F83C00 		ldrb	r0, [r0, #60]	@ zero_extendqisi2
 1371              	.LVL82:
 724:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1372              		.loc 1 724 3 is_stmt 0 view .LVU556
 1373 000e 0128     		cmp	r0, #1
 1374 0010 65D0     		beq	.L106
 712:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   MDMA_LinkNodeTypeDef *pNode;
 1375              		.loc 1 712 1 view .LVU557
 1376 0012 F0B4     		push	{r4, r5, r6, r7}
 1377              		.cfi_def_cfa_offset 16
 1378              		.cfi_offset 4, -16
 1379              		.cfi_offset 5, -12
 1380              		.cfi_offset 6, -8
 1381              		.cfi_offset 7, -4
 724:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1382              		.loc 1 724 3 is_stmt 1 discriminator 2 view .LVU558
 1383 0014 0120     		movs	r0, #1
 1384 0016 83F83C00 		strb	r0, [r3, #60]
 724:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1385              		.loc 1 724 3 view .LVU559
 726:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1386              		.loc 1 726 3 view .LVU560
 726:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1387              		.loc 1 726 35 is_stmt 0 view .LVU561
 1388 001a 93F83D40 		ldrb	r4, [r3, #61]	@ zero_extendqisi2
 1389 001e E0B2     		uxtb	r0, r4
 726:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1390              		.loc 1 726 5 view .LVU562
 1391 0020 012C     		cmp	r4, #1
 1392 0022 05D0     		beq	.L115
 828:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1393              		.loc 1 828 5 is_stmt 1 view .LVU563
 828:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1394              		.loc 1 828 5 view .LVU564
 1395 0024 0022     		movs	r2, #0
 1396              	.LVL83:
 828:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1397              		.loc 1 828 5 is_stmt 0 view .LVU565
 1398 0026 83F83C20 		strb	r2, [r3, #60]
 828:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1399              		.loc 1 828 5 is_stmt 1 view .LVU566
 831:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1400              		.loc 1 831 5 view .LVU567
 831:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1401              		.loc 1 831 12 is_stmt 0 view .LVU568
 1402 002a 0220     		movs	r0, #2
 1403              	.LVL84:
 1404              	.L91:
 833:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1405              		.loc 1 833 1 view .LVU569
 1406 002c F0BC     		pop	{r4, r5, r6, r7}
 1407              		.cfi_remember_state
 1408              		.cfi_restore 7
 1409              		.cfi_restore 6
 1410              		.cfi_restore 5
 1411              		.cfi_restore 4
 1412              		.cfi_def_cfa_offset 0
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 67


 1413 002e 7047     		bx	lr
 1414              	.LVL85:
 1415              	.L115:
 1416              		.cfi_restore_state
 729:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1417              		.loc 1 729 5 is_stmt 1 view .LVU570
 729:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1418              		.loc 1 729 18 is_stmt 0 view .LVU571
 1419 0030 0224     		movs	r4, #2
 1420 0032 83F83D40 		strb	r4, [r3, #61]
 732:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 1421              		.loc 1 732 5 is_stmt 1 view .LVU572
 732:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 1422              		.loc 1 732 23 is_stmt 0 view .LVU573
 1423 0036 DF6D     		ldr	r7, [r3, #92]
 732:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 1424              		.loc 1 732 7 view .LVU574
 1425 0038 2FB1     		cbz	r7, .L116
 756:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 1426              		.loc 1 756 10 is_stmt 1 view .LVU575
 756:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 1427              		.loc 1 756 12 is_stmt 0 view .LVU576
 1428 003a 8F42     		cmp	r7, r1
 1429 003c 46D0     		beq	.L94
 759:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       while((counter < hmdma->LinkedListNodeCounter) && (hal_status == HAL_OK))
 1430              		.loc 1 759 13 view .LVU577
 1431 003e 3C46     		mov	r4, r7
 715:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1432              		.loc 1 715 21 view .LVU578
 1433 0040 0026     		movs	r6, #0
 714:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   HAL_StatusTypeDef hal_status = HAL_OK;
 1434              		.loc 1 714 12 view .LVU579
 1435 0042 B446     		mov	ip, r6
 1436 0044 0DE0     		b	.L95
 1437              	.L116:
 734:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 1438              		.loc 1 734 7 is_stmt 1 view .LVU580
 734:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 1439              		.loc 1 734 9 is_stmt 0 view .LVU581
 1440 0046 002A     		cmp	r2, #0
 1441 0048 40D1     		bne	.L94
 739:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Set the MDMA handle First linked List node*/
 1442              		.loc 1 739 9 is_stmt 1 view .LVU582
 739:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Set the MDMA handle First linked List node*/
 1443              		.loc 1 739 14 is_stmt 0 view .LVU583
 1444 004a 1A68     		ldr	r2, [r3]
 1445              	.LVL86:
 739:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Set the MDMA handle First linked List node*/
 1446              		.loc 1 739 31 view .LVU584
 1447 004c 5162     		str	r1, [r2, #36]
 741:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1448              		.loc 1 741 9 is_stmt 1 view .LVU585
 741:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1449              		.loc 1 741 43 is_stmt 0 view .LVU586
 1450 004e D965     		str	r1, [r3, #92]
 744:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1451              		.loc 1 744 9 is_stmt 1 view .LVU587
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 68


 744:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1452              		.loc 1 744 24 is_stmt 0 view .LVU588
 1453 0050 0020     		movs	r0, #0
 1454 0052 4861     		str	r0, [r1, #20]
 747:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1455              		.loc 1 747 9 is_stmt 1 view .LVU589
 747:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1456              		.loc 1 747 42 is_stmt 0 view .LVU590
 1457 0054 1966     		str	r1, [r3, #96]
 749:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 1458              		.loc 1 749 9 is_stmt 1 view .LVU591
 749:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 1459              		.loc 1 749 38 is_stmt 0 view .LVU592
 1460 0056 0122     		movs	r2, #1
 1461 0058 5A66     		str	r2, [r3, #100]
 1462 005a 37E0     		b	.L94
 1463              	.LVL87:
 1464              	.L96:
 766:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         counter++;
 1465              		.loc 1 766 9 is_stmt 1 view .LVU593
 766:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         counter++;
 1466              		.loc 1 766 46 is_stmt 0 view .LVU594
 1467 005c 6469     		ldr	r4, [r4, #20]
 1468              	.LVL88:
 767:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 1469              		.loc 1 767 9 is_stmt 1 view .LVU595
 767:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 1470              		.loc 1 767 16 is_stmt 0 view .LVU596
 1471 005e 0CF1010C 		add	ip, ip, #1
 1472              	.LVL89:
 1473              	.L95:
 760:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 1474              		.loc 1 760 54 is_stmt 1 view .LVU597
 760:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 1475              		.loc 1 760 29 is_stmt 0 view .LVU598
 1476 0062 5D6E     		ldr	r5, [r3, #100]
 760:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 1477              		.loc 1 760 54 view .LVU599
 1478 0064 6545     		cmp	r5, ip
 1479 0066 05D9     		bls	.L97
 760:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 1480              		.loc 1 760 54 discriminator 1 view .LVU600
 1481 0068 26B9     		cbnz	r6, .L97
 762:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
 1482              		.loc 1 762 9 is_stmt 1 view .LVU601
 762:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
 1483              		.loc 1 762 17 is_stmt 0 view .LVU602
 1484 006a 6569     		ldr	r5, [r4, #20]
 762:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
 1485              		.loc 1 762 11 view .LVU603
 1486 006c 8D42     		cmp	r5, r1
 1487 006e F5D1     		bne	.L96
 764:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         }
 1488              		.loc 1 764 22 view .LVU604
 1489 0070 0646     		mov	r6, r0
 1490              	.LVL90:
 764:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         }
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 69


 1491              		.loc 1 764 22 view .LVU605
 1492 0072 F3E7     		b	.L96
 1493              	.LVL91:
 1494              	.L97:
 770:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 1495              		.loc 1 770 7 is_stmt 1 view .LVU606
 770:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 1496              		.loc 1 770 9 is_stmt 0 view .LVU607
 1497 0074 4EBB     		cbnz	r6, .L109
 773:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
 1498              		.loc 1 773 9 is_stmt 1 view .LVU608
 773:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
 1499              		.loc 1 773 31 is_stmt 0 view .LVU609
 1500 0076 1C6E     		ldr	r4, [r3, #96]
 1501              	.LVL92:
 773:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
 1502              		.loc 1 773 11 view .LVU610
 1503 0078 9442     		cmp	r4, r2
 1504 007a 04D0     		beq	.L99
 773:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
 1505              		.loc 1 773 60 discriminator 1 view .LVU611
 1506 007c 1AB1     		cbz	r2, .L99
 714:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   HAL_StatusTypeDef hal_status = HAL_OK;
 1507              		.loc 1 714 25 view .LVU612
 1508 007e 4FF0000C 		mov	ip, #0
 1509              	.LVL93:
 787:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           while((counter < hmdma->LinkedListNodeCounter) && (nodeInserted == 0U))
 1510              		.loc 1 787 19 view .LVU613
 1511 0082 6446     		mov	r4, ip
 1512 0084 11E0     		b	.L100
 1513              	.LVL94:
 1514              	.L99:
 776:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           hmdma->LastLinkedListNodeAddress->CLAR = (uint32_t)pNewNode;
 1515              		.loc 1 776 11 is_stmt 1 view .LVU614
 776:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           hmdma->LastLinkedListNodeAddress->CLAR = (uint32_t)pNewNode;
 1516              		.loc 1 776 60 is_stmt 0 view .LVU615
 1517 0086 6269     		ldr	r2, [r4, #20]
 1518              	.LVL95:
 776:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           hmdma->LastLinkedListNodeAddress->CLAR = (uint32_t)pNewNode;
 1519              		.loc 1 776 26 view .LVU616
 1520 0088 4A61     		str	r2, [r1, #20]
 777:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           /* Update the Handle last node address */
 1521              		.loc 1 777 11 is_stmt 1 view .LVU617
 777:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           /* Update the Handle last node address */
 1522              		.loc 1 777 16 is_stmt 0 view .LVU618
 1523 008a 1A6E     		ldr	r2, [r3, #96]
 777:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           /* Update the Handle last node address */
 1524              		.loc 1 777 50 view .LVU619
 1525 008c 5161     		str	r1, [r2, #20]
 779:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           /* Increment the linked list node counter */
 1526              		.loc 1 779 11 is_stmt 1 view .LVU620
 779:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           /* Increment the linked list node counter */
 1527              		.loc 1 779 44 is_stmt 0 view .LVU621
 1528 008e 1966     		str	r1, [r3, #96]
 781:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         }
 1529              		.loc 1 781 11 is_stmt 1 view .LVU622
 781:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         }
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 70


 1530              		.loc 1 781 16 is_stmt 0 view .LVU623
 1531 0090 5A6E     		ldr	r2, [r3, #100]
 781:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         }
 1532              		.loc 1 781 39 view .LVU624
 1533 0092 0132     		adds	r2, r2, #1
 1534 0094 5A66     		str	r2, [r3, #100]
 1535 0096 3046     		mov	r0, r6
 1536 0098 18E0     		b	.L94
 1537              	.LVL96:
 1538              	.L117:
 794:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               pNode->CLAR = (uint32_t)pNewNode;
 1539              		.loc 1 794 15 is_stmt 1 view .LVU625
 794:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               pNode->CLAR = (uint32_t)pNewNode;
 1540              		.loc 1 794 37 is_stmt 0 view .LVU626
 1541 009a 7D69     		ldr	r5, [r7, #20]
 794:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               pNode->CLAR = (uint32_t)pNewNode;
 1542              		.loc 1 794 30 view .LVU627
 1543 009c 4D61     		str	r5, [r1, #20]
 795:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               /* Increment the linked list node counter */
 1544              		.loc 1 795 15 is_stmt 1 view .LVU628
 795:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               /* Increment the linked list node counter */
 1545              		.loc 1 795 27 is_stmt 0 view .LVU629
 1546 009e 7961     		str	r1, [r7, #20]
 797:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               nodeInserted = 1;
 1547              		.loc 1 797 15 is_stmt 1 view .LVU630
 797:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               nodeInserted = 1;
 1548              		.loc 1 797 20 is_stmt 0 view .LVU631
 1549 00a0 5D6E     		ldr	r5, [r3, #100]
 797:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****               nodeInserted = 1;
 1550              		.loc 1 797 43 view .LVU632
 1551 00a2 0135     		adds	r5, r5, #1
 1552 00a4 5D66     		str	r5, [r3, #100]
 798:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             }
 1553              		.loc 1 798 15 is_stmt 1 view .LVU633
 1554              	.LVL97:
 798:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             }
 1555              		.loc 1 798 28 is_stmt 0 view .LVU634
 1556 00a6 4FF0010C 		mov	ip, #1
 1557              	.LVL98:
 1558              	.L100:
 788:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           {
 1559              		.loc 1 788 58 is_stmt 1 view .LVU635
 1560 00aa 5D6E     		ldr	r5, [r3, #100]
 1561 00ac A542     		cmp	r5, r4
 1562 00ae 07D9     		bls	.L103
 788:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           {
 1563              		.loc 1 788 58 is_stmt 0 discriminator 1 view .LVU636
 1564 00b0 BCF1000F 		cmp	ip, #0
 1565 00b4 04D1     		bne	.L103
 790:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             if(pNode == pPrevNode)
 1566              		.loc 1 790 13 is_stmt 1 view .LVU637
 790:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             if(pNode == pPrevNode)
 1567              		.loc 1 790 20 is_stmt 0 view .LVU638
 1568 00b6 0134     		adds	r4, r4, #1
 1569              	.LVL99:
 791:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             {
 1570              		.loc 1 791 13 is_stmt 1 view .LVU639
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 71


 791:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             {
 1571              		.loc 1 791 15 is_stmt 0 view .LVU640
 1572 00b8 9742     		cmp	r7, r2
 1573 00ba EED0     		beq	.L117
 802:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             }
 1574              		.loc 1 802 15 is_stmt 1 view .LVU641
 802:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             }
 1575              		.loc 1 802 52 is_stmt 0 view .LVU642
 1576 00bc 7F69     		ldr	r7, [r7, #20]
 1577              	.LVL100:
 802:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****             }
 1578              		.loc 1 802 52 view .LVU643
 1579 00be F4E7     		b	.L100
 1580              	.L103:
 806:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           {
 1581              		.loc 1 806 11 is_stmt 1 view .LVU644
 806:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           {
 1582              		.loc 1 806 13 is_stmt 0 view .LVU645
 1583 00c0 BCF1000F 		cmp	ip, #0
 1584 00c4 02D0     		beq	.L94
 1585 00c6 3046     		mov	r0, r6
 1586 00c8 00E0     		b	.L94
 1587              	.LVL101:
 1588              	.L109:
 806:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           {
 1589              		.loc 1 806 13 view .LVU646
 1590 00ca 3046     		mov	r0, r6
 1591              	.LVL102:
 1592              	.L94:
 819:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1593              		.loc 1 819 5 is_stmt 1 view .LVU647
 819:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1594              		.loc 1 819 5 view .LVU648
 1595 00cc 0022     		movs	r2, #0
 1596 00ce 83F83C20 		strb	r2, [r3, #60]
 819:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1597              		.loc 1 819 5 view .LVU649
 821:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1598              		.loc 1 821 5 view .LVU650
 821:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1599              		.loc 1 821 18 is_stmt 0 view .LVU651
 1600 00d2 0122     		movs	r2, #1
 1601 00d4 83F83D20 		strb	r2, [r3, #61]
 823:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1602              		.loc 1 823 5 is_stmt 1 view .LVU652
 823:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1603              		.loc 1 823 12 is_stmt 0 view .LVU653
 1604 00d8 A8E7     		b	.L91
 1605              	.LVL103:
 1606              	.L105:
 1607              		.cfi_def_cfa_offset 0
 1608              		.cfi_restore 4
 1609              		.cfi_restore 5
 1610              		.cfi_restore 6
 1611              		.cfi_restore 7
 720:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1612              		.loc 1 720 12 view .LVU654
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 72


 1613 00da 0120     		movs	r0, #1
 1614              	.LVL104:
 720:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1615              		.loc 1 720 12 view .LVU655
 1616 00dc 7047     		bx	lr
 1617              	.LVL105:
 1618              	.L106:
 724:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1619              		.loc 1 724 3 discriminator 1 view .LVU656
 1620 00de 0220     		movs	r0, #2
 833:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1621              		.loc 1 833 1 view .LVU657
 1622 00e0 7047     		bx	lr
 1623              		.cfi_endproc
 1624              	.LFE341:
 1626              		.section	.text.HAL_MDMA_LinkedList_RemoveNode,"ax",%progbits
 1627              		.align	1
 1628              		.global	HAL_MDMA_LinkedList_RemoveNode
 1629              		.syntax unified
 1630              		.thumb
 1631              		.thumb_func
 1633              	HAL_MDMA_LinkedList_RemoveNode:
 1634              	.LVL106:
 1635              	.LFB342:
 845:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   MDMA_LinkNodeTypeDef *ptmpNode;
 1636              		.loc 1 845 1 is_stmt 1 view -0
 1637              		.cfi_startproc
 1638              		@ args = 0, pretend = 0, frame = 0
 1639              		@ frame_needed = 0, uses_anonymous_args = 0
 1640              		@ link register save eliminated.
 846:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t counter = 0, nodeDeleted = 0;
 1641              		.loc 1 846 3 view .LVU659
 847:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   HAL_StatusTypeDef hal_status = HAL_OK;
 1642              		.loc 1 847 3 view .LVU660
 848:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1643              		.loc 1 848 3 view .LVU661
 851:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1644              		.loc 1 851 3 view .LVU662
 851:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1645              		.loc 1 851 5 is_stmt 0 view .LVU663
 1646 0000 0029     		cmp	r1, #0
 1647 0002 18BF     		it	ne
 1648 0004 0028     		cmpne	r0, #0
 1649 0006 5DD0     		beq	.L130
 1650 0008 0346     		mov	r3, r0
 857:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1651              		.loc 1 857 3 is_stmt 1 view .LVU664
 857:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1652              		.loc 1 857 3 view .LVU665
 1653 000a 90F83C20 		ldrb	r2, [r0, #60]	@ zero_extendqisi2
 1654 000e 012A     		cmp	r2, #1
 1655 0010 5AD0     		beq	.L131
 857:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1656              		.loc 1 857 3 discriminator 2 view .LVU666
 1657 0012 0122     		movs	r2, #1
 1658 0014 80F83C20 		strb	r2, [r0, #60]
 857:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 73


 1659              		.loc 1 857 3 view .LVU667
 859:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1660              		.loc 1 859 3 view .LVU668
 859:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1661              		.loc 1 859 35 is_stmt 0 view .LVU669
 1662 0018 90F83D20 		ldrb	r2, [r0, #61]	@ zero_extendqisi2
 1663 001c D0B2     		uxtb	r0, r2
 1664              	.LVL107:
 859:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1665              		.loc 1 859 5 view .LVU670
 1666 001e 012A     		cmp	r2, #1
 1667 0020 04D0     		beq	.L137
 944:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1668              		.loc 1 944 5 is_stmt 1 view .LVU671
 944:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1669              		.loc 1 944 5 view .LVU672
 1670 0022 0022     		movs	r2, #0
 1671 0024 83F83C20 		strb	r2, [r3, #60]
 944:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1672              		.loc 1 944 5 view .LVU673
 947:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1673              		.loc 1 947 5 view .LVU674
 947:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1674              		.loc 1 947 12 is_stmt 0 view .LVU675
 1675 0028 0220     		movs	r0, #2
 1676 002a 7047     		bx	lr
 1677              	.L137:
 845:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   MDMA_LinkNodeTypeDef *ptmpNode;
 1678              		.loc 1 845 1 view .LVU676
 1679 002c 30B4     		push	{r4, r5}
 1680              		.cfi_def_cfa_offset 8
 1681              		.cfi_offset 4, -8
 1682              		.cfi_offset 5, -4
 862:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1683              		.loc 1 862 5 is_stmt 1 view .LVU677
 862:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1684              		.loc 1 862 18 is_stmt 0 view .LVU678
 1685 002e 0222     		movs	r2, #2
 1686 0030 83F83D20 		strb	r2, [r3, #61]
 865:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 1687              		.loc 1 865 5 is_stmt 1 view .LVU679
 865:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 1688              		.loc 1 865 24 is_stmt 0 view .LVU680
 1689 0034 DA6D     		ldr	r2, [r3, #92]
 865:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 1690              		.loc 1 865 7 view .LVU681
 1691 0036 002A     		cmp	r2, #0
 1692 0038 3CD0     		beq	.L121
 865:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 1693              		.loc 1 865 79 discriminator 1 view .LVU682
 1694 003a 1C6E     		ldr	r4, [r3, #96]
 865:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 1695              		.loc 1 865 60 discriminator 1 view .LVU683
 1696 003c 002C     		cmp	r4, #0
 1697 003e 39D0     		beq	.L121
 865:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 1698              		.loc 1 865 123 discriminator 2 view .LVU684
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 74


 1699 0040 5D6E     		ldr	r5, [r3, #100]
 865:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 1700              		.loc 1 865 114 discriminator 2 view .LVU685
 1701 0042 002D     		cmp	r5, #0
 1702 0044 36D0     		beq	.L121
 869:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 1703              		.loc 1 869 10 is_stmt 1 view .LVU686
 869:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 1704              		.loc 1 869 12 is_stmt 0 view .LVU687
 1705 0046 8A42     		cmp	r2, r1
 1706 0048 02D0     		beq	.L138
 847:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   HAL_StatusTypeDef hal_status = HAL_OK;
 1707              		.loc 1 847 25 view .LVU688
 1708 004a 0025     		movs	r5, #0
 847:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   HAL_StatusTypeDef hal_status = HAL_OK;
 1709              		.loc 1 847 12 view .LVU689
 1710 004c AC46     		mov	ip, r5
 1711 004e 22E0     		b	.L122
 1712              	.L138:
 872:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 1713              		.loc 1 872 7 is_stmt 1 view .LVU690
 872:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 1714              		.loc 1 872 9 is_stmt 0 view .LVU691
 1715 0050 8C42     		cmp	r4, r1
 1716 0052 0DD0     		beq	.L139
 885:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
 1717              		.loc 1 885 9 is_stmt 1 view .LVU692
 885:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
 1718              		.loc 1 885 91 is_stmt 0 view .LVU693
 1719 0054 6069     		ldr	r0, [r4, #20]
 885:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
 1720              		.loc 1 885 11 view .LVU694
 1721 0056 8242     		cmp	r2, r0
 1722 0058 11D0     		beq	.L140
 1723              	.L124:
 894:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->FirstLinkedListNodeAddress = (MDMA_LinkNodeTypeDef *)hmdma->Instance->CLAR;
 1724              		.loc 1 894 9 is_stmt 1 view .LVU695
 894:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->FirstLinkedListNodeAddress = (MDMA_LinkNodeTypeDef *)hmdma->Instance->CLAR;
 1725              		.loc 1 894 14 is_stmt 0 view .LVU696
 1726 005a 1A68     		ldr	r2, [r3]
 894:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->FirstLinkedListNodeAddress = (MDMA_LinkNodeTypeDef *)hmdma->Instance->CLAR;
 1727              		.loc 1 894 38 view .LVU697
 1728 005c 4969     		ldr	r1, [r1, #20]
 1729              	.LVL108:
 894:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->FirstLinkedListNodeAddress = (MDMA_LinkNodeTypeDef *)hmdma->Instance->CLAR;
 1730              		.loc 1 894 31 view .LVU698
 1731 005e 5162     		str	r1, [r2, #36]
 895:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Update the Handle node counter */
 1732              		.loc 1 895 9 is_stmt 1 view .LVU699
 895:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Update the Handle node counter */
 1733              		.loc 1 895 74 is_stmt 0 view .LVU700
 1734 0060 1A68     		ldr	r2, [r3]
 895:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Update the Handle node counter */
 1735              		.loc 1 895 84 view .LVU701
 1736 0062 526A     		ldr	r2, [r2, #36]
 895:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         /* Update the Handle node counter */
 1737              		.loc 1 895 43 view .LVU702
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 75


 1738 0064 DA65     		str	r2, [r3, #92]
 897:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 1739              		.loc 1 897 9 is_stmt 1 view .LVU703
 897:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 1740              		.loc 1 897 14 is_stmt 0 view .LVU704
 1741 0066 5A6E     		ldr	r2, [r3, #100]
 897:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 1742              		.loc 1 897 37 view .LVU705
 1743 0068 013A     		subs	r2, r2, #1
 1744 006a 5A66     		str	r2, [r3, #100]
 848:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1745              		.loc 1 848 21 view .LVU706
 1746 006c 0020     		movs	r0, #0
 1747 006e 21E0     		b	.L121
 1748              	.LVL109:
 1749              	.L139:
 877:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->LastLinkedListNodeAddress  = 0;
 1750              		.loc 1 877 9 is_stmt 1 view .LVU707
 877:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->LastLinkedListNodeAddress  = 0;
 1751              		.loc 1 877 43 is_stmt 0 view .LVU708
 1752 0070 0020     		movs	r0, #0
 1753 0072 D865     		str	r0, [r3, #92]
 878:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->LinkedListNodeCounter = 0;
 1754              		.loc 1 878 9 is_stmt 1 view .LVU709
 878:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         hmdma->LinkedListNodeCounter = 0;
 1755              		.loc 1 878 43 is_stmt 0 view .LVU710
 1756 0074 1866     		str	r0, [r3, #96]
 879:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1757              		.loc 1 879 9 is_stmt 1 view .LVU711
 879:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1758              		.loc 1 879 38 is_stmt 0 view .LVU712
 1759 0076 5866     		str	r0, [r3, #100]
 881:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 1760              		.loc 1 881 9 is_stmt 1 view .LVU713
 881:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 1761              		.loc 1 881 14 is_stmt 0 view .LVU714
 1762 0078 1A68     		ldr	r2, [r3]
 881:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 1763              		.loc 1 881 31 view .LVU715
 1764 007a 5062     		str	r0, [r2, #36]
 1765 007c 1AE0     		b	.L121
 1766              	.L140:
 888:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         }
 1767              		.loc 1 888 11 is_stmt 1 view .LVU716
 888:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         }
 1768              		.loc 1 888 57 is_stmt 0 view .LVU717
 1769 007e 4A69     		ldr	r2, [r1, #20]
 888:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         }
 1770              		.loc 1 888 50 view .LVU718
 1771 0080 6261     		str	r2, [r4, #20]
 1772 0082 EAE7     		b	.L124
 1773              	.LVL110:
 1774              	.L142:
 910:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           {
 1775              		.loc 1 910 11 is_stmt 1 view .LVU719
 910:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           {
 1776              		.loc 1 910 28 is_stmt 0 view .LVU720
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 76


 1777 0084 1C6E     		ldr	r4, [r3, #96]
 910:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           {
 1778              		.loc 1 910 13 view .LVU721
 1779 0086 8C42     		cmp	r4, r1
 1780 0088 10D0     		beq	.L141
 1781              	.L126:
 916:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           nodeDeleted = 1;
 1782              		.loc 1 916 11 is_stmt 1 view .LVU722
 916:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           nodeDeleted = 1;
 1783              		.loc 1 916 33 is_stmt 0 view .LVU723
 1784 008a 4C69     		ldr	r4, [r1, #20]
 916:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           nodeDeleted = 1;
 1785              		.loc 1 916 26 view .LVU724
 1786 008c 5461     		str	r4, [r2, #20]
 917:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           /* Update the Handle node counter */
 1787              		.loc 1 917 11 is_stmt 1 view .LVU725
 1788              	.LVL111:
 919:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         }
 1789              		.loc 1 919 11 view .LVU726
 919:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         }
 1790              		.loc 1 919 16 is_stmt 0 view .LVU727
 1791 008e 5C6E     		ldr	r4, [r3, #100]
 919:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         }
 1792              		.loc 1 919 39 view .LVU728
 1793 0090 013C     		subs	r4, r4, #1
 1794 0092 5C66     		str	r4, [r3, #100]
 917:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           /* Update the Handle node counter */
 1795              		.loc 1 917 23 view .LVU729
 1796 0094 0125     		movs	r5, #1
 1797              	.LVL112:
 1798              	.L122:
 904:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 1799              		.loc 1 904 54 is_stmt 1 view .LVU730
 1800 0096 5C6E     		ldr	r4, [r3, #100]
 1801 0098 6445     		cmp	r4, ip
 1802 009a 09D9     		bls	.L128
 904:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 1803              		.loc 1 904 54 is_stmt 0 discriminator 1 view .LVU731
 1804 009c 45B9     		cbnz	r5, .L128
 906:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         if(ptmpNode->CLAR == ((uint32_t)pNode))
 1805              		.loc 1 906 9 is_stmt 1 view .LVU732
 906:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         if(ptmpNode->CLAR == ((uint32_t)pNode))
 1806              		.loc 1 906 16 is_stmt 0 view .LVU733
 1807 009e 0CF1010C 		add	ip, ip, #1
 1808              	.LVL113:
 907:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
 1809              		.loc 1 907 9 is_stmt 1 view .LVU734
 907:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
 1810              		.loc 1 907 20 is_stmt 0 view .LVU735
 1811 00a2 5469     		ldr	r4, [r2, #20]
 907:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
 1812              		.loc 1 907 11 view .LVU736
 1813 00a4 8C42     		cmp	r4, r1
 1814 00a6 EDD0     		beq	.L142
 923:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         }
 1815              		.loc 1 923 11 is_stmt 1 view .LVU737
 923:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         }
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 77


 1816              		.loc 1 923 54 is_stmt 0 view .LVU738
 1817 00a8 5269     		ldr	r2, [r2, #20]
 1818              	.LVL114:
 923:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         }
 1819              		.loc 1 923 54 view .LVU739
 1820 00aa F4E7     		b	.L122
 1821              	.L141:
 913:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           }
 1822              		.loc 1 913 13 is_stmt 1 view .LVU740
 913:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****           }
 1823              		.loc 1 913 46 is_stmt 0 view .LVU741
 1824 00ac 1A66     		str	r2, [r3, #96]
 1825 00ae ECE7     		b	.L126
 1826              	.L128:
 927:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 1827              		.loc 1 927 7 is_stmt 1 view .LVU742
 927:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 1828              		.loc 1 927 9 is_stmt 0 view .LVU743
 1829 00b0 05B1     		cbz	r5, .L121
 848:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1830              		.loc 1 848 21 view .LVU744
 1831 00b2 0020     		movs	r0, #0
 1832              	.LVL115:
 1833              	.L121:
 935:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1834              		.loc 1 935 5 is_stmt 1 view .LVU745
 935:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1835              		.loc 1 935 5 view .LVU746
 1836 00b4 0022     		movs	r2, #0
 1837 00b6 83F83C20 		strb	r2, [r3, #60]
 935:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1838              		.loc 1 935 5 view .LVU747
 937:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1839              		.loc 1 937 5 view .LVU748
 937:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1840              		.loc 1 937 18 is_stmt 0 view .LVU749
 1841 00ba 0122     		movs	r2, #1
 1842 00bc 83F83D20 		strb	r2, [r3, #61]
 939:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1843              		.loc 1 939 5 is_stmt 1 view .LVU750
 949:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1844              		.loc 1 949 1 is_stmt 0 view .LVU751
 1845 00c0 30BC     		pop	{r4, r5}
 1846              		.cfi_restore 5
 1847              		.cfi_restore 4
 1848              		.cfi_def_cfa_offset 0
 1849 00c2 7047     		bx	lr
 1850              	.LVL116:
 1851              	.L130:
 853:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1852              		.loc 1 853 12 view .LVU752
 1853 00c4 0120     		movs	r0, #1
 1854              	.LVL117:
 853:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1855              		.loc 1 853 12 view .LVU753
 1856 00c6 7047     		bx	lr
 1857              	.LVL118:
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 78


 1858              	.L131:
 857:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1859              		.loc 1 857 3 discriminator 1 view .LVU754
 1860 00c8 0220     		movs	r0, #2
 1861              	.LVL119:
 949:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1862              		.loc 1 949 1 view .LVU755
 1863 00ca 7047     		bx	lr
 1864              		.cfi_endproc
 1865              	.LFE342:
 1867              		.section	.text.HAL_MDMA_LinkedList_EnableCircularMode,"ax",%progbits
 1868              		.align	1
 1869              		.global	HAL_MDMA_LinkedList_EnableCircularMode
 1870              		.syntax unified
 1871              		.thumb
 1872              		.thumb_func
 1874              	HAL_MDMA_LinkedList_EnableCircularMode:
 1875              	.LVL120:
 1876              	.LFB343:
 958:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   HAL_StatusTypeDef hal_status = HAL_OK;
 1877              		.loc 1 958 1 is_stmt 1 view -0
 1878              		.cfi_startproc
 1879              		@ args = 0, pretend = 0, frame = 0
 1880              		@ frame_needed = 0, uses_anonymous_args = 0
 1881              		@ link register save eliminated.
 959:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1882              		.loc 1 959 3 view .LVU757
 962:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1883              		.loc 1 962 3 view .LVU758
 962:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1884              		.loc 1 962 5 is_stmt 0 view .LVU759
 1885 0000 30B3     		cbz	r0, .L146
 1886 0002 0346     		mov	r3, r0
 968:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1887              		.loc 1 968 3 is_stmt 1 view .LVU760
 968:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1888              		.loc 1 968 3 view .LVU761
 1889 0004 90F83C20 		ldrb	r2, [r0, #60]	@ zero_extendqisi2
 1890 0008 012A     		cmp	r2, #1
 1891 000a 23D0     		beq	.L147
 958:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   HAL_StatusTypeDef hal_status = HAL_OK;
 1892              		.loc 1 958 1 is_stmt 0 view .LVU762
 1893 000c 10B4     		push	{r4}
 1894              		.cfi_def_cfa_offset 4
 1895              		.cfi_offset 4, -4
 968:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1896              		.loc 1 968 3 is_stmt 1 discriminator 2 view .LVU763
 1897 000e 0122     		movs	r2, #1
 1898 0010 80F83C20 		strb	r2, [r0, #60]
 968:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1899              		.loc 1 968 3 view .LVU764
 970:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1900              		.loc 1 970 3 view .LVU765
 970:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1901              		.loc 1 970 35 is_stmt 0 view .LVU766
 1902 0014 90F83D20 		ldrb	r2, [r0, #61]	@ zero_extendqisi2
 1903 0018 D0B2     		uxtb	r0, r2
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 79


 1904              	.LVL121:
 970:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1905              		.loc 1 970 5 view .LVU767
 1906 001a 012A     		cmp	r2, #1
 1907 001c 09D0     		beq	.L153
 959:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1908              		.loc 1 959 21 view .LVU768
 1909 001e 0020     		movs	r0, #0
 1910              	.L145:
 1911              	.LVL122:
 988:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1912              		.loc 1 988 3 is_stmt 1 view .LVU769
 988:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1913              		.loc 1 988 3 view .LVU770
 1914 0020 0022     		movs	r2, #0
 1915 0022 83F83C20 		strb	r2, [r3, #60]
 988:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1916              		.loc 1 988 3 view .LVU771
 990:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1917              		.loc 1 990 3 view .LVU772
 990:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1918              		.loc 1 990 16 is_stmt 0 view .LVU773
 1919 0026 0122     		movs	r2, #1
 1920 0028 83F83D20 		strb	r2, [r3, #61]
 992:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 1921              		.loc 1 992 3 is_stmt 1 view .LVU774
 993:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1922              		.loc 1 993 1 is_stmt 0 view .LVU775
 1923 002c 5DF8044B 		ldr	r4, [sp], #4
 1924              		.cfi_remember_state
 1925              		.cfi_restore 4
 1926              		.cfi_def_cfa_offset 0
 1927 0030 7047     		bx	lr
 1928              	.LVL123:
 1929              	.L153:
 1930              		.cfi_restore_state
 973:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1931              		.loc 1 973 5 is_stmt 1 view .LVU776
 973:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1932              		.loc 1 973 18 is_stmt 0 view .LVU777
 1933 0032 0222     		movs	r2, #2
 1934 0034 83F83D20 		strb	r2, [r3, #61]
 976:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 1935              		.loc 1 976 5 is_stmt 1 view .LVU778
 976:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 1936              		.loc 1 976 24 is_stmt 0 view .LVU779
 1937 0038 DA6D     		ldr	r2, [r3, #92]
 976:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 1938              		.loc 1 976 7 view .LVU780
 1939 003a 002A     		cmp	r2, #0
 1940 003c F0D0     		beq	.L145
 976:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 1941              		.loc 1 976 79 discriminator 1 view .LVU781
 1942 003e 196E     		ldr	r1, [r3, #96]
 976:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 1943              		.loc 1 976 60 discriminator 1 view .LVU782
 1944 0040 0029     		cmp	r1, #0
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 80


 1945 0042 EDD0     		beq	.L145
 976:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 1946              		.loc 1 976 114 discriminator 2 view .LVU783
 1947 0044 5C6E     		ldr	r4, [r3, #100]
 1948 0046 002C     		cmp	r4, #0
 1949 0048 EAD0     		beq	.L145
 983:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 1950              		.loc 1 983 7 is_stmt 1 view .LVU784
 983:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 1951              		.loc 1 983 46 is_stmt 0 view .LVU785
 1952 004a 4A61     		str	r2, [r1, #20]
 959:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1953              		.loc 1 959 21 view .LVU786
 1954 004c 0020     		movs	r0, #0
 1955 004e E7E7     		b	.L145
 1956              	.LVL124:
 1957              	.L146:
 1958              		.cfi_def_cfa_offset 0
 1959              		.cfi_restore 4
 964:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1960              		.loc 1 964 12 view .LVU787
 1961 0050 0120     		movs	r0, #1
 1962              	.LVL125:
 964:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 1963              		.loc 1 964 12 view .LVU788
 1964 0052 7047     		bx	lr
 1965              	.LVL126:
 1966              	.L147:
 968:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1967              		.loc 1 968 3 discriminator 1 view .LVU789
 1968 0054 0220     		movs	r0, #2
 1969              	.LVL127:
 993:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1970              		.loc 1 993 1 view .LVU790
 1971 0056 7047     		bx	lr
 1972              		.cfi_endproc
 1973              	.LFE343:
 1975              		.section	.text.HAL_MDMA_LinkedList_DisableCircularMode,"ax",%progbits
 1976              		.align	1
 1977              		.global	HAL_MDMA_LinkedList_DisableCircularMode
 1978              		.syntax unified
 1979              		.thumb
 1980              		.thumb_func
 1982              	HAL_MDMA_LinkedList_DisableCircularMode:
 1983              	.LVL128:
 1984              	.LFB344:
1002:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   HAL_StatusTypeDef hal_status = HAL_OK;
 1985              		.loc 1 1002 1 is_stmt 1 view -0
 1986              		.cfi_startproc
 1987              		@ args = 0, pretend = 0, frame = 0
 1988              		@ frame_needed = 0, uses_anonymous_args = 0
 1989              		@ link register save eliminated.
1003:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1990              		.loc 1 1003 3 view .LVU792
1006:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 1991              		.loc 1 1006 3 view .LVU793
1006:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 81


 1992              		.loc 1 1006 5 is_stmt 0 view .LVU794
 1993 0000 0346     		mov	r3, r0
 1994 0002 10B3     		cbz	r0, .L157
1012:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1995              		.loc 1 1012 3 is_stmt 1 view .LVU795
1012:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 1996              		.loc 1 1012 3 view .LVU796
 1997 0004 90F83C20 		ldrb	r2, [r0, #60]	@ zero_extendqisi2
 1998 0008 012A     		cmp	r2, #1
 1999 000a 20D0     		beq	.L158
1012:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2000              		.loc 1 1012 3 discriminator 2 view .LVU797
 2001 000c 0122     		movs	r2, #1
 2002 000e 80F83C20 		strb	r2, [r0, #60]
1012:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2003              		.loc 1 1012 3 view .LVU798
1014:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2004              		.loc 1 1014 3 view .LVU799
1014:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2005              		.loc 1 1014 35 is_stmt 0 view .LVU800
 2006 0012 90F83D20 		ldrb	r2, [r0, #61]	@ zero_extendqisi2
 2007 0016 D0B2     		uxtb	r0, r2
 2008              	.LVL129:
1014:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2009              		.loc 1 1014 5 view .LVU801
 2010 0018 012A     		cmp	r2, #1
 2011 001a 07D0     		beq	.L160
1003:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2012              		.loc 1 1003 21 view .LVU802
 2013 001c 0020     		movs	r0, #0
 2014              	.L156:
 2015              	.LVL130:
1032:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2016              		.loc 1 1032 3 is_stmt 1 view .LVU803
1032:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2017              		.loc 1 1032 3 view .LVU804
 2018 001e 0022     		movs	r2, #0
 2019 0020 83F83C20 		strb	r2, [r3, #60]
1032:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2020              		.loc 1 1032 3 view .LVU805
1034:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2021              		.loc 1 1034 3 view .LVU806
1034:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2022              		.loc 1 1034 16 is_stmt 0 view .LVU807
 2023 0024 0122     		movs	r2, #1
 2024 0026 83F83D20 		strb	r2, [r3, #61]
1036:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 2025              		.loc 1 1036 3 is_stmt 1 view .LVU808
1036:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 2026              		.loc 1 1036 10 is_stmt 0 view .LVU809
 2027 002a 7047     		bx	lr
 2028              	.LVL131:
 2029              	.L160:
1017:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2030              		.loc 1 1017 5 is_stmt 1 view .LVU810
1017:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2031              		.loc 1 1017 18 is_stmt 0 view .LVU811
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 82


 2032 002c 0222     		movs	r2, #2
 2033 002e 83F83D20 		strb	r2, [r3, #61]
1020:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2034              		.loc 1 1020 5 is_stmt 1 view .LVU812
1020:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2035              		.loc 1 1020 24 is_stmt 0 view .LVU813
 2036 0032 DA6D     		ldr	r2, [r3, #92]
1020:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2037              		.loc 1 1020 7 view .LVU814
 2038 0034 002A     		cmp	r2, #0
 2039 0036 F2D0     		beq	.L156
1020:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2040              		.loc 1 1020 79 discriminator 1 view .LVU815
 2041 0038 1A6E     		ldr	r2, [r3, #96]
1020:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2042              		.loc 1 1020 60 discriminator 1 view .LVU816
 2043 003a 002A     		cmp	r2, #0
 2044 003c EFD0     		beq	.L156
1020:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2045              		.loc 1 1020 123 discriminator 2 view .LVU817
 2046 003e 596E     		ldr	r1, [r3, #100]
1020:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2047              		.loc 1 1020 114 discriminator 2 view .LVU818
 2048 0040 0029     		cmp	r1, #0
 2049 0042 ECD0     		beq	.L156
1027:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 2050              		.loc 1 1027 7 is_stmt 1 view .LVU819
1027:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 2051              		.loc 1 1027 46 is_stmt 0 view .LVU820
 2052 0044 0020     		movs	r0, #0
 2053 0046 5061     		str	r0, [r2, #20]
 2054 0048 E9E7     		b	.L156
 2055              	.LVL132:
 2056              	.L157:
1008:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2057              		.loc 1 1008 12 view .LVU821
 2058 004a 0120     		movs	r0, #1
 2059              	.LVL133:
1008:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2060              		.loc 1 1008 12 view .LVU822
 2061 004c 7047     		bx	lr
 2062              	.LVL134:
 2063              	.L158:
1012:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2064              		.loc 1 1012 3 discriminator 1 view .LVU823
 2065 004e 0220     		movs	r0, #2
 2066              	.LVL135:
1037:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2067              		.loc 1 1037 1 view .LVU824
 2068 0050 7047     		bx	lr
 2069              		.cfi_endproc
 2070              	.LFE344:
 2072              		.section	.text.HAL_MDMA_Start,"ax",%progbits
 2073              		.align	1
 2074              		.global	HAL_MDMA_Start
 2075              		.syntax unified
 2076              		.thumb
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 83


 2077              		.thumb_func
 2079              	HAL_MDMA_Start:
 2080              	.LVL136:
 2081              	.LFB345:
1073:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the parameters */
 2082              		.loc 1 1073 1 is_stmt 1 view -0
 2083              		.cfi_startproc
 2084              		@ args = 4, pretend = 0, frame = 0
 2085              		@ frame_needed = 0, uses_anonymous_args = 0
1075:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_BLOCK_COUNT(BlockCount));
 2086              		.loc 1 1075 3 view .LVU826
1076:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2087              		.loc 1 1076 3 view .LVU827
1079:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2088              		.loc 1 1079 3 view .LVU828
1079:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2089              		.loc 1 1079 5 is_stmt 0 view .LVU829
 2090 0000 0028     		cmp	r0, #0
 2091 0002 34D0     		beq	.L164
1073:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the parameters */
 2092              		.loc 1 1073 1 view .LVU830
 2093 0004 30B5     		push	{r4, r5, lr}
 2094              		.cfi_def_cfa_offset 12
 2095              		.cfi_offset 4, -12
 2096              		.cfi_offset 5, -8
 2097              		.cfi_offset 14, -4
 2098 0006 83B0     		sub	sp, sp, #12
 2099              		.cfi_def_cfa_offset 24
 2100 0008 0446     		mov	r4, r0
1085:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2101              		.loc 1 1085 3 is_stmt 1 view .LVU831
1085:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2102              		.loc 1 1085 3 view .LVU832
 2103 000a 90F83C00 		ldrb	r0, [r0, #60]	@ zero_extendqisi2
 2104              	.LVL137:
1085:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2105              		.loc 1 1085 3 is_stmt 0 view .LVU833
 2106 000e 0128     		cmp	r0, #1
 2107 0010 2FD0     		beq	.L165
1085:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2108              		.loc 1 1085 3 is_stmt 1 discriminator 2 view .LVU834
 2109 0012 0120     		movs	r0, #1
 2110 0014 84F83C00 		strb	r0, [r4, #60]
1085:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2111              		.loc 1 1085 3 view .LVU835
1087:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2112              		.loc 1 1087 3 view .LVU836
1087:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2113              		.loc 1 1087 35 is_stmt 0 view .LVU837
 2114 0018 94F83D00 		ldrb	r0, [r4, #61]	@ zero_extendqisi2
1087:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2115              		.loc 1 1087 5 view .LVU838
 2116 001c 0128     		cmp	r0, #1
 2117 001e 05D0     		beq	.L171
1113:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2118              		.loc 1 1113 5 is_stmt 1 view .LVU839
1113:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 84


 2119              		.loc 1 1113 5 view .LVU840
 2120 0020 0023     		movs	r3, #0
 2121              	.LVL138:
1113:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2122              		.loc 1 1113 5 is_stmt 0 view .LVU841
 2123 0022 84F83C30 		strb	r3, [r4, #60]
1113:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2124              		.loc 1 1113 5 is_stmt 1 view .LVU842
1116:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2125              		.loc 1 1116 5 view .LVU843
1116:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2126              		.loc 1 1116 12 is_stmt 0 view .LVU844
 2127 0026 0220     		movs	r0, #2
 2128              	.LVL139:
 2129              	.L162:
1120:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2130              		.loc 1 1120 1 view .LVU845
 2131 0028 03B0     		add	sp, sp, #12
 2132              		.cfi_remember_state
 2133              		.cfi_def_cfa_offset 12
 2134              		@ sp needed
 2135 002a 30BD     		pop	{r4, r5, pc}
 2136              	.LVL140:
 2137              	.L171:
 2138              		.cfi_restore_state
1090:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2139              		.loc 1 1090 5 is_stmt 1 view .LVU846
1090:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2140              		.loc 1 1090 18 is_stmt 0 view .LVU847
 2141 002c 0220     		movs	r0, #2
 2142 002e 84F83D00 		strb	r0, [r4, #61]
1093:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2143              		.loc 1 1093 5 is_stmt 1 view .LVU848
1093:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2144              		.loc 1 1093 22 is_stmt 0 view .LVU849
 2145 0032 0020     		movs	r0, #0
 2146 0034 A066     		str	r0, [r4, #104]
1096:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2147              		.loc 1 1096 5 is_stmt 1 view .LVU850
 2148 0036 2568     		ldr	r5, [r4]
 2149 0038 E868     		ldr	r0, [r5, #12]
 2150 003a 20F00100 		bic	r0, r0, #1
 2151 003e E860     		str	r0, [r5, #12]
1099:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2152              		.loc 1 1099 5 view .LVU851
 2153 0040 0698     		ldr	r0, [sp, #24]
 2154 0042 0090     		str	r0, [sp]
 2155 0044 2046     		mov	r0, r4
 2156 0046 FFF7FEFF 		bl	MDMA_SetConfig
 2157              	.LVL141:
1102:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2158              		.loc 1 1102 5 view .LVU852
 2159 004a 2268     		ldr	r2, [r4]
 2160 004c D368     		ldr	r3, [r2, #12]
 2161 004e 43F00103 		orr	r3, r3, #1
 2162 0052 D360     		str	r3, [r2, #12]
1104:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 85


 2163              		.loc 1 1104 5 view .LVU853
1104:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2164              		.loc 1 1104 19 is_stmt 0 view .LVU854
 2165 0054 6368     		ldr	r3, [r4, #4]
1104:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2166              		.loc 1 1104 7 view .LVU855
 2167 0056 B3F1804F 		cmp	r3, #1073741824
 2168 005a 01D0     		beq	.L172
1119:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 2169              		.loc 1 1119 10 view .LVU856
 2170 005c 0020     		movs	r0, #0
 2171 005e E3E7     		b	.L162
 2172              	.L172:
1107:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 2173              		.loc 1 1107 7 is_stmt 1 view .LVU857
1107:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 2174              		.loc 1 1107 12 is_stmt 0 view .LVU858
 2175 0060 2268     		ldr	r2, [r4]
1107:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 2176              		.loc 1 1107 22 view .LVU859
 2177 0062 D368     		ldr	r3, [r2, #12]
1107:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 2178              		.loc 1 1107 28 view .LVU860
 2179 0064 43F48033 		orr	r3, r3, #65536
 2180 0068 D360     		str	r3, [r2, #12]
1119:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 2181              		.loc 1 1119 10 view .LVU861
 2182 006a 0020     		movs	r0, #0
 2183 006c DCE7     		b	.L162
 2184              	.LVL142:
 2185              	.L164:
 2186              		.cfi_def_cfa_offset 0
 2187              		.cfi_restore 4
 2188              		.cfi_restore 5
 2189              		.cfi_restore 14
1081:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2190              		.loc 1 1081 12 view .LVU862
 2191 006e 0120     		movs	r0, #1
 2192              	.LVL143:
1120:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2193              		.loc 1 1120 1 view .LVU863
 2194 0070 7047     		bx	lr
 2195              	.LVL144:
 2196              	.L165:
 2197              		.cfi_def_cfa_offset 24
 2198              		.cfi_offset 4, -12
 2199              		.cfi_offset 5, -8
 2200              		.cfi_offset 14, -4
1085:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2201              		.loc 1 1085 3 discriminator 1 view .LVU864
 2202 0072 0220     		movs	r0, #2
 2203 0074 D8E7     		b	.L162
 2204              		.cfi_endproc
 2205              	.LFE345:
 2207              		.section	.text.HAL_MDMA_Start_IT,"ax",%progbits
 2208              		.align	1
 2209              		.global	HAL_MDMA_Start_IT
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 86


 2210              		.syntax unified
 2211              		.thumb
 2212              		.thumb_func
 2214              	HAL_MDMA_Start_IT:
 2215              	.LVL145:
 2216              	.LFB346:
1133:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the parameters */
 2217              		.loc 1 1133 1 is_stmt 1 view -0
 2218              		.cfi_startproc
 2219              		@ args = 4, pretend = 0, frame = 0
 2220              		@ frame_needed = 0, uses_anonymous_args = 0
1135:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   assert_param(IS_MDMA_BLOCK_COUNT(BlockCount));
 2221              		.loc 1 1135 3 view .LVU866
1136:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2222              		.loc 1 1136 3 view .LVU867
1139:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2223              		.loc 1 1139 3 view .LVU868
1139:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2224              		.loc 1 1139 5 is_stmt 0 view .LVU869
 2225 0000 0028     		cmp	r0, #0
 2226 0002 4ED0     		beq	.L179
1133:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the parameters */
 2227              		.loc 1 1133 1 view .LVU870
 2228 0004 30B5     		push	{r4, r5, lr}
 2229              		.cfi_def_cfa_offset 12
 2230              		.cfi_offset 4, -12
 2231              		.cfi_offset 5, -8
 2232              		.cfi_offset 14, -4
 2233 0006 83B0     		sub	sp, sp, #12
 2234              		.cfi_def_cfa_offset 24
 2235 0008 0446     		mov	r4, r0
1145:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2236              		.loc 1 1145 3 is_stmt 1 view .LVU871
1145:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2237              		.loc 1 1145 3 view .LVU872
 2238 000a 90F83C00 		ldrb	r0, [r0, #60]	@ zero_extendqisi2
 2239              	.LVL146:
1145:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2240              		.loc 1 1145 3 is_stmt 0 view .LVU873
 2241 000e 0128     		cmp	r0, #1
 2242 0010 49D0     		beq	.L180
1145:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2243              		.loc 1 1145 3 is_stmt 1 discriminator 2 view .LVU874
 2244 0012 0120     		movs	r0, #1
 2245 0014 84F83C00 		strb	r0, [r4, #60]
1145:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2246              		.loc 1 1145 3 view .LVU875
1147:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2247              		.loc 1 1147 3 view .LVU876
1147:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2248              		.loc 1 1147 35 is_stmt 0 view .LVU877
 2249 0018 94F83D00 		ldrb	r0, [r4, #61]	@ zero_extendqisi2
1147:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2250              		.loc 1 1147 5 view .LVU878
 2251 001c 0128     		cmp	r0, #1
 2252 001e 05D0     		beq	.L186
1194:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 87


 2253              		.loc 1 1194 5 is_stmt 1 view .LVU879
1194:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2254              		.loc 1 1194 5 view .LVU880
 2255 0020 0023     		movs	r3, #0
 2256              	.LVL147:
1194:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2257              		.loc 1 1194 5 is_stmt 0 view .LVU881
 2258 0022 84F83C30 		strb	r3, [r4, #60]
1194:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2259              		.loc 1 1194 5 is_stmt 1 view .LVU882
1197:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2260              		.loc 1 1197 5 view .LVU883
1197:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2261              		.loc 1 1197 12 is_stmt 0 view .LVU884
 2262 0026 0220     		movs	r0, #2
 2263              	.LVL148:
 2264              	.L174:
1201:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2265              		.loc 1 1201 1 view .LVU885
 2266 0028 03B0     		add	sp, sp, #12
 2267              		.cfi_remember_state
 2268              		.cfi_def_cfa_offset 12
 2269              		@ sp needed
 2270 002a 30BD     		pop	{r4, r5, pc}
 2271              	.LVL149:
 2272              	.L186:
 2273              		.cfi_restore_state
1150:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2274              		.loc 1 1150 5 is_stmt 1 view .LVU886
1150:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2275              		.loc 1 1150 18 is_stmt 0 view .LVU887
 2276 002c 0220     		movs	r0, #2
 2277 002e 84F83D00 		strb	r0, [r4, #61]
1153:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2278              		.loc 1 1153 5 is_stmt 1 view .LVU888
1153:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2279              		.loc 1 1153 22 is_stmt 0 view .LVU889
 2280 0032 0020     		movs	r0, #0
 2281 0034 A066     		str	r0, [r4, #104]
1156:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2282              		.loc 1 1156 5 is_stmt 1 view .LVU890
 2283 0036 2568     		ldr	r5, [r4]
 2284 0038 E868     		ldr	r0, [r5, #12]
 2285 003a 20F00100 		bic	r0, r0, #1
 2286 003e E860     		str	r0, [r5, #12]
1159:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2287              		.loc 1 1159 5 view .LVU891
 2288 0040 0698     		ldr	r0, [sp, #24]
 2289 0042 0090     		str	r0, [sp]
 2290 0044 2046     		mov	r0, r4
 2291 0046 FFF7FEFF 		bl	MDMA_SetConfig
 2292              	.LVL150:
1162:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2293              		.loc 1 1162 5 view .LVU892
 2294 004a 2268     		ldr	r2, [r4]
 2295 004c D368     		ldr	r3, [r2, #12]
 2296 004e 43F00603 		orr	r3, r3, #6
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 88


 2297 0052 D360     		str	r3, [r2, #12]
1164:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2298              		.loc 1 1164 5 view .LVU893
1164:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2299              		.loc 1 1164 13 is_stmt 0 view .LVU894
 2300 0054 E36C     		ldr	r3, [r4, #76]
1164:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2301              		.loc 1 1164 7 view .LVU895
 2302 0056 23B1     		cbz	r3, .L176
1167:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 2303              		.loc 1 1167 7 is_stmt 1 view .LVU896
 2304 0058 2268     		ldr	r2, [r4]
 2305 005a D368     		ldr	r3, [r2, #12]
 2306 005c 43F01003 		orr	r3, r3, #16
 2307 0060 D360     		str	r3, [r2, #12]
 2308              	.L176:
1170:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2309              		.loc 1 1170 5 view .LVU897
1170:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2310              		.loc 1 1170 13 is_stmt 0 view .LVU898
 2311 0062 236D     		ldr	r3, [r4, #80]
1170:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2312              		.loc 1 1170 7 view .LVU899
 2313 0064 23B1     		cbz	r3, .L177
1173:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 2314              		.loc 1 1173 7 is_stmt 1 view .LVU900
 2315 0066 2268     		ldr	r2, [r4]
 2316 0068 D368     		ldr	r3, [r2, #12]
 2317 006a 43F00803 		orr	r3, r3, #8
 2318 006e D360     		str	r3, [r2, #12]
 2319              	.L177:
1176:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2320              		.loc 1 1176 5 view .LVU901
1176:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2321              		.loc 1 1176 13 is_stmt 0 view .LVU902
 2322 0070 A36C     		ldr	r3, [r4, #72]
1176:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2323              		.loc 1 1176 7 view .LVU903
 2324 0072 23B1     		cbz	r3, .L178
1179:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 2325              		.loc 1 1179 7 is_stmt 1 view .LVU904
 2326 0074 2268     		ldr	r2, [r4]
 2327 0076 D368     		ldr	r3, [r2, #12]
 2328 0078 43F02003 		orr	r3, r3, #32
 2329 007c D360     		str	r3, [r2, #12]
 2330              	.L178:
1183:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2331              		.loc 1 1183 5 view .LVU905
 2332 007e 2268     		ldr	r2, [r4]
 2333 0080 D368     		ldr	r3, [r2, #12]
 2334 0082 43F00103 		orr	r3, r3, #1
 2335 0086 D360     		str	r3, [r2, #12]
1185:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2336              		.loc 1 1185 5 view .LVU906
1185:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2337              		.loc 1 1185 19 is_stmt 0 view .LVU907
 2338 0088 6368     		ldr	r3, [r4, #4]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 89


1185:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2339              		.loc 1 1185 7 view .LVU908
 2340 008a B3F1804F 		cmp	r3, #1073741824
 2341 008e 01D0     		beq	.L187
1200:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 2342              		.loc 1 1200 10 view .LVU909
 2343 0090 0020     		movs	r0, #0
 2344 0092 C9E7     		b	.L174
 2345              	.L187:
1188:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 2346              		.loc 1 1188 7 is_stmt 1 view .LVU910
1188:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 2347              		.loc 1 1188 12 is_stmt 0 view .LVU911
 2348 0094 2268     		ldr	r2, [r4]
1188:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 2349              		.loc 1 1188 22 view .LVU912
 2350 0096 D368     		ldr	r3, [r2, #12]
1188:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 2351              		.loc 1 1188 28 view .LVU913
 2352 0098 43F48033 		orr	r3, r3, #65536
 2353 009c D360     		str	r3, [r2, #12]
1200:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 2354              		.loc 1 1200 10 view .LVU914
 2355 009e 0020     		movs	r0, #0
 2356 00a0 C2E7     		b	.L174
 2357              	.LVL151:
 2358              	.L179:
 2359              		.cfi_def_cfa_offset 0
 2360              		.cfi_restore 4
 2361              		.cfi_restore 5
 2362              		.cfi_restore 14
1141:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2363              		.loc 1 1141 12 view .LVU915
 2364 00a2 0120     		movs	r0, #1
 2365              	.LVL152:
1201:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2366              		.loc 1 1201 1 view .LVU916
 2367 00a4 7047     		bx	lr
 2368              	.LVL153:
 2369              	.L180:
 2370              		.cfi_def_cfa_offset 24
 2371              		.cfi_offset 4, -12
 2372              		.cfi_offset 5, -8
 2373              		.cfi_offset 14, -4
1145:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2374              		.loc 1 1145 3 discriminator 1 view .LVU917
 2375 00a6 0220     		movs	r0, #2
 2376 00a8 BEE7     		b	.L174
 2377              		.cfi_endproc
 2378              	.LFE346:
 2380              		.section	.text.HAL_MDMA_Abort,"ax",%progbits
 2381              		.align	1
 2382              		.global	HAL_MDMA_Abort
 2383              		.syntax unified
 2384              		.thumb
 2385              		.thumb_func
 2387              	HAL_MDMA_Abort:
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 90


 2388              	.LVL154:
 2389              	.LFB347:
1216:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t tickstart =  HAL_GetTick();
 2390              		.loc 1 1216 1 is_stmt 1 view -0
 2391              		.cfi_startproc
 2392              		@ args = 0, pretend = 0, frame = 0
 2393              		@ frame_needed = 0, uses_anonymous_args = 0
1216:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t tickstart =  HAL_GetTick();
 2394              		.loc 1 1216 1 is_stmt 0 view .LVU919
 2395 0000 38B5     		push	{r3, r4, r5, lr}
 2396              		.cfi_def_cfa_offset 16
 2397              		.cfi_offset 3, -16
 2398              		.cfi_offset 4, -12
 2399              		.cfi_offset 5, -8
 2400              		.cfi_offset 14, -4
 2401 0002 0446     		mov	r4, r0
1217:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2402              		.loc 1 1217 3 is_stmt 1 view .LVU920
1217:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2403              		.loc 1 1217 25 is_stmt 0 view .LVU921
 2404 0004 FFF7FEFF 		bl	HAL_GetTick
 2405              	.LVL155:
1220:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2406              		.loc 1 1220 3 is_stmt 1 view .LVU922
1220:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2407              		.loc 1 1220 5 is_stmt 0 view .LVU923
 2408 0008 002C     		cmp	r4, #0
 2409 000a 34D0     		beq	.L193
 2410 000c 0546     		mov	r5, r0
1225:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2411              		.loc 1 1225 3 is_stmt 1 view .LVU924
1225:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2412              		.loc 1 1225 34 is_stmt 0 view .LVU925
 2413 000e 94F83D30 		ldrb	r3, [r4, #61]	@ zero_extendqisi2
1225:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2414              		.loc 1 1225 5 view .LVU926
 2415 0012 022B     		cmp	r3, #2
 2416 0014 06D0     		beq	.L190
1227:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2417              		.loc 1 1227 5 is_stmt 1 view .LVU927
1227:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2418              		.loc 1 1227 22 is_stmt 0 view .LVU928
 2419 0016 8023     		movs	r3, #128
 2420 0018 A366     		str	r3, [r4, #104]
1230:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2421              		.loc 1 1230 5 is_stmt 1 view .LVU929
1230:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2422              		.loc 1 1230 5 view .LVU930
 2423 001a 0023     		movs	r3, #0
 2424 001c 84F83C30 		strb	r3, [r4, #60]
1230:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2425              		.loc 1 1230 5 view .LVU931
1232:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2426              		.loc 1 1232 5 view .LVU932
1232:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2427              		.loc 1 1232 12 is_stmt 0 view .LVU933
 2428 0020 0120     		movs	r0, #1
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 91


 2429              	.LVL156:
 2430              	.L189:
1272:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2431              		.loc 1 1272 1 view .LVU934
 2432 0022 38BD     		pop	{r3, r4, r5, pc}
 2433              	.LVL157:
 2434              	.L190:
1237:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2435              		.loc 1 1237 5 is_stmt 1 view .LVU935
 2436 0024 2268     		ldr	r2, [r4]
 2437 0026 D368     		ldr	r3, [r2, #12]
 2438 0028 23F03E03 		bic	r3, r3, #62
 2439 002c D360     		str	r3, [r2, #12]
1240:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2440              		.loc 1 1240 5 view .LVU936
 2441 002e 2268     		ldr	r2, [r4]
 2442 0030 D368     		ldr	r3, [r2, #12]
 2443 0032 23F00103 		bic	r3, r3, #1
 2444 0036 D360     		str	r3, [r2, #12]
1243:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2445              		.loc 1 1243 5 view .LVU937
 2446              	.LVL158:
 2447              	.L191:
1243:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2448              		.loc 1 1243 48 view .LVU938
1243:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2449              		.loc 1 1243 17 is_stmt 0 view .LVU939
 2450 0038 2368     		ldr	r3, [r4]
1243:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2451              		.loc 1 1243 27 view .LVU940
 2452 003a DA68     		ldr	r2, [r3, #12]
1243:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2453              		.loc 1 1243 48 view .LVU941
 2454 003c 12F0010F 		tst	r2, #1
 2455 0040 10D0     		beq	.L195
1246:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 2456              		.loc 1 1246 7 is_stmt 1 view .LVU942
1246:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 2457              		.loc 1 1246 12 is_stmt 0 view .LVU943
 2458 0042 FFF7FEFF 		bl	HAL_GetTick
 2459              	.LVL159:
1246:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 2460              		.loc 1 1246 27 discriminator 1 view .LVU944
 2461 0046 431B     		subs	r3, r0, r5
1246:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 2462              		.loc 1 1246 9 discriminator 1 view .LVU945
 2463 0048 052B     		cmp	r3, #5
 2464 004a F5D9     		bls	.L191
1249:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2465              		.loc 1 1249 9 is_stmt 1 view .LVU946
1249:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2466              		.loc 1 1249 14 is_stmt 0 view .LVU947
 2467 004c A36E     		ldr	r3, [r4, #104]
1249:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2468              		.loc 1 1249 26 view .LVU948
 2469 004e 43F04003 		orr	r3, r3, #64
 2470 0052 A366     		str	r3, [r4, #104]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 92


1252:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2471              		.loc 1 1252 9 is_stmt 1 view .LVU949
1252:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2472              		.loc 1 1252 9 view .LVU950
 2473 0054 0023     		movs	r3, #0
 2474 0056 84F83C30 		strb	r3, [r4, #60]
1252:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2475              		.loc 1 1252 9 view .LVU951
1255:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2476              		.loc 1 1255 9 view .LVU952
1255:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2477              		.loc 1 1255 22 is_stmt 0 view .LVU953
 2478 005a 0323     		movs	r3, #3
 2479 005c 84F83D30 		strb	r3, [r4, #61]
1257:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 2480              		.loc 1 1257 9 is_stmt 1 view .LVU954
1257:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 2481              		.loc 1 1257 16 is_stmt 0 view .LVU955
 2482 0060 0120     		movs	r0, #1
 2483 0062 DEE7     		b	.L189
 2484              	.L195:
1262:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2485              		.loc 1 1262 5 is_stmt 1 view .LVU956
 2486 0064 1F22     		movs	r2, #31
 2487 0066 5A60     		str	r2, [r3, #4]
1265:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2488              		.loc 1 1265 5 view .LVU957
1265:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2489              		.loc 1 1265 5 view .LVU958
 2490 0068 0020     		movs	r0, #0
 2491 006a 84F83C00 		strb	r0, [r4, #60]
1265:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2492              		.loc 1 1265 5 view .LVU959
1268:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2493              		.loc 1 1268 5 view .LVU960
1268:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2494              		.loc 1 1268 18 is_stmt 0 view .LVU961
 2495 006e 0123     		movs	r3, #1
 2496 0070 84F83D30 		strb	r3, [r4, #61]
1271:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 2497              		.loc 1 1271 3 is_stmt 1 view .LVU962
1271:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 2498              		.loc 1 1271 10 is_stmt 0 view .LVU963
 2499 0074 D5E7     		b	.L189
 2500              	.LVL160:
 2501              	.L193:
1222:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2502              		.loc 1 1222 12 view .LVU964
 2503 0076 0120     		movs	r0, #1
 2504              	.LVL161:
1222:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2505              		.loc 1 1222 12 view .LVU965
 2506 0078 D3E7     		b	.L189
 2507              		.cfi_endproc
 2508              	.LFE347:
 2510              		.section	.text.HAL_MDMA_Abort_IT,"ax",%progbits
 2511              		.align	1
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 93


 2512              		.global	HAL_MDMA_Abort_IT
 2513              		.syntax unified
 2514              		.thumb
 2515              		.thumb_func
 2517              	HAL_MDMA_Abort_IT:
 2518              	.LVL162:
 2519              	.LFB348:
1281:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   /* Check the MDMA peripheral handle */
 2520              		.loc 1 1281 1 is_stmt 1 view -0
 2521              		.cfi_startproc
 2522              		@ args = 0, pretend = 0, frame = 0
 2523              		@ frame_needed = 0, uses_anonymous_args = 0
 2524              		@ link register save eliminated.
1283:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2525              		.loc 1 1283 3 view .LVU967
1283:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2526              		.loc 1 1283 5 is_stmt 0 view .LVU968
 2527 0000 88B1     		cbz	r0, .L199
1288:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2528              		.loc 1 1288 3 is_stmt 1 view .LVU969
1288:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2529              		.loc 1 1288 34 is_stmt 0 view .LVU970
 2530 0002 90F83D20 		ldrb	r2, [r0, #61]	@ zero_extendqisi2
1288:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2531              		.loc 1 1288 5 view .LVU971
 2532 0006 022A     		cmp	r2, #2
 2533 0008 03D0     		beq	.L198
1291:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2534              		.loc 1 1291 5 is_stmt 1 view .LVU972
1291:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2535              		.loc 1 1291 22 is_stmt 0 view .LVU973
 2536 000a 8022     		movs	r2, #128
 2537 000c 8266     		str	r2, [r0, #104]
1293:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2538              		.loc 1 1293 5 is_stmt 1 view .LVU974
1293:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2539              		.loc 1 1293 12 is_stmt 0 view .LVU975
 2540 000e 0120     		movs	r0, #1
 2541              	.LVL163:
1293:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2542              		.loc 1 1293 12 view .LVU976
 2543 0010 7047     		bx	lr
 2544              	.LVL164:
 2545              	.L198:
1298:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2546              		.loc 1 1298 5 is_stmt 1 view .LVU977
1298:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2547              		.loc 1 1298 18 is_stmt 0 view .LVU978
 2548 0012 0422     		movs	r2, #4
 2549 0014 80F83D20 		strb	r2, [r0, #61]
1301:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2550              		.loc 1 1301 5 is_stmt 1 view .LVU979
 2551 0018 0268     		ldr	r2, [r0]
 2552 001a D368     		ldr	r3, [r2, #12]
 2553 001c 23F00103 		bic	r3, r3, #1
 2554 0020 D360     		str	r3, [r2, #12]
1304:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 94


 2555              		.loc 1 1304 3 view .LVU980
1304:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 2556              		.loc 1 1304 10 is_stmt 0 view .LVU981
 2557 0022 0020     		movs	r0, #0
 2558              	.LVL165:
1304:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 2559              		.loc 1 1304 10 view .LVU982
 2560 0024 7047     		bx	lr
 2561              	.LVL166:
 2562              	.L199:
1285:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2563              		.loc 1 1285 12 view .LVU983
 2564 0026 0120     		movs	r0, #1
 2565              	.LVL167:
1305:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2566              		.loc 1 1305 1 view .LVU984
 2567 0028 7047     		bx	lr
 2568              		.cfi_endproc
 2569              	.LFE348:
 2571              		.section	.text.HAL_MDMA_PollForTransfer,"ax",%progbits
 2572              		.align	1
 2573              		.global	HAL_MDMA_PollForTransfer
 2574              		.syntax unified
 2575              		.thumb
 2576              		.thumb_func
 2578              	HAL_MDMA_PollForTransfer:
 2579              	.LVL168:
 2580              	.LFB349:
1316:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t levelFlag, errorFlag;
 2581              		.loc 1 1316 1 is_stmt 1 view -0
 2582              		.cfi_startproc
 2583              		@ args = 0, pretend = 0, frame = 0
 2584              		@ frame_needed = 0, uses_anonymous_args = 0
1317:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t tickstart;
 2585              		.loc 1 1317 3 view .LVU986
1318:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2586              		.loc 1 1318 3 view .LVU987
1321:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2587              		.loc 1 1321 3 view .LVU988
1324:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2588              		.loc 1 1324 3 view .LVU989
1324:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2589              		.loc 1 1324 5 is_stmt 0 view .LVU990
 2590 0000 0028     		cmp	r0, #0
 2591 0002 00F08880 		beq	.L220
1316:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t levelFlag, errorFlag;
 2592              		.loc 1 1316 1 view .LVU991
 2593 0006 2DE9F843 		push	{r3, r4, r5, r6, r7, r8, r9, lr}
 2594              		.cfi_def_cfa_offset 32
 2595              		.cfi_offset 3, -32
 2596              		.cfi_offset 4, -28
 2597              		.cfi_offset 5, -24
 2598              		.cfi_offset 6, -20
 2599              		.cfi_offset 7, -16
 2600              		.cfi_offset 8, -12
 2601              		.cfi_offset 9, -8
 2602              		.cfi_offset 14, -4
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 95


 2603 000a 0F46     		mov	r7, r1
 2604 000c 1646     		mov	r6, r2
 2605 000e 0546     		mov	r5, r0
1329:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2606              		.loc 1 1329 3 is_stmt 1 view .LVU992
1329:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2607              		.loc 1 1329 34 is_stmt 0 view .LVU993
 2608 0010 90F83D30 		ldrb	r3, [r0, #61]	@ zero_extendqisi2
1329:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2609              		.loc 1 1329 5 view .LVU994
 2610 0014 022B     		cmp	r3, #2
 2611 0016 04D0     		beq	.L202
1332:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2612              		.loc 1 1332 5 is_stmt 1 view .LVU995
1332:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2613              		.loc 1 1332 22 is_stmt 0 view .LVU996
 2614 0018 8023     		movs	r3, #128
 2615 001a 8366     		str	r3, [r0, #104]
1334:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2616              		.loc 1 1334 5 is_stmt 1 view .LVU997
1334:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2617              		.loc 1 1334 12 is_stmt 0 view .LVU998
 2618 001c 0120     		movs	r0, #1
 2619              	.LVL169:
 2620              	.L201:
1454:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2621              		.loc 1 1454 1 view .LVU999
 2622 001e BDE8F883 		pop	{r3, r4, r5, r6, r7, r8, r9, pc}
 2623              	.LVL170:
 2624              	.L202:
1338:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****                (CompleteLevel == HAL_MDMA_BUFFER_TRANSFER)? MDMA_FLAG_BFTC : \
 2625              		.loc 1 1338 3 is_stmt 1 view .LVU1000
 2626 0022 0129     		cmp	r1, #1
 2627 0024 24D0     		beq	.L221
 2628 0026 0229     		cmp	r1, #2
 2629 0028 25D0     		beq	.L222
 2630 002a 39BB     		cbnz	r1, .L223
1329:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2631              		.loc 1 1329 5 is_stmt 0 view .LVU1001
 2632 002c 4FF00208 		mov	r8, #2
 2633              	.L203:
 2634              	.LVL171:
1345:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2635              		.loc 1 1345 3 is_stmt 1 view .LVU1002
1345:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2636              		.loc 1 1345 15 is_stmt 0 view .LVU1003
 2637 0030 FFF7FEFF 		bl	HAL_GetTick
 2638              	.LVL172:
1345:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2639              		.loc 1 1345 15 view .LVU1004
 2640 0034 8146     		mov	r9, r0
 2641              	.LVL173:
1347:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2642              		.loc 1 1347 3 is_stmt 1 view .LVU1005
 2643              	.L212:
1347:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2644              		.loc 1 1347 47 view .LVU1006
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 96


1347:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2645              		.loc 1 1347 9 is_stmt 0 view .LVU1007
 2646 0036 2B68     		ldr	r3, [r5]
 2647 0038 1C68     		ldr	r4, [r3]
1347:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2648              		.loc 1 1347 47 view .LVU1008
 2649 003a 14EA080F 		tst	r4, r8
 2650 003e 4ED1     		bne	.L229
1349:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2651              		.loc 1 1349 5 is_stmt 1 view .LVU1009
1349:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2652              		.loc 1 1349 9 is_stmt 0 view .LVU1010
 2653 0040 1C68     		ldr	r4, [r3]
1349:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2654              		.loc 1 1349 7 view .LVU1011
 2655 0042 14F0010F 		tst	r4, #1
 2656 0046 1CD1     		bne	.L230
1403:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2657              		.loc 1 1403 5 is_stmt 1 view .LVU1012
1403:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 2658              		.loc 1 1403 7 is_stmt 0 view .LVU1013
 2659 0048 B6F1FF3F 		cmp	r6, #-1
 2660 004c F3D0     		beq	.L212
1405:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 2661              		.loc 1 1405 7 is_stmt 1 view .LVU1014
1405:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 2662              		.loc 1 1405 12 is_stmt 0 view .LVU1015
 2663 004e FFF7FEFF 		bl	HAL_GetTick
 2664              	.LVL174:
1405:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 2665              		.loc 1 1405 26 discriminator 1 view .LVU1016
 2666 0052 A0EB0900 		sub	r0, r0, r9
1405:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 2667              		.loc 1 1405 9 discriminator 1 view .LVU1017
 2668 0056 B042     		cmp	r0, r6
 2669 0058 01D8     		bhi	.L213
1405:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 2670              		.loc 1 1405 51 discriminator 1 view .LVU1018
 2671 005a 002E     		cmp	r6, #0
 2672 005c EBD1     		bne	.L212
 2673              	.L213:
1408:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2674              		.loc 1 1408 9 is_stmt 1 view .LVU1019
1408:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2675              		.loc 1 1408 14 is_stmt 0 view .LVU1020
 2676 005e AB6E     		ldr	r3, [r5, #104]
1408:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2677              		.loc 1 1408 26 view .LVU1021
 2678 0060 43F04003 		orr	r3, r3, #64
 2679 0064 AB66     		str	r3, [r5, #104]
1410:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2680              		.loc 1 1410 9 is_stmt 1 view .LVU1022
1410:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2681              		.loc 1 1410 16 is_stmt 0 view .LVU1023
 2682 0066 2846     		mov	r0, r5
 2683 0068 FFF7FEFF 		bl	HAL_MDMA_Abort
 2684              	.LVL175:
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 97


1419:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 2685              		.loc 1 1419 9 is_stmt 1 view .LVU1024
1419:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 2686              		.loc 1 1419 16 is_stmt 0 view .LVU1025
 2687 006c 0120     		movs	r0, #1
 2688 006e D6E7     		b	.L201
 2689              	.LVL176:
 2690              	.L221:
1329:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2691              		.loc 1 1329 5 view .LVU1026
 2692 0070 4FF01008 		mov	r8, #16
 2693 0074 DCE7     		b	.L203
 2694              	.L222:
 2695 0076 4FF00808 		mov	r8, #8
 2696 007a D9E7     		b	.L203
 2697              	.L223:
 2698 007c 4FF00408 		mov	r8, #4
 2699 0080 D6E7     		b	.L203
 2700              	.LVL177:
 2701              	.L230:
1352:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2702              		.loc 1 1352 7 is_stmt 1 view .LVU1027
1352:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2703              		.loc 1 1352 17 is_stmt 0 view .LVU1028
 2704 0082 9B68     		ldr	r3, [r3, #8]
 2705              	.LVL178:
1354:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 2706              		.loc 1 1354 7 is_stmt 1 view .LVU1029
1354:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 2707              		.loc 1 1354 9 is_stmt 0 view .LVU1030
 2708 0084 13F0800F 		tst	r3, #128
 2709 0088 24D1     		bne	.L206
1357:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 2710              		.loc 1 1357 9 is_stmt 1 view .LVU1031
1357:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 2711              		.loc 1 1357 14 is_stmt 0 view .LVU1032
 2712 008a AA6E     		ldr	r2, [r5, #104]
1357:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 2713              		.loc 1 1357 26 view .LVU1033
 2714 008c 42F00102 		orr	r2, r2, #1
 2715 0090 AA66     		str	r2, [r5, #104]
 2716              	.L207:
1365:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 2717              		.loc 1 1365 7 is_stmt 1 view .LVU1034
1365:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 2718              		.loc 1 1365 9 is_stmt 0 view .LVU1035
 2719 0092 13F4007F 		tst	r3, #512
 2720 0096 03D0     		beq	.L208
1368:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 2721              		.loc 1 1368 9 is_stmt 1 view .LVU1036
1368:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 2722              		.loc 1 1368 14 is_stmt 0 view .LVU1037
 2723 0098 AA6E     		ldr	r2, [r5, #104]
1368:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 2724              		.loc 1 1368 26 view .LVU1038
 2725 009a 42F00402 		orr	r2, r2, #4
 2726 009e AA66     		str	r2, [r5, #104]
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 98


 2727              	.L208:
1371:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 2728              		.loc 1 1371 7 is_stmt 1 view .LVU1039
1371:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 2729              		.loc 1 1371 9 is_stmt 0 view .LVU1040
 2730 00a0 13F4807F 		tst	r3, #256
 2731 00a4 03D0     		beq	.L209
1374:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 2732              		.loc 1 1374 9 is_stmt 1 view .LVU1041
1374:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 2733              		.loc 1 1374 14 is_stmt 0 view .LVU1042
 2734 00a6 AA6E     		ldr	r2, [r5, #104]
1374:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 2735              		.loc 1 1374 26 view .LVU1043
 2736 00a8 42F00802 		orr	r2, r2, #8
 2737 00ac AA66     		str	r2, [r5, #104]
 2738              	.L209:
1377:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 2739              		.loc 1 1377 7 is_stmt 1 view .LVU1044
1377:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 2740              		.loc 1 1377 9 is_stmt 0 view .LVU1045
 2741 00ae 13F4806F 		tst	r3, #1024
 2742 00b2 03D0     		beq	.L210
1380:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 2743              		.loc 1 1380 9 is_stmt 1 view .LVU1046
1380:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 2744              		.loc 1 1380 14 is_stmt 0 view .LVU1047
 2745 00b4 AA6E     		ldr	r2, [r5, #104]
1380:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 2746              		.loc 1 1380 26 view .LVU1048
 2747 00b6 42F01002 		orr	r2, r2, #16
 2748 00ba AA66     		str	r2, [r5, #104]
 2749              	.L210:
1383:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 2750              		.loc 1 1383 7 is_stmt 1 view .LVU1049
1383:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 2751              		.loc 1 1383 9 is_stmt 0 view .LVU1050
 2752 00bc 13F4006F 		tst	r3, #2048
 2753 00c0 03D0     		beq	.L211
1386:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 2754              		.loc 1 1386 9 is_stmt 1 view .LVU1051
1386:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 2755              		.loc 1 1386 14 is_stmt 0 view .LVU1052
 2756 00c2 AB6E     		ldr	r3, [r5, #104]
 2757              	.LVL179:
1386:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 2758              		.loc 1 1386 26 view .LVU1053
 2759 00c4 43F02003 		orr	r3, r3, #32
 2760 00c8 AB66     		str	r3, [r5, #104]
 2761              	.L211:
1389:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2762              		.loc 1 1389 7 is_stmt 1 view .LVU1054
1389:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2763              		.loc 1 1389 14 is_stmt 0 view .LVU1055
 2764 00ca 2846     		mov	r0, r5
 2765 00cc FFF7FEFF 		bl	HAL_MDMA_Abort
 2766              	.LVL180:
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 99


1398:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2767              		.loc 1 1398 7 is_stmt 1 view .LVU1056
1398:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2768              		.loc 1 1398 14 is_stmt 0 view .LVU1057
 2769 00d0 0120     		movs	r0, #1
 2770 00d2 A4E7     		b	.L201
 2771              	.LVL181:
 2772              	.L206:
1362:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 2773              		.loc 1 1362 9 is_stmt 1 view .LVU1058
1362:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 2774              		.loc 1 1362 14 is_stmt 0 view .LVU1059
 2775 00d4 AA6E     		ldr	r2, [r5, #104]
1362:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 2776              		.loc 1 1362 26 view .LVU1060
 2777 00d6 42F00202 		orr	r2, r2, #2
 2778 00da AA66     		str	r2, [r5, #104]
 2779 00dc D9E7     		b	.L207
 2780              	.LVL182:
 2781              	.L229:
1425:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2782              		.loc 1 1425 3 is_stmt 1 view .LVU1061
 2783 00de 032F     		cmp	r7, #3
 2784 00e0 1BD8     		bhi	.L224
 2785 00e2 DFE807F0 		tbb	[pc, r7]
 2786              	.L216:
 2787 00e6 0E       		.byte	(.L219-.L216)/2
 2788 00e7 02       		.byte	(.L218-.L216)/2
 2789 00e8 06       		.byte	(.L217-.L216)/2
 2790 00e9 0A       		.byte	(.L215-.L216)/2
 2791              		.p2align 1
 2792              	.L218:
1427:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2793              		.loc 1 1427 5 view .LVU1062
 2794 00ea 1022     		movs	r2, #16
 2795 00ec 5A60     		str	r2, [r3, #4]
1453:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 2796              		.loc 1 1453 10 is_stmt 0 view .LVU1063
 2797 00ee 0020     		movs	r0, #0
 2798 00f0 95E7     		b	.L201
 2799              	.L217:
1432:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2800              		.loc 1 1432 5 is_stmt 1 view .LVU1064
 2801 00f2 1822     		movs	r2, #24
 2802 00f4 5A60     		str	r2, [r3, #4]
1453:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 2803              		.loc 1 1453 10 is_stmt 0 view .LVU1065
 2804 00f6 0020     		movs	r0, #0
 2805 00f8 91E7     		b	.L201
 2806              	.L215:
1437:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2807              		.loc 1 1437 5 is_stmt 1 view .LVU1066
 2808 00fa 1C22     		movs	r2, #28
 2809 00fc 5A60     		str	r2, [r3, #4]
1453:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 2810              		.loc 1 1453 10 is_stmt 0 view .LVU1067
 2811 00fe 0020     		movs	r0, #0
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 100


 2812 0100 8DE7     		b	.L201
 2813              	.L219:
1441:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2814              		.loc 1 1441 5 is_stmt 1 view .LVU1068
 2815 0102 1E22     		movs	r2, #30
 2816 0104 5A60     		str	r2, [r3, #4]
1444:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2817              		.loc 1 1444 5 view .LVU1069
1444:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2818              		.loc 1 1444 5 view .LVU1070
 2819 0106 0023     		movs	r3, #0
 2820 0108 85F83C30 		strb	r3, [r5, #60]
1444:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2821              		.loc 1 1444 5 view .LVU1071
1446:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2822              		.loc 1 1446 5 view .LVU1072
1446:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2823              		.loc 1 1446 18 is_stmt 0 view .LVU1073
 2824 010c 0123     		movs	r3, #1
 2825 010e 85F83D30 		strb	r3, [r5, #61]
1453:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 2826              		.loc 1 1453 10 view .LVU1074
 2827 0112 3846     		mov	r0, r7
 2828 0114 83E7     		b	.L201
 2829              	.LVL183:
 2830              	.L220:
 2831              		.cfi_def_cfa_offset 0
 2832              		.cfi_restore 3
 2833              		.cfi_restore 4
 2834              		.cfi_restore 5
 2835              		.cfi_restore 6
 2836              		.cfi_restore 7
 2837              		.cfi_restore 8
 2838              		.cfi_restore 9
 2839              		.cfi_restore 14
1326:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2840              		.loc 1 1326 12 view .LVU1075
 2841 0116 0120     		movs	r0, #1
 2842              	.LVL184:
1454:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2843              		.loc 1 1454 1 view .LVU1076
 2844 0118 7047     		bx	lr
 2845              	.LVL185:
 2846              	.L224:
 2847              		.cfi_def_cfa_offset 32
 2848              		.cfi_offset 3, -32
 2849              		.cfi_offset 4, -28
 2850              		.cfi_offset 5, -24
 2851              		.cfi_offset 6, -20
 2852              		.cfi_offset 7, -16
 2853              		.cfi_offset 8, -12
 2854              		.cfi_offset 9, -8
 2855              		.cfi_offset 14, -4
1347:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2856              		.loc 1 1347 47 view .LVU1077
 2857 011a 0120     		movs	r0, #1
 2858 011c 7FE7     		b	.L201
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 101


 2859              		.cfi_endproc
 2860              	.LFE349:
 2862              		.section	.text.HAL_MDMA_GenerateSWRequest,"ax",%progbits
 2863              		.align	1
 2864              		.global	HAL_MDMA_GenerateSWRequest
 2865              		.syntax unified
 2866              		.thumb
 2867              		.thumb_func
 2869              	HAL_MDMA_GenerateSWRequest:
 2870              	.LVL186:
 2871              	.LFB350:
1463:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t request_mode;
 2872              		.loc 1 1463 1 is_stmt 1 view -0
 2873              		.cfi_startproc
 2874              		@ args = 0, pretend = 0, frame = 0
 2875              		@ frame_needed = 0, uses_anonymous_args = 0
 2876              		@ link register save eliminated.
1464:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2877              		.loc 1 1464 3 view .LVU1079
1467:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2878              		.loc 1 1467 3 view .LVU1080
1467:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2879              		.loc 1 1467 5 is_stmt 0 view .LVU1081
 2880 0000 0146     		mov	r1, r0
 2881 0002 D8B1     		cbz	r0, .L236
1473:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2882              		.loc 1 1473 3 is_stmt 1 view .LVU1082
1473:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2883              		.loc 1 1473 23 is_stmt 0 view .LVU1083
 2884 0004 0368     		ldr	r3, [r0]
1473:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2885              		.loc 1 1473 33 view .LVU1084
 2886 0006 1A69     		ldr	r2, [r3, #16]
1473:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2887              		.loc 1 1473 16 view .LVU1085
 2888 0008 02F08042 		and	r2, r2, #1073741824
 2889              	.LVL187:
1475:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2890              		.loc 1 1475 3 is_stmt 1 view .LVU1086
1475:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2891              		.loc 1 1475 22 is_stmt 0 view .LVU1087
 2892 000c D868     		ldr	r0, [r3, #12]
 2893              	.LVL188:
1475:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2894              		.loc 1 1475 5 view .LVU1088
 2895 000e 10F0010F 		tst	r0, #1
 2896 0012 09D0     		beq	.L237
1482:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2897              		.loc 1 1482 8 is_stmt 1 view .LVU1089
1482:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2898              		.loc 1 1482 28 is_stmt 0 view .LVU1090
 2899 0014 1868     		ldr	r0, [r3]
1482:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2900              		.loc 1 1482 10 view .LVU1091
 2901 0016 10F4803F 		tst	r0, #65536
 2902 001a 00D1     		bne	.L234
1482:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 102


 2903              		.loc 1 1482 61 discriminator 1 view .LVU1092
 2904 001c 42B9     		cbnz	r2, .L235
 2905              	.L234:
1485:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2906              		.loc 1 1485 5 is_stmt 1 view .LVU1093
1485:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2907              		.loc 1 1485 22 is_stmt 0 view .LVU1094
 2908 001e 4FF48073 		mov	r3, #256
 2909 0022 8B66     		str	r3, [r1, #104]
1487:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2910              		.loc 1 1487 5 is_stmt 1 view .LVU1095
1487:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2911              		.loc 1 1487 12 is_stmt 0 view .LVU1096
 2912 0024 0120     		movs	r0, #1
 2913 0026 7047     		bx	lr
 2914              	.L237:
1478:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2915              		.loc 1 1478 5 is_stmt 1 view .LVU1097
1478:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2916              		.loc 1 1478 22 is_stmt 0 view .LVU1098
 2917 0028 8023     		movs	r3, #128
 2918 002a 8B66     		str	r3, [r1, #104]
1480:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2919              		.loc 1 1480 5 is_stmt 1 view .LVU1099
1480:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2920              		.loc 1 1480 12 is_stmt 0 view .LVU1100
 2921 002c 0120     		movs	r0, #1
 2922 002e 7047     		bx	lr
 2923              	.L235:
1492:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2924              		.loc 1 1492 5 is_stmt 1 view .LVU1101
1492:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2925              		.loc 1 1492 20 is_stmt 0 view .LVU1102
 2926 0030 DA68     		ldr	r2, [r3, #12]
 2927              	.LVL189:
1492:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2928              		.loc 1 1492 26 view .LVU1103
 2929 0032 42F48032 		orr	r2, r2, #65536
 2930 0036 DA60     		str	r2, [r3, #12]
1494:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2931              		.loc 1 1494 5 is_stmt 1 view .LVU1104
1494:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2932              		.loc 1 1494 12 is_stmt 0 view .LVU1105
 2933 0038 0020     		movs	r0, #0
 2934 003a 7047     		bx	lr
 2935              	.LVL190:
 2936              	.L236:
1469:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   }
 2937              		.loc 1 1469 12 view .LVU1106
 2938 003c 0120     		movs	r0, #1
 2939              	.LVL191:
1496:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2940              		.loc 1 1496 1 view .LVU1107
 2941 003e 7047     		bx	lr
 2942              		.cfi_endproc
 2943              	.LFE350:
 2945              		.section	.text.HAL_MDMA_IRQHandler,"ax",%progbits
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 103


 2946              		.align	1
 2947              		.global	HAL_MDMA_IRQHandler
 2948              		.syntax unified
 2949              		.thumb
 2950              		.thumb_func
 2952              	HAL_MDMA_IRQHandler:
 2953              	.LVL192:
 2954              	.LFB351:
1505:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __IO uint32_t count = 0;
 2955              		.loc 1 1505 1 is_stmt 1 view -0
 2956              		.cfi_startproc
 2957              		@ args = 0, pretend = 0, frame = 8
 2958              		@ frame_needed = 0, uses_anonymous_args = 0
1505:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   __IO uint32_t count = 0;
 2959              		.loc 1 1505 1 is_stmt 0 view .LVU1109
 2960 0000 30B5     		push	{r4, r5, lr}
 2961              		.cfi_def_cfa_offset 12
 2962              		.cfi_offset 4, -12
 2963              		.cfi_offset 5, -8
 2964              		.cfi_offset 14, -4
 2965 0002 83B0     		sub	sp, sp, #12
 2966              		.cfi_def_cfa_offset 24
1506:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t timeout = SystemCoreClock / 9600U;
 2967              		.loc 1 1506 3 is_stmt 1 view .LVU1110
1506:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   uint32_t timeout = SystemCoreClock / 9600U;
 2968              		.loc 1 1506 17 is_stmt 0 view .LVU1111
 2969 0004 0023     		movs	r3, #0
 2970 0006 0193     		str	r3, [sp, #4]
1507:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2971              		.loc 1 1507 3 is_stmt 1 view .LVU1112
1507:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2972              		.loc 1 1507 38 is_stmt 0 view .LVU1113
 2973 0008 664B     		ldr	r3, .L259
 2974 000a 1D68     		ldr	r5, [r3]
1507:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2975              		.loc 1 1507 12 view .LVU1114
 2976 000c 664B     		ldr	r3, .L259+4
 2977 000e A3FB0535 		umull	r3, r5, r3, r5
 2978              	.LVL193:
1509:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 2979              		.loc 1 1509 3 is_stmt 1 view .LVU1115
1512:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((MDMA->GISR0 & generalIntFlag) == 0U)
 2980              		.loc 1 1512 3 view .LVU1116
1512:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((MDMA->GISR0 & generalIntFlag) == 0U)
 2981              		.loc 1 1512 46 is_stmt 0 view .LVU1117
 2982 0012 0168     		ldr	r1, [r0]
1512:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((MDMA->GISR0 & generalIntFlag) == 0U)
 2983              		.loc 1 1512 57 view .LVU1118
 2984 0014 654B     		ldr	r3, .L259+8
 2985 0016 0B44     		add	r3, r3, r1
1512:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((MDMA->GISR0 & generalIntFlag) == 0U)
 2986              		.loc 1 1512 109 view .LVU1119
 2987 0018 C3F38413 		ubfx	r3, r3, #6, #5
1512:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   if((MDMA->GISR0 & generalIntFlag) == 0U)
 2988              		.loc 1 1512 18 view .LVU1120
 2989 001c 0122     		movs	r2, #1
 2990 001e 02FA03F3 		lsl	r3, r2, r3
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 104


 2991              	.LVL194:
1513:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2992              		.loc 1 1513 3 is_stmt 1 view .LVU1121
1513:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2993              		.loc 1 1513 11 is_stmt 0 view .LVU1122
 2994 0022 4FF0A442 		mov	r2, #1375731712
 2995 0026 1268     		ldr	r2, [r2]
1513:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 2996              		.loc 1 1513 5 view .LVU1123
 2997 0028 1A42     		tst	r2, r3
 2998 002a 00F0A480 		beq	.L238
 2999 002e 0446     		mov	r4, r0
 3000 0030 AD0A     		lsrs	r5, r5, #10
 3001              	.LVL195:
1519:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 3002              		.loc 1 1519 3 is_stmt 1 view .LVU1124
1519:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 3003              		.loc 1 1519 7 is_stmt 0 view .LVU1125
 3004 0032 0B68     		ldr	r3, [r1]
 3005              	.LVL196:
1519:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 3006              		.loc 1 1519 5 view .LVU1126
 3007 0034 13F0010F 		tst	r3, #1
 3008 0038 2FD0     		beq	.L240
1521:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 3009              		.loc 1 1521 5 is_stmt 1 view .LVU1127
1521:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 3010              		.loc 1 1521 8 is_stmt 0 view .LVU1128
 3011 003a CB68     		ldr	r3, [r1, #12]
1521:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 3012              		.loc 1 1521 7 view .LVU1129
 3013 003c 13F0020F 		tst	r3, #2
 3014 0040 2BD0     		beq	.L240
1524:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3015              		.loc 1 1524 7 is_stmt 1 view .LVU1130
 3016 0042 CB68     		ldr	r3, [r1, #12]
 3017 0044 23F00203 		bic	r3, r3, #2
 3018 0048 CB60     		str	r3, [r1, #12]
1527:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3019              		.loc 1 1527 7 view .LVU1131
1527:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3020              		.loc 1 1527 24 is_stmt 0 view .LVU1132
 3021 004a 0268     		ldr	r2, [r0]
1527:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3022              		.loc 1 1527 17 view .LVU1133
 3023 004c 9368     		ldr	r3, [r2, #8]
 3024              	.LVL197:
1529:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3025              		.loc 1 1529 7 is_stmt 1 view .LVU1134
1529:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3026              		.loc 1 1529 9 is_stmt 0 view .LVU1135
 3027 004e 13F0800F 		tst	r3, #128
 3028 0052 40F09280 		bne	.L241
1532:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3029              		.loc 1 1532 9 is_stmt 1 view .LVU1136
1532:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3030              		.loc 1 1532 14 is_stmt 0 view .LVU1137
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 105


 3031 0056 816E     		ldr	r1, [r0, #104]
 3032              	.LVL198:
1532:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3033              		.loc 1 1532 26 view .LVU1138
 3034 0058 41F00101 		orr	r1, r1, #1
 3035 005c 8166     		str	r1, [r0, #104]
 3036              	.L242:
1540:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3037              		.loc 1 1540 7 is_stmt 1 view .LVU1139
1540:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3038              		.loc 1 1540 9 is_stmt 0 view .LVU1140
 3039 005e 13F4007F 		tst	r3, #512
 3040 0062 03D0     		beq	.L243
1543:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3041              		.loc 1 1543 9 is_stmt 1 view .LVU1141
1543:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3042              		.loc 1 1543 14 is_stmt 0 view .LVU1142
 3043 0064 A16E     		ldr	r1, [r4, #104]
1543:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3044              		.loc 1 1543 26 view .LVU1143
 3045 0066 41F00401 		orr	r1, r1, #4
 3046 006a A166     		str	r1, [r4, #104]
 3047              	.L243:
1546:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3048              		.loc 1 1546 7 is_stmt 1 view .LVU1144
1546:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3049              		.loc 1 1546 9 is_stmt 0 view .LVU1145
 3050 006c 13F4807F 		tst	r3, #256
 3051 0070 03D0     		beq	.L244
1549:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3052              		.loc 1 1549 9 is_stmt 1 view .LVU1146
1549:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3053              		.loc 1 1549 14 is_stmt 0 view .LVU1147
 3054 0072 A16E     		ldr	r1, [r4, #104]
1549:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3055              		.loc 1 1549 26 view .LVU1148
 3056 0074 41F00801 		orr	r1, r1, #8
 3057 0078 A166     		str	r1, [r4, #104]
 3058              	.L244:
1552:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3059              		.loc 1 1552 7 is_stmt 1 view .LVU1149
1552:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3060              		.loc 1 1552 9 is_stmt 0 view .LVU1150
 3061 007a 13F4806F 		tst	r3, #1024
 3062 007e 03D0     		beq	.L245
1555:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3063              		.loc 1 1555 9 is_stmt 1 view .LVU1151
1555:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3064              		.loc 1 1555 14 is_stmt 0 view .LVU1152
 3065 0080 A16E     		ldr	r1, [r4, #104]
1555:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3066              		.loc 1 1555 26 view .LVU1153
 3067 0082 41F01001 		orr	r1, r1, #16
 3068 0086 A166     		str	r1, [r4, #104]
 3069              	.L245:
1558:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3070              		.loc 1 1558 7 is_stmt 1 view .LVU1154
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 106


1558:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3071              		.loc 1 1558 9 is_stmt 0 view .LVU1155
 3072 0088 13F4006F 		tst	r3, #2048
 3073 008c 03D0     		beq	.L246
1561:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3074              		.loc 1 1561 9 is_stmt 1 view .LVU1156
1561:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3075              		.loc 1 1561 14 is_stmt 0 view .LVU1157
 3076 008e A36E     		ldr	r3, [r4, #104]
 3077              	.LVL199:
1561:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3078              		.loc 1 1561 26 view .LVU1158
 3079 0090 43F02003 		orr	r3, r3, #32
 3080 0094 A366     		str	r3, [r4, #104]
 3081              	.L246:
1565:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 3082              		.loc 1 1565 7 is_stmt 1 view .LVU1159
 3083 0096 0123     		movs	r3, #1
1565:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 3084              		.loc 1 1565 7 is_stmt 0 view .LVU1160
 3085 0098 5360     		str	r3, [r2, #4]
 3086              	.LVL200:
 3087              	.L240:
1570:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 3088              		.loc 1 1570 3 is_stmt 1 view .LVU1161
1570:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 3089              		.loc 1 1570 7 is_stmt 0 view .LVU1162
 3090 009a 2368     		ldr	r3, [r4]
 3091 009c 1A68     		ldr	r2, [r3]
1570:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 3092              		.loc 1 1570 5 view .LVU1163
 3093 009e 12F0100F 		tst	r2, #16
 3094 00a2 09D0     		beq	.L247
1572:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 3095              		.loc 1 1572 5 is_stmt 1 view .LVU1164
1572:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 3096              		.loc 1 1572 8 is_stmt 0 view .LVU1165
 3097 00a4 DA68     		ldr	r2, [r3, #12]
1572:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 3098              		.loc 1 1572 7 view .LVU1166
 3099 00a6 12F0200F 		tst	r2, #32
 3100 00aa 05D0     		beq	.L247
1575:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3101              		.loc 1 1575 7 is_stmt 1 view .LVU1167
 3102 00ac 1022     		movs	r2, #16
 3103 00ae 5A60     		str	r2, [r3, #4]
1577:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3104              		.loc 1 1577 7 view .LVU1168
1577:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3105              		.loc 1 1577 15 is_stmt 0 view .LVU1169
 3106 00b0 A36C     		ldr	r3, [r4, #72]
1577:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3107              		.loc 1 1577 9 view .LVU1170
 3108 00b2 0BB1     		cbz	r3, .L247
1580:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3109              		.loc 1 1580 9 is_stmt 1 view .LVU1171
 3110 00b4 2046     		mov	r0, r4
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 107


 3111              	.LVL201:
1580:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3112              		.loc 1 1580 9 is_stmt 0 view .LVU1172
 3113 00b6 9847     		blx	r3
 3114              	.LVL202:
 3115              	.L247:
1586:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 3116              		.loc 1 1586 3 is_stmt 1 view .LVU1173
1586:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 3117              		.loc 1 1586 7 is_stmt 0 view .LVU1174
 3118 00b8 2368     		ldr	r3, [r4]
 3119 00ba 1A68     		ldr	r2, [r3]
1586:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 3120              		.loc 1 1586 5 view .LVU1175
 3121 00bc 12F0080F 		tst	r2, #8
 3122 00c0 09D0     		beq	.L248
1588:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 3123              		.loc 1 1588 5 is_stmt 1 view .LVU1176
1588:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 3124              		.loc 1 1588 8 is_stmt 0 view .LVU1177
 3125 00c2 DA68     		ldr	r2, [r3, #12]
1588:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 3126              		.loc 1 1588 7 view .LVU1178
 3127 00c4 12F0100F 		tst	r2, #16
 3128 00c8 05D0     		beq	.L248
1591:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3129              		.loc 1 1591 7 is_stmt 1 view .LVU1179
 3130 00ca 0822     		movs	r2, #8
 3131 00cc 5A60     		str	r2, [r3, #4]
1593:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3132              		.loc 1 1593 7 view .LVU1180
1593:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3133              		.loc 1 1593 15 is_stmt 0 view .LVU1181
 3134 00ce E36C     		ldr	r3, [r4, #76]
1593:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3135              		.loc 1 1593 9 view .LVU1182
 3136 00d0 0BB1     		cbz	r3, .L248
1596:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3137              		.loc 1 1596 9 is_stmt 1 view .LVU1183
 3138 00d2 2046     		mov	r0, r4
 3139 00d4 9847     		blx	r3
 3140              	.LVL203:
 3141              	.L248:
1602:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 3142              		.loc 1 1602 3 view .LVU1184
1602:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 3143              		.loc 1 1602 7 is_stmt 0 view .LVU1185
 3144 00d6 2368     		ldr	r3, [r4]
 3145 00d8 1A68     		ldr	r2, [r3]
1602:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 3146              		.loc 1 1602 5 view .LVU1186
 3147 00da 12F0040F 		tst	r2, #4
 3148 00de 09D0     		beq	.L249
1604:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 3149              		.loc 1 1604 5 is_stmt 1 view .LVU1187
1604:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 3150              		.loc 1 1604 8 is_stmt 0 view .LVU1188
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 108


 3151 00e0 DA68     		ldr	r2, [r3, #12]
1604:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 3152              		.loc 1 1604 7 view .LVU1189
 3153 00e2 12F0080F 		tst	r2, #8
 3154 00e6 05D0     		beq	.L249
1607:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3155              		.loc 1 1607 7 is_stmt 1 view .LVU1190
 3156 00e8 0422     		movs	r2, #4
 3157 00ea 5A60     		str	r2, [r3, #4]
1609:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3158              		.loc 1 1609 7 view .LVU1191
1609:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3159              		.loc 1 1609 15 is_stmt 0 view .LVU1192
 3160 00ec 236D     		ldr	r3, [r4, #80]
1609:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3161              		.loc 1 1609 9 view .LVU1193
 3162 00ee 0BB1     		cbz	r3, .L249
1612:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3163              		.loc 1 1612 9 is_stmt 1 view .LVU1194
 3164 00f0 2046     		mov	r0, r4
 3165 00f2 9847     		blx	r3
 3166              	.LVL204:
 3167              	.L249:
1618:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 3168              		.loc 1 1618 3 view .LVU1195
1618:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 3169              		.loc 1 1618 7 is_stmt 0 view .LVU1196
 3170 00f4 2368     		ldr	r3, [r4]
 3171 00f6 1A68     		ldr	r2, [r3]
1618:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 3172              		.loc 1 1618 5 view .LVU1197
 3173 00f8 12F0020F 		tst	r2, #2
 3174 00fc 18D0     		beq	.L250
1620:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 3175              		.loc 1 1620 5 is_stmt 1 view .LVU1198
1620:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 3176              		.loc 1 1620 8 is_stmt 0 view .LVU1199
 3177 00fe DA68     		ldr	r2, [r3, #12]
1620:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 3178              		.loc 1 1620 7 view .LVU1200
 3179 0100 12F0040F 		tst	r2, #4
 3180 0104 14D0     		beq	.L250
1623:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3181              		.loc 1 1623 7 is_stmt 1 view .LVU1201
 3182 0106 DA68     		ldr	r2, [r3, #12]
 3183 0108 22F03E02 		bic	r2, r2, #62
 3184 010c DA60     		str	r2, [r3, #12]
1625:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3185              		.loc 1 1625 7 view .LVU1202
1625:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3186              		.loc 1 1625 39 is_stmt 0 view .LVU1203
 3187 010e 94F83D30 		ldrb	r3, [r4, #61]	@ zero_extendqisi2
1625:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3188              		.loc 1 1625 9 view .LVU1204
 3189 0112 042B     		cmp	r3, #4
 3190 0114 36D0     		beq	.L258
1641:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 109


 3191              		.loc 1 1641 7 is_stmt 1 view .LVU1205
 3192 0116 2368     		ldr	r3, [r4]
 3193 0118 0222     		movs	r2, #2
 3194 011a 5A60     		str	r2, [r3, #4]
1644:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3195              		.loc 1 1644 7 view .LVU1206
1644:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3196              		.loc 1 1644 7 view .LVU1207
 3197 011c 0023     		movs	r3, #0
 3198 011e 84F83C30 		strb	r3, [r4, #60]
1644:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3199              		.loc 1 1644 7 view .LVU1208
1647:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3200              		.loc 1 1647 7 view .LVU1209
1647:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3201              		.loc 1 1647 20 is_stmt 0 view .LVU1210
 3202 0122 0123     		movs	r3, #1
1647:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3203              		.loc 1 1647 20 view .LVU1211
 3204 0124 84F83D30 		strb	r3, [r4, #61]
1649:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3205              		.loc 1 1649 7 is_stmt 1 view .LVU1212
1649:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3206              		.loc 1 1649 15 is_stmt 0 view .LVU1213
 3207 0128 636C     		ldr	r3, [r4, #68]
1649:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3208              		.loc 1 1649 9 view .LVU1214
 3209 012a 0BB1     		cbz	r3, .L250
1652:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3210              		.loc 1 1652 9 is_stmt 1 view .LVU1215
 3211 012c 2046     		mov	r0, r4
 3212 012e 9847     		blx	r3
 3213              	.LVL205:
 3214              	.L250:
1658:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 3215              		.loc 1 1658 3 view .LVU1216
1658:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 3216              		.loc 1 1658 11 is_stmt 0 view .LVU1217
 3217 0130 A36E     		ldr	r3, [r4, #104]
1658:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   {
 3218              		.loc 1 1658 5 view .LVU1218
 3219 0132 03B3     		cbz	r3, .L238
1660:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3220              		.loc 1 1660 5 is_stmt 1 view .LVU1219
1660:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3221              		.loc 1 1660 18 is_stmt 0 view .LVU1220
 3222 0134 0423     		movs	r3, #4
 3223 0136 84F83D30 		strb	r3, [r4, #61]
1663:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3224              		.loc 1 1663 5 is_stmt 1 view .LVU1221
 3225 013a 2268     		ldr	r2, [r4]
 3226 013c D368     		ldr	r3, [r2, #12]
 3227 013e 23F00103 		bic	r3, r3, #1
 3228 0142 D360     		str	r3, [r2, #12]
 3229              	.L254:
1665:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 3230              		.loc 1 1665 5 view .LVU1222
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 110


1667:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3231              		.loc 1 1667 7 view .LVU1223
1667:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3232              		.loc 1 1667 11 is_stmt 0 view .LVU1224
 3233 0144 019B     		ldr	r3, [sp, #4]
 3234 0146 0133     		adds	r3, r3, #1
1667:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       {
 3235              		.loc 1 1667 10 view .LVU1225
 3236 0148 0193     		str	r3, [sp, #4]
 3237 014a AB42     		cmp	r3, r5
 3238 014c 04D8     		bhi	.L253
1672:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3239              		.loc 1 1672 48 is_stmt 1 view .LVU1226
1672:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3240              		.loc 1 1672 17 is_stmt 0 view .LVU1227
 3241 014e 2368     		ldr	r3, [r4]
1672:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3242              		.loc 1 1672 27 view .LVU1228
 3243 0150 DB68     		ldr	r3, [r3, #12]
1672:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3244              		.loc 1 1672 48 view .LVU1229
 3245 0152 13F0010F 		tst	r3, #1
 3246 0156 F5D1     		bne	.L254
 3247              	.L253:
1675:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3248              		.loc 1 1675 5 is_stmt 1 view .LVU1230
1675:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3249              		.loc 1 1675 5 view .LVU1231
 3250 0158 0023     		movs	r3, #0
 3251 015a 84F83C30 		strb	r3, [r4, #60]
1675:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3252              		.loc 1 1675 5 view .LVU1232
1677:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 3253              		.loc 1 1677 5 view .LVU1233
1677:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 3254              		.loc 1 1677 14 is_stmt 0 view .LVU1234
 3255 015e 2368     		ldr	r3, [r4]
1677:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 3256              		.loc 1 1677 24 view .LVU1235
 3257 0160 DB68     		ldr	r3, [r3, #12]
1677:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 3258              		.loc 1 1677 7 view .LVU1236
 3259 0162 13F0010F 		tst	r3, #1
 3260 0166 19D0     		beq	.L255
1680:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 3261              		.loc 1 1680 7 is_stmt 1 view .LVU1237
1680:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 3262              		.loc 1 1680 20 is_stmt 0 view .LVU1238
 3263 0168 0323     		movs	r3, #3
 3264 016a 84F83D30 		strb	r3, [r4, #61]
 3265              	.L256:
1689:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 3266              		.loc 1 1689 5 is_stmt 1 view .LVU1239
1689:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
 3267              		.loc 1 1689 14 is_stmt 0 view .LVU1240
 3268 016e 636D     		ldr	r3, [r4, #84]
1689:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     {
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 111


 3269              		.loc 1 1689 8 view .LVU1241
 3270 0170 0BB1     		cbz	r3, .L238
1692:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 3271              		.loc 1 1692 7 is_stmt 1 view .LVU1242
 3272 0172 2046     		mov	r0, r4
 3273 0174 9847     		blx	r3
 3274              	.LVL206:
 3275              	.L238:
1695:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3276              		.loc 1 1695 1 is_stmt 0 view .LVU1243
 3277 0176 03B0     		add	sp, sp, #12
 3278              		.cfi_remember_state
 3279              		.cfi_def_cfa_offset 12
 3280              		@ sp needed
 3281 0178 30BD     		pop	{r4, r5, pc}
 3282              	.LVL207:
 3283              	.L241:
 3284              		.cfi_restore_state
1537:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3285              		.loc 1 1537 9 is_stmt 1 view .LVU1244
1537:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3286              		.loc 1 1537 14 is_stmt 0 view .LVU1245
 3287 017a 816E     		ldr	r1, [r0, #104]
 3288              	.LVL208:
1537:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3289              		.loc 1 1537 26 view .LVU1246
 3290 017c 41F00201 		orr	r1, r1, #2
 3291 0180 8166     		str	r1, [r0, #104]
 3292 0182 6CE7     		b	.L242
 3293              	.LVL209:
 3294              	.L258:
1628:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3295              		.loc 1 1628 9 is_stmt 1 view .LVU1247
1628:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3296              		.loc 1 1628 9 view .LVU1248
 3297 0184 0023     		movs	r3, #0
 3298 0186 84F83C30 		strb	r3, [r4, #60]
1628:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3299              		.loc 1 1628 9 view .LVU1249
1631:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3300              		.loc 1 1631 9 view .LVU1250
1631:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3301              		.loc 1 1631 22 is_stmt 0 view .LVU1251
 3302 018a 0123     		movs	r3, #1
1631:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3303              		.loc 1 1631 22 view .LVU1252
 3304 018c 84F83D30 		strb	r3, [r4, #61]
1633:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
 3305              		.loc 1 1633 9 is_stmt 1 view .LVU1253
1633:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
 3306              		.loc 1 1633 17 is_stmt 0 view .LVU1254
 3307 0190 A36D     		ldr	r3, [r4, #88]
1633:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         {
 3308              		.loc 1 1633 11 view .LVU1255
 3309 0192 002B     		cmp	r3, #0
 3310 0194 EFD0     		beq	.L238
1635:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****         }
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 112


 3311              		.loc 1 1635 11 is_stmt 1 view .LVU1256
 3312 0196 2046     		mov	r0, r4
 3313 0198 9847     		blx	r3
 3314              	.LVL210:
1637:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****       }
 3315              		.loc 1 1637 9 view .LVU1257
 3316 019a ECE7     		b	.L238
 3317              	.L255:
1685:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 3318              		.loc 1 1685 7 view .LVU1258
1685:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 3319              		.loc 1 1685 20 is_stmt 0 view .LVU1259
 3320 019c 0123     		movs	r3, #1
1685:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****     }
 3321              		.loc 1 1685 20 view .LVU1260
 3322 019e 84F83D30 		strb	r3, [r4, #61]
 3323 01a2 E4E7     		b	.L256
 3324              	.L260:
 3325              		.align	2
 3326              	.L259:
 3327 01a4 00000000 		.word	SystemCoreClock
 3328 01a8 B5814E1B 		.word	458129845
 3329 01ac C0FFFFAD 		.word	-1375731776
 3330              		.cfi_endproc
 3331              	.LFE351:
 3333              		.section	.text.HAL_MDMA_GetState,"ax",%progbits
 3334              		.align	1
 3335              		.global	HAL_MDMA_GetState
 3336              		.syntax unified
 3337              		.thumb
 3338              		.thumb_func
 3340              	HAL_MDMA_GetState:
 3341              	.LVL211:
 3342              	.LFB352:
1723:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   return hmdma->State;
 3343              		.loc 1 1723 1 is_stmt 1 view -0
 3344              		.cfi_startproc
 3345              		@ args = 0, pretend = 0, frame = 0
 3346              		@ frame_needed = 0, uses_anonymous_args = 0
 3347              		@ link register save eliminated.
1724:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 3348              		.loc 1 1724 3 view .LVU1262
1724:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 3349              		.loc 1 1724 15 is_stmt 0 view .LVU1263
 3350 0000 90F83D00 		ldrb	r0, [r0, #61]	@ zero_extendqisi2
 3351              	.LVL212:
1725:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3352              		.loc 1 1725 1 view .LVU1264
 3353 0004 7047     		bx	lr
 3354              		.cfi_endproc
 3355              	.LFE352:
 3357              		.section	.text.HAL_MDMA_GetError,"ax",%progbits
 3358              		.align	1
 3359              		.global	HAL_MDMA_GetError
 3360              		.syntax unified
 3361              		.thumb
 3362              		.thumb_func
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 113


 3364              	HAL_MDMA_GetError:
 3365              	.LVL213:
 3366              	.LFB353:
1734:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c ****   return hmdma->ErrorCode;
 3367              		.loc 1 1734 1 is_stmt 1 view -0
 3368              		.cfi_startproc
 3369              		@ args = 0, pretend = 0, frame = 0
 3370              		@ frame_needed = 0, uses_anonymous_args = 0
 3371              		@ link register save eliminated.
1735:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 3372              		.loc 1 1735 3 view .LVU1266
1735:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** }
 3373              		.loc 1 1735 15 is_stmt 0 view .LVU1267
 3374 0000 806E     		ldr	r0, [r0, #104]
 3375              	.LVL214:
1736:Drivers/STM32H7xx_HAL_Driver/Src/stm32h7xx_hal_mdma.c **** 
 3376              		.loc 1 1736 1 view .LVU1268
 3377 0002 7047     		bx	lr
 3378              		.cfi_endproc
 3379              	.LFE353:
 3381              		.text
 3382              	.Letext0:
 3383              		.file 2 "C:/Users/lenex/AppData/Roaming/Code/User/globalStorage/bmd.stm32-for-vscode/@xpack-dev-to
 3384              		.file 3 "C:/Users/lenex/AppData/Roaming/Code/User/globalStorage/bmd.stm32-for-vscode/@xpack-dev-to
 3385              		.file 4 "Drivers/CMSIS/Device/ST/STM32H7xx/Include/stm32h7a3xx.h"
 3386              		.file 5 "Drivers/STM32H7xx_HAL_Driver/Inc/stm32h7xx_hal_def.h"
 3387              		.file 6 "Drivers/STM32H7xx_HAL_Driver/Inc/stm32h7xx_hal_mdma.h"
 3388              		.file 7 "Drivers/CMSIS/Device/ST/STM32H7xx/Include/system_stm32h7xx.h"
 3389              		.file 8 "Drivers/STM32H7xx_HAL_Driver/Inc/stm32h7xx_hal.h"
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 114


DEFINED SYMBOLS
                            *ABS*:00000000 stm32h7xx_hal_mdma.c
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:20     .text.MDMA_SetConfig:00000000 $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:25     .text.MDMA_SetConfig:00000000 MDMA_SetConfig
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:158    .text.MDMA_SetConfig:0000008c $d
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:163    .text.MDMA_Init:00000000 $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:168    .text.MDMA_Init:00000000 MDMA_Init
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:367    .text.HAL_MDMA_Init:00000000 $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:373    .text.HAL_MDMA_Init:00000000 HAL_MDMA_Init
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:495    .text.HAL_MDMA_DeInit:00000000 $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:501    .text.HAL_MDMA_DeInit:00000000 HAL_MDMA_DeInit
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:609    .text.HAL_MDMA_ConfigPostRequestMask:00000000 $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:615    .text.HAL_MDMA_ConfigPostRequestMask:00000000 HAL_MDMA_ConfigPostRequestMask
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:749    .text.HAL_MDMA_RegisterCallback:00000000 $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:755    .text.HAL_MDMA_RegisterCallback:00000000 HAL_MDMA_RegisterCallback
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:806    .text.HAL_MDMA_RegisterCallback:0000002c $d
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:812    .text.HAL_MDMA_RegisterCallback:00000032 $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:887    .text.HAL_MDMA_UnRegisterCallback:00000000 $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:893    .text.HAL_MDMA_UnRegisterCallback:00000000 HAL_MDMA_UnRegisterCallback
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:943    .text.HAL_MDMA_UnRegisterCallback:00000030 $d
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:1036   .text.HAL_MDMA_LinkedList_CreateNode:00000000 $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:1042   .text.HAL_MDMA_LinkedList_CreateNode:00000000 HAL_MDMA_LinkedList_CreateNode
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:1344   .text.HAL_MDMA_LinkedList_AddNode:00000000 $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:1350   .text.HAL_MDMA_LinkedList_AddNode:00000000 HAL_MDMA_LinkedList_AddNode
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:1627   .text.HAL_MDMA_LinkedList_RemoveNode:00000000 $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:1633   .text.HAL_MDMA_LinkedList_RemoveNode:00000000 HAL_MDMA_LinkedList_RemoveNode
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:1868   .text.HAL_MDMA_LinkedList_EnableCircularMode:00000000 $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:1874   .text.HAL_MDMA_LinkedList_EnableCircularMode:00000000 HAL_MDMA_LinkedList_EnableCircularMode
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:1976   .text.HAL_MDMA_LinkedList_DisableCircularMode:00000000 $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:1982   .text.HAL_MDMA_LinkedList_DisableCircularMode:00000000 HAL_MDMA_LinkedList_DisableCircularMode
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:2073   .text.HAL_MDMA_Start:00000000 $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:2079   .text.HAL_MDMA_Start:00000000 HAL_MDMA_Start
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:2208   .text.HAL_MDMA_Start_IT:00000000 $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:2214   .text.HAL_MDMA_Start_IT:00000000 HAL_MDMA_Start_IT
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:2381   .text.HAL_MDMA_Abort:00000000 $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:2387   .text.HAL_MDMA_Abort:00000000 HAL_MDMA_Abort
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:2511   .text.HAL_MDMA_Abort_IT:00000000 $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:2517   .text.HAL_MDMA_Abort_IT:00000000 HAL_MDMA_Abort_IT
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:2572   .text.HAL_MDMA_PollForTransfer:00000000 $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:2578   .text.HAL_MDMA_PollForTransfer:00000000 HAL_MDMA_PollForTransfer
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:2787   .text.HAL_MDMA_PollForTransfer:000000e6 $d
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:2791   .text.HAL_MDMA_PollForTransfer:000000ea $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:2863   .text.HAL_MDMA_GenerateSWRequest:00000000 $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:2869   .text.HAL_MDMA_GenerateSWRequest:00000000 HAL_MDMA_GenerateSWRequest
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:2946   .text.HAL_MDMA_IRQHandler:00000000 $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:2952   .text.HAL_MDMA_IRQHandler:00000000 HAL_MDMA_IRQHandler
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:3327   .text.HAL_MDMA_IRQHandler:000001a4 $d
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:3334   .text.HAL_MDMA_GetState:00000000 $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:3340   .text.HAL_MDMA_GetState:00000000 HAL_MDMA_GetState
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:3358   .text.HAL_MDMA_GetError:00000000 $t
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:3364   .text.HAL_MDMA_GetError:00000000 HAL_MDMA_GetError
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:950    .text.HAL_MDMA_UnRegisterCallback:00000037 $d
C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s:950    .text.HAL_MDMA_UnRegisterCallback:00000038 $t

UNDEFINED SYMBOLS
HAL_GetTick
SystemCoreClock
ARM GAS  C:\Users\lenex\AppData\Local\Temp\ccYIolaq.s 			page 115


