(module "Micro Mate-N-Lok 4-Pol" (layer F.Cu) (tedit 5CE9F407)
  (fp_text reference REF** (at 0 6) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "Micro Mate-N-Lok 4-Pol" (at 0 -8) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0 -6.6) (end 8 -6.6) (layer F.CrtYd) (width 0.15))
  (fp_line (start 8 -6.6) (end 8 4.6) (layer F.CrtYd) (width 0.15))
  (fp_line (start 8 4.6) (end -8 4.6) (layer F.CrtYd) (width 0.15))
  (fp_line (start -8 4.6) (end -8 -6.6) (layer F.CrtYd) (width 0.15))
  (fp_line (start -8 -6.6) (end 0 -6.6) (layer F.CrtYd) (width 0.15))
  (pad "" smd rect (at -8.2 0.4) (size 3.43 1.65) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 4.5 -5.08) (size 1.27 3) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 1.5 -5.08) (size 1.27 3) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.5 -5.08) (size 1.27 3) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -4.5 -5.08) (size 1.27 3) (layers F.Cu F.Paste F.Mask))
  (pad "" smd rect (at 8.21 0.4) (size 3.43 1.65) (layers F.Cu F.Paste F.Mask))
)
