(footprint "WCAP-ASLI_12.5" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -7.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3cee2c0b-8b35-4535-853d-df8ade17e4aa)
  )
  (fp_text value "WCAP-ASLI_12.5" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4628875b-f092-48f6-8e44-ec3b9c04543a)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e160328d-39ef-438b-a66b-60d815eef80a)
  )
  (fp_line (start -6.5 -6.5) (end 4.5 -6.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 3f123ee9-28d5-4f79-bcaf-c275979fdb1e))
  (fp_line (start -6.5 -1.7) (end -6.5 -6.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 6c0a3388-d539-414d-bb9e-53a279ec79d6))
  (fp_line (start -6.5 1.7) (end -6.5 6.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp dbcee1c4-42fe-4b03-8b35-37b8775bf28e))
  (fp_line (start -6.5 6.5) (end 4.5 6.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 64091fe8-2c7f-4b79-903f-43b7efe3e556))
  (fp_line (start 4.5 -6.5) (end 6.5 -4.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 8e8606d6-a6a6-415d-aa0b-d73d31eb7140))
  (fp_line (start 4.5 6.5) (end 6.5 4.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp a8c0d90e-2d70-4413-ab60-2591449a98c1))
  (fp_line (start 6.5 -4.5) (end 6.5 -1.7)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 28800248-08d3-44a9-9fd5-8fafd30f651b))
  (fp_line (start 6.5 4.5) (end 6.5 1.7)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp af4b0a40-afe6-4cb9-b6ec-d6790150b401))
  (fp_rect (start -8.2 -6.8) (end 8.2 6.7)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 3f398354-17e2-4891-96bb-d0b72d6e3f85))
  (pad "1" smd roundrect (at 5.05 0) (size 5.8 2.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.12)
    (thermal_bridge_angle 45) (tstamp 251fa680-5c21-47a1-ac86-de7b148e68fe))
  (pad "2" smd roundrect (at -5.05 0) (size 5.8 2.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.12)
    (thermal_bridge_angle 45) (tstamp cf6b6522-ea88-4837-94cf-95442cfd10d9))
)
