(footprint "WireHole_2x02_P2.54mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
	(tags "Through hole pin header THT 2x02 2.54mm double row")
	(property "Reference" "J1"
		(at 1 -4 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "ee40b56e-91b3-468c-aa95-b962b40d4e1a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Conn_01x04_Male"
		(at 1 17.5 180)
		(layer "F.Fab")
		(uuid "38a70129-eca5-4f6c-9812-806afdc0ba48")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "BLI:WireHole_2x02_P2.54mm"
		(at 0 -7.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "84606a78-1bd3-445f-8ebf-0f9a132e36ed")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "cd081a85-ac12-4b01-8c3a-172416a8990a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Generic connector, double row, 02x02, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
		(at 12.5 10.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "89d93fa8-6cc1-4801-b54e-1cd2fde023a9")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -1.8 -1.8)
		(end -1.8 4.35)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2ac14706-1e31-44be-9b2f-08a764be0341")
	)
	(fp_line
		(start -1.8 4.35)
		(end 4.35 4.35)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ee20101a-4c25-4ce5-8a6a-ef2b9d14a480")
	)
	(fp_line
		(start 4.35 -1.8)
		(end -1.8 -1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "98d96541-9129-4b07-be26-0f09b7241783")
	)
	(fp_line
		(start 4.35 4.35)
		(end 4.35 -1.8)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "37a77b34-edf4-496e-993c-80f83987010d")
	)
	(fp_line
		(start -1.27 0)
		(end 0 -1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "823f2b72-85a8-4de2-98bc-188bbb56f308")
	)
	(fp_line
		(start -1.27 3.81)
		(end -1.27 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ca877fa7-0fac-457c-8e43-67223021610c")
	)
	(fp_line
		(start 0 -1.27)
		(end 3.81 -1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "aa10dd5c-a3f5-4ee6-a11b-c5898d4beb23")
	)
	(fp_line
		(start 3.81 -1.27)
		(end 3.81 3.81)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d6443d8d-2c62-49d2-a75a-63ee08cba44d")
	)
	(fp_line
		(start 3.81 3.81)
		(end -1.27 3.81)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b0ba3f26-1b9d-47c5-8cbd-38fcf12191a4")
	)
	(fp_text user "${REFERENCE}"
		(at 10 2 90)
		(layer "F.Fab")
		(uuid "ba43d901-161f-43d9-aea1-bf0f5f4a44df")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 5)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "5bfc6ab7-1efd-4b67-b14e-84e856bca500")
	)
	(pad "2" thru_hole oval
		(at 2.5 1.5)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 5)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "f285ecf6-f489-4178-bb7a-b72daac7e2e0")
	)
	(pad "3" thru_hole oval
		(at 0 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 5)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "5c4b5232-71e0-4b12-af77-b7fdaa593e63")
	)
	(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
