(footprint "Micro_Mate-N-Lok_2p_vertical" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 6222BBBC)
  (attr smd)
  (fp_text reference "REF**" (at 0 3.81 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 42713045-fffd-4b2d-ae1e-7232d705fb12)
  )
  (fp_text value "Micro_Mate-N-Lok_2p_vertical" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c0515cd2-cdaa-467e-8354-0f6eadfa35c9)
  )
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1bf544e3-5940-4576-9291-2464e95c0ee2)
  )
  (fp_line (start -0.5 -3.25) (end 0.5 -3.25) (layer "F.SilkS") (width 0.12) (tstamp 16b71e23-859c-4e16-8af1-5d30a5c2b726))
  (fp_line (start -3.75 2.54) (end 3.75 2.5) (layer "F.SilkS") (width 0.12) (tstamp 1afdd221-608b-420b-8eb2-861de263adb5))
  (fp_line (start -3.75 -2.5) (end -2.5 -2.5) (layer "F.SilkS") (width 0.12) (tstamp 3742a313-c63e-4807-a7bf-be5a0ae2c781))
  (fp_line (start -3.75 -1.25) (end -3.75 -2.5) (layer "F.SilkS") (width 0.12) (tstamp 5e27f565-c85a-4f3b-9862-58c0accdd5e3))
  (fp_line (start 3.75 1.25) (end 5 1.25) (layer "F.SilkS") (width 0.12) (tstamp 5e3106c4-aefe-4ef5-8aa8-6f8a9c16fe7d))
  (fp_line (start -3.75 1.25) (end -5 1.25) (layer "F.SilkS") (width 0.12) (tstamp 8c5a6fce-194d-4416-8856-cb66ff818319))
  (fp_line (start 3.75 -1.25) (end 5 -1.25) (layer "F.SilkS") (width 0.12) (tstamp 917603e2-441d-4888-a037-0b830871fafd))
  (fp_line (start 3.75 2.5) (end 3.75 1.25) (layer "F.SilkS") (width 0.12) (tstamp 9d7822b4-339e-43c0-b115-d4b16189cc93))
  (fp_line (start -3.75 -1.25) (end -5 -1.25) (layer "F.SilkS") (width 0.12) (tstamp a6e79250-4ea1-4a1f-b168-c1d347acb43a))
  (fp_line (start 3.75 -2.5) (end 2.5 -2.5) (layer "F.SilkS") (width 0.12) (tstamp b4e13e2a-b1f5-417e-8d80-b3e4cb5e5e55))
  (fp_line (start 3.75 -1.25) (end 3.75 -2.5) (layer "F.SilkS") (width 0.12) (tstamp d2fb2423-7bf4-4222-994d-25a9683eab67))
  (fp_line (start -3.75 1.25) (end -3.75 2.54) (layer "F.SilkS") (width 0.12) (tstamp ed74c2b7-a3ac-4886-84f5-377b5e1bbbfc))
  (fp_circle (center 4.75 -3.5) (end 5.25 -3.5) (layer "F.SilkS") (width 0.12) (fill solid) (tstamp 63489ebf-0f52-43a6-a0ab-158b1a7d4988))
  (fp_rect (start -7 -4.58) (end 7 2.54) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 312474c5-a081-4cd1-b2e6-730f0718514a))
  (fp_line (start 4.318 1.27) (end 5.08 1.27) (layer "F.Fab") (width 0.1) (tstamp c6462399-f2e4-4f1a-b34a-b49a04c8bdb9))
  (fp_line (start 4.318 1.778) (end 4.318 1.27) (layer "F.Fab") (width 0.1) (tstamp f284b1e2-75a4-4a3f-a5f4-6f05f15fb4f5))
  (pad "" smd roundrect (at -5.2 0) (size 3.43 1.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1f3003e6-dce5-420f-906b-3f1e92b67249))
  (pad "" smd roundrect (at 5.2 0) (size 3.43 1.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 378af8b4-af3d-46e7-89ae-deff12ca9067))
  (pad "1" smd roundrect (at 1.5 -3.2) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8c0807a7-765b-4fa5-baaa-e09a2b610e6b))
  (pad "2" smd roundrect (at -1.5 -3.2) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ebd06df3-d52b-4cff-99a2-a771df6d3733))
  (model "${KIPRJMOD}/libraries/FaSTTUBe_connectors_3dmodels/Micro_Mate-N-Lok_2p_vertical.stp"
    (offset (xyz 0 0 9.24))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 180))
  )
)
