;Proteus Design Interchange Format
(PDIF
 (vendor "SamacSys Limited")
 (version 1 0)
 (library
  (part "3386F-1-105LF"
   (description "1M Through Hole Trimmer Resistor 0.5W Top Adjust Bourns 3386 Series")
   (family "ANA")
   (package "3386F1153")
   (attribute "Datasheet Link" "https://www.bourns.com/pdfs/3386.pdf")
   (attribute "Geometry.Height" "4.83mm")
   (attribute "Manufacturer_Name" "Bourns")
   (attribute "Manufacturer_Part_Number" "3386F-1-105LF")
   (attribute "Mouser Part Number" "652-3386F-1-105LF")
   (attribute "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Bourns/3386F-1-105LF?qs=nE0RJHjSZ6W2MHhpfLC%252BRw%3D%3D")
   (attribute "Arrow Part Number" "3386F-1-105LF")
   (attribute "Arrow Price/Stock" "https://www.arrow.com/en/products/3386f-1-105lf/bourns?region=nac")
   (gate
    (symbol "3386F-1-105LF")
    (pin "CCW" 1 PS)
    (pin "WIPER" 2 PS)
    (pin "CW" 3 PS)
   )
  )
  (symbol "3386F-1-105LF"
   (units THOU)
   (origin (pt 0 0))
   (graphic
    (stroke 10)
    (path (pt 200 100) (pt 900 100) (pt 900 -200) (pt 200 -200) (pt 200 100) (closed))
   )
   (terminal
    (body (symbol "PIN") (pt 0 -100) (rot 0) (mir 0) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 1100 0) (rot 0) (mir X) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 0 0) (rot 0) (mir 0) (visible true))
    (name (pt 230 0) (rot 0) (just MIDDLE LEFT) (visible true))
    (number (pt 140 20) (rot 0) (just BOTTOM RIGHT) (visible true)))
  )
  (symbol "PIN"
   (units THOU)
   (origin (pt 0 0))
   (graphic
    (stroke 10)
    (path (pt 0 0) (pt 200 0))))
  (symbol "PINSHORT"
   (units THOU)
   (origin (pt 0 0))
   (graphic
    (stroke 10)
    (path (pt 0 0) (pt 100 0))))
  (package "3386F1153"
   (units MM)
   (layer TASM
    (graphic
     (stroke 0.2)
     (path
      (closed true)
      (pt -7.305 -2.11)
      (pt 2.225 -2.11)
      (pt 2.225 7.42)
      (pt -7.305 7.42)
      (pt -7.305 -2.11))))
   (layer TSLK
    (graphic
     (stroke 0.1)
     (path
      (closed true)
      (pt -7.305 -2.11)
      (pt 2.225 -2.11)
      (pt 2.225 7.42)
      (pt -7.305 7.42)
      (pt -7.305 -2.11))))
   (layer OCCA
    (graphic
     (stroke 0.1)
     (path
      (closed true)
      (pt -8.305 -3.11)
      (pt 3.8 -3.11)
      (pt 3.8 8.42)
      (pt -8.305 8.42)
      (pt -8.305 -3.11))))
   (layer TSLK
    (graphic
     (stroke 0.2)
     (path
      (closed true)
      (pt 2.7 -0.1)
      (arc (pt 2.700 -0.100) (pt 2.600 0.100) (pt 2.800 -0.100) (start -180.0) (sweep -90.0))
      (pt 2.7 0.1)
      (arc (pt 2.700 0.100) (pt 2.600 0.100) (pt 2.800 -0.100) (start -180.0) (sweep 90.0))
      (pt 2.7 -0.1))))
   (leg 1 (pt 0.000 0.000) (padstack 0))
   (leg 2 (pt -2.540 5.080) (padstack 0))
   (leg 3 (pt -5.080 0.000) (padstack 0))
   (padstack 0
    (hole 0.76)
    (plated true)
    (pad (layer TCOP) (round 1.303))
    (pad (layer INNER) (round 1.303))
    (pad (layer BCOP) (round 1.303))
   )
   (model "3386F-1-105LF.stp"
    (euler 0 0 180)
    (offset -2.3399999141693115 2.7100000381469727 0)
   )
  )
 )
)
