SamacSys ECAD Model
760783/1031803/2.50/3/4/Variable Resistor

DESIGNSPARK_INTERMEDIATE_ASCII

(asciiHeader
	(fileUnits MM)
)
(library Library_1
	(padStyleDef "c130.3_h76"
		(holeDiam 0.76)
		(padShape (layerNumRef 1) (padShapeType Ellipse)  (shapeWidth 1.303) (shapeHeight 1.303))
		(padShape (layerNumRef 16) (padShapeType Ellipse)  (shapeWidth 1.303) (shapeHeight 1.303))
	)
	(textStyleDef "Default"
		(font
			(fontType Stroke)
			(fontFace "Helvetica")
			(fontHeight 50 mils)
			(strokeWidth 5 mils)
		)
	)
	(patternDef "3386F1153" (originalName "3386F1153")
		(multiLayer
			(pad (padNum 1) (padStyleRef c130.3_h76) (pt 0.000, 0.000) (rotation 90))
			(pad (padNum 2) (padStyleRef c130.3_h76) (pt -2.540, 5.080) (rotation 90))
			(pad (padNum 3) (padStyleRef c130.3_h76) (pt -5.080, 0.000) (rotation 90))
		)
		(layerContents (layerNumRef 18)
			(attr "RefDes" "RefDes" (pt -2.253, 2.655) (textStyleRef "Default") (isVisible True))
		)
		(layerContents (layerNumRef 28)
			(line (pt -7.305 -2.11) (pt 2.225 -2.11) (width 0.2))
		)
		(layerContents (layerNumRef 28)
			(line (pt 2.225 -2.11) (pt 2.225 7.42) (width 0.2))
		)
		(layerContents (layerNumRef 28)
			(line (pt 2.225 7.42) (pt -7.305 7.42) (width 0.2))
		)
		(layerContents (layerNumRef 28)
			(line (pt -7.305 7.42) (pt -7.305 -2.11) (width 0.2))
		)
		(layerContents (layerNumRef 18)
			(line (pt -7.305 -2.11) (pt 2.225 -2.11) (width 0.1))
		)
		(layerContents (layerNumRef 18)
			(line (pt 2.225 -2.11) (pt 2.225 7.42) (width 0.1))
		)
		(layerContents (layerNumRef 18)
			(line (pt 2.225 7.42) (pt -7.305 7.42) (width 0.1))
		)
		(layerContents (layerNumRef 18)
			(line (pt -7.305 7.42) (pt -7.305 -2.11) (width 0.1))
		)
		(layerContents (layerNumRef 30)
			(line (pt -8.305 -3.11) (pt 3.8 -3.11) (width 0.1))
		)
		(layerContents (layerNumRef 30)
			(line (pt 3.8 -3.11) (pt 3.8 8.42) (width 0.1))
		)
		(layerContents (layerNumRef 30)
			(line (pt 3.8 8.42) (pt -8.305 8.42) (width 0.1))
		)
		(layerContents (layerNumRef 30)
			(line (pt -8.305 8.42) (pt -8.305 -3.11) (width 0.1))
		)
		(layerContents (layerNumRef 18)
			(line (pt 2.7 -0.1) (pt 2.7 -0.1) (width 0.2))
		)
		(layerContents (layerNumRef 18)
			(arc (pt 2.7, 0) (radius 0.1) (startAngle 270) (sweepAngle -180.0) (width 0.2))
		)
		(layerContents (layerNumRef 18)
			(line (pt 2.7 0.1) (pt 2.7 0.1) (width 0.2))
		)
		(layerContents (layerNumRef 18)
			(arc (pt 2.7, 0) (radius 0.1) (startAngle 90.0) (sweepAngle -180.0) (width 0.2))
		)
	)
	(symbolDef "3386F-1-105LF" (originalName "3386F-1-105LF")

		(pin (pinNum 1) (pt 0 mils -100 mils) (rotation 0) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 230 mils -125 mils) (rotation 0]) (justify "Left") (textStyleRef "Default"))
		))
		(pin (pinNum 2) (pt 1100 mils 0 mils) (rotation 180) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 870 mils -25 mils) (rotation 0]) (justify "Right") (textStyleRef "Default"))
		))
		(pin (pinNum 3) (pt 0 mils 0 mils) (rotation 0) (pinLength 200 mils) (pinDisplay (dispPinName true)) (pinName (text (pt 230 mils -25 mils) (rotation 0]) (justify "Left") (textStyleRef "Default"))
		))
		(line (pt 200 mils 100 mils) (pt 900 mils 100 mils) (width 6 mils))
		(line (pt 900 mils 100 mils) (pt 900 mils -200 mils) (width 6 mils))
		(line (pt 900 mils -200 mils) (pt 200 mils -200 mils) (width 6 mils))
		(line (pt 200 mils -200 mils) (pt 200 mils 100 mils) (width 6 mils))
		(attr "RefDes" "RefDes" (pt 950 mils 300 mils) (justify Left) (isVisible True) (textStyleRef "Default"))

	)
	(compDef "3386F-1-105LF" (originalName "3386F-1-105LF") (compHeader (numPins 3) (numParts 1) (refDesPrefix VR)
		)
		(compPin "1" (pinName "CCW") (partNum 1) (symPinNum 1) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "2" (pinName "WIPER") (partNum 1) (symPinNum 2) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(compPin "3" (pinName "CW") (partNum 1) (symPinNum 3) (gateEq 0) (pinEq 0) (pinType Bidirectional))
		(attachedSymbol (partNum 1) (altType Normal) (symbolName "3386F-1-105LF"))
		(attachedPattern (patternNum 1) (patternName "3386F1153")
			(numPads 3)
			(padPinMap
				(padNum 1) (compPinRef "1")
				(padNum 2) (compPinRef "2")
				(padNum 3) (compPinRef "3")
			)
		)
		(attr "Manufacturer_Name" "Bourns")
		(attr "Manufacturer_Part_Number" "3386F-1-105LF")
		(attr "Mouser Part Number" "652-3386F-1-105LF")
		(attr "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Bourns/3386F-1-105LF?qs=nE0RJHjSZ6W2MHhpfLC%252BRw%3D%3D")
		(attr "Arrow Part Number" "3386F-1-105LF")
		(attr "Arrow Price/Stock" "https://www.arrow.com/en/products/3386f-1-105lf/bourns?region=nac")
		(attr "Description" "1M Through Hole Trimmer Resistor 0.5W Top Adjust Bourns 3386 Series")
		(attr "Datasheet Link" "https://www.bourns.com/pdfs/3386.pdf")
		(attr "Height" "4.83 mm")
	)

)
