(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "SN75LVDS83B" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 68.58 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SN75LVDS83B" (at 0 71.12 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Package_SO:TSSOP-56_6.1x14mm_P0.5mm" (at 0 68.58 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 68.58 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SN75LVDS83B_0_1"
      (rectangle (start -13.97 60.96) (end 13.97 -62.23)
        (stroke (width 0) (type default))
        (fill (type background))
      )
    )
    (symbol "SN75LVDS83B_1_1"
      (pin power_in line (at -7.62 63.5 270) (length 2.54)
        (name "IOVCC" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 -43.18 0) (length 2.54)
        (name "D11" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 8.89 0) (length 2.54)
        (name "D12/G3" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 6.35 0) (length 2.54)
        (name "D13/G4" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -8.89 -64.77 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 3.81 0) (length 2.54)
        (name "D14/G5" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 -1.27 0) (length 2.54)
        (name "D15/B0" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 -45.72 0) (length 2.54)
        (name "D16" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 -27.94 0) (length 2.54)
        (name "CLKSEL" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 -48.26 0) (length 2.54)
        (name "D17" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 -3.81 0) (length 2.54)
        (name "D18/B1" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 -38.1 0) (length 2.54)
        (name "D5" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 -6.35 0) (length 2.54)
        (name "D19/B2" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -6.35 -64.77 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 -8.89 0) (length 2.54)
        (name "D20/B3" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 -11.43 0) (length 2.54)
        (name "D21/B4" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 -13.97 0) (length 2.54)
        (name "D22/B5" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 -50.8 0) (length 2.54)
        (name "D23" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.08 63.5 270) (length 2.54)
        (name "IOVCC" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 39.37 0) (length 2.54)
        (name "D24/HSYNC" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 44.45 0) (length 2.54)
        (name "D25/VSYNC" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -3.81 -64.77 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 21.59 0) (length 2.54)
        (name "D6/R5" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 41.91 0) (length 2.54)
        (name "D26/ENABLE" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 46.99 0) (length 2.54)
        (name "CLKIN" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 -22.86 0) (length 2.54)
        (name "~{SHTDN}" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -1.27 -64.77 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 7.62 63.5 270) (length 2.54)
        (name "PLLVCC" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 1.27 -64.77 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 3.81 -64.77 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 16.51 -3.81 180) (length 2.54)
        (name "Y3P" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 16.51 -1.27 180) (length 2.54)
        (name "Y3M" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 16.51 5.08 180) (length 2.54)
        (name "CLKOUTP" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 16.51 0) (length 2.54)
        (name "D7/G0" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 16.51 7.62 180) (length 2.54)
        (name "CLKOUTM" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 16.51 13.97 180) (length 2.54)
        (name "Y2P" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 16.51 16.51 180) (length 2.54)
        (name "Y2M" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 6.35 -64.77 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 5.08 63.5 270) (length 2.54)
        (name "LCDSVCC" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 16.51 22.86 180) (length 2.54)
        (name "Y1P" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 16.51 25.4 180) (length 2.54)
        (name "Y1M" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 16.51 31.75 180) (length 2.54)
        (name "Y0P" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 16.51 34.29 180) (length 2.54)
        (name "Y0M" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 8.89 -64.77 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -11.43 -64.77 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 -35.56 0) (length 2.54)
        (name "D27" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 34.29 0) (length 2.54)
        (name "D0/R0" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 31.75 0) (length 2.54)
        (name "D1/R1" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 11.43 -64.77 90) (length 2.54)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 29.21 0) (length 2.54)
        (name "D2/R2" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 26.67 0) (length 2.54)
        (name "D3/R3" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 24.13 0) (length 2.54)
        (name "D4/R4" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 13.97 0) (length 2.54)
        (name "D8/G1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 11.43 0) (length 2.54)
        (name "D9/G2" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -16.51 -40.64 0) (length 2.54)
        (name "D10" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 63.5 270) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
