(footprint "WF100-06S" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp 41467782-87ec-47cd-85a7-ccf56567d8df)
  )
  (fp_text value "WF100-06S" (at 0 1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 97ae9d9d-f6ff-4306-82f2-44ffe9f903ba)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 10629d22-87a6-4bc3-ba37-c0b3592380f4)
  )
  (fp_line (start -8 -3.5) (end -4 -3.5)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 025d5c49-a934-4277-9087-98866ddf4049))
  (fp_line (start -8 2) (end -8 -3.5)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 7f2c722b-561a-46c6-84a3-9a54a8fc2ec6))
  (fp_line (start -8 2) (end -8 2.5)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp f1597424-cecf-48e2-ad3b-05b0757f4080))
  (fp_line (start -8 2.5) (end 8 2.5)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp b3c436d1-887b-44bd-a9cc-73e9f9e4dfe9))
  (fp_line (start -4 -5.5) (end 4 -5.5)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp f7926a91-c733-4e2e-8aa5-a83aa82f717c))
  (fp_line (start -4 -3.5) (end -4 -5.5)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp b6944733-2903-4a40-8aee-2c61c20ab71c))
  (fp_line (start 4 -5.5) (end 4 -3.5)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp f6938fa9-5c5b-4a71-aec3-8e167ed70100))
  (fp_line (start 4 -3.5) (end 8 -3.5)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp e9c4dc66-0120-47ae-ac08-8268de1d50ca))
  (fp_line (start 8 -3.5) (end 8 2)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 65f997fa-eae8-4258-9f0b-8b96d2bec05d))
  (fp_line (start 8 2.5) (end 8 2)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 4743f283-5723-4303-b9a4-d38740798331))
  (fp_line (start -7.5 -3) (end -3.5 -3)
    (stroke (width 0.1) (type default)) (layer "F.CrtYd") (tstamp 9b74d177-f58b-4738-8ecb-e98d6619aff8))
  (fp_line (start -7.5 2) (end -7.5 -3)
    (stroke (width 0.1) (type default)) (layer "F.CrtYd") (tstamp bdd2e99e-2b43-4670-a8ac-e546f9eacc95))
  (fp_line (start -3.5 -5) (end 3.5 -5)
    (stroke (width 0.1) (type default)) (layer "F.CrtYd") (tstamp a4e11d30-d35a-4b80-a97f-8782128d6afc))
  (fp_line (start -3.5 -4.5) (end -3.5 -5)
    (stroke (width 0.1) (type default)) (layer "F.CrtYd") (tstamp 6c40c509-1aac-43dc-b15b-c8c51380ec37))
  (fp_line (start -3.5 -3) (end -3.5 -4.5)
    (stroke (width 0.1) (type default)) (layer "F.CrtYd") (tstamp 42b54cd1-0704-4ed8-b52c-10c6eeaf568e))
  (fp_line (start 3.5 -5) (end 3.5 -3)
    (stroke (width 0.1) (type default)) (layer "F.CrtYd") (tstamp 53f656c9-4901-4824-884b-075ce3d99193))
  (fp_line (start 3.5 -3) (end 7.5 -3)
    (stroke (width 0.1) (type default)) (layer "F.CrtYd") (tstamp ffc1d84a-9e15-40a6-ba1c-5b01b23edd7e))
  (fp_line (start 7.5 -3) (end 7.5 2)
    (stroke (width 0.1) (type default)) (layer "F.CrtYd") (tstamp cadca4ad-74f0-4687-b8dd-9a5c09558519))
  (fp_line (start 7.5 2) (end -7.5 2)
    (stroke (width 0.1) (type default)) (layer "F.CrtYd") (tstamp b7735400-8a78-4109-aebb-6593350d9250))
  (pad "" smd rect (at -5.95 -0.425) (size 2.1 4.3) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 6c478f06-3d43-43bd-a8c7-28b9332be749))
  (pad "" smd rect (at 5.95 -0.425) (size 2.1 4.3) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp e14491fd-6ec7-4622-aa67-a1e0ba049576))
  (pad "1" smd rect (at -2.5 -3.5) (size 0.6 1.85) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp f7f0a05d-ce51-4716-b64b-1c58c9c71ca6))
  (pad "2" smd rect (at -1.5 -3.5) (size 0.6 1.85) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 59c827f4-2309-41d3-8b43-3a774fb8cd5d))
  (pad "3" smd rect (at -0.5 -3.5) (size 0.6 1.85) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 89f020ae-7f36-4129-aac9-658ec0c79116))
  (pad "4" smd rect (at 0.5 -3.5) (size 0.6 1.85) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp d19e0f18-b6ea-4748-9ef2-cc972a2382bb))
  (pad "5" smd rect (at 1.5 -3.5) (size 0.6 1.85) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp be2eb44b-12e0-4980-acc6-c2e6381c710c))
  (pad "6" smd rect (at 2.5 -3.5) (size 0.6 1.85) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 769acce3-2117-4573-891e-0165630ac0c6))
)
