(CADSTARPCB
 (HEADER
  (FORMAT LIBRARY 2 18)
  (JOBFILE "")
  (JOBTITLE "")
  (GENERATOR "")
  (RESOLUTION
   (METRIC HUNDREDTH MICRON)
  )
  (TIMESTAMP 2025 02 01 05 40 22)
 )
 (ASSIGNMENTS
  (LAYERDEFS
   (LAYERSTACK LAY7 LAY9 LAY12 LAY14 LAY18 LAY10 LAY16 LAY6 LAY8 LAY17
     LAY11 LAY19 LAY15 LAY13
   )
   (LAYER LAY0 "(All Layers)"
    (ALLLAYER)
   )
   (LAYER LAY1 "(All Electrical Layers)"
    (ALLELEC)
   )
   (LAYER LAY2 "(All Documentation Layers)"
    (ALLDOC)
   )
   (LAYER LAY3 "(Undefined)"
    (NOLAYER)
   )
   (LAYER LAY4 "(Component Copper)"
    (ASSCOMPCOPP)
   )
   (LAYER LAY5 "(Jumper)"
    (JUMPERLAYER)
   )
   (LAYER LAY6 "Top Elec"
    (ELEC 1
     (BIAS UNBIASED)
     (LAYERHEIGHT 0)
    )
   )
   (LAYER LAY7 "Construction"
    (DOC)
   )
   (LAYER LAY8 "Bottom Elec"
    (ELEC 2
     (BIAS UNBIASED)
     (LAYERHEIGHT 0)
    )
   )
   (LAYER LAY9 "Drill Drawing"
    (DOC)
   )
   (LAYER LAY10 "Top silk"
    (NONELEC 1)
    (LASUBTYP LAYERSUBTYPE_SILKSCREEN)
   )
   (LAYER LAY11 "Bottom silk"
    (NONELEC 2)
    (LASUBTYP LAYERSUBTYPE_SILKSCREEN)
   )
   (LAYER LAY12 "Top Placement"
    (NONELEC 1)
    (LASUBTYP LAYERSUBTYPE_PLACEMENT)
   )
   (LAYER LAY13 "Bottom Placement"
    (NONELEC 2)
    (LASUBTYP LAYERSUBTYPE_PLACEMENT)
   )
   (LAYER LAY14 "Top Assembly"
    (NONELEC 1)
    (LASUBTYP LAYERSUBTYPE_ASSEMBLY)
   )
   (LAYER LAY15 "Bottom Assembly"
    (NONELEC 2)
    (LASUBTYP LAYERSUBTYPE_ASSEMBLY)
   )
   (LAYER LAY16 "Top Solder Resist"
    (NONELEC 1)
    (LASUBTYP LAYERSUBTYPE_SOLDERRESIST)
   )
   (LAYER LAY17 "Bottom Solder Resist"
    (NONELEC 2)
    (LASUBTYP LAYERSUBTYPE_SOLDERRESIST)
   )
   (LAYER LAY18 "Top Paste"
    (NONELEC 1)
    (LASUBTYP LAYERSUBTYPE_PASTE)
   )
   (LAYER LAY19 "Bottom Paste"
    (NONELEC 2)
    (LASUBTYP LAYERSUBTYPE_PASTE)
   )
  )
  (CODEDEFS
   (LINECODE LC11 "Silkscreen Outline 1" 2540
    (STYLE SOLID)
   )
   (LINECODE LC14 "Assembly Outline 1" 2540
    (STYLE SOLID)
   )
   (LINECODE LC15 "Placement Outline 1" 2540
    (STYLE SOLID)
   )
   (TEXTCODE TC10 "Component Name" 3000 60000 40000)
   (SPACINGCODE P_P 100000)
   (SPACINGCODE P_C 100000)
   (SPACINGCODE C_C 100000)
   (SPACINGCODE H_H 100000)
   (PADCODE PC0 "r129.5_60"
    (RECTANGLE 60000 34750 34750)
   )
   (ATTRNAME AT0 "Component Category"
    (ATTROWNER COMPONENT)
   )
   (ATTRNAME AT1 "assembly_name"
    (ATTROWNER COMPONENT)
   )
   (ATTRNAME AT2 "Value"
    (ATTROWNER COMPONENT)
   )
   (ATTRNAME AT3 "thm_power_diss"
    (ATTROWNER COMPONENT)
   )
   (ATTRNAME AT4 "placement"
    (ATTROWNER COMPONENT)
   )
   (ATTRNAME AT5 "silkscrn_name"
    (ATTROWNER COMPONENT)
   )
   (ATTRNAME AT6 "Manufacturers Part Number"
    (ATTROWNER COMPONENT)
   )
   (ATTRNAME AT7 "Height"
    (ATTROWNER SYMDEF)
   )
   (ATTRNAME AT8 "Drawing_Name"
    (ATTROWNER DOCSYMBOL)
   )
   (ATTRNAME AT9 "Client"
    (ATTROWNER DOCSYMBOL)
   )
   (ATTRNAME AT10 "RefDes"
    (ATTROWNER COMPONENT)
   )
  )
  (TECHNOLOGY
   (UNITS MM)
   (UNITSPRECISION 2)
   (INTERLINEGAP 20)
   (BARLINEGAP 20)
   (ALLOWBARTEXT)
   (ANGULARPRECISION 1)
   (MAXPHYSLAYER 2)
   (DESIGNORIGIN (PT 0 0))
   (DESIGNAREA (PT 0 0) (PT 100000000 100000000))
   (PINNOOFFSET 50800)
   (PINNOANGLE 0)
   (DESIGNLIMIT (PT 100000000 100000000))
  )
 )
 (LIBRARY
  (HIERARCHY
   (ROOTFOLDER F0 "root"
    (SYMDEFLIST L0)
   )
  )
  (SYMDEF L0 "SOP80P1176X120-54N" "" (PT 50000000 50000000)
   (VERSION 1)
   (FIGURE FIG0 LC15 LAY12
    (OUTLINE (PT 49337500 51142500) (PT 50662500 51142500) (PT 50662500 48857500) (PT 49337500 48857500) (PT 49337500 51142500))
   )
   (FIGURE FIG1 LC14 LAY14
    (OUTLINE (PT 49492000 51111000) (PT 50508000 51111000) (PT 50508000 48889000) (PT 49492000 48889000) (PT 49492000 51111000))
   )
   (FIGURE FIG2 LC14 LAY14
    (OPENSHAPE (PT 49492000 51031000) (PT 49572000 51111000))
   )
   (FIGURE FIG3 LC11 LAY10
    (OUTLINE (PT 49527000 51111000) (PT 50473000 51111000) (PT 50473000 48889000) (PT 49527000 48889000) (PT 49527000 51111000))
   )
   (FIGURE FIG4 LC11 LAY10
    (OPENSHAPE (PT 49362500 51105000) (PT 49492000 51105000))
   )
   (PAD 1 (PT 49427200 51040000) PC0 TOP
    (FIRSTPAD)
    (PADIDENTIFIER "1")
   )
   (PAD 2 (PT 49427200 50960000) PC0 TOP
    (PADIDENTIFIER "2")
   )
   (PAD 3 (PT 49427200 50880000) PC0 TOP
    (PADIDENTIFIER "3")
   )
   (PAD 4 (PT 49427200 50800000) PC0 TOP
    (PADIDENTIFIER "4")
   )
   (PAD 5 (PT 49427200 50720000) PC0 TOP
    (PADIDENTIFIER "5")
   )
   (PAD 6 (PT 49427200 50640000) PC0 TOP
    (PADIDENTIFIER "6")
   )
   (PAD 7 (PT 49427200 50560000) PC0 TOP
    (PADIDENTIFIER "7")
   )
   (PAD 8 (PT 49427200 50480000) PC0 TOP
    (PADIDENTIFIER "8")
   )
   (PAD 9 (PT 49427200 50400000) PC0 TOP
    (PADIDENTIFIER "9")
   )
   (PAD 10 (PT 49427200 50320000) PC0 TOP
    (PADIDENTIFIER "10")
   )
   (PAD 11 (PT 49427200 50240000) PC0 TOP
    (PADIDENTIFIER "11")
   )
   (PAD 12 (PT 49427200 50160000) PC0 TOP
    (PADIDENTIFIER "12")
   )
   (PAD 13 (PT 49427200 50080000) PC0 TOP
    (PADIDENTIFIER "13")
   )
   (PAD 14 (PT 49427200 50000000) PC0 TOP
    (PADIDENTIFIER "14")
   )
   (PAD 15 (PT 49427200 49920000) PC0 TOP
    (PADIDENTIFIER "15")
   )
   (PAD 16 (PT 49427200 49840000) PC0 TOP
    (PADIDENTIFIER "16")
   )
   (PAD 17 (PT 49427200 49760000) PC0 TOP
    (PADIDENTIFIER "17")
   )
   (PAD 18 (PT 49427200 49680000) PC0 TOP
    (PADIDENTIFIER "18")
   )
   (PAD 19 (PT 49427200 49600000) PC0 TOP
    (PADIDENTIFIER "19")
   )
   (PAD 20 (PT 49427200 49520000) PC0 TOP
    (PADIDENTIFIER "20")
   )
   (PAD 21 (PT 49427200 49440000) PC0 TOP
    (PADIDENTIFIER "21")
   )
   (PAD 22 (PT 49427200 49360000) PC0 TOP
    (PADIDENTIFIER "22")
   )
   (PAD 23 (PT 49427200 49280000) PC0 TOP
    (PADIDENTIFIER "23")
   )
   (PAD 24 (PT 49427200 49200000) PC0 TOP
    (PADIDENTIFIER "24")
   )
   (PAD 25 (PT 49427200 49120000) PC0 TOP
    (PADIDENTIFIER "25")
   )
   (PAD 26 (PT 49427200 49040000) PC0 TOP
    (PADIDENTIFIER "26")
   )
   (PAD 27 (PT 49427200 48960000) PC0 TOP
    (PADIDENTIFIER "27")
   )
   (PAD 28 (PT 50572800 48960000) PC0 TOP
    (PADIDENTIFIER "28")
   )
   (PAD 29 (PT 50572800 49040000) PC0 TOP
    (PADIDENTIFIER "29")
   )
   (PAD 30 (PT 50572800 49120000) PC0 TOP
    (PADIDENTIFIER "30")
   )
   (PAD 31 (PT 50572800 49200000) PC0 TOP
    (PADIDENTIFIER "31")
   )
   (PAD 32 (PT 50572800 49280000) PC0 TOP
    (PADIDENTIFIER "32")
   )
   (PAD 33 (PT 50572800 49360000) PC0 TOP
    (PADIDENTIFIER "33")
   )
   (PAD 34 (PT 50572800 49440000) PC0 TOP
    (PADIDENTIFIER "34")
   )
   (PAD 35 (PT 50572800 49520000) PC0 TOP
    (PADIDENTIFIER "35")
   )
   (PAD 36 (PT 50572800 49600000) PC0 TOP
    (PADIDENTIFIER "36")
   )
   (PAD 37 (PT 50572800 49680000) PC0 TOP
    (PADIDENTIFIER "37")
   )
   (PAD 38 (PT 50572800 49760000) PC0 TOP
    (PADIDENTIFIER "38")
   )
   (PAD 39 (PT 50572800 49840000) PC0 TOP
    (PADIDENTIFIER "39")
   )
   (PAD 40 (PT 50572800 49920000) PC0 TOP
    (PADIDENTIFIER "40")
   )
   (PAD 41 (PT 50572800 50000000) PC0 TOP
    (PADIDENTIFIER "41")
   )
   (PAD 42 (PT 50572800 50080000) PC0 TOP
    (PADIDENTIFIER "42")
   )
   (PAD 43 (PT 50572800 50160000) PC0 TOP
    (PADIDENTIFIER "43")
   )
   (PAD 44 (PT 50572800 50240000) PC0 TOP
    (PADIDENTIFIER "44")
   )
   (PAD 45 (PT 50572800 50320000) PC0 TOP
    (PADIDENTIFIER "45")
   )
   (PAD 46 (PT 50572800 50400000) PC0 TOP
    (PADIDENTIFIER "46")
   )
   (PAD 47 (PT 50572800 50480000) PC0 TOP
    (PADIDENTIFIER "47")
   )
   (PAD 48 (PT 50572800 50560000) PC0 TOP
    (PADIDENTIFIER "48")
   )
   (PAD 49 (PT 50572800 50640000) PC0 TOP
    (PADIDENTIFIER "49")
   )
   (PAD 50 (PT 50572800 50720000) PC0 TOP
    (PADIDENTIFIER "50")
   )
   (PAD 51 (PT 50572800 50800000) PC0 TOP
    (PADIDENTIFIER "51")
   )
   (PAD 52 (PT 50572800 50880000) PC0 TOP
    (PADIDENTIFIER "52")
   )
   (PAD 53 (PT 50572800 50960000) PC0 TOP
    (PADIDENTIFIER "53")
   )
   (PAD 54 (PT 50572800 51040000) PC0 TOP
    (PADIDENTIFIER "54")
   )
   (TEXTLOC COMP_NAME TC10 LAY10 (PT 50000000 50000000)
    (ALIGN CENTERCENTER)
   )
  )
 )
)
