(kicad_symbol_lib
	(version 20231120)
	(generator "kicad_symbol_editor")
	(generator_version "8.0")
	(symbol "ESP32-WROOM-32-DevKit-30Pin"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U9"
			(at -6.985 26.035 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "ESP32-WROOM-32-DevKit-30Pin"
			(at 5.08 -25.4 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Charger:ESP32-WROOM-32-DevKit-30Pin"
			(at 0 -27.94 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32_datasheet_en.pdf"
			(at 0 -30.48 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "RF Radio BT ESP ESP32 Espressif onboard PCB antenna"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "ESP32?WROOM?32*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "ESP32-WROOM-32-DevKit-30Pin_0_1"
			(rectangle
				(start -12.7 21.59)
				(end 12.7 -21.59)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(text "VReg on board\nsupply only VIN or 3V3"
				(at 0 15.24 0)
				(effects
					(font
						(size 1 1)
					)
				)
			)
		)
		(symbol "ESP32-WROOM-32-DevKit-30Pin_1_1"
			(pin power_in line
				(at -1.27 24.13 270)
				(length 2.54)
				(name "VIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "D32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "D35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "D34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "D39/VN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "D36/VP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "D23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "D22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "TX0/D1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "RX0/D3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -1.27 -24.13 90)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "D21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "D19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "D18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "D5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "TX2/D17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "RX2/D16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "D4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "D2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "D15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 1.27 -24.13 90)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "D13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 1.27 24.13 270)
				(length 2.54)
				(name "3V3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "D12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "D14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "D27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "D26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "D25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "D33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "SN75LVDS83B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U14"
			(at 14.605 57.15 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "SN75LVDS83B"
			(at 14.605 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_SO:TSSOP-56_6.1x14mm_P0.5mm"
			(at 0 68.58 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn75lvds83b.pdf?ts=1730295288259&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FSN75LVDS83B"
			(at 0 68.58 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "SN75LVDS83B_0_1"
			(rectangle
				(start -13.97 58.42)
				(end 13.97 -58.42)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(symbol "SN75LVDS83B_1_1"
			(pin power_in line
				(at -7.62 60.96 270)
				(length 2.54)
				(name "IOVCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 -8.89 0)
				(length 2.54)
				(name "D11/G7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 1.27 0)
				(length 2.54)
				(name "D12/G3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 -1.27 0)
				(length 2.54)
				(name "D13/G4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 0 -60.96 90)
				(length 2.54) hide
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 -3.81 0)
				(length 2.54)
				(name "D14/G5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 -16.51 0)
				(length 2.54)
				(name "D15/B0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 -31.75 0)
				(length 2.54)
				(name "D16/B6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 -45.72 0)
				(length 2.54)
				(name "CLKSEL"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 -34.29 0)
				(length 2.54)
				(name "D17/B7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 -19.05 0)
				(length 2.54)
				(name "D18/B1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 16.51 0)
				(length 2.54)
				(name "D5/R7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 -21.59 0)
				(length 2.54)
				(name "D19/B2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 0 -60.96 90)
				(length 2.54) hide
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 -24.13 0)
				(length 2.54)
				(name "D20/B3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 -26.67 0)
				(length 2.54)
				(name "D21/B4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 -29.21 0)
				(length 2.54)
				(name "D22/B5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 -49.53 0)
				(length 2.54)
				(name "D23/RSVD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 60.96 270)
				(length 2.54) hide
				(name "IOVCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 41.91 0)
				(length 2.54)
				(name "D24/HSYNC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 46.99 0)
				(length 2.54)
				(name "D25/VSYNC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 0 -60.96 90)
				(length 2.54) hide
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 21.59 0)
				(length 2.54)
				(name "D6/R5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 44.45 0)
				(length 2.54)
				(name "D26/ENABLE"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 49.53 0)
				(length 2.54)
				(name "CLKIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 -41.91 0)
				(length 2.54)
				(name "~{SHTDN}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 0 -60.96 90)
				(length 2.54) hide
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 7.62 60.96 270)
				(length 2.54)
				(name "PLLVCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 0 -60.96 90)
				(length 2.54) hide
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 0 -60.96 90)
				(length 2.54) hide
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 16.51 5.08 180)
				(length 2.54)
				(name "Y3P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 16.51 7.62 180)
				(length 2.54)
				(name "Y3M"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 16.51 -3.81 180)
				(length 2.54)
				(name "CLKOUTP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 8.89 0)
				(length 2.54)
				(name "D7/G0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 16.51 -1.27 180)
				(length 2.54)
				(name "CLKOUTM"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 16.51 13.97 180)
				(length 2.54)
				(name "Y2P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 16.51 16.51 180)
				(length 2.54)
				(name "Y2M"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 0 -60.96 90)
				(length 2.54) hide
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 60.96 270)
				(length 2.54)
				(name "LCDSVCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 16.51 22.86 180)
				(length 2.54)
				(name "Y1P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 16.51 25.4 180)
				(length 2.54)
				(name "Y1M"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 16.51 31.75 180)
				(length 2.54)
				(name "Y0P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 16.51 34.29 180)
				(length 2.54)
				(name "Y0M"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 0 -60.96 90)
				(length 2.54) hide
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "49"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 0 -60.96 90)
				(length 2.54)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 19.05 0)
				(length 2.54)
				(name "D27/R6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "50"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 34.29 0)
				(length 2.54)
				(name "D0/R0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "51"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 31.75 0)
				(length 2.54)
				(name "D1/R1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "52"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 0 -60.96 90)
				(length 2.54) hide
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "53"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 29.21 0)
				(length 2.54)
				(name "D2/R2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "54"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 26.67 0)
				(length 2.54)
				(name "D3/R3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "55"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 24.13 0)
				(length 2.54)
				(name "D4/R4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "56"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 6.35 0)
				(length 2.54)
				(name "D8/G1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 3.81 0)
				(length 2.54)
				(name "D9/G2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -16.51 -6.35 0)
				(length 2.54)
				(name "D10/G6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -2.54 60.96 270)
				(length 2.54)
				(name "VCC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "STM32H753IITx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U4"
			(at 0 42.545 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "STM32H753IITx"
			(at 0 40.005 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_QFP:LQFP-176_24x24mm_P0.5mm"
			(at 21.336 47.244 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h753ii.pdf"
			(at -3.556 43.18 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M7 MCU, 2048KB flash, 1024KB RAM, 480 MHz, 1.62-3.6V, 140 GPIO, LQFP176"
			(at -3.556 43.18 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_keywords" "Arm Cortex-M7 STM32H7 STM32H743/753"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_fp_filters" "LQFP*24x24mm*P0.5mm*"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "STM32H753IITx_1_1"
			(rectangle
				(start -10.16 30.48)
				(end 10.16 -30.48)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at -15.24 1.27 0)
				(length 5.08) hide
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "102"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 3.81 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "103"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -15.24 1.27 0)
				(length 5.08) hide
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "113"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 -11.43 180)
				(length 5.08)
				(name "VDD33_USB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "114"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 15.24 -24.13 180)
				(length 5.08)
				(name "VCAP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "125"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -15.24 1.27 0)
				(length 5.08) hide
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "126"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 1.27 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "127"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -15.24 1.27 0)
				(length 5.08) hide
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "135"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 -1.27 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "136"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -15.24 1.27 0)
				(length 5.08)
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -15.24 1.27 0)
				(length 5.08) hide
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "148"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 -3.81 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "149"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 24.13 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -15.24 1.27 0)
				(length 5.08) hide
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "158"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 -6.35 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "159"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 -8.89 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "172"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -15.24 1.27 0)
				(length 5.08) hide
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 21.59 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 19.05 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -15.24 -1.27 0)
				(length 5.08)
				(name "VSSA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 15.24 -19.05 180)
				(length 5.08)
				(name "VREF+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin power_in line
				(at 15.24 -13.97 180)
				(length 5.08)
				(name "VDDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -15.24 1.27 0)
				(length 5.08) hide
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 16.51 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "49"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 26.67 180)
				(length 5.08)
				(name "VBAT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -15.24 1.27 0)
				(length 5.08) hide
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "61"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 13.97 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "62"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -15.24 1.27 0)
				(length 5.08) hide
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "71"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 11.43 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "72"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 15.24 -26.67 180)
				(length 5.08)
				(name "VCAP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "81"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 8.89 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "82"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -15.24 1.27 0)
				(length 5.08) hide
				(name "VSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "90"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 15.24 6.35 180)
				(length 5.08)
				(name "VDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "91"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "STM32H753IITx_2_1"
			(rectangle
				(start -10.16 31.75)
				(end 10.16 -31.75)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 5.08)
				(name "PE2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI4_CK1" bidirectional line)
				(alternate "SAI4_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 5.08)
				(name "PD12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "100"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 5.08)
				(name "PD13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "101"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 5.08)
				(name "PG3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "107"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FMC_A13" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_BKIN2_COMP1" bidirectional line)
				(alternate "TIM8_BKIN2_COMP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 5.08)
				(name "PI9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D30" bidirectional line)
				(alternate "LTDC_VSYNC" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "PC6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "115"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "HRTIM_CHA1" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LTDC_HSYNC" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "SWPMI1_IO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "PC7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "116"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "HRTIM_CHA2" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LTDC_G6" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "SWPMI1_TX" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "PC8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "117"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "HRTIM_CHB1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SWPMI1_RX" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 5.08)
				(name "PA10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "121"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D1" bidirectional line)
				(alternate "HRTIM_CHC2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LTDC_B1" bidirectional line)
				(alternate "LTDC_B4" bidirectional line)
				(alternate "MDIOS_MDIO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_FS_ID" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "PH15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "130"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "FMC_D23" bidirectional line)
				(alternate "LTDC_G4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 5.08)
				(name "PI0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "131"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_D24" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LTDC_G5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 5.08)
				(name "PI1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "132"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D8" bidirectional line)
				(alternate "FMC_D25" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LTDC_G6" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_BKIN2_COMP1" bidirectional line)
				(alternate "TIM8_BKIN2_COMP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 5.08)
				(name "PI3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "134"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_D27" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 5.08)
				(name "PA15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "138"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "HRTIM_FLT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "PC10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "139"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D8" bidirectional line)
				(alternate "DFSDM1_CKIN5" bidirectional line)
				(alternate "HRTIM_EEV1" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LTDC_R2" bidirectional line)
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "PC11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "140"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DFSDM1_DATIN5" bidirectional line)
				(alternate "HRTIM_FLT2" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "QUADSPI_BK2_NCS" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 5.08)
				(name "PD3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "145"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LTDC_G7" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 5.08)
				(name "PD4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "146"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "HRTIM_FLT3" bidirectional line)
				(alternate "SAI3_FS_A" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 5.08)
				(name "PD7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "151"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "DFSDM1_DATIN4" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPDIFRX1_IN0" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "PG9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "152"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "QUADSPI_BK2_IO2" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPDIFRX1_IN3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 5.08)
				(name "PG13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "156"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "HRTIM_EEV10" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LTDC_R0" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 5.08)
				(name "PG14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "157"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LTDC_B0" bidirectional line)
				(alternate "QUADSPI_BK2_IO3" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 5.08)
				(name "PB5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "163"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "HRTIM_EEV7" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D7" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 5.08)
				(name "PI6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "175"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FMC_D28" bidirectional line)
				(alternate "LTDC_B6" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 5.08)
				(name "PI7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "176"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FMC_D29" bidirectional line)
				(alternate "LTDC_B7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 5.08)
				(name "PE3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SAI4_SD_B" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 5.08)
				(name "PF6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC3_INN4" bidirectional line)
				(alternate "ADC3_INP8" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SAI4_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 5.08)
				(name "PF7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC3_INP3" bidirectional line)
				(alternate "QUADSPI_BK1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SAI4_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 5.08)
				(name "PF8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC3_INN3" bidirectional line)
				(alternate "ADC3_INP7" bidirectional line)
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SAI4_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 5.08)
				(name "PF9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC3_INP2" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "QUADSPI_BK1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SAI4_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 5.08)
				(name "PB2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "58"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI4_D1" bidirectional line)
				(alternate "SAI4_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 5.08)
				(name "PI8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "PC13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "PH6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "83"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "PH7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "84"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "PH9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "86"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_D17" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LTDC_R3" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "PH10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "87"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FMC_D18" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LTDC_R4" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "PH11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "88"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_D19" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LTDC_R5" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "PH12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "89"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_D20" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LTDC_R6" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 5.08)
				(name "PD11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "99"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
		)
		(symbol "STM32H753IITx_3_1"
			(rectangle
				(start -6.35 38.1)
				(end 6.35 -38.1)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(text "LTDC"
				(at -2.54 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(pin bidirectional line
				(at 11.43 -3.81 180)
				(length 5.08)
				(name "PG6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "110"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "HRTIM_CHE1" bidirectional line)
				(alternate "LTDC_R7" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 -6.35 180)
				(length 5.08)
				(name "PG7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "111"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "HRTIM_CHE2" bidirectional line)
				(alternate "LTDC_CLK" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 8.89 180)
				(length 5.08)
				(name "PC9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "118"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S_CKIN" bidirectional line)
				(alternate "LTDC_B2" bidirectional line)
				(alternate "LTDC_G3" bidirectional line)
				(alternate "QUADSPI_BK1_IO0" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "SWPMI1_SUSPEND" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 26.67 180)
				(length 5.08)
				(name "PA8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "119"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "HRTIM_CHB2" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LTDC_B3" bidirectional line)
				(alternate "LTDC_R6" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_BKIN2_COMP1" bidirectional line)
				(alternate "TIM8_BKIN2_COMP2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_OTG_FS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 -31.75 180)
				(length 5.08)
				(name "PI10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "FMC_D31" bidirectional line)
				(alternate "LTDC_HSYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 -34.29 180)
				(length 5.08)
				(name "PI11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "LTDC_G6" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 -24.13 180)
				(length 5.08)
				(name "PI2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "133"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D9" bidirectional line)
				(alternate "FMC_D26" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LTDC_G7" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 -8.89 180)
				(length 5.08)
				(name "PG10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "153"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "HRTIM_FLT5" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "LTDC_B2" bidirectional line)
				(alternate "LTDC_G3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 -11.43 180)
				(length 5.08)
				(name "PG12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "155"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "HRTIM_EEV5" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LTDC_B1" bidirectional line)
				(alternate "LTDC_B4" bidirectional line)
				(alternate "SPDIFRX1_IN1" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 19.05 180)
				(length 5.08)
				(name "PB8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "167"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DFSDM1_CKIN7" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LTDC_B6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SDMMC2_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 16.51 180)
				(length 5.08)
				(name "PB9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "168"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DFSDM1_DATIN7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LTDC_B7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 -26.67 180)
				(length 5.08)
				(name "PI4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "173"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_NBL2" bidirectional line)
				(alternate "LTDC_B4" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_BKIN_COMP1" bidirectional line)
				(alternate "TIM8_BKIN_COMP2" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 -29.21 180)
				(length 5.08)
				(name "PI5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "174"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NBL3" bidirectional line)
				(alternate "LTDC_B5" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 -1.27 180)
				(length 5.08)
				(name "PF10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC3_INN2" bidirectional line)
				(alternate "ADC3_INP6" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "LTDC_DE" bidirectional line)
				(alternate "QUADSPI_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI4_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 6.35 180)
				(length 5.08)
				(name "PE4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "LTDC_B0" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SAI4_D2" bidirectional line)
				(alternate "SAI4_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 11.43 180)
				(length 5.08)
				(name "PC0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "ADC3_INP10" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "DFSDM1_DATIN4" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "LTDC_R5" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_STP" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 3.81 180)
				(length 5.08)
				(name "PE5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "LTDC_G0" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SAI4_CK2" bidirectional line)
				(alternate "SAI4_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 -13.97 180)
				(length 5.08)
				(name "PH2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC3_INP13" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LTDC_R0" bidirectional line)
				(alternate "QUADSPI_BK2_IO0" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 -16.51 180)
				(length 5.08)
				(name "PH3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC3_INN13" bidirectional line)
				(alternate "ADC3_INP14" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "LTDC_R1" bidirectional line)
				(alternate "QUADSPI_BK2_IO1" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 -19.05 180)
				(length 5.08)
				(name "PH4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC3_INN14" bidirectional line)
				(alternate "ADC3_INP15" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LTDC_G4" bidirectional line)
				(alternate "LTDC_G5" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 1.27 180)
				(length 5.08)
				(name "PE6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "LTDC_G1" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SAI4_D1" bidirectional line)
				(alternate "SAI4_SD_A" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_BKIN2_COMP1" bidirectional line)
				(alternate "TIM1_BKIN2_COMP2" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 34.29 180)
				(length 5.08)
				(name "PA4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "50"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LTDC_VSYNC" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USB_OTG_HS_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 31.75 180)
				(length 5.08)
				(name "PA5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "51"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LTDC_R4" bidirectional line)
				(alternate "PWR_NDSTOP2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 29.21 180)
				(length 5.08)
				(name "PA6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "52"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "LTDC_G2" bidirectional line)
				(alternate "MDIOS_MDC" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_BKIN_COMP1" bidirectional line)
				(alternate "TIM1_BKIN_COMP2" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_BKIN_COMP1" bidirectional line)
				(alternate "TIM8_BKIN_COMP2" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 24.13 180)
				(length 5.08)
				(name "PB0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "56"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LTDC_G1" bidirectional line)
				(alternate "LTDC_R3" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D1" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 21.59 180)
				(length 5.08)
				(name "PB1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "57"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LTDC_G0" bidirectional line)
				(alternate "LTDC_R6" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D2" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 13.97 180)
				(length 5.08)
				(name "PB10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "79"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DFSDM1_DATIN7" bidirectional line)
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "HRTIM_SCOUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LTDC_G4" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D3" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 -21.59 180)
				(length 5.08)
				(name "PH8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "85"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "FMC_D16" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LTDC_R2" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
			)
		)
		(symbol "STM32H753IITx_4_1"
			(rectangle
				(start -6.35 12.7)
				(end 6.35 -12.7)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(text "ETH"
				(at -2.032 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(pin bidirectional line
				(at 11.43 -5.08 180)
				(length 5.08)
				(name "PC1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "ADC3_INN10" bidirectional line)
				(alternate "ADC3_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "DFSDM1_CKIN4" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "MDIOS_MDC" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI4_D1" bidirectional line)
				(alternate "SAI4_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 10.16 180)
				(length 5.08)
				(name "PA1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_INN16" bidirectional line)
				(alternate "ADC1_INP17" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LTDC_R2" bidirectional line)
				(alternate "QUADSPI_BK1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 7.62 180)
				(length 5.08)
				(name "PA2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "LTDC_R1" bidirectional line)
				(alternate "MDIOS_MDIO" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 5.08 180)
				(length 5.08)
				(name "PA7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "53"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 -7.62 180)
				(length 5.08)
				(name "PC4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "54"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SPDIFRX1_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 -10.16 180)
				(length 5.08)
				(name "PC5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "55"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI4_D3" bidirectional line)
				(alternate "SPDIFRX1_IN3" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 2.54 180)
				(length 5.08)
				(name "PB11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "80"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DFSDM1_CKIN7" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "HRTIM_SCIN" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LTDC_G5" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D4" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 0 180)
				(length 5.08)
				(name "PB12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "92"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_BKIN_COMP1" bidirectional line)
				(alternate "TIM1_BKIN_COMP2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USB_OTG_HS_ID" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 11.43 -2.54 180)
				(length 5.08)
				(name "PB13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "93"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D6" bidirectional line)
				(alternate "USB_OTG_HS_VBUS" bidirectional line)
			)
		)
		(symbol "STM32H753IITx_5_1"
			(rectangle
				(start -7.62 27.94)
				(end 7.62 -27.94)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(text "FMC"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "PD14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "104"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "SAI3_MCLK_B" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "PD15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "105"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "SAI3_MCLK_A" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -11.43 0)
				(length 5.08)
				(name "PG2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "106"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FMC_A12" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_BKIN_COMP1" bidirectional line)
				(alternate "TIM8_BKIN_COMP2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -13.97 0)
				(length 5.08)
				(name "PG4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "108"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_BKIN2_COMP1" bidirectional line)
				(alternate "TIM1_BKIN2_COMP2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -16.51 0)
				(length 5.08)
				(name "PG5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "109"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -19.05 0)
				(length 5.08)
				(name "PG8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "112"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "LTDC_G7" bidirectional line)
				(alternate "SPDIFRX1_IN2" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 5.08)
				(name "PD0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "142"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DFSDM1_CKIN6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "SAI3_SCK_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "PD1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "143"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DFSDM1_DATIN6" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "SAI3_SD_A" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 21.59 0)
				(length 5.08)
				(name "PF0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -21.59 0)
				(length 5.08)
				(name "PG15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "160"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 5.08)
				(name "PE0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "169"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "HRTIM_SCIN" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 19.05 0)
				(length 5.08)
				(name "PF1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "PE1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "170"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "HRTIM_SCOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 16.51 0)
				(length 5.08)
				(name "PF2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 13.97 0)
				(length 5.08)
				(name "PF3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC3_INP5" bidirectional line)
				(alternate "FMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 11.43 0)
				(length 5.08)
				(name "PF4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC3_INN5" bidirectional line)
				(alternate "ADC3_INP9" bidirectional line)
				(alternate "FMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 8.89 0)
				(length 5.08)
				(name "PF5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC3_INP4" bidirectional line)
				(alternate "FMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 5.08)
				(name "PC2_C"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC3_INN1" bidirectional line)
				(alternate "ADC3_INP0" bidirectional line)
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 5.08)
				(name "PC3_C"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC3_INP1" bidirectional line)
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -24.13 0)
				(length 5.08)
				(name "PH5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC3_INN15" bidirectional line)
				(alternate "ADC3_INP16" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 6.35 0)
				(length 5.08)
				(name "PF11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "59"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 3.81 0)
				(length 5.08)
				(name "PF12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "60"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 1.27 0)
				(length 5.08)
				(name "PF13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "63"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "DFSDM1_DATIN6" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -1.27 0)
				(length 5.08)
				(name "PF14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "64"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "DFSDM1_CKIN6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -3.81 0)
				(length 5.08)
				(name "PF15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "65"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -6.35 0)
				(length 5.08)
				(name "PG0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "66"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -8.89 0)
				(length 5.08)
				(name "PG1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "67"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FMC_A11" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "PE7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "68"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "QUADSPI_BK2_IO0" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "PE8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "69"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "OPAMP2_VINM0" bidirectional line)
				(alternate "QUADSPI_BK2_IO1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "PE9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "70"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "QUADSPI_BK2_IO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 5.08)
				(name "PE10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "73"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DFSDM1_DATIN4" bidirectional line)
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "QUADSPI_BK2_IO3" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 5.08)
				(name "PE11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "74"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DFSDM1_CKIN4" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "LTDC_G3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 5.08)
				(name "PE12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "75"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DFSDM1_DATIN5" bidirectional line)
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "LTDC_B4" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 5.08)
				(name "PE13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "76"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "DFSDM1_CKIN5" bidirectional line)
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "LTDC_DE" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 5.08)
				(name "PE14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "77"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "LTDC_CLK" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 24.13 0)
				(length 5.08)
				(name "PE15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "78"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "LTDC_R7" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_BKIN_COMP1" bidirectional line)
				(alternate "TIM1_BKIN_COMP2" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "PD8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "96"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "SAI3_SCK_B" bidirectional line)
				(alternate "SPDIFRX1_IN1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "PD9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "97"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "SAI3_SD_B" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "PD10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "98"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LTDC_B3" bidirectional line)
				(alternate "SAI3_FS_B" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
		)
		(symbol "STM32H753IITx_6_1"
			(rectangle
				(start -7.62 19.05)
				(end 7.62 -19.05)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "PC15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "PA13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "124"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "PA14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "137"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 5.08)
				(name "PB3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "161"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "HRTIM_FLT4" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "BOOT0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "166"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "PDR_ON"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "171"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 5.08)
				(name "PH0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 5.08)
				(name "PH1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "NRST"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "PC14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
		)
		(symbol "STM32H753IITx_7_1"
			(rectangle
				(start -7.62 30.48)
				(end 7.62 -30.48)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(text "CAN"
				(at -2.54 15.494 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(text "I2C"
				(at -2.032 -25.654 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(text "SDMMC"
				(at -2.54 2.54 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(text "UART"
				(at -2.032 -10.668 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(text "USART"
				(at -2.032 -18.288 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(text "USB"
				(at -2.54 25.908 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(pin bidirectional line
				(at 12.7 26.67 180)
				(length 5.08)
				(name "PA9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "120"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "HRTIM_CHC1" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LTDC_R5" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USB_OTG_FS_VBUS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 24.13 180)
				(length 5.08)
				(name "PA11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "122"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "HRTIM_CHD1" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "LTDC_R4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_OTG_FS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 21.59 180)
				(length 5.08)
				(name "PA12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "123"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "HRTIM_CHD2" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LTDC_R5" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_OTG_FS_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 16.51 180)
				(length 5.08)
				(name "PH13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "128"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D21" bidirectional line)
				(alternate "LTDC_G2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 13.97 180)
				(length 5.08)
				(name "PH14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "129"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D22" bidirectional line)
				(alternate "LTDC_G3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -8.89 180)
				(length 5.08)
				(name "PC12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "141"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "HRTIM_EEV2" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -11.43 180)
				(length 5.08)
				(name "PD2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "144"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -19.05 180)
				(length 5.08)
				(name "PD5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "147"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "HRTIM_EEV3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -1.27 180)
				(length 5.08)
				(name "PD6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "150"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_D10" bidirectional line)
				(alternate "DFSDM1_CKIN4" bidirectional line)
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LTDC_B2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI4_D1" bidirectional line)
				(alternate "SAI4_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -3.81 180)
				(length 5.08)
				(name "PG11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "154"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ADC3_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "HRTIM_EEV4" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LTDC_B3" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPDIFRX1_IN0" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 6.35 180)
				(length 5.08)
				(name "PB4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "162"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "HRTIM_EEV6" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -24.13 180)
				(length 5.08)
				(name "PB6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "164"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "DFSDM1_DATIN5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "HRTIM_EEV8" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "QUADSPI_BK1_NCS" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -26.67 180)
				(length 5.08)
				(name "PB7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "165"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "DFSDM1_CKIN5" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "HRTIM_EEV9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 8.89 180)
				(length 5.08)
				(name "PA0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_INP16" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -16.51 180)
				(length 5.08)
				(name "PA3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "LPTIM5_OUT" bidirectional line)
				(alternate "LTDC_B2" bidirectional line)
				(alternate "LTDC_B5" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USB_OTG_HS_ULPI_D0" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 3.81 180)
				(length 5.08)
				(name "PB14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "94"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USB_OTG_HS_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 1.27 180)
				(length 5.08)
				(name "PB15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "95"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC3_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USB_OTG_HS_DP" bidirectional line)
			)
		)
	)
	(symbol "TPS65105"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U1"
			(at -0.635 41.275 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "TPS65105"
			(at -0.635 38.735 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_SO:HTSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.4x7.8mm_Mask2.4x4.68mm"
			(at 0 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps65101.pdf?HQS=dis-mous-null-mousermode-dsf-pf-null-wwe&ts=1672757737464&ref_url=https%253A%252F%252Fwww.mouser.co.uk%252F"
			(at 0 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "TPS65105_1_1"
			(rectangle
				(start -10.16 36.83)
				(end 8.89 -38.1)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin input line
				(at 11.43 26.67 180)
				(length 2.54)
				(name "FB1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 11.43 -29.21 180)
				(length 2.54)
				(name "VCOM"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 11.43 15.24 180)
				(length 2.54)
				(name "VCOMIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 11.43 -21.59 180)
				(length 2.54)
				(name "FB3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 11.43 -16.51 180)
				(length 2.54)
				(name "OUT3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "C2+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "C2-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "C1+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "C1-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 11.43 8.89 180)
				(length 2.54)
				(name "DRV"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 1.27 -40.64 90)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -12.7 -29.21 0)
				(length 2.54)
				(name "FB4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 11.43 -6.35 180)
				(length 2.54)
				(name "REF"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 11.43 -1.27 180)
				(length 2.54)
				(name "FB2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at -12.7 24.13 0)
				(length 2.54)
				(name "COMP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "ENR"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 3.81 -40.64 90)
				(length 2.54)
				(name "PGND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at -12.7 -21.59 0)
				(length 2.54)
				(name "BASE"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "VIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 11.43 33.02 180)
				(length 2.54)
				(name "SW"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 11.43 30.48 180)
				(length 2.54)
				(name "SW"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -3.81 -40.64 90)
				(length 2.54)
				(name "PGND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -1.27 -40.64 90)
				(length 2.54)
				(name "PGND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 11.43 22.86 180)
				(length 2.54)
				(name "SUP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
)
