EESchema-DOCLIB  Version 2.0
#
$CMP SN75LVDS83BDGGR
D 10- to 135-MHz 28-bit LVDS transmitter/serializer & FlatLink integrated circuit
K
F https://www.ti.com/lit/gpn/SN75LVDS83B
$ENDCMP
#
#End Doc Library
