(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(uuid "0dca9b66-f638-4727-874b-1b91b6921c17")
	(paper "A4")
	(lib_symbols
		(symbol "Jumper:SolderJumper_3_Open"
			(pin_names
				(offset 0) hide)
			(exclude_from_sim yes)
			(in_bom no)
			(on_board yes)
			(property "Reference" "JP"
				(at -2.54 -2.54 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Value" "SolderJumper_3_Open"
				(at 0 2.794 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Footprint" ""
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "Solder Jumper, 3-pole, open"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_keywords" "Solder Jumper SPDT"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_fp_filters" "SolderJumper*Open*"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "SolderJumper_3_Open_0_1"
				(arc
					(start -1.016 1.016)
					(mid -2.0276 0)
					(end -1.016 -1.016)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start -1.016 1.016)
					(mid -2.0276 0)
					(end -1.016 -1.016)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -0.508 1.016)
					(end 0.508 -1.016)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -2.54 0) (xy -2.032 0)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.016 1.016) (xy -1.016 -1.016)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -1.27) (xy 0 -1.016)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 1.016) (xy 1.016 -1.016)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 0) (xy 2.032 0)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 1.016 -1.016)
					(mid 2.0276 0)
					(end 1.016 1.016)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 1.016 -1.016)
					(mid 2.0276 0)
					(end 1.016 1.016)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type outline)
					)
				)
			)
			(symbol "SolderJumper_3_Open_1_1"
				(pin passive line
					(at -5.08 0 0)
					(length 2.54)
					(name "A"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.54)
					(name "C"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 5.08 0 180)
					(length 2.54)
					(name "B"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "3"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
		)
		(symbol "power:+3V3"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Value" "+3V3"
				(at 0 3.556 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Footprint" ""
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" ""
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "Power symbol creates a global label with name \"+3V3\""
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "+3V3_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+3V3_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
		)
	)
	(junction
		(at 125.095 47.625)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "bcf88112-9e4f-4fa6-ad5c-4e11aab62804")
	)
	(wire
		(pts
			(xy 177.8 44.45) (xy 190.5 44.45)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "0cacb7b2-828e-468a-b028-da22591d57ac")
	)
	(wire
		(pts
			(xy 177.8 46.99) (xy 190.5 46.99)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "14d286a6-18ee-41d3-9a4d-773df509b7ca")
	)
	(wire
		(pts
			(xy 177.8 93.98) (xy 190.5 93.98)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "17e6f2b8-d691-4b5e-8551-54bce877833e")
	)
	(wire
		(pts
			(xy 177.8 130.81) (xy 190.5 130.81)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "26d4ad7c-b89d-4f97-affc-bf4b88d71548")
	)
	(wire
		(pts
			(xy 182.88 54.61) (xy 190.5 54.61)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "2afaf6e6-2157-4183-93e5-6357c3ab0ce2")
	)
	(wire
		(pts
			(xy 190.5 57.15) (xy 185.42 57.15)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "3bfb4c24-2752-416c-8624-7565e129dea8")
	)
	(wire
		(pts
			(xy 114.3 47.625) (xy 125.095 47.625)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "4bf57c7e-ab34-4063-b1fb-aa53287e6f4c")
	)
	(wire
		(pts
			(xy 177.8 91.44) (xy 190.5 91.44)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "5dd1b8d0-fb3c-4461-b61f-5abdfee04be4")
	)
	(wire
		(pts
			(xy 125.095 46.355) (xy 125.095 47.625)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "6025be00-c80f-456e-a00d-ec207ce81eac")
	)
	(wire
		(pts
			(xy 177.8 120.65) (xy 190.5 120.65)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "60f05adb-f60d-4875-8c08-177356e7200b")
	)
	(wire
		(pts
			(xy 177.8 77.47) (xy 182.88 77.47)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "7315155a-effe-46a2-a26c-29dea0224f4b")
	)
	(wire
		(pts
			(xy 177.8 138.43) (xy 190.5 138.43)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "7e3895eb-2358-4d1c-a72b-a571c054d981")
	)
	(wire
		(pts
			(xy 114.3 38.735) (xy 115.57 38.735)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "9821429e-68b7-4497-be1c-49c9c317e73a")
	)
	(wire
		(pts
			(xy 114.3 43.815) (xy 127 43.815)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "98fab502-4b37-4104-812a-28817f22f655")
	)
	(wire
		(pts
			(xy 127 46.355) (xy 125.095 46.355)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "9e9c8201-c0ba-45b7-8641-b4442e035449")
	)
	(wire
		(pts
			(xy 177.8 140.97) (xy 190.5 140.97)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "9fe83f71-9eab-4af6-8f62-4d9d37b78249")
	)
	(wire
		(pts
			(xy 182.88 77.47) (xy 182.88 54.61)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "aa2f43ad-7b2a-4e57-abd6-75993e299d19")
	)
	(wire
		(pts
			(xy 114.3 51.435) (xy 127 51.435)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "ad1cecd8-688d-46cd-b2d2-90564d76996e")
	)
	(wire
		(pts
			(xy 177.8 135.89) (xy 190.5 135.89)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "b216a0b9-561b-4a06-b6f6-a94249af4b25")
	)
	(wire
		(pts
			(xy 185.42 80.01) (xy 177.8 80.01)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "b75f1298-18fc-40f9-9756-b213d5f217ef")
	)
	(wire
		(pts
			(xy 153.67 60.96) (xy 153.67 73.66)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "ba840715-3e40-401c-9d02-6a24f9976ffc")
	)
	(wire
		(pts
			(xy 185.42 57.15) (xy 185.42 80.01)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "c0ebe27d-fb7d-4269-966d-e4c93372f711")
	)
	(wire
		(pts
			(xy 125.095 48.895) (xy 127 48.895)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "c4b687e4-363f-4e9a-8780-a69070456447")
	)
	(wire
		(pts
			(xy 158.75 60.96) (xy 158.75 73.66)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "d7ec212e-a90d-46b4-beb0-d322de6d3cb0")
	)
	(wire
		(pts
			(xy 161.29 60.96) (xy 161.29 73.66)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "d97b5ce5-48e8-4f17-ab96-c4ac65bfcaf7")
	)
	(wire
		(pts
			(xy 177.8 143.51) (xy 190.5 143.51)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "dcc71353-6f59-48c1-abf6-9615e09c65b6")
	)
	(wire
		(pts
			(xy 114.3 41.275) (xy 127 41.275)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "e4336981-5782-49ce-ad45-6e4bc8e6a28c")
	)
	(wire
		(pts
			(xy 125.095 47.625) (xy 125.095 48.895)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "ec081ed6-f16b-4763-9b7a-7dbf465c90af")
	)
	(wire
		(pts
			(xy 177.8 123.19) (xy 190.5 123.19)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "f3a35937-8835-45c7-9edd-4c16204460b4")
	)
	(wire
		(pts
			(xy 125.73 38.735) (xy 127 38.735)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "f4342269-3fd4-434b-b954-44565e85c6c1")
	)
	(wire
		(pts
			(xy 177.8 128.27) (xy 190.5 128.27)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "fc87f22e-7de3-46a8-9429-a26dc52e1f56")
	)
	(text "TODO:\n4. REFCLK0 pull-up?\n5. 5.6.3 ~{RST}\n6. series termination calculation\n8. ethernet ~{RST} discharge?\n12. DS90C385A?\n13. routing guidelines"
		(exclude_from_sim no)
		(at 74.93 182.118 0)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify left)
		)
		(uuid "b77f9553-b64d-4a04-bcaa-eb156863248b")
	)
	(symbol
		(lib_id "Jumper:SolderJumper_3_Open")
		(at 120.65 38.735 180)
		(unit 1)
		(exclude_from_sim yes)
		(in_bom no)
		(on_board yes)
		(dnp no)
		(uuid "4bb7830d-92cf-4db4-b890-6f418ae6fb60")
		(property "Reference" "JP1"
			(at 122.555 35.56 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "SolderJumper_3_Open"
			(at 124.46 26.035 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 120.65 38.735 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "~"
			(at 120.65 38.735 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Solder Jumper, 3-pole, open"
			(at 120.65 38.735 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "b19ccb07-8f92-4c19-8ac9-bafe24cdd7b8")
		)
		(pin "3"
			(uuid "815d8bda-b1a9-4f8a-a5b8-10e75e7d2ad3")
		)
		(pin "2"
			(uuid "a688e533-6a17-4690-9dac-ec41122ec8c5")
		)
		(instances
			(project ""
				(path "/0dca9b66-f638-4727-874b-1b91b6921c17"
					(reference "JP1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+3V3")
		(at 120.65 34.925 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "ed95c26d-df04-4bbd-8d92-ffd282e0abb3")
		(property "Reference" "#PWR01"
			(at 120.65 38.735 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" "+3V3"
			(at 120.65 29.845 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 120.65 34.925 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 120.65 34.925 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"+3V3\""
			(at 120.65 34.925 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "bd206165-8e5c-490e-8f6c-ed736ed737c9")
		)
		(instances
			(project "FT25-Charger"
				(path "/0dca9b66-f638-4727-874b-1b91b6921c17"
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(sheet
		(at 63.5 73.66)
		(size 50.546 30.48)
		(fields_autoplaced yes)
		(stroke
			(width 0.1524)
			(type solid)
		)
		(fill
			(color 0 0 0 0.0000)
		)
		(uuid "128393d2-6dd9-44f0-979c-682ff9f03572")
		(property "Sheetname" "SDRAM"
			(at 63.5 72.9484 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Sheetfile" "SDRAM.kicad_sch"
			(at 63.5 104.7246 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left top)
			)
		)
		(instances
			(project "FT25-Charger"
				(path "/0dca9b66-f638-4727-874b-1b91b6921c17"
					(page "9")
				)
			)
		)
	)
	(sheet
		(at 127 30.48)
		(size 50.8 30.48)
		(fields_autoplaced yes)
		(stroke
			(width 0.1524)
			(type solid)
		)
		(fill
			(color 0 0 0 0.0000)
		)
		(uuid "34256820-5635-4c85-a70b-596b3ee01bd0")
		(property "Sheetname" "Display"
			(at 127 29.7684 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Sheetfile" "Display.kicad_sch"
			(at 127 61.5446 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left top)
			)
		)
		(property "Field2" ""
			(at 127 30.48 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "VCOM" input
			(at 127 51.435 180)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "3816bc7e-ee37-4195-854a-ef6440631568")
		)
		(pin "LCD_VDD" input
			(at 127 38.735 180)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "833577a5-95dc-4c3f-9b0a-2b6806adc8ae")
		)
		(pin "LED+" input
			(at 127 48.895 180)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "5bec4186-7cff-4de9-87d8-239b46e1f0de")
		)
		(pin "I2C_SCL" input
			(at 177.8 46.99 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
			(uuid "f4c38e29-beea-44cb-a561-64f5a9911c76")
		)
		(pin "PCAP_Int" input
			(at 158.75 60.96 270)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "62b05ffa-2d66-4e71-9358-b43a1080656d")
		)
		(pin "I2C_SDA" bidirectional
			(at 177.8 44.45 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
			(uuid "b126d798-02d8-4942-b520-01e739e24e0a")
		)
		(pin "PCAP_RST" input
			(at 161.29 60.96 270)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "20210132-3e45-49eb-a1f2-812fa35e183e")
		)
		(pin "LCD_VGH" input
			(at 127 41.275 180)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "9a2964f7-dcb3-435b-8dcf-65450fec93a9")
		)
		(pin "LCD_VGL" input
			(at 127 43.815 180)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "b49a99ac-0f56-4aeb-91e1-d7644aa1a90c")
		)
		(pin "LCD_AVDD" input
			(at 127 46.355 180)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "61e5f3b9-926b-4d1e-820d-2bd639b67b0d")
		)
		(pin "LCD_Reset" input
			(at 153.67 60.96 270)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "fbf4a5ae-f8cf-4900-8590-f1eac8b3cee6")
		)
		(instances
			(project "FT25-Charger"
				(path "/0dca9b66-f638-4727-874b-1b91b6921c17"
					(page "9")
				)
			)
		)
	)
	(sheet
		(at 127 73.66)
		(size 50.8 73.66)
		(fields_autoplaced yes)
		(stroke
			(width 0.1524)
			(type solid)
		)
		(fill
			(color 0 0 0 0.0000)
		)
		(uuid "486f4a0e-b8d5-42cd-a726-c7aa5b0383fd")
		(property "Sheetname" "Core"
			(at 127 72.9484 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Sheetfile" "Core.kicad_sch"
			(at 127 147.9046 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left top)
			)
		)
		(pin "PCAP_RST" input
			(at 161.29 73.66 90)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
			(uuid "e3e18945-5024-4afa-9e6f-aa2e6a66cfd9")
		)
		(pin "PCAP_Int" input
			(at 158.75 73.66 90)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
			(uuid "4fa40e5f-480b-449b-b67c-c814866b6a63")
		)
		(pin "CANH" output
			(at 177.8 77.47 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
			(uuid "ba745a4d-2cfb-45af-9f1b-6faa6f0aa196")
		)
		(pin "CANL" output
			(at 177.8 80.01 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
			(uuid "4e93f07a-4621-403e-b26f-1cdd4043fdb1")
		)
		(pin "~{AMS_Error_LED}" output
			(at 177.8 120.65 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
			(uuid "0427c85c-84e6-48df-8d01-b094dc2312cc")
		)
		(pin "~{IMD_Error_LED}" output
			(at 177.8 123.19 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
			(uuid "71aea406-8d39-4bbc-a9e2-404317dfcf03")
		)
		(pin "SDC_enable" output
			(at 177.8 135.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
			(uuid "356e7d39-23fd-4cfb-b0ab-b26eeff80d0e")
		)
		(pin "AMS_Reset_out" input
			(at 177.8 130.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
			(uuid "f9ab0224-1e57-46a2-932c-8d13e647087b")
		)
		(pin "SDC_Voltage" input
			(at 177.8 143.51 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
			(uuid "09f8fc16-df20-4353-a0a3-3ff148136c7c")
		)
		(pin "SDC_in" input
			(at 177.8 138.43 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
			(uuid "39b1d835-1b17-4353-a561-530cfdbb07f3")
		)
		(pin "SDC_out" output
			(at 177.8 140.97 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
			(uuid "462dc091-717e-445c-9ccb-bcf244e3bcea")
		)
		(pin "AMS_Reset_in" output
			(at 177.8 128.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
			(uuid "9cb065ba-4d91-4a96-9a5a-6e77d7cfe390")
		)
		(pin "EV_Start_Charging" output
			(at 177.8 93.98 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
			(uuid "79bf9d22-0a93-4215-b737-9b2992bb6c6d")
		)
		(pin "Charging_Point_PWM" input
			(at 177.8 91.44 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
			(uuid "400055eb-9354-43a6-bbb6-e6f49a622ed5")
		)
		(pin "LCD_Reset" output
			(at 153.67 73.66 90)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
			(uuid "45810262-42ca-4bf5-b56c-adb2ac7bafc9")
		)
		(instances
			(project "FT25-Charger"
				(path "/0dca9b66-f638-4727-874b-1b91b6921c17"
					(page "4")
				)
			)
		)
	)
	(sheet
		(at 63.5 116.84)
		(size 50.8 30.48)
		(fields_autoplaced yes)
		(stroke
			(width 0.1524)
			(type solid)
		)
		(fill
			(color 0 0 0 0.0000)
		)
		(uuid "5469580a-3180-4bfd-8660-e5a4628a92d9")
		(property "Sheetname" "Ethernet"
			(at 63.5 116.1284 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Sheetfile" "Ethernet.kicad_sch"
			(at 63.5 147.9046 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left top)
			)
		)
		(instances
			(project "FT25-Charger"
				(path "/0dca9b66-f638-4727-874b-1b91b6921c17"
					(page "4")
				)
			)
		)
	)
	(sheet
		(at 190.5 116.84)
		(size 50.8 30.48)
		(fields_autoplaced yes)
		(stroke
			(width 0.1524)
			(type solid)
		)
		(fill
			(color 0 0 0 0.0000)
		)
		(uuid "75c94037-2217-4879-97cf-1bc2976ef0dc")
		(property "Sheetname" "SDC_and_SCS"
			(at 190.5 116.1284 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Sheetfile" "SDC_and_SCS.kicad_sch"
			(at 190.5 147.9046 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left top)
			)
		)
		(property "Field2" ""
			(at 190.5 116.84 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "~{IMD_Error_LED}" input
			(at 190.5 123.19 180)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "efb58820-83bc-424b-95f3-2fb058914d3e")
		)
		(pin "~{AMS_Error_LED}" input
			(at 190.5 120.65 180)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "a159e626-fcc3-4e1f-909e-a5917b863ccb")
		)
		(pin "AMS_Reset_in" input
			(at 190.5 128.27 180)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "1cf3b872-e697-433b-8dbd-7195a9e73264")
		)
		(pin "AMS_Reset_out" output
			(at 190.5 130.81 180)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "545ea471-bf17-44d3-99c8-fe48c00fd893")
		)
		(pin "SDC_enable" input
			(at 190.5 135.89 180)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "a8abaeea-a668-46bb-b5e7-f3cf1ce07f0b")
		)
		(pin "SDC_in" output
			(at 190.5 138.43 180)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "15c9950c-ec3e-4af1-bf46-01d63abf5762")
		)
		(pin "SDC_Voltage" output
			(at 190.5 143.51 180)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "5c6d18a7-241d-4ab1-b3d3-3581f6a2cef2")
		)
		(pin "SDC_out" input
			(at 190.5 140.97 180)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "420b0c15-b784-4095-8679-fb98ddcf85a2")
		)
		(instances
			(project "FT25-Charger"
				(path "/0dca9b66-f638-4727-874b-1b91b6921c17"
					(page "7")
				)
			)
		)
	)
	(sheet
		(at 190.5 30.48)
		(size 50.8 30.48)
		(fields_autoplaced yes)
		(stroke
			(width 0.1524)
			(type solid)
		)
		(fill
			(color 0 0 0 0.0000)
		)
		(uuid "80927836-8e39-47ea-8430-ab9d018fcb5d")
		(property "Sheetname" "Peripherals"
			(at 190.5 29.7684 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Sheetfile" "Peripherals.kicad_sch"
			(at 190.5 61.5446 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left top)
			)
		)
		(property "Field2" ""
			(at 190.5 30.48 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "CANL" output
			(at 190.5 57.15 180)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "594eae58-b3ae-495d-a6f8-492ba17e0522")
		)
		(pin "I2C_SDA" bidirectional
			(at 190.5 44.45 180)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "e1a21df7-7d3f-45fa-b65a-8b054068756f")
		)
		(pin "I2C_SCL" output
			(at 190.5 46.99 180)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "dd32d4ab-dc8a-451d-b1e5-8d92fc8fc43e")
		)
		(pin "CANH" output
			(at 190.5 54.61 180)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "27e51e44-3361-47de-b3d3-8491ec931bf7")
		)
		(instances
			(project "FT25-Charger"
				(path "/0dca9b66-f638-4727-874b-1b91b6921c17"
					(page "10")
				)
			)
		)
	)
	(sheet
		(at 190.5 73.66)
		(size 50.8 30.48)
		(fields_autoplaced yes)
		(stroke
			(width 0.1524)
			(type solid)
		)
		(fill
			(color 0 0 0 0.0000)
		)
		(uuid "821f8254-7e97-454c-9aee-86b4ab099a85")
		(property "Sheetname" "IEC_Charging_Circuit"
			(at 190.5 72.9484 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Sheetfile" "IEC_Charging_Circuit.kicad_sch"
			(at 190.5 104.7246 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left top)
			)
		)
		(property "Field2" ""
			(at 190.5 73.66 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "Charging_Point_PWM" output
			(at 190.5 91.44 180)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "2af6d41f-5d0e-41ad-99d0-1e60204cd27a")
		)
		(pin "EV_Start_Charging" input
			(at 190.5 93.98 180)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
			(uuid "b48fa48c-d674-409b-9ecd-d2e98dbc2adb")
		)
		(instances
			(project "FT25-Charger"
				(path "/0dca9b66-f638-4727-874b-1b91b6921c17"
					(page "6")
				)
			)
		)
	)
	(sheet
		(at 63.5 30.48)
		(size 50.8 30.48)
		(fields_autoplaced yes)
		(stroke
			(width 0.1524)
			(type solid)
		)
		(fill
			(color 0 0 0 0.0000)
		)
		(uuid "91c9895f-7dce-429f-866f-2980d966c967")
		(property "Sheetname" "Power"
			(at 63.5 29.7684 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Sheetfile" "Power.kicad_sch"
			(at 63.5 61.5446 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left top)
			)
		)
		(pin "3V3_Display" output
			(at 114.3 38.735 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
			(uuid "469f8fab-9bfc-4dc8-b9d7-c6d54d1a2584")
		)
		(pin "3V8" output
			(at 114.3 51.435 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
			(uuid "73449056-44d4-480a-b05b-850ea7f4a374")
		)
		(pin "18V" output
			(at 114.3 41.275 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
			(uuid "67dcf555-c746-42de-9a09-3853531a0eab")
		)
		(pin "-6V" output
			(at 114.3 43.815 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
			(uuid "53710fa2-9707-4618-8292-bf60fe93736f")
		)
		(pin "9V6" output
			(at 114.3 47.625 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
			(uuid "6985c10b-c346-4576-830b-9256c7d72372")
		)
		(instances
			(project "FT25-Charger"
				(path "/0dca9b66-f638-4727-874b-1b91b6921c17"
					(page "3")
				)
			)
		)
	)
	(sheet_instances
		(path "/"
			(page "1")
		)
	)
)
