(module Binder_M12-A_12P_Female_NoSilk (layer F.Cu) (tedit 61C3AB96)
  (fp_text reference J1 (at 0 -10.045) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Conn_01x12_Male (at 0 10.045) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 0 0) (end 9 0) (layer Dwgs.User) (width 0.1))
  (fp_circle (center 0 0) (end 0 9.37) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 0 -0.1) (end 0 -4.2) (layer F.Fab) (width 0.12))
  (fp_line (start 0.6 -3.7) (end 0.6 -4.1) (layer F.Fab) (width 0.12))
  (fp_line (start -0.6 -3.7) (end -0.6 -4.1) (layer F.Fab) (width 0.12))
  (fp_arc (start 0 -3.7) (end -0.6 -3.7) (angle -180) (layer F.Fab) (width 0.12))
  (pad 10 thru_hole circle (at 0 -1.1) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at 0.952627 0.549999) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at -0.952627 0.55) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -1.428 -2.524) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 1.428 -2.524) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 2.672 -1.127) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 2.804 0.738) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 1.77 2.297) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 0 2.9) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at -1.77 2.297) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at -2.804 0.738) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at -2.672 -1.127) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask))
  (model ${KIPRJMOD}/packages3d/Binder.3dshapes/Binder_SACC-DSI-M12MS-12CON-M16.stp
    (offset (xyz 12.7 0 -2.45))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 -180 -45))
  )
)
