(footprint "Phoenix_SACC-DSI-M8FS-8CON-M10"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -6 -2.75 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "b51065ed-ca1f-4093-8840-ee80a59c40bc")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "Phoenix_SACC-DSI-M8FS-8CON-M10"
		(at 0 4.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "50bdfe40-c0fa-43dd-957d-85fdc45bdb50")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "82a2213b-8d82-4892-9bbc-094b84015dd0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "90b4b0ee-d93b-48f6-a14a-a4d68f2e1c20")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "cba8b3c1-a062-4ba6-bce0-2debfeb73050")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_circle
		(center 0 0)
		(end 4 0)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "24848760-8873-4982-988c-833114c85a89")
	)
	(fp_circle
		(center 0 0)
		(end -6.25 0)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "6aaa6ba1-e153-49bb-8d52-8eb67d06ab0a")
	)
	(fp_text user "${REFERENCE}"
		(at 0 6 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "0da35195-988e-4351-8f90-cea69edc6416")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0.9 1.65)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "87a51578-6db1-4bde-8524-7d58da71d926")
	)
	(pad "2" thru_hole circle
		(at -0.9 1.65)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ff00cf00-759c-4704-9e3e-84f25eae3b0c")
	)
	(pad "3" thru_hole circle
		(at -1.85 0.35)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0f1b3ffc-b1b3-4b03-b461-7ca8af67c2f6")
	)
	(pad "4" thru_hole circle
		(at -1.45 -1.2)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "15cb901b-5956-4d34-9c88-4602c8b1328d")
	)
	(pad "5" thru_hole circle
		(at 0 -1.85)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "23e609eb-b984-4087-b890-eb8e16a508e5")
	)
	(pad "6" thru_hole circle
		(at 1.45 -1.2)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f88fab65-8381-4777-aa29-c230bd2d5b23")
	)
	(pad "7" thru_hole circle
		(at 1.85 0.35)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6af93209-f318-417f-b347-7be737afcb2a")
	)
	(pad "8" thru_hole circle
		(at 0 0)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "bb79a8fc-d9bb-458d-b33c-59362a722424")
	)
	(pad "MP" thru_hole circle
		(at -6.25 0)
		(size 3.6 3.6)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3b80d336-5e33-4b32-b49a-7f4fb60bd3e7")
	)
	(pad "MP" thru_hole circle
		(at 6.25 0)
		(size 3.6 3.6)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b67b52ac-70c3-4a8b-b4bf-f3a92a82506e")
	)
	(model "${KIPRJMOD}/3d/pxc_1424235_03_00_SACC-DSI-M8FS-8CON-M10-L180-SH_3D.stp"
		(offset
			(xyz 0 0 -2.7)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 180)
		)
	)
)
