(footprint "WE-LQS_8040"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "<b>WE-LQS SMD Power Inductor<br></b><br></b>Size: 8040, SMT, 2pins<br>LxWxH= 8mmx8mmx4.2mm")
	(property "Reference" "REF**"
		(at 0 -5.435 0)
		(layer "F.SilkS")
		(uuid "eb17e6d5-08db-4185-b94b-43e0e7fca1f3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "WE-LQS_8040"
		(at 0 5.365 0)
		(layer "F.Fab")
		(uuid "3874ce6d-ca6b-4177-a594-9326eb6acedb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "96cb8930-032d-4b62-b605-eb2591763655")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "3649e519-47d8-4d8b-9475-ebe3e5c118e2")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -4 -4.1)
		(end 4 -4.1)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "590392f2-1210-4f62-866f-247a10032d44")
	)
	(fp_line
		(start -4 4.1)
		(end 4 4.1)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2371d563-a955-4732-9227-3e22d4015c7f")
	)
	(fp_circle
		(center 5.2 3.5)
		(end 5.4 3.5)
		(stroke
			(width 0.4)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "34350fbc-278f-42f7-ac21-7901cb868f5a")
	)
	(fp_poly
		(pts
			(xy -4.5 -4.3) (xy 4.5 -4.3) (xy 4.5 4.3) (xy -4.5 4.3)
		)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill yes)
		(layer "F.CrtYd")
		(uuid "01e3dbc1-771e-4130-9298-72657eb269b2")
	)
	(fp_line
		(start -4 -4)
		(end -4 4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8bf950bd-dd63-4867-acc7-bae821daf188")
	)
	(fp_line
		(start -4 -4)
		(end 4 -4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4cf898db-a037-45da-b1fc-f92b0d5cfde1")
	)
	(fp_line
		(start -4 4)
		(end 4 4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "bab663bd-de57-4589-96c1-8218ffe9b71a")
	)
	(fp_line
		(start 4 -4)
		(end 4 4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f7f79822-fa8f-4790-a653-4242529be305")
	)
	(pad "1" smd rect
		(at -3.1 0)
		(size 2.4 7.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
		(uuid "48ca0e82-6d8a-4b2b-bdf8-2f5f5999004e")
	)
	(pad "2" smd rect
		(at 3.1 0)
		(size 2.4 7.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
		(uuid "6a045b5b-9be6-4ffe-87c9-c2b71c945644")
	)
	(embedded_fonts no)
	(model "C:/Users/georg/git/fsim_ff/fsim_ff.pretty/WE-LQS_8040_LQS (rev1).stp"
		(offset
			(xyz 0 0 2.2)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -90)
		)
	)
)
