(module "DIOM5226X244N" (layer F.Cu)
  (descr "3SMAJ5934B-TP")
  (tags "Zener Diode")
  (attr smd)
  (fp_text reference Z** (at 0 0) (layer F.SilkS)
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_text value "DIOM5226X244N" (at 0 0) (layer F.SilkS) hide
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_line (start -3.575 -1.71) (end 3.575 -1.71) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.575 -1.71) (end 3.575 1.71) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.575 1.71) (end -3.575 1.71) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.575 1.71) (end -3.575 -1.71) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.598 -1.292) (end 2.598 -1.292) (layer F.Fab) (width 0.1))
  (fp_line (start 2.598 -1.292) (end 2.598 1.292) (layer F.Fab) (width 0.1))
  (fp_line (start 2.598 1.292) (end -2.598 1.292) (layer F.Fab) (width 0.1))
  (fp_line (start -2.598 1.292) (end -2.598 -1.292) (layer F.Fab) (width 0.1))
  (fp_line (start -2.598 -0.518) (end -1.822 -1.292) (layer F.Fab) (width 0.1))
  (fp_line (start 2.598 -1.292) (end -2.925 -1.292) (layer F.SilkS) (width 0.2))
  (fp_line (start -2.598 1.292) (end 2.598 1.292) (layer F.SilkS) (width 0.2))
  (pad 1 smd rect (at -2.15 0 90) (size 1.55 2.35) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 2.15 0 90) (size 1.55 2.35) (layers F.Cu F.Paste F.Mask))
  (model 3SMAJ5934B-TP.stp
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
