(module "CAPAE830X900N" (layer F.Cu)
  (descr "8*8.7MM")
  (tags "Capacitor Polarised")
  (attr smd)
  (fp_text reference C** (at 0 0) (layer F.SilkS)
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_text value "CAPAE830X900N" (at 0 0) (layer F.SilkS) hide
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_line (start -5.475 -4.75) (end 5.475 -4.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.475 -4.75) (end 5.475 4.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.475 4.75) (end -5.475 4.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.475 4.75) (end -5.475 -4.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.15 -4.15) (end -2.075 -4.15) (layer F.Fab) (width 0.1))
  (fp_line (start -2.075 -4.15) (end -4.15 -2.075) (layer F.Fab) (width 0.1))
  (fp_line (start -4.15 -2.075) (end -4.15 2.075) (layer F.Fab) (width 0.1))
  (fp_line (start -4.15 2.075) (end -2.075 4.15) (layer F.Fab) (width 0.1))
  (fp_line (start -2.075 4.15) (end 4.15 4.15) (layer F.Fab) (width 0.1))
  (fp_line (start 4.15 4.15) (end 4.15 -4.15) (layer F.Fab) (width 0.1))
  (fp_line (start -4.975 -4.15) (end 4.15 -4.15) (layer F.SilkS) (width 0.2))
  (fp_line (start -2.075 4.15) (end 4.15 4.15) (layer F.SilkS) (width 0.2))
  (pad 1 smd rect (at -3.2 0 90) (size 2.15 3.55) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 3.2 0 90) (size 2.15 3.55) (layers F.Cu F.Paste F.Mask))
  (model 875115852001.stp
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
