(footprint "LFXTAL081781RL3K"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "crystal Epson Toyocom FA-238 https://support.epson.biz/td/api/doc_check.php?dl=brief_fa-238v_en.pdf, 3.2x2.5mm^2 package")
	(tags "SMD SMT crystal")
	(property "Reference" "REF**"
		(at -0.075 -1.775 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "5f5e01d8-9d8d-4443-a209-6125dd425c9f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "LFXTAL081781RL3K"
		(at 0 2.45 0)
		(layer "F.Fab")
		(uuid "11d05367-caf3-4ce6-ad30-324fe6c8f655")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "394ac66d-d65e-49cb-b386-a6091e701b03")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "eb633373-b3d5-4385-b8c9-d84762d16190")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2f7b7400-f7ed-430f-b053-9f995dbbd428")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2 -0.85)
		(end -2 1.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2d4e5054-1ea8-4447-a374-cc871a70fb67")
	)
	(fp_line
		(start -2 1.6)
		(end 0.95 1.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d3ddc131-349e-484f-bc56-0bf0736cafa5")
	)
	(fp_line
		(start -2.1 -1.025)
		(end -2.1 1.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "3cf55d7f-695b-4bf8-a5ce-e512c3a3dc2a")
	)
	(fp_line
		(start -2.1 -1.025)
		(end 1.1 -1.025)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f1202206-8d36-4629-9ba7-784207b91e0d")
	)
	(fp_line
		(start -2.1 1.7)
		(end 1.1 1.7)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "8ddb9a7d-d2a8-4751-baf2-7d175211ce92")
	)
	(fp_line
		(start 1.1 -1.025)
		(end 1.1 1.6875)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c644e145-6a4e-497f-a6de-ccb9a6f7f68d")
	)
	(fp_line
		(start -1.6 -0.525)
		(end -1.5 -0.625)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "23ee9dc6-949f-4fe4-bc99-e6db53643eb7")
	)
	(fp_line
		(start -1.6 1.15)
		(end -1.6 -0.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a748639f-b71e-4259-a8db-e457693bb542")
	)
	(fp_line
		(start -1.5 -0.625)
		(end 0.575 -0.625)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1ae6bf33-82fc-4219-8842-031340933f0a")
	)
	(fp_line
		(start -1.5 1.25)
		(end -1.6 1.15)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5281ffb8-4661-4366-90e1-14eb88360e47")
	)
	(fp_line
		(start 0.55 1.25)
		(end -1.5 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e41db710-f5c2-4645-8470-1585b4c67ac3")
	)
	(fp_line
		(start 0.575 -0.625)
		(end 0.675 -0.525)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8ec5fcb3-611c-491c-ae2f-9ebfb5e396f6")
	)
	(fp_line
		(start 0.675 1.15)
		(end 0.575 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a877f32c-4d4e-4f97-9c6f-4c1ebc2993df")
	)
	(fp_line
		(start 0.675 1.15)
		(end 0.675 -0.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "67f4ef23-f5ad-44a6-9621-e992a3fc7bc7")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "1004a732-1e38-4a14-bc5e-29d57b1f8922")
		(effects
			(font
				(size 0.7 0.7)
				(thickness 0.105)
			)
		)
	)
	(pad "1" smd rect
		(at -1.1 -0.175)
		(size 0.875 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "0a5d0c31-e576-4298-9e66-34475b922ba8")
	)
	(pad "2" smd rect
		(at 0.175 -0.175)
		(size 0.875 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "32284a40-dc90-406b-b2da-600e01fe8a46")
	)
	(pad "3" smd rect
		(at 0.175 0.8)
		(size 0.875 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "7009403b-7fe8-4a9d-8ec0-6c330492b524")
	)
	(pad "4" smd rect
		(at -1.1 0.8)
		(size 0.875 0.775)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "1b45d612-87af-40c6-a2b0-9b7a8eaaf98b")
	)
	(model "${KICAD8_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_SeikoEpson_FA238-4Pin_3.2x2.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
