;Proteus Design Interchange Format
(PDIF
 (vendor "SamacSys Limited")
 (version 1 0)
 (library
  (part "IHLP2525CZER100M11"
   (description "Vishay IHLP2525CZ-11 Series Shielded Wire-wound SMD Inductor with a Metal Composite Core, 10 uH +/-20% Wire-Wound 4A Idc")
   (family "IND")
   (package "INDPM6965X300N")
   (attribute "Datasheet Link" "https://componentsearchengine.com/Datasheets/2/IHLP2525CZER100M11.pdf")
   (attribute "Geometry.Height" "3mm")
   (attribute "Manufacturer_Name" "Vishay")
   (attribute "Manufacturer_Part_Number" "IHLP2525CZER100M11")
   (attribute "Mouser Part Number" "70-IHLP2525CZER100M1")
   (attribute "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Vishay-Dale/IHLP2525CZER100M11?qs=gMuw6kkpPFi7WFZ9cEKRAA%3D%3D")
   (attribute "Arrow Part Number" "IHLP2525CZER100M11")
   (attribute "Arrow Price/Stock" "https://www.arrow.com/en/products/ihlp2525czer100m11/vishay?region=nac")
   (gate
    (symbol "IHLP2525CZER100M11")
    (pin "1" 1 PS)
    (pin "2" 2 PS)
   )
  )
  (symbol "IHLP2525CZER100M11"
   (units THOU)
   (origin (pt 0 0))
   (graphic
    (stroke 10)
    (path
     (arc (pt 200 0) (pt 200 -52) (pt 300 48) (start -175.4) (sweep 177.7)) (pt 300 0))
   )
   (graphic
    (stroke 10)
    (path
     (arc (pt 300 0) (pt 300 -52) (pt 400 48) (start -175.4) (sweep 177.7)) (pt 400 0))
   )
   (graphic
    (stroke 10)
    (path
     (arc (pt 400 0) (pt 400 -52) (pt 500 48) (start -175.4) (sweep 177.7)) (pt 500 0))
   )
   (graphic
    (stroke 10)
    (path
     (arc (pt 500 0) (pt 500 -52) (pt 600 48) (start -175.4) (sweep 177.7)) (pt 600 0))
   )
   (terminal
    (body (symbol "PIN") (pt 0 0) (rot 0) (mir 0) (visible true))
    (name (pt 0 -10) (rot 0) (just TOP LEFT) (visible false))
    (number (pt 0 10) (rot 0) (just BOTTOM LEFT) (visible true)))
   (terminal
    (body (symbol "PIN") (pt 800 0) (rot 0) (mir X) (visible true))
    (name (pt 0 -10) (rot 0) (just TOP LEFT) (visible false))
    (number (pt 0 10) (rot 0) (just BOTTOM LEFT) (visible true)))
  )
  (symbol "PIN"
   (units THOU)
   (origin (pt 0 0))
   (graphic
    (stroke 10)
    (path (pt 0 0) (pt 200 0))))
  (symbol "PINSHORT"
   (units THOU)
   (origin (pt 0 0))
   (graphic
    (stroke 10)
    (path (pt 0 0) (pt 100 0))))
  (package "INDPM6965X300N"
   (units MM)
   (layer OCCA
    (graphic
     (stroke 0.05)
     (path
      (closed true)
      (pt -4.35 3.612)
      (pt 4.35 3.612)
      (pt 4.35 -3.612)
      (pt -4.35 -3.612)
      (pt -4.35 3.612))))
   (layer TASM
    (graphic
     (stroke 0.1)
     (path
      (closed true)
      (pt -3.43 3.235)
      (pt 3.43 3.235)
      (pt 3.43 -3.235)
      (pt -3.43 -3.235)
      (pt -3.43 3.235))))
   (layer TSLK
    (graphic
     (stroke 0.2)
     (path
      (closed false)
      (pt 3.43 3.235)
      (pt -3.43 3.235))))
   (layer TSLK
    (graphic
     (stroke 0.2)
     (path
      (closed false)
      (pt -3.43 -3.235)
      (pt 3.43 -3.235))))
   (leg 1 (pt -2.9 0) (padstack 0))
   (leg 2 (pt 2.9 0) (padstack 0))
   (padstack 0
    (plated false)
    (pad (layer TCOP) (rectf 2.4 3.4 0 0 90))
   )
   (model "IHLP2525CZER100M11.stp"
    (euler 90 0 0)
    (offset -1.4900000095367432 5.329999923706055 -2.4000000953674316)
   )
  )
 )
)
