(footprint "Socket_Harwin_S9091-46R" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at 0 3.25 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2ad483ea-4498-4295-a713-0cc8ba79be85)
  )
  (fp_text value "Socket_Harwin_S9091-46R" (at 0 4.75 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 633b7c84-97e9-4c98-8816-1ec7536436d7)
  )
  (fp_text user "${REFERENCE}" (at 0 3.25 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b1cf610b-548b-484d-b718-a091a010f9fa)
  )
  (fp_rect (start -3.25 -1.25) (end 3.25 1.25) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 66f52706-4907-4a41-8441-30c7f991332a))
  (pad "" np_thru_hole circle (at 0 0) (size 3.8 3.8) (drill 3.8) (layers *.Mask) (tstamp f1ee6fa7-0015-4933-b8fe-bfff70212ff0))
  (pad "1" smd roundrect (at -2.5 0 90) (size 2 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b418fe9a-1d85-4120-8490-128f67095786))
  (pad "1" smd roundrect (at 2.5 0 90) (size 2 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f596af2e-0245-4273-808f-0cf71de56de3))
)
