(module "XTPS56637RPAT" (layer F.Cu)
  (descr "RPA0010A")
  (tags "Integrated Circuit")
  (attr smd)
  (fp_text reference IC** (at -0.010 -0) (layer F.SilkS)
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_text user %R (at -0.010 -0) (layer F.Fab)
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_text value "XTPS56637RPAT" (at -0.010 -0) (layer F.SilkS) hide
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_line (start -1.5 -1.5) (end 1.5 -1.5) (layer F.Fab) (width 0.2))
  (fp_line (start 1.5 -1.5) (end 1.5 1.5) (layer F.Fab) (width 0.2))
  (fp_line (start 1.5 1.5) (end -1.5 1.5) (layer F.Fab) (width 0.2))
  (fp_line (start -1.5 1.5) (end -1.5 -1.5) (layer F.Fab) (width 0.2))
  (fp_line (start -2.41 -2.4) (end 2.39 -2.4) (layer F.CrtYd) (width 0.1))
  (fp_line (start 2.39 -2.4) (end 2.39 2.4) (layer F.CrtYd) (width 0.1))
  (fp_line (start 2.39 2.4) (end -2.41 2.4) (layer F.CrtYd) (width 0.1))
  (fp_line (start -2.41 2.4) (end -2.41 -2.4) (layer F.CrtYd) (width 0.1))
  (fp_line (start -1.5 -1.25) (end -1.5 -1.4) (layer F.SilkS) (width 0.1))
  (fp_line (start -1.5 -1.4) (end -1.5 -1.5) (layer F.SilkS) (width 0.1))
  (fp_line (start -1.5 -1.5) (end -1.25 -1.5) (layer F.SilkS) (width 0.1))
  (fp_line (start 1.5 -1.5) (end 1.5 -1.25) (layer F.SilkS) (width 0.1))
  (fp_line (start -1.5 1.25) (end -1.5 1.5) (layer F.SilkS) (width 0.1))
  (fp_line (start -1.5 1.5) (end -1.25 1.5) (layer F.SilkS) (width 0.1))
  (fp_line (start 1.5 1.5) (end 1.5 0.85) (layer F.SilkS) (width 0.1))
  (fp_line (start 0.5 -1.5) (end 0.25 -1.5) (layer F.SilkS) (width 0.1))
  (fp_line (start -0.5 1.5) (end 0 1.5) (layer F.SilkS) (width 0.1))
  (fp_line (start -2 -0.75) (end -2 -0.75) (layer F.SilkS) (width 0.2))
  (fp_line (start -2.1 -0.75) (end -2.1 -0.75) (layer F.SilkS) (width 0.2))
  (fp_arc (start -2.05 -0.75) (end -2.000 -0.75) (angle -180) (layer F.SilkS) (width 0.2))
  (fp_arc (start -2.05 -0.75) (end -2.100 -0.75) (angle -180) (layer F.SilkS) (width 0.2))
  (pad 1 smd rect (at -1.410 -0.75 90) (size 0.250 0.600) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.410 -0.25 90) (size 0.250 0.600) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.410 0.25 90) (size 0.250 0.600) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.410 0.75 90) (size 0.250 0.600) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -0.940 1.4 0) (size 0.250 0.600) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 0.360 0.85 0) (size 0.250 1.700) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 0.860 1.4 0) (size 0.250 0.600) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 0.940 -0.65 0) (size 0.400 2.100) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -0.220 -0.65 0) (size 0.400 2.100) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -0.940 -1.4 0) (size 0.250 0.600) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 1.410 0.25 90) (size 0.250 0.560) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 1.410 -0.25 90) (size 0.250 0.560) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 1.410 -0.75 90) (size 0.250 0.560) (layers F.Cu F.Paste F.Mask))
  (model TPS56837RPAR.stp
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
