FILE_TYPE = MULTI_PHYS_TABLE;

PART 'LM5122MH_NOPB'
CLASS = IC
{========================================================================================}
:"MANUFACTURER_NAME", "MANUFACTURER_PART_NUMBER"= "PART_NUMBER", "JEDEC_TYPE", "PACK_TYPE", "MOUSER_PART_NUMBER", "MOUSER_PRICE/STOCK", "ARROW_PART_NUMBER", "ARROW_PRICE/STOCK", "DESCRIPTION", "DATASHEET", "HEIGHT";
{========================================================================================}
 "Texas Instruments", "LM5122MH/NOPB" (!) = "", "SOP65P640X110-21N", "Small Outline Packages", "595-LM5122MH/NOPB", "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/LM5122MH-NOPB?qs=iIeLWXrA%252B1WObMiZ4L5hVQ%3D%3D", "LM5122MH/NOPB", "https://www.arrow.com/en/products/lm5122mhnopb/texas-instruments?region=nac", "65V Boost Controller with Phase HTSSOP20 LM5122MH/NOPB, DC-DC Controller, 15A, 65 V Step-Up, 250 kHz, 20-Pin, HTTSOP", "https://datasheet.datasheetarchive.com/originals/distributors/Datasheets-SFU2/DSASFU100037250.pdf", "1.1 mm"
END_PART

END.
