(module "SODFL1608X77N" (layer F.Cu)
  (descr "DYA0002A")
  (tags "TVS Diode (Uni-directional)")
  (attr smd)
  (fp_text reference D** (at 0 0) (layer F.SilkS)
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_text value "SODFL1608X77N" (at 0 0) (layer F.SilkS) hide
    (effects (font (size 1.27 1.27) (thickness 0.254)))
  )
  (fp_line (start -1.21 -0.575) (end 1.21 -0.575) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.21 -0.575) (end 1.21 0.575) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.21 0.575) (end -1.21 0.575) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.21 0.575) (end -1.21 -0.575) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.6 -0.4) (end 0.6 -0.4) (layer F.Fab) (width 0.1))
  (fp_line (start 0.6 -0.4) (end 0.6 0.4) (layer F.Fab) (width 0.1))
  (fp_line (start 0.6 0.4) (end -0.6 0.4) (layer F.Fab) (width 0.1))
  (fp_line (start -0.6 0.4) (end -0.6 -0.4) (layer F.Fab) (width 0.1))
  (fp_line (start -0.6 -0.065) (end -0.265 -0.4) (layer F.Fab) (width 0.1))
  (fp_line (start -1.06 -0.4) (end 0.6 -0.4) (layer F.SilkS) (width 0.2))
  (fp_line (start -0.6 0.4) (end 0.6 0.4) (layer F.SilkS) (width 0.2))
  (pad 1 smd rect (at -0.725 0 90) (size 0.42 0.67) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0.725 0 90) (size 0.42 0.67) (layers F.Cu F.Paste F.Mask))
  (model ESD321DYAR.stp
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
