(footprint "WL-SFTW_RGB"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "http://cdn.sparkfun.com/datasheets/Components/LED/5060BRG4.pdf")
	(tags "RGB LED 5050-6")
	(property "Reference" "D4"
		(at 0 -3.5 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "34152d2b-cca3-4d7e-9e5f-9fb4cc26dd7e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "150505M173300"
		(at 0 3.3 180)
		(layer "F.Fab")
		(uuid "cd5c531f-b622-4d9c-9a7c-708543ef048f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "LED_SMD:LED_RGB_5050-6"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a4b02bbd-4800-43cc-9f69-fa987f14f18b")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://www.we-online.com/components/products/datasheet/150505M173300.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "750eb887-7fd6-46dc-8864-57e08d751ef0")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "RGB LED, PLCC-6"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4e14cd30-864d-42f8-88c0-4e81e9231d57")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -3.6 -2.7)
		(end 2.5 -2.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2821be64-6735-423b-b880-31f8444e212e")
	)
	(fp_line
		(start -3.6 -1.6)
		(end -3.6 -2.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "02b509bb-54a7-4f72-b7ab-72a93b1892c5")
	)
	(fp_line
		(start 2.5 2.7)
		(end -2.5 2.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "da461e0f-12a6-44c6-9e3d-647cc54ac3ca")
	)
	(fp_line
		(start -3.65 -2.75)
		(end -3.65 2.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "8147028a-b302-42e9-9c71-a9f5a8ba34b5")
	)
	(fp_line
		(start -3.65 2.75)
		(end 3.65 2.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f2fadcb0-b5f7-4cb4-b370-64cc20c9f53f")
	)
	(fp_line
		(start 3.65 -2.75)
		(end -3.65 -2.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "02a927da-7952-4379-83c3-29a93043ae9f")
	)
	(fp_line
		(start 3.65 2.75)
		(end 3.65 -2.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c522f134-c57d-4d72-aa6a-82af1b6ca86b")
	)
	(fp_line
		(start -2.5 -2.5)
		(end -2.5 2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5e2641f1-4e9f-474f-b310-f5151027f765")
	)
	(fp_line
		(start -2.5 -1.9)
		(end -1.9 -2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "191503aa-4f41-4c07-8b94-87297a65e7cc")
	)
	(fp_line
		(start -2.5 2.5)
		(end 2.5 2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "abf53099-5a91-4507-8132-9613f8bf2694")
	)
	(fp_line
		(start 2.5 -2.5)
		(end -2.5 -2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b6f88d53-fd60-41c5-a8d9-9dd756ab7735")
	)
	(fp_line
		(start 2.5 2.5)
		(end 2.5 -2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "91e2abb4-0725-4bd6-aef0-97e62c67bb6c")
	)
	(fp_circle
		(center 0 0)
		(end 0 -1.9)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "37f8f067-44f6-42e9-a5ea-db93eeddef69")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
		(uuid "d44ddea9-db94-4569-8a56-c110000206f6")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.06)
			)
		)
	)
	(pad "1" smd rect
		(at -2.4 -1.7 90)
		(size 1.1 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "cfe67ca2-16ee-40dc-9557-33c2781a0464")
	)
	(pad "2" smd rect
		(at 2.4 -1.7 90)
		(size 1.1 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "1b6efcfd-0694-4ffa-b0a2-ee35704f4992")
	)
	(pad "3" smd rect
		(at -2.4 0 90)
		(size 1.1 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "ff29aa26-6c19-4757-a371-7e816dc7be2b")
	)
	(pad "4" smd rect
		(at 2.4 0 90)
		(size 1.1 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "7a8946fe-506f-41f1-be78-e999f7d1de01")
	)
	(pad "5" smd rect
		(at -2.4 1.7 90)
		(size 1.1 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "9fe7feff-362c-47d9-9372-8b23fa3cb2d3")
	)
	(pad "6" smd rect
		(at 2.4 1.7 90)
		(size 1.1 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "a47906e0-3459-48be-91c2-52688f7e4027")
	)
	(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_RGB_5050-6.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
