11-05 15:38:48 com_github_MitjaNemec_ReplicateLayout.action_replicate_layout 392:Plugin executed on: 'linux'
11-05 15:38:48 com_github_MitjaNemec_ReplicateLayout.action_replicate_layout 393:Plugin executed with python version: '3.12.6 (main, Sep  8 2024, 13:18:56) [GCC 14.2.1 20240805]'
11-05 15:38:48 com_github_MitjaNemec_ReplicateLayout.action_replicate_layout 394:KiCad build version: 8.0.5
11-05 15:38:48 com_github_MitjaNemec_ReplicateLayout.action_replicate_layout 395:Plugin version: 3.0.2
11-05 15:38:48 com_github_MitjaNemec_ReplicateLayout.action_replicate_layout 396:Frame repr: <wx._core.Frame object at 0x74ad84dc8b00>
11-05 15:38:48 com_github_MitjaNemec_ReplicateLayout.action_replicate_layout 420:Preparing replicator with D15 as a reference
11-05 15:38:48 com_github_MitjaNemec_ReplicateLayout.replicate_layout 117:getting a list of all footprints on board
11-05 15:38:48 com_github_MitjaNemec_ReplicateLayout.action_replicate_layout 468:source anchor footprint is 'D15'
Located on: ['Double GPIO Protection']
With filenames: ['GPIOProt.kicad_sch']
With sheet_id:['Double GPIO Protection']
11-05 15:38:48 com_github_MitjaNemec_ReplicateLayout.action_replicate_layout 475:Corresponding footprints are 
[('D21', ['Double GPIO Protection3']), ('D17', ['Double GPIO Protection1']), ('D15', ['Double GPIO Protection']), ('D19', ['Double GPIO Protection2'])]
11-05 15:38:48 com_github_MitjaNemec_ReplicateLayout.action_replicate_layout 487:Showing dialog
11-05 15:38:48 com_github_MitjaNemec_ReplicateLayout.replicate_layout 462:constructing a list of sheets suitable for replication on level:'Double GPIO Protection', file:'GPIOProt.kicad_sch'
11-05 15:38:48 com_github_MitjaNemec_ReplicateLayout.replicate_layout 499:suitable sheets are:[['Double GPIO Protection1'], ['Double GPIO Protection2'], ['Double GPIO Protection3']]
11-05 15:38:49 com_github_MitjaNemec_ReplicateLayout.replicate_layout 1503:Level selected: ['Double GPIO Protection']
11-05 15:38:49 com_github_MitjaNemec_ReplicateLayout.replicate_layout 1327:Filtering list of tracks
11-05 15:38:49 com_github_MitjaNemec_ReplicateLayout.action_replicate_layout 493:Toolbar position: wx.Point(1878, 99)
11-05 15:38:49 com_github_MitjaNemec_ReplicateLayout.action_replicate_layout 498:Dialog position: wx.Point(1439, 99)
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 462:constructing a list of sheets suitable for replication on level:'Double GPIO Protection', file:'GPIOProt.kicad_sch'
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 499:suitable sheets are:[['Double GPIO Protection1'], ['Double GPIO Protection2'], ['Double GPIO Protection3']]
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.action_replicate_layout 240:Replicating layout
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 278:Starting replication of sheets: [['Double GPIO Protection1'], ['Double GPIO Protection2'], ['Double GPIO Protection3']]
on level: ['Double GPIO Protection']
with tracks=True, zone=True, text=True, text=True, intersecting=False, remove=False, locked footprints=False, group_only=False
11-05 15:38:51 root 332:updating GUI message: 'Preparing for replication'
11-05 15:38:51 root 337:updating GUI with: 0
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 348:Getting the list of source footprints
11-05 15:38:51 root 337:updating GUI with: 0
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 358:Getting the list of all the remaining footprints
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 365:Getting source tracks
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 1327:Filtering list of tracks
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 369:Getting source zones
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 373:Getting source text items
11-05 15:38:51 root 337:updating GUI with: 66
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 377:Getting source drawing items
11-05 15:38:51 root 332:updating GUI message: 'Replicating footprints'
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 844:Replicating footprints
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 851:Replicating footprints on sheet ['Double GPIO Protection1']
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 851:Replicating footprints on sheet ['Double GPIO Protection2']
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 851:Replicating footprints on sheet ['Double GPIO Protection3']
11-05 15:38:51 root 332:updating GUI message: 'Replicating tracks'
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 1005:Replicating tracks
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 1011:Replicating tracks on sheet ['Double GPIO Protection1']
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D4'] and dst net: ['', 'D6'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.75
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D5'] and dst net: ['', 'WS2'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.50
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D4'] and dst net: ['', 'D6'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.75
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D5'] and dst net: ['', 'WS2'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.50
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 804:Net pairs for sheet ['Double GPIO Protection1'] :[('/Double GPIO Protection/In 2', '/Double GPIO Protection1/In 2'), ('', ''), ('/D4', '/D6'), ('+5V', '+5V'), ('/D5', '/WS2'), ('GND', 'GND'), ('/Double GPIO Protection/In 1', '/Double GPIO Protection1/In 1')]
11-05 15:38:51 root 337:updating GUI with: 1
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 1011:Replicating tracks on sheet ['Double GPIO Protection2']
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D4'] and dst net: ['', 'D1'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.75
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D5'] and dst net: ['', 'D2'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.75
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D4'] and dst net: ['', 'D1'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.75
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D5'] and dst net: ['', 'D2'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.75
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 804:Net pairs for sheet ['Double GPIO Protection2'] :[('/D4', '/D1'), ('', ''), ('/Double GPIO Protection/In 1', '/Double GPIO Protection2/In 1'), ('/Double GPIO Protection/In 2', '/Double GPIO Protection2/In 2'), ('/D5', '/D2'), ('+5V', '+5V'), ('GND', 'GND')]
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 1011:Replicating tracks on sheet ['Double GPIO Protection3']
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D4'] and dst net: ['', 'D3'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.75
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D5'] and dst net: ['', 'WS1'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.50
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D4'] and dst net: ['', 'D3'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.75
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D5'] and dst net: ['', 'WS1'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.50
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 804:Net pairs for sheet ['Double GPIO Protection3'] :[('/D5', '/WS1'), ('/D4', '/D3'), ('', ''), ('/Double GPIO Protection/In 1', '/Double GPIO Protection3/In 1'), ('+5V', '+5V'), ('/Double GPIO Protection/In 2', '/Double GPIO Protection3/In 2'), ('GND', 'GND')]
11-05 15:38:51 root 332:updating GUI message: 'Replicating zones'
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 1075:Replicating zones
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 1082:Replicating zones on sheet ['Double GPIO Protection1']
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D4'] and dst net: ['', 'D6'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.75
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D5'] and dst net: ['', 'WS2'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.50
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D4'] and dst net: ['', 'D6'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.75
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D5'] and dst net: ['', 'WS2'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.50
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 804:Net pairs for sheet ['Double GPIO Protection1'] :[('/Double GPIO Protection/In 2', '/Double GPIO Protection1/In 2'), ('', ''), ('/D4', '/D6'), ('+5V', '+5V'), ('/D5', '/WS2'), ('GND', 'GND'), ('/Double GPIO Protection/In 1', '/Double GPIO Protection1/In 1')]
11-05 15:38:51 root 337:updating GUI with: 33
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 1082:Replicating zones on sheet ['Double GPIO Protection2']
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D4'] and dst net: ['', 'D1'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.75
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D5'] and dst net: ['', 'D2'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.75
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D4'] and dst net: ['', 'D1'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.75
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D5'] and dst net: ['', 'D2'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.75
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 804:Net pairs for sheet ['Double GPIO Protection2'] :[('/D4', '/D1'), ('', ''), ('/Double GPIO Protection/In 1', '/Double GPIO Protection2/In 1'), ('/Double GPIO Protection/In 2', '/Double GPIO Protection2/In 2'), ('/D5', '/D2'), ('+5V', '+5V'), ('GND', 'GND')]
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 1082:Replicating zones on sheet ['Double GPIO Protection3']
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D4'] and dst net: ['', 'D3'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.75
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D5'] and dst net: ['', 'WS1'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.50
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D4'] and dst net: ['', 'D3'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.75
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 788:Significant difference between src net: ['', 'D5'] and dst net: ['', 'WS1'], with src_net_depth=2, dst_net_depth=2, src_fp_depth=1, dst_fp_depth=1, match level 0.50
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 804:Net pairs for sheet ['Double GPIO Protection3'] :[('/D5', '/WS1'), ('/D4', '/D3'), ('', ''), ('/Double GPIO Protection/In 1', '/Double GPIO Protection3/In 1'), ('+5V', '+5V'), ('/Double GPIO Protection/In 2', '/Double GPIO Protection3/In 2'), ('GND', 'GND')]
11-05 15:38:51 root 332:updating GUI message: 'Replicating text'
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 1164:Replicating text
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 1171:Replicating text on sheet ['Double GPIO Protection1']
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 1171:Replicating text on sheet ['Double GPIO Protection2']
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 1171:Replicating text on sheet ['Double GPIO Protection3']
11-05 15:38:51 root 332:updating GUI message: 'Replicating drawings'
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 1215:Replicating drawings
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 1221:Replicating drawings on sheet ['Double GPIO Protection1']
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 1221:Replicating drawings on sheet ['Double GPIO Protection2']
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.replicate_layout 1221:Replicating drawings on sheet ['Double GPIO Protection3']
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.action_replicate_layout 256:Replication complete
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.action_replicate_layout 259:Letting the user know there are some issues with replicated design
11-05 15:38:51 com_github_MitjaNemec_ReplicateLayout.action_replicate_layout 263:Looks like the design has an exotic connectivity that the plugin might not handle properly
 Make sure that you check the connectivity around:
Footprint D19, pad 1
Footprint Q2, pad 4
Footprint D19, pad 4
Footprint D17, pad 4
Footprint Q2, pad 1
Footprint D17, pad 1
Footprint Q3, pad 4
Footprint Q4, pad 1
Footprint Q3, pad 1
Footprint Q4, pad 4
Footprint D21, pad 4
Footprint D21, pad 1

