ARM GAS  /tmp/ccqUhOmw.s 			page 1


   1              		.cpu cortex-m4
   2              		.arch armv7e-m
   3              		.fpu fpv4-sp-d16
   4              		.eabi_attribute 27, 1
   5              		.eabi_attribute 28, 1
   6              		.eabi_attribute 20, 1
   7              		.eabi_attribute 21, 1
   8              		.eabi_attribute 23, 3
   9              		.eabi_attribute 24, 1
  10              		.eabi_attribute 25, 1
  11              		.eabi_attribute 26, 1
  12              		.eabi_attribute 30, 1
  13              		.eabi_attribute 34, 1
  14              		.eabi_attribute 18, 4
  15              		.file	"stm32f3xx_hal_spi.c"
  16              		.text
  17              	.Ltext0:
  18              		.cfi_sections	.debug_frame
  19              		.file 1 "Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c"
  20              		.section	.text.SPI_WaitFlagStateUntilTimeout,"ax",%progbits
  21              		.align	1
  22              		.syntax unified
  23              		.thumb
  24              		.thumb_func
  26              	SPI_WaitFlagStateUntilTimeout:
  27              	.LVL0:
  28              	.LFB177:
   1:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
   2:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   ******************************************************************************
   3:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @file    stm32f3xx_hal_spi.c
   4:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @author  MCD Application Team
   5:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief   SPI HAL module driver.
   6:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *          This file provides firmware functions to manage the following
   7:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *          functionalities of the Serial Peripheral Interface (SPI) peripheral:
   8:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           + Initialization and de-initialization functions
   9:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           + IO operation functions
  10:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           + Peripheral Control functions
  11:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           + Peripheral State functions
  12:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *
  13:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   @verbatim
  14:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   ==============================================================================
  15:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                         ##### How to use this driver #####
  16:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   ==============================================================================
  17:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     [..]
  18:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       The SPI HAL driver can be used as follows:
  19:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
  20:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (#) Declare a SPI_HandleTypeDef handle structure, for example:
  21:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           SPI_HandleTypeDef  hspi;
  22:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
  23:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (#)Initialize the SPI low level resources by implementing the HAL_SPI_MspInit() API:
  24:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           (##) Enable the SPIx interface clock
  25:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           (##) SPI pins configuration
  26:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               (+++) Enable the clock for the SPI GPIOs
  27:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               (+++) Configure these SPI pins as alternate function push-pull
  28:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           (##) NVIC configuration if you need to use interrupt process
  29:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               (+++) Configure the SPIx interrupt priority
  30:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               (+++) Enable the NVIC SPI IRQ handle
ARM GAS  /tmp/ccqUhOmw.s 			page 2


  31:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           (##) DMA Configuration if you need to use DMA process
  32:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               (+++) Declare a DMA_HandleTypeDef handle structure for the transmit or receive Stream
  33:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               (+++) Enable the DMAx clock
  34:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               (+++) Configure the DMA handle parameters
  35:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               (+++) Configure the DMA Tx or Rx Stream/Channel
  36:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               (+++) Associate the initialized hdma_tx(or _rx)  handle to the hspi DMA Tx or Rx hand
  37:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               (+++) Configure the priority and enable the NVIC for the transfer complete interrupt 
  38:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
  39:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (#) Program the Mode, BidirectionalMode , Data size, Baudrate Prescaler, NSS
  40:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           management, Clock polarity and phase, FirstBit and CRC configuration in the hspi Init str
  41:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
  42:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (#) Initialize the SPI registers by calling the HAL_SPI_Init() API:
  43:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           (++) This API configures also the low level Hardware GPIO, CLOCK, CORTEX...etc)
  44:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               by calling the customized HAL_SPI_MspInit() API.
  45:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****      [..]
  46:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        Circular mode restriction:
  47:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (#) The DMA circular mode cannot be used when the SPI is configured in these modes:
  48:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           (##) Master 2Lines RxOnly
  49:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           (##) Master 1Line Rx
  50:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (#) The CRC feature is not managed when the DMA circular mode is enabled
  51:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (#) When the SPI DMA Pause/Stop features are used, we must use the following APIs
  52:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           the HAL_SPI_DMAPause()/ HAL_SPI_DMAStop() only under the SPI callbacks
  53:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****      [..]
  54:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        Master Receive mode restriction:
  55:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (#) In Master unidirectional receive-only mode (MSTR =1, BIDIMODE=0, RXONLY=1) or
  56:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           bidirectional receive mode (MSTR=1, BIDIMODE=1, BIDIOE=0), to ensure that the SPI
  57:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           does not initiate a new transfer the following procedure has to be respected:
  58:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           (##) HAL_SPI_DeInit()
  59:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           (##) HAL_SPI_Init()
  60:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****      [..]
  61:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        Callback registration:
  62:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
  63:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (#) The compilation flag USE_HAL_SPI_REGISTER_CALLBACKS when set to 1U
  64:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           allows the user to configure dynamically the driver callbacks.
  65:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           Use Functions HAL_SPI_RegisterCallback() to register an interrupt callback.
  66:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
  67:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           Function HAL_SPI_RegisterCallback() allows to register following callbacks:
  68:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) TxCpltCallback        : SPI Tx Completed callback
  69:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) RxCpltCallback        : SPI Rx Completed callback
  70:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) TxRxCpltCallback      : SPI TxRx Completed callback
  71:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) TxHalfCpltCallback    : SPI Tx Half Completed callback
  72:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) RxHalfCpltCallback    : SPI Rx Half Completed callback
  73:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) TxRxHalfCpltCallback  : SPI TxRx Half Completed callback
  74:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) ErrorCallback         : SPI Error callback
  75:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) AbortCpltCallback     : SPI Abort callback
  76:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) MspInitCallback       : SPI Msp Init callback
  77:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) MspDeInitCallback     : SPI Msp DeInit callback
  78:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           This function takes as parameters the HAL peripheral handle, the Callback ID
  79:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           and a pointer to the user callback function.
  80:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
  81:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
  82:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (#) Use function HAL_SPI_UnRegisterCallback to reset a callback to the default
  83:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           weak function.
  84:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           HAL_SPI_UnRegisterCallback takes as parameters the HAL peripheral handle,
  85:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           and the Callback ID.
  86:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           This function allows to reset following callbacks:
  87:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) TxCpltCallback        : SPI Tx Completed callback
ARM GAS  /tmp/ccqUhOmw.s 			page 3


  88:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) RxCpltCallback        : SPI Rx Completed callback
  89:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) TxRxCpltCallback      : SPI TxRx Completed callback
  90:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) TxHalfCpltCallback    : SPI Tx Half Completed callback
  91:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) RxHalfCpltCallback    : SPI Rx Half Completed callback
  92:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) TxRxHalfCpltCallback  : SPI TxRx Half Completed callback
  93:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) ErrorCallback         : SPI Error callback
  94:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) AbortCpltCallback     : SPI Abort callback
  95:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) MspInitCallback       : SPI Msp Init callback
  96:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (++) MspDeInitCallback     : SPI Msp DeInit callback
  97:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
  98:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        [..]
  99:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        By default, after the HAL_SPI_Init() and when the state is HAL_SPI_STATE_RESET
 100:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        all callbacks are set to the corresponding weak functions:
 101:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        examples HAL_SPI_MasterTxCpltCallback(), HAL_SPI_MasterRxCpltCallback().
 102:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        Exception done for MspInit and MspDeInit functions that are
 103:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        reset to the legacy weak functions in the HAL_SPI_Init()/ HAL_SPI_DeInit() only when
 104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        these callbacks are null (not registered beforehand).
 105:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        If MspInit or MspDeInit are not null, the HAL_SPI_Init()/ HAL_SPI_DeInit()
 106:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        keep and use the user MspInit/MspDeInit callbacks (registered beforehand) whatever the state
 107:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 108:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        [..]
 109:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        Callbacks can be registered/unregistered in HAL_SPI_STATE_READY state only.
 110:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        Exception done MspInit/MspDeInit functions that can be registered/unregistered
 111:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        in HAL_SPI_STATE_READY or HAL_SPI_STATE_RESET state,
 112:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        thus registered (user) MspInit/DeInit callbacks can be used during the Init/DeInit.
 113:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        Then, the user first registers the MspInit/MspDeInit user callbacks
 114:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        using HAL_SPI_RegisterCallback() before calling HAL_SPI_DeInit()
 115:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        or HAL_SPI_Init() function.
 116:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 117:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        [..]
 118:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        When the compilation define USE_HAL_PPP_REGISTER_CALLBACKS is set to 0 or
 119:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        not defined, the callback registering feature is not available
 120:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        and weak (surcharged) callbacks are used.
 121:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 122:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****      [..]
 123:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        Using the HAL it is not possible to reach all supported SPI frequency with the different SPI
 124:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        the following table resume the max SPI frequency reached with data size 8bits/16bits,
 125:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****          according to frequency of the APBx Peripheral Clock (fPCLK) used by the SPI instance.
 126:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 127:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   @endverbatim
 128:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 129:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   Additional table :
 130:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 131:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        DataSize = SPI_DATASIZE_8BIT:
 132:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        +-------------------------------------------------------------------------------------------
 133:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |                | 2Lines Fullduplex   |     2Lines RxOnly    |         1Line     
 134:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        | Process | Transfer mode  |---------------------|----------------------|-------------------
 135:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |                |  Master  |  Slave   |  Master   |  Slave   |  Master   |  Slave
 136:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |===========================================================================================
 137:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    T    |     Polling    | Fpclk/4  | Fpclk/8  |    NA     |    NA    |    NA     |   NA  
 138:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    X    |----------------|----------|----------|-----------|----------|-----------|-------
 139:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    /    |     Interrupt  | Fpclk/4  | Fpclk/16 |    NA     |    NA    |    NA     |   NA  
 140:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    R    |----------------|----------|----------|-----------|----------|-----------|-------
 141:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    X    |       DMA      | Fpclk/2  | Fpclk/2  |    NA     |    NA    |    NA     |   NA  
 142:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |=========|================|==========|==========|===========|==========|===========|=======
 143:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |     Polling    | Fpclk/4  | Fpclk/8  | Fpclk/16  | Fpclk/8  | Fpclk/8   | Fpclk/
 144:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |----------------|----------|----------|-----------|----------|-----------|-------
ARM GAS  /tmp/ccqUhOmw.s 			page 4


 145:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    R    |     Interrupt  | Fpclk/8  | Fpclk/16 | Fpclk/8   | Fpclk/8  | Fpclk/8   | Fpclk/
 146:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    X    |----------------|----------|----------|-----------|----------|-----------|-------
 147:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |       DMA      | Fpclk/4  | Fpclk/2  | Fpclk/2   | Fpclk/16 | Fpclk/2   | Fpclk/
 148:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |=========|================|==========|==========|===========|==========|===========|=======
 149:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |     Polling    | Fpclk/8  | Fpclk/2  |     NA    |    NA    | Fpclk/8   | Fpclk/
 150:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |----------------|----------|----------|-----------|----------|-----------|-------
 151:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    T    |     Interrupt  | Fpclk/2  | Fpclk/4  |     NA    |    NA    | Fpclk/16  | Fpclk/
 152:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    X    |----------------|----------|----------|-----------|----------|-----------|-------
 153:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |       DMA      | Fpclk/2  | Fpclk/2  |     NA    |    NA    | Fpclk/8   | Fpclk/
 154:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        +-------------------------------------------------------------------------------------------
 155:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 156:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        DataSize = SPI_DATASIZE_16BIT:
 157:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        +-------------------------------------------------------------------------------------------
 158:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |                | 2Lines Fullduplex   |     2Lines RxOnly    |         1Line     
 159:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        | Process | Transfer mode  |---------------------|----------------------|-------------------
 160:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |                |  Master  |  Slave   |  Master   |  Slave   |  Master   |  Slave
 161:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |===========================================================================================
 162:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    T    |     Polling    | Fpclk/4  | Fpclk/8  |    NA     |    NA    |    NA     |   NA  
 163:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    X    |----------------|----------|----------|-----------|----------|-----------|-------
 164:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    /    |     Interrupt  | Fpclk/4  | Fpclk/16 |    NA     |    NA    |    NA     |   NA  
 165:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    R    |----------------|----------|----------|-----------|----------|-----------|-------
 166:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    X    |       DMA      | Fpclk/2  | Fpclk/2  |    NA     |    NA    |    NA     |   NA  
 167:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |=========|================|==========|==========|===========|==========|===========|=======
 168:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |     Polling    | Fpclk/4  | Fpclk/8  | Fpclk/16  | Fpclk/8  | Fpclk/8   | Fpclk/
 169:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |----------------|----------|----------|-----------|----------|-----------|-------
 170:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    R    |     Interrupt  | Fpclk/8  | Fpclk/16 | Fpclk/8   | Fpclk/8  | Fpclk/8   | Fpclk/
 171:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    X    |----------------|----------|----------|-----------|----------|-----------|-------
 172:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |       DMA      | Fpclk/4  | Fpclk/2  | Fpclk/2   | Fpclk/16 | Fpclk/2   | Fpclk/
 173:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |=========|================|==========|==========|===========|==========|===========|=======
 174:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |     Polling    | Fpclk/8  | Fpclk/2  |     NA    |    NA    | Fpclk/8   | Fpclk/
 175:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |----------------|----------|----------|-----------|----------|-----------|-------
 176:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    T    |     Interrupt  | Fpclk/2  | Fpclk/4  |     NA    |    NA    | Fpclk/16  | Fpclk/
 177:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |    X    |----------------|----------|----------|-----------|----------|-----------|-------
 178:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        |         |       DMA      | Fpclk/2  | Fpclk/2  |     NA    |    NA    | Fpclk/8   | Fpclk/
 179:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        +-------------------------------------------------------------------------------------------
 180:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        @note The max SPI frequency depend on SPI data size (4bits, 5bits,..., 8bits,...15bits, 16bi
 181:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****              SPI mode(2 Lines fullduplex, 2 lines RxOnly, 1 line TX/RX) and Process mode (Polling, 
 182:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        @note
 183:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (#) TX/RX processes are HAL_SPI_TransmitReceive(), HAL_SPI_TransmitReceive_IT() and HAL
 184:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (#) RX processes are HAL_SPI_Receive(), HAL_SPI_Receive_IT() and HAL_SPI_Receive_DMA()
 185:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             (#) TX processes are HAL_SPI_Transmit(), HAL_SPI_Transmit_IT() and HAL_SPI_Transmit_DMA
 186:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 187:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   ******************************************************************************
 188:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @attention
 189:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *
 190:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * <h2><center>&copy; Copyright (c) 2016 STMicroelectronics.
 191:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * All rights reserved.</center></h2>
 192:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *
 193:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * This software component is licensed by ST under BSD 3-Clause license,
 194:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * the "License"; You may not use this file except in compliance with the
 195:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * License. You may obtain a copy of the License at:
 196:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *                        opensource.org/licenses/BSD-3-Clause
 197:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *
 198:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   ******************************************************************************
 199:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 200:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 201:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /* Includes ------------------------------------------------------------------*/
ARM GAS  /tmp/ccqUhOmw.s 			page 5


 202:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #include "stm32f3xx_hal.h"
 203:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 204:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /** @addtogroup STM32F3xx_HAL_Driver
 205:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @{
 206:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 207:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 208:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /** @defgroup SPI SPI
 209:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief SPI HAL module driver
 210:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @{
 211:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 212:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #ifdef HAL_SPI_MODULE_ENABLED
 213:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 214:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /* Private typedef -----------------------------------------------------------*/
 215:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /* Private defines -----------------------------------------------------------*/
 216:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /** @defgroup SPI_Private_Constants SPI Private Constants
 217:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @{
 218:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 219:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #define SPI_DEFAULT_TIMEOUT 100U
 220:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
 221:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @}
 222:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 223:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 224:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /* Private macros ------------------------------------------------------------*/
 225:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /* Private variables ---------------------------------------------------------*/
 226:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /* Private function prototypes -----------------------------------------------*/
 227:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /** @defgroup SPI_Private_Functions SPI Private Functions
 228:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @{
 229:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 230:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMATransmitCplt(DMA_HandleTypeDef *hdma);
 231:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAReceiveCplt(DMA_HandleTypeDef *hdma);
 232:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMATransmitReceiveCplt(DMA_HandleTypeDef *hdma);
 233:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAHalfTransmitCplt(DMA_HandleTypeDef *hdma);
 234:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAHalfReceiveCplt(DMA_HandleTypeDef *hdma);
 235:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAHalfTransmitReceiveCplt(DMA_HandleTypeDef *hdma);
 236:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAError(DMA_HandleTypeDef *hdma);
 237:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAAbortOnError(DMA_HandleTypeDef *hdma);
 238:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMATxAbortCallback(DMA_HandleTypeDef *hdma);
 239:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMARxAbortCallback(DMA_HandleTypeDef *hdma);
 240:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static HAL_StatusTypeDef SPI_WaitFlagStateUntilTimeout(SPI_HandleTypeDef *hspi, uint32_t Flag, Flag
 241:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                        uint32_t Timeout, uint32_t Tickstart);
 242:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static HAL_StatusTypeDef SPI_WaitFifoStateUntilTimeout(SPI_HandleTypeDef *hspi, uint32_t Fifo, uint
 243:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                        uint32_t Timeout, uint32_t Tickstart);
 244:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_TxISR_8BIT(struct __SPI_HandleTypeDef *hspi);
 245:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_TxISR_16BIT(struct __SPI_HandleTypeDef *hspi);
 246:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_RxISR_8BIT(struct __SPI_HandleTypeDef *hspi);
 247:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_RxISR_16BIT(struct __SPI_HandleTypeDef *hspi);
 248:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesRxISR_8BIT(struct __SPI_HandleTypeDef *hspi);
 249:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesTxISR_8BIT(struct __SPI_HandleTypeDef *hspi);
 250:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesTxISR_16BIT(struct __SPI_HandleTypeDef *hspi);
 251:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesRxISR_16BIT(struct __SPI_HandleTypeDef *hspi);
 252:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 253:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_RxISR_8BITCRC(struct __SPI_HandleTypeDef *hspi);
 254:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_RxISR_16BITCRC(struct __SPI_HandleTypeDef *hspi);
 255:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesRxISR_8BITCRC(struct __SPI_HandleTypeDef *hspi);
 256:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesRxISR_16BITCRC(struct __SPI_HandleTypeDef *hspi);
 257:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 258:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_AbortRx_ISR(SPI_HandleTypeDef *hspi);
ARM GAS  /tmp/ccqUhOmw.s 			page 6


 259:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_AbortTx_ISR(SPI_HandleTypeDef *hspi);
 260:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_CloseRxTx_ISR(SPI_HandleTypeDef *hspi);
 261:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_CloseRx_ISR(SPI_HandleTypeDef *hspi);
 262:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_CloseTx_ISR(SPI_HandleTypeDef *hspi);
 263:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static HAL_StatusTypeDef SPI_EndRxTransaction(SPI_HandleTypeDef *hspi, uint32_t Timeout, uint32_t T
 264:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static HAL_StatusTypeDef SPI_EndRxTxTransaction(SPI_HandleTypeDef *hspi, uint32_t Timeout, uint32_t
 265:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
 266:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @}
 267:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 268:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 269:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /* Exported functions --------------------------------------------------------*/
 270:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /** @defgroup SPI_Exported_Functions SPI Exported Functions
 271:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @{
 272:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 273:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 274:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /** @defgroup SPI_Exported_Functions_Group1 Initialization and de-initialization functions
 275:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *  @brief    Initialization and Configuration functions
 276:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *
 277:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** @verbatim
 278:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****  ===============================================================================
 279:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****               ##### Initialization and de-initialization functions #####
 280:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****  ===============================================================================
 281:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     [..]  This subsection provides a set of functions allowing to initialize and
 282:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           de-initialize the SPIx peripheral:
 283:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 284:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (+) User must implement HAL_SPI_MspInit() function in which he configures
 285:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           all related peripherals resources (CLOCK, GPIO, DMA, IT and NVIC ).
 286:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 287:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (+) Call the function HAL_SPI_Init() to configure the selected device with
 288:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           the selected configuration:
 289:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) Mode
 290:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) Direction
 291:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) Data Size
 292:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) Clock Polarity and Phase
 293:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) NSS Management
 294:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) BaudRate Prescaler
 295:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) FirstBit
 296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) TIMode
 297:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) CRC Calculation
 298:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) CRC Polynomial if CRC enabled
 299:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) CRC Length, used only with Data8 and Data16
 300:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (++) FIFO reception threshold
 301:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 302:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (+) Call the function HAL_SPI_DeInit() to restore the default configuration
 303:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           of the selected SPIx peripheral.
 304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 305:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** @endverbatim
 306:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @{
 307:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 308:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 309:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
 310:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Initialize the SPI according to the specified parameters
 311:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         in the SPI_InitTypeDef and initialize the associated handle.
 312:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
 313:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
 314:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
 315:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
ARM GAS  /tmp/ccqUhOmw.s 			page 7


 316:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Init(SPI_HandleTypeDef *hspi)
 317:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
 318:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t frxth;
 319:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 320:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the SPI handle allocation */
 321:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi == NULL)
 322:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 323:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_ERROR;
 324:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 325:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 326:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the parameters */
 327:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_ALL_INSTANCE(hspi->Instance));
 328:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_MODE(hspi->Init.Mode));
 329:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION(hspi->Init.Direction));
 330:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DATASIZE(hspi->Init.DataSize));
 331:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_NSS(hspi->Init.NSS));
 332:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_NSSP(hspi->Init.NSSPMode));
 333:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_BAUDRATE_PRESCALER(hspi->Init.BaudRatePrescaler));
 334:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_FIRST_BIT(hspi->Init.FirstBit));
 335:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_TIMODE(hspi->Init.TIMode));
 336:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.TIMode == SPI_TIMODE_DISABLE)
 337:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 338:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     assert_param(IS_SPI_CPOL(hspi->Init.CLKPolarity));
 339:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     assert_param(IS_SPI_CPHA(hspi->Init.CLKPhase));
 340:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 341:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.Mode == SPI_MODE_MASTER)
 342:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 343:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       assert_param(IS_SPI_BAUDRATE_PRESCALER(hspi->Init.BaudRatePrescaler));
 344:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 345:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     else
 346:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 347:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Baudrate prescaler not use in Motoraola Slave mode. force to default value */
 348:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->Init.BaudRatePrescaler = SPI_BAUDRATEPRESCALER_2;
 349:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 350:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 351:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
 352:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 353:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     assert_param(IS_SPI_BAUDRATE_PRESCALER(hspi->Init.BaudRatePrescaler));
 354:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 355:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Force polarity and phase to TI protocaol requirements */
 356:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->Init.CLKPolarity = SPI_POLARITY_LOW;
 357:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->Init.CLKPhase    = SPI_PHASE_1EDGE;
 358:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 359:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_CRC_CALCULATION(hspi->Init.CRCCalculation));
 361:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
 362:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 363:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     assert_param(IS_SPI_CRC_POLYNOMIAL(hspi->Init.CRCPolynomial));
 364:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     assert_param(IS_SPI_CRC_LENGTH(hspi->Init.CRCLength));
 365:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 366:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
 367:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->Init.CRCCalculation = SPI_CRCCALCULATION_DISABLE;
 368:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 369:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 370:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->State == HAL_SPI_STATE_RESET)
 371:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 372:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Allocate lock resource and initialize it */
ARM GAS  /tmp/ccqUhOmw.s 			page 8


 373:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->Lock = HAL_UNLOCKED;
 374:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 375:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
 376:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Init the SPI Callback settings */
 377:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxCpltCallback       = HAL_SPI_TxCpltCallback;       /* Legacy weak TxCpltCallback       
 378:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxCpltCallback       = HAL_SPI_RxCpltCallback;       /* Legacy weak RxCpltCallback       
 379:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxRxCpltCallback     = HAL_SPI_TxRxCpltCallback;     /* Legacy weak TxRxCpltCallback     
 380:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxHalfCpltCallback   = HAL_SPI_TxHalfCpltCallback;   /* Legacy weak TxHalfCpltCallback   
 381:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxHalfCpltCallback   = HAL_SPI_RxHalfCpltCallback;   /* Legacy weak RxHalfCpltCallback   
 382:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxRxHalfCpltCallback = HAL_SPI_TxRxHalfCpltCallback; /* Legacy weak TxRxHalfCpltCallback 
 383:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCallback        = HAL_SPI_ErrorCallback;        /* Legacy weak ErrorCallback        
 384:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->AbortCpltCallback    = HAL_SPI_AbortCpltCallback;    /* Legacy weak AbortCpltCallback    
 385:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 386:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->MspInitCallback == NULL)
 387:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 388:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->MspInitCallback = HAL_SPI_MspInit; /* Legacy weak MspInit  */
 389:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 390:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 391:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Init the low level hardware : GPIO, CLOCK, NVIC... */
 392:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->MspInitCallback(hspi);
 393:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
 394:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Init the low level hardware : GPIO, CLOCK, NVIC... */
 395:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     HAL_SPI_MspInit(hspi);
 396:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 397:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 398:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_BUSY;
 400:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 401:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable the selected SPI peripheral */
 402:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_DISABLE(hspi);
 403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 404:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Align by default the rs fifo threshold on the data size */
 405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
 406:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 407:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     frxth = SPI_RXFIFO_THRESHOLD_HF;
 408:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 409:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
 410:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     frxth = SPI_RXFIFO_THRESHOLD_QF;
 412:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 413:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 414:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* CRC calculation is valid only for 16Bit and 8 Bit */
 415:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.DataSize != SPI_DATASIZE_16BIT) && (hspi->Init.DataSize != SPI_DATASIZE_8BIT))
 416:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 417:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* CRC must be disabled */
 418:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->Init.CRCCalculation = SPI_CRCCALCULATION_DISABLE;
 419:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 420:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 421:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /*----------------------- SPIx CR1 & CR2 Configuration ---------------------*/
 422:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Configure : SPI Mode, Communication Mode, Clock polarity and phase, NSS management,
 423:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   Communication speed, First bit and CRC calculation state */
 424:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   WRITE_REG(hspi->Instance->CR1, ((hspi->Init.Mode & (SPI_CR1_MSTR | SPI_CR1_SSI)) |
 425:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.Direction & (SPI_CR1_RXONLY | SPI_CR1_BIDIMODE)) |
 426:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.CLKPolarity & SPI_CR1_CPOL) |
 427:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.CLKPhase & SPI_CR1_CPHA) |
 428:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.NSS & SPI_CR1_SSM) |
 429:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.BaudRatePrescaler & SPI_CR1_BR_Msk) |
ARM GAS  /tmp/ccqUhOmw.s 			page 9


 430:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.FirstBit  & SPI_CR1_LSBFIRST) |
 431:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.CRCCalculation & SPI_CR1_CRCEN)));
 432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 433:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /*---------------------------- SPIx CRCL Configuration -------------------*/
 434:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
 435:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 436:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Align the CRC Length on the data size */
 437:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCLength == SPI_CRC_LENGTH_DATASIZE)
 438:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 439:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* CRC Length aligned on the data size : value set by default */
 440:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
 441:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 442:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->Init.CRCLength = SPI_CRC_LENGTH_16BIT;
 443:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 444:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
 445:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 446:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->Init.CRCLength = SPI_CRC_LENGTH_8BIT;
 447:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 448:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 449:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 450:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Configure : CRC Length */
 451:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCLength == SPI_CRC_LENGTH_16BIT)
 452:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 453:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCL);
 454:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 455:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 456:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 457:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 458:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Configure : NSS management, TI Mode, NSS Pulse, Data size and Rx Fifo threshold */
 459:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   WRITE_REG(hspi->Instance->CR2, (((hspi->Init.NSS >> 16U) & SPI_CR2_SSOE) |
 460:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.TIMode & SPI_CR2_FRF) |
 461:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.NSSPMode & SPI_CR2_NSSP) |
 462:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.DataSize & SPI_CR2_DS_Msk) |
 463:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (frxth & SPI_CR2_FRXTH)));
 464:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 465:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 466:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /*---------------------------- SPIx CRCPOLY Configuration ------------------*/
 467:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Configure : CRC Polynomial */
 468:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
 469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 470:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     WRITE_REG(hspi->Instance->CRCPR, (hspi->Init.CRCPolynomial & SPI_CRCPR_CRCPOLY_Msk));
 471:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 472:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 473:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 474:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if defined(SPI_I2SCFGR_I2SMOD)
 475:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Activate the SPI mode (Make sure that I2SMOD bit in I2SCFGR register is reset) */
 476:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->I2SCFGR, SPI_I2SCFGR_I2SMOD);
 477:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* SPI_I2SCFGR_I2SMOD */
 478:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 479:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode = HAL_SPI_ERROR_NONE;
 480:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State     = HAL_SPI_STATE_READY;
 481:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 482:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return HAL_OK;
 483:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 484:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 485:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
 486:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  De-Initialize the SPI peripheral.
ARM GAS  /tmp/ccqUhOmw.s 			page 10


 487:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
 488:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
 489:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
 490:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 491:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_DeInit(SPI_HandleTypeDef *hspi)
 492:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
 493:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the SPI handle allocation */
 494:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi == NULL)
 495:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 496:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_ERROR;
 497:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 498:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 499:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check SPI Instance parameter */
 500:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_ALL_INSTANCE(hspi->Instance));
 501:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 502:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_BUSY;
 503:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 504:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable the SPI Peripheral Clock */
 505:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_DISABLE(hspi);
 506:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 507:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
 508:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->MspDeInitCallback == NULL)
 509:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 510:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->MspDeInitCallback = HAL_SPI_MspDeInit; /* Legacy weak MspDeInit  */
 511:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 512:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 513:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* DeInit the low level hardware: GPIO, CLOCK, NVIC... */
 514:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->MspDeInitCallback(hspi);
 515:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
 516:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* DeInit the low level hardware: GPIO, CLOCK, NVIC... */
 517:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_MspDeInit(hspi);
 518:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 519:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 520:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode = HAL_SPI_ERROR_NONE;
 521:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_RESET;
 522:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 523:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Release Lock */
 524:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
 525:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 526:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return HAL_OK;
 527:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 528:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 529:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
 530:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Initialize the SPI MSP.
 531:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
 532:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
 533:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
 534:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 535:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** __weak void HAL_SPI_MspInit(SPI_HandleTypeDef *hspi)
 536:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
 537:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 538:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(hspi);
 539:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 540:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
 541:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             the HAL_SPI_MspInit should be implemented in the user file
 542:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****    */
 543:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
ARM GAS  /tmp/ccqUhOmw.s 			page 11


 544:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 545:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
 546:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  De-Initialize the SPI MSP.
 547:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
 548:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
 549:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
 550:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 551:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** __weak void HAL_SPI_MspDeInit(SPI_HandleTypeDef *hspi)
 552:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
 553:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 554:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(hspi);
 555:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 556:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
 557:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             the HAL_SPI_MspDeInit should be implemented in the user file
 558:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****    */
 559:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 560:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 561:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
 562:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
 563:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Register a User SPI Callback
 564:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         To be used instead of the weak predefined callback
 565:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi Pointer to a SPI_HandleTypeDef structure that contains
 566:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *                the configuration information for the specified SPI.
 567:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  CallbackID ID of the callback to be registered
 568:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pCallback pointer to the Callback function
 569:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
 570:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 571:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_RegisterCallback(SPI_HandleTypeDef *hspi, HAL_SPI_CallbackIDTypeDef Callb
 572:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                            pSPI_CallbackTypeDef pCallback)
 573:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
 574:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef status = HAL_OK;
 575:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 576:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (pCallback == NULL)
 577:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 578:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Update the error code */
 579:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode |= HAL_SPI_ERROR_INVALID_CALLBACK;
 580:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 581:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_ERROR;
 582:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 583:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process locked */
 584:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
 585:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 586:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_SPI_STATE_READY == hspi->State)
 587:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 588:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     switch (CallbackID)
 589:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 590:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_TX_COMPLETE_CB_ID :
 591:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxCpltCallback = pCallback;
 592:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 593:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 594:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_RX_COMPLETE_CB_ID :
 595:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxCpltCallback = pCallback;
 596:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 597:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 598:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_TX_RX_COMPLETE_CB_ID :
 599:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxRxCpltCallback = pCallback;
 600:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
ARM GAS  /tmp/ccqUhOmw.s 			page 12


 601:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 602:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_TX_HALF_COMPLETE_CB_ID :
 603:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxHalfCpltCallback = pCallback;
 604:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 605:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 606:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_RX_HALF_COMPLETE_CB_ID :
 607:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxHalfCpltCallback = pCallback;
 608:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 609:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 610:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_TX_RX_HALF_COMPLETE_CB_ID :
 611:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxRxHalfCpltCallback = pCallback;
 612:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 613:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 614:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_ERROR_CB_ID :
 615:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCallback = pCallback;
 616:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 617:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 618:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_ABORT_CB_ID :
 619:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->AbortCpltCallback = pCallback;
 620:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 621:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 622:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_MSPINIT_CB_ID :
 623:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->MspInitCallback = pCallback;
 624:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 625:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 626:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_MSPDEINIT_CB_ID :
 627:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->MspDeInitCallback = pCallback;
 628:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 629:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 630:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       default :
 631:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Update the error code */
 632:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_INVALID_CALLBACK);
 633:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 634:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Return error status */
 635:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         status =  HAL_ERROR;
 636:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 637:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 638:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 639:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else if (HAL_SPI_STATE_RESET == hspi->State)
 640:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 641:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     switch (CallbackID)
 642:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 643:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_MSPINIT_CB_ID :
 644:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->MspInitCallback = pCallback;
 645:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 646:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 647:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_MSPDEINIT_CB_ID :
 648:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->MspDeInitCallback = pCallback;
 649:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 650:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 651:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       default :
 652:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Update the error code */
 653:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_INVALID_CALLBACK);
 654:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 655:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Return error status */
 656:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         status =  HAL_ERROR;
 657:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
ARM GAS  /tmp/ccqUhOmw.s 			page 13


 658:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 659:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 660:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
 661:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 662:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Update the error code */
 663:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_INVALID_CALLBACK);
 664:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 665:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Return error status */
 666:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     status =  HAL_ERROR;
 667:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 668:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 669:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Release Lock */
 670:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
 671:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return status;
 672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 673:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 674:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
 675:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Unregister an SPI Callback
 676:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         SPI callback is redirected to the weak predefined callback
 677:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi Pointer to a SPI_HandleTypeDef structure that contains
 678:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *                the configuration information for the specified SPI.
 679:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  CallbackID ID of the callback to be unregistered
 680:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
 681:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 682:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_UnRegisterCallback(SPI_HandleTypeDef *hspi, HAL_SPI_CallbackIDTypeDef Cal
 683:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
 684:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef status = HAL_OK;
 685:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 686:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process locked */
 687:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
 688:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 689:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_SPI_STATE_READY == hspi->State)
 690:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 691:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     switch (CallbackID)
 692:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 693:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_TX_COMPLETE_CB_ID :
 694:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxCpltCallback = HAL_SPI_TxCpltCallback;             /* Legacy weak TxCpltCallback   
 695:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 696:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 697:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_RX_COMPLETE_CB_ID :
 698:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxCpltCallback = HAL_SPI_RxCpltCallback;             /* Legacy weak RxCpltCallback   
 699:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 700:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 701:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_TX_RX_COMPLETE_CB_ID :
 702:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxRxCpltCallback = HAL_SPI_TxRxCpltCallback;         /* Legacy weak TxRxCpltCallback 
 703:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 704:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 705:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_TX_HALF_COMPLETE_CB_ID :
 706:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxHalfCpltCallback = HAL_SPI_TxHalfCpltCallback;     /* Legacy weak TxHalfCpltCallbac
 707:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 708:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 709:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_RX_HALF_COMPLETE_CB_ID :
 710:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxHalfCpltCallback = HAL_SPI_RxHalfCpltCallback;     /* Legacy weak RxHalfCpltCallbac
 711:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 712:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 713:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_TX_RX_HALF_COMPLETE_CB_ID :
 714:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxRxHalfCpltCallback = HAL_SPI_TxRxHalfCpltCallback; /* Legacy weak TxRxHalfCpltCallb
ARM GAS  /tmp/ccqUhOmw.s 			page 14


 715:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 716:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 717:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_ERROR_CB_ID :
 718:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCallback = HAL_SPI_ErrorCallback;               /* Legacy weak ErrorCallback    
 719:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 720:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 721:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_ABORT_CB_ID :
 722:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->AbortCpltCallback = HAL_SPI_AbortCpltCallback;       /* Legacy weak AbortCpltCallback
 723:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 724:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 725:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_MSPINIT_CB_ID :
 726:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->MspInitCallback = HAL_SPI_MspInit;                   /* Legacy weak MspInit          
 727:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 728:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 729:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_MSPDEINIT_CB_ID :
 730:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->MspDeInitCallback = HAL_SPI_MspDeInit;               /* Legacy weak MspDeInit        
 731:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 732:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 733:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       default :
 734:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Update the error code */
 735:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_INVALID_CALLBACK);
 736:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 737:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Return error status */
 738:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         status =  HAL_ERROR;
 739:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 740:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 741:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 742:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else if (HAL_SPI_STATE_RESET == hspi->State)
 743:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 744:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     switch (CallbackID)
 745:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 746:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_MSPINIT_CB_ID :
 747:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->MspInitCallback = HAL_SPI_MspInit;                   /* Legacy weak MspInit          
 748:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 749:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 750:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       case HAL_SPI_MSPDEINIT_CB_ID :
 751:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->MspDeInitCallback = HAL_SPI_MspDeInit;               /* Legacy weak MspDeInit        
 752:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 753:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 754:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       default :
 755:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Update the error code */
 756:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_INVALID_CALLBACK);
 757:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 758:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Return error status */
 759:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         status =  HAL_ERROR;
 760:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 761:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 762:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 763:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
 764:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 765:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Update the error code */
 766:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_INVALID_CALLBACK);
 767:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 768:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Return error status */
 769:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     status =  HAL_ERROR;
 770:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 771:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/ccqUhOmw.s 			page 15


 772:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Release Lock */
 773:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
 774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return status;
 775:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 776:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 777:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
 778:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @}
 779:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 780:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 781:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /** @defgroup SPI_Exported_Functions_Group2 IO operation functions
 782:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *  @brief   Data transfers functions
 783:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *
 784:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** @verbatim
 785:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   ==============================================================================
 786:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                       ##### IO operation functions #####
 787:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****  ===============================================================================
 788:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****  [..]
 789:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     This subsection provides a set of functions allowing to manage the SPI
 790:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     data transfers.
 791:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 792:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     [..] The SPI supports master and slave mode :
 793:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 794:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     (#) There are two modes of transfer:
 795:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        (++) Blocking mode: The communication is performed in polling mode.
 796:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             The HAL status of all data processing is returned by the same function
 797:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             after finishing transfer.
 798:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        (++) No-Blocking mode: The communication is performed using Interrupts
 799:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             or DMA, These APIs return the HAL status.
 800:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             The end of the data processing will be indicated through the
 801:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             dedicated SPI IRQ when using Interrupt mode or the DMA IRQ when
 802:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             using DMA mode.
 803:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             The HAL_SPI_TxCpltCallback(), HAL_SPI_RxCpltCallback() and HAL_SPI_TxRxCpltCallback() u
 804:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             will be executed respectively at the end of the transmit or Receive process
 805:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             The HAL_SPI_ErrorCallback()user callback will be executed when a communication error is
 806:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 807:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     (#) APIs provided for these 2 transfer modes (Blocking mode or Non blocking mode using either I
 808:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         exist for 1Line (simplex) and 2Lines (full duplex) modes.
 809:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 810:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** @endverbatim
 811:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @{
 812:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 813:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 814:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
 815:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Transmit an amount of data in blocking mode.
 816:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
 817:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
 818:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pData pointer to data buffer
 819:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Size amount of data to be sent
 820:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Timeout Timeout duration
 821:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
 822:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
 823:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Transmit(SPI_HandleTypeDef *hspi, uint8_t *pData, uint16_t Size, uint32_t
 824:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
 825:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 826:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 827:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint16_t initial_TxXferCount;
 828:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/ccqUhOmw.s 			page 16


 829:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check Direction parameter */
 830:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION_2LINES_OR_1LINE(hspi->Init.Direction));
 831:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 832:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Locked */
 833:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
 834:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 835:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init tickstart for timeout management*/
 836:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tickstart = HAL_GetTick();
 837:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   initial_TxXferCount = Size;
 838:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 839:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_READY)
 840:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 841:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_BUSY;
 842:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 843:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 844:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 845:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((pData == NULL) || (Size == 0U))
 846:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 847:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
 848:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 849:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 850:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 851:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the transaction information */
 852:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State       = HAL_SPI_STATE_BUSY_TX;
 853:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 854:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pData;
 855:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 856:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 857:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 858:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /*Init field not used in handle to zero */
 859:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)NULL;
 860:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = 0U;
 861:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
 862:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 863:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
 864:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 865:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Configure communication direction : 1Line */
 866:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.Direction == SPI_DIRECTION_1LINE)
 867:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 868:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable SPI Peripheral before set 1Line direction (BIDIOE bit) */
 869:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE(hspi);
 870:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_TX(hspi);
 871:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 872:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 873:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 874:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Reset CRC Calculation */
 875:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
 876:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 877:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_RESET_CRC(hspi);
 878:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 879:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 880:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 881:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if the SPI is already enabled */
 882:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Instance->CR1 & SPI_CR1_SPE) != SPI_CR1_SPE)
 883:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 884:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Enable SPI peripheral */
 885:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_ENABLE(hspi);
ARM GAS  /tmp/ccqUhOmw.s 			page 17


 886:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 887:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 888:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in 16 Bit mode */
 889:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
 890:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 891:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if ((hspi->Init.Mode == SPI_MODE_SLAVE) || (initial_TxXferCount == 0x01U))
 892:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->Instance->DR = *((uint16_t *)hspi->pTxBuffPtr);
 894:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
 895:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount--;
 896:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 897:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Transmit data in 16 Bit mode */
 898:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     while (hspi->TxXferCount > 0U)
 899:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 900:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Wait until TXE flag is set to send data */
 901:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_TXE))
 902:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 903:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->Instance->DR = *((uint16_t *)hspi->pTxBuffPtr);
 904:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 905:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 906:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 907:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
 908:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 909:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Timeout management */
 910:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if ((((HAL_GetTick() - tickstart) >=  Timeout) && (Timeout != HAL_MAX_DELAY)) || (Timeout =
 911:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 912:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           errorcode = HAL_TIMEOUT;
 913:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
 914:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 915:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 916:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 917:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 918:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in 8 Bit mode */
 919:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
 920:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 921:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if ((hspi->Init.Mode == SPI_MODE_SLAVE) || (initial_TxXferCount == 0x01U))
 922:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 923:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (hspi->TxXferCount > 1U)
 924:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 925:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* write on the data register in packing mode */
 926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->Instance->DR = *((uint16_t *)hspi->pTxBuffPtr);
 927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 928:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount -= 2U;
 929:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 930:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
 931:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 932:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         *((__IO uint8_t *)&hspi->Instance->DR) = (*hspi->pTxBuffPtr);
 933:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr ++;
 934:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 935:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 936:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 937:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     while (hspi->TxXferCount > 0U)
 938:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 939:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Wait until TXE flag is set to send data */
 940:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_TXE))
 941:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 942:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (hspi->TxXferCount > 1U)
ARM GAS  /tmp/ccqUhOmw.s 			page 18


 943:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 944:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* write on the data register in packing mode */
 945:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->Instance->DR = *((uint16_t *)hspi->pTxBuffPtr);
 946:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint16_t);
 947:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount -= 2U;
 948:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 949:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         else
 950:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 951:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           *((__IO uint8_t *)&hspi->Instance->DR) = (*hspi->pTxBuffPtr);
 952:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr++;
 953:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount--;
 954:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 955:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 956:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
 957:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 958:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Timeout management */
 959:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if ((((HAL_GetTick() - tickstart) >=  Timeout) && (Timeout != HAL_MAX_DELAY)) || (Timeout =
 960:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 961:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           errorcode = HAL_TIMEOUT;
 962:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
 963:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 964:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 965:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 966:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 967:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 968:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable CRC Transmission */
 969:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
 970:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 971:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCNEXT);
 972:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 973:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 974:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 975:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the end of the transaction */
 976:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_EndRxTxTransaction(hspi, Timeout, tickstart) != HAL_OK)
 977:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 978:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_FLAG;
 979:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 980:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 981:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Clear overrun flag in 2 Lines communication mode because received is not read */
 982:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.Direction == SPI_DIRECTION_2LINES)
 983:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 984:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_OVRFLAG(hspi);
 985:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 986:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 987:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
 988:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 989:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
 990:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 991:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 992:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** error:
 993:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
 994:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Unlocked */
 995:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
 996:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 997:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 998:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 999:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
ARM GAS  /tmp/ccqUhOmw.s 			page 19


1000:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Receive an amount of data in blocking mode.
1001:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
1002:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
1003:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pData pointer to data buffer
1004:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Size amount of data to be received
1005:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Timeout Timeout duration
1006:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
1007:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
1008:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Receive(SPI_HandleTypeDef *hspi, uint8_t *pData, uint16_t Size, uint32_t 
1009:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
1010:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1011:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t tmpreg = 0U;
1012:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  * ptmpreg8;
1013:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  tmpreg8 = 0;
1014:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1015:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
1016:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
1017:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1018:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.Mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES))
1019:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1020:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_BUSY_RX;
1021:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Call transmit-receive function to send Dummy data on Tx line and generate clock on CLK line 
1022:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_SPI_TransmitReceive(hspi, pData, pData, Size, Timeout);
1023:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1024:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1025:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Locked */
1026:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
1027:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1028:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init tickstart for timeout management*/
1029:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tickstart = HAL_GetTick();
1030:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1031:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_READY)
1032:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1033:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_BUSY;
1034:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1035:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1036:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1037:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((pData == NULL) || (Size == 0U))
1038:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1039:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
1040:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1041:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1042:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1043:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the transaction information */
1044:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State       = HAL_SPI_STATE_BUSY_RX;
1045:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
1046:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
1047:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
1048:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
1049:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1050:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /*Init field not used in handle to zero */
1051:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)NULL;
1052:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = 0U;
1053:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
1054:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
1055:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
1056:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/ccqUhOmw.s 			page 20


1057:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1058:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Reset CRC Calculation */
1059:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
1060:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1061:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_RESET_CRC(hspi);
1062:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* this is done to handle the CRCNEXT before the latest data */
1063:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount--;
1064:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1065:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1066:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1067:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the Rx Fifo threshold */
1068:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
1069:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1070:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set RX Fifo threshold according the reception data length: 16bit */
1071:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     CLEAR_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
1072:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1073:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
1074:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1075:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set RX Fifo threshold according the reception data length: 8bit */
1076:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
1077:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1078:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1079:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Configure communication direction: 1Line */
1080:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.Direction == SPI_DIRECTION_1LINE)
1081:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1082:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable SPI Peripheral before set 1Line direction (BIDIOE bit) */
1083:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE(hspi);
1084:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_RX(hspi);
1085:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1086:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1087:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if the SPI is already enabled */
1088:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Instance->CR1 & SPI_CR1_SPE) != SPI_CR1_SPE)
1089:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1090:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Enable SPI peripheral */
1091:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_ENABLE(hspi);
1092:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1093:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1094:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Receive data in 8 Bit mode */
1095:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.DataSize <= SPI_DATASIZE_8BIT)
1096:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1097:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Transfer loop */
1098:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     while (hspi->RxXferCount > 0U)
1099:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1100:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Check the RXNE flag */
1101:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_RXNE))
1102:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1103:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* read the received data */
1104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         (* (uint8_t *)hspi->pRxBuffPtr) = *(__IO uint8_t *)&hspi->Instance->DR;
1105:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
1106:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
1107:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1108:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
1109:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1110:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Timeout management */
1111:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if ((((HAL_GetTick() - tickstart) >=  Timeout) && (Timeout != HAL_MAX_DELAY)) || (Timeout =
1112:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
1113:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           errorcode = HAL_TIMEOUT;
ARM GAS  /tmp/ccqUhOmw.s 			page 21


1114:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
1115:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
1116:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1117:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1118:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1119:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
1120:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1121:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Transfer loop */
1122:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     while (hspi->RxXferCount > 0U)
1123:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1124:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Check the RXNE flag */
1125:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_RXNE))
1126:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1127:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         *((uint16_t *)hspi->pRxBuffPtr) = (uint16_t)hspi->Instance->DR;
1128:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
1129:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
1130:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1131:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
1132:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1133:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Timeout management */
1134:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if ((((HAL_GetTick() - tickstart) >=  Timeout) && (Timeout != HAL_MAX_DELAY)) || (Timeout =
1135:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
1136:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           errorcode = HAL_TIMEOUT;
1137:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
1138:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
1139:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1140:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1141:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1142:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1143:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1144:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Handle the CRC Transmission */
1145:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
1146:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1147:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* freeze the CRC before the latest data */
1148:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCNEXT);
1149:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1150:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Read the latest data */
1151:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_RXNE, SET, Timeout, tickstart) != HAL_OK)
1152:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1153:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* the latest data has not been received */
1154:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       errorcode = HAL_TIMEOUT;
1155:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       goto error;
1156:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1157:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1158:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Receive last data in 16 Bit mode */
1159:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
1160:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1161:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       *((uint16_t *)hspi->pRxBuffPtr) = (uint16_t)hspi->Instance->DR;
1162:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1163:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Receive last data in 8 Bit mode */
1164:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     else
1165:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1166:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (*(uint8_t *)hspi->pRxBuffPtr) = *(__IO uint8_t *)&hspi->Instance->DR;
1167:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1168:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1169:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait the CRC data */
1170:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_RXNE, SET, Timeout, tickstart) != HAL_OK)
ARM GAS  /tmp/ccqUhOmw.s 			page 22


1171:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1172:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
1173:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       errorcode = HAL_TIMEOUT;
1174:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       goto error;
1175:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1176:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1177:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Read CRC to Flush DR and RXNE flag */
1178:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.DataSize == SPI_DATASIZE_16BIT)
1179:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1180:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Read 16bit CRC */
1181:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       tmpreg = READ_REG(hspi->Instance->DR);
1182:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* To avoid GCC warning */
1183:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       UNUSED(tmpreg);
1184:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1185:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     else
1186:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1187:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Initialize the 8bit temporary pointer */
1188:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       ptmpreg8 = (__IO uint8_t *)&hspi->Instance->DR;
1189:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Read 8bit CRC */
1190:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       tmpreg8 = *ptmpreg8;
1191:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* To avoid GCC warning */
1192:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       UNUSED(tmpreg8);
1193:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1194:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((hspi->Init.DataSize == SPI_DATASIZE_8BIT) && (hspi->Init.CRCLength == SPI_CRC_LENGTH_16B
1195:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1196:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_RXNE, SET, Timeout, tickstart) != HAL_OK)
1197:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
1198:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Error on the CRC reception */
1199:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
1200:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           errorcode = HAL_TIMEOUT;
1201:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
1202:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
1203:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Read 8bit CRC again in case of 16bit CRC in 8bit Data mode */
1204:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         tmpreg8 = *ptmpreg8;
1205:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* To avoid GCC warning */
1206:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         UNUSED(tmpreg8);
1207:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1208:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1209:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1210:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1211:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1212:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the end of the transaction */
1213:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_EndRxTransaction(hspi, Timeout, tickstart) != HAL_OK)
1214:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1215:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_FLAG;
1216:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1217:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1218:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1219:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if CRC error occurred */
1220:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_CRCERR))
1221:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1222:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
1223:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_CRCERRFLAG(hspi);
1224:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1225:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1226:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1227:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
ARM GAS  /tmp/ccqUhOmw.s 			page 23


1228:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1229:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
1230:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1231:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1232:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** error :
1233:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
1234:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
1235:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
1236:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
1237:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1238:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
1239:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Transmit and Receive an amount of data in blocking mode.
1240:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
1241:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
1242:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pTxData pointer to transmission data buffer
1243:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pRxData pointer to reception data buffer
1244:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Size amount of data to be sent and received
1245:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Timeout Timeout duration
1246:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
1247:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
1248:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_TransmitReceive(SPI_HandleTypeDef *hspi, uint8_t *pTxData, uint8_t *pRxDa
1249:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                           uint32_t Timeout)
1250:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
1251:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint16_t             initial_TxXferCount;
1252:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint16_t             initial_RxXferCount;
1253:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             tmp_mode;
1254:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_StateTypeDef tmp_state;
1255:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             tickstart;
1256:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1257:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t tmpreg = 0U;
1258:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             spi_cr1;
1259:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             spi_cr2;
1260:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  * ptmpreg8;
1261:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  tmpreg8 = 0;
1262:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1263:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1264:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Variable used to alternate Rx and Tx during transfer */
1265:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             txallowed = 1U;
1266:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef    errorcode = HAL_OK;
1267:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1268:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check Direction parameter */
1269:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION_2LINES(hspi->Init.Direction));
1270:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1271:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Locked */
1272:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
1273:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1274:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init tickstart for timeout management*/
1275:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tickstart = HAL_GetTick();
1276:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1277:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init temporary variables */
1278:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_state           = hspi->State;
1279:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_mode            = hspi->Init.Mode;
1280:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   initial_TxXferCount = Size;
1281:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   initial_RxXferCount = Size;
1282:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1283:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   spi_cr1             = READ_REG(hspi->Instance->CR1);
1284:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   spi_cr2             = READ_REG(hspi->Instance->CR2);
ARM GAS  /tmp/ccqUhOmw.s 			page 24


1285:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1286:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1287:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (!((tmp_state == HAL_SPI_STATE_READY) || \
1288:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
1289:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1290:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_BUSY;
1291:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1292:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1293:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1294:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((pTxData == NULL) || (pRxData == NULL) || (Size == 0U))
1295:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
1297:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1298:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1299:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1300:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Don't overwrite in case of HAL_SPI_STATE_BUSY_RX */
1301:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_BUSY_RX)
1302:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1303:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_BUSY_TX_RX;
1304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1305:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1306:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the transaction information */
1307:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
1308:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
1309:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
1310:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
1311:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pTxData;
1312:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
1313:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
1314:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1315:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /*Init field not used in handle to zero */
1316:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
1317:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
1318:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1319:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1320:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Reset CRC Calculation */
1321:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
1322:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1323:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_RESET_CRC(hspi);
1324:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1325:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1326:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1327:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the Rx Fifo threshold */
1328:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) || (initial_RxXferCount > 1U))
1329:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1330:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set fiforxthreshold according the reception data length: 16bit */
1331:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     CLEAR_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
1332:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1333:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
1334:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1335:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set fiforxthreshold according the reception data length: 8bit */
1336:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
1337:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1338:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1339:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if the SPI is already enabled */
1340:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Instance->CR1 & SPI_CR1_SPE) != SPI_CR1_SPE)
1341:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/ccqUhOmw.s 			page 25


1342:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Enable SPI peripheral */
1343:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_ENABLE(hspi);
1344:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1345:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1346:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit and Receive data in 16 Bit mode */
1347:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
1348:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1349:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if ((hspi->Init.Mode == SPI_MODE_SLAVE) || (initial_TxXferCount == 0x01U))
1350:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1351:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->Instance->DR = *((uint16_t *)hspi->pTxBuffPtr);
1352:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
1353:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount--;
1354:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1355:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     while ((hspi->TxXferCount > 0U) || (hspi->RxXferCount > 0U))
1356:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1357:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Check TXE flag */
1358:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_TXE)) && (hspi->TxXferCount > 0U) && (txallowed == 1U)
1359:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->Instance->DR = *((uint16_t *)hspi->pTxBuffPtr);
1361:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
1362:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
1363:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Next Data is a reception (Rx). Tx not allowed */
1364:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         txallowed = 0U;
1365:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1366:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1367:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Enable CRC Transmission */
1368:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if ((hspi->TxXferCount == 0U) && (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE))
1369:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
1370:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Set NSS Soft to received correctly the CRC on slave mode with NSS pulse activated */
1371:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if ((READ_BIT(spi_cr1, SPI_CR1_MSTR) == 0U) && (READ_BIT(spi_cr2, SPI_CR2_NSSP) == SPI_CR
1372:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
1373:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             SET_BIT(hspi->Instance->CR1, SPI_CR1_SSM);
1374:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           }
1375:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCNEXT);
1376:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
1377:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1378:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1379:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1380:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Check RXNE flag */
1381:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_RXNE)) && (hspi->RxXferCount > 0U))
1382:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1383:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         *((uint16_t *)hspi->pRxBuffPtr) = (uint16_t)hspi->Instance->DR;
1384:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
1385:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
1386:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Next Data is a Transmission (Tx). Tx is allowed */
1387:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         txallowed = 1U;
1388:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1389:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (((HAL_GetTick() - tickstart) >=  Timeout) && (Timeout != HAL_MAX_DELAY))
1390:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1391:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         errorcode = HAL_TIMEOUT;
1392:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         goto error;
1393:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1394:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1395:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1396:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit and Receive data in 8 Bit mode */
1397:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
1398:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/ccqUhOmw.s 			page 26


1399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if ((hspi->Init.Mode == SPI_MODE_SLAVE) || (initial_TxXferCount == 0x01U))
1400:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1401:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (hspi->TxXferCount > 1U)
1402:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->Instance->DR = *((uint16_t *)hspi->pTxBuffPtr);
1404:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
1405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount -= 2U;
1406:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1407:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
1408:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1409:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         *(__IO uint8_t *)&hspi->Instance->DR = (*hspi->pTxBuffPtr);
1410:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr++;
1411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
1412:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1413:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1414:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     while ((hspi->TxXferCount > 0U) || (hspi->RxXferCount > 0U))
1415:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1416:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Check TXE flag */
1417:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_TXE)) && (hspi->TxXferCount > 0U) && (txallowed == 1U)
1418:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1419:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (hspi->TxXferCount > 1U)
1420:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
1421:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->Instance->DR = *((uint16_t *)hspi->pTxBuffPtr);
1422:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint16_t);
1423:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount -= 2U;
1424:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
1425:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         else
1426:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
1427:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           *(__IO uint8_t *)&hspi->Instance->DR = (*hspi->pTxBuffPtr);
1428:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr++;
1429:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount--;
1430:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
1431:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Next Data is a reception (Rx). Tx not allowed */
1432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         txallowed = 0U;
1433:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1434:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1435:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Enable CRC Transmission */
1436:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if ((hspi->TxXferCount == 0U) && (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE))
1437:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
1438:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Set NSS Soft to received correctly the CRC on slave mode with NSS pulse activated */
1439:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if ((READ_BIT(spi_cr1, SPI_CR1_MSTR) == 0U) && (READ_BIT(spi_cr2, SPI_CR2_NSSP) == SPI_CR
1440:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
1441:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             SET_BIT(hspi->Instance->CR1, SPI_CR1_SSM);
1442:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           }
1443:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCNEXT);
1444:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
1445:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1446:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1447:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1448:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Wait until RXNE flag is reset */
1449:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_RXNE)) && (hspi->RxXferCount > 0U))
1450:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1451:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (hspi->RxXferCount > 1U)
1452:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
1453:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           *((uint16_t *)hspi->pRxBuffPtr) = (uint16_t)hspi->Instance->DR;
1454:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint16_t);
1455:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->RxXferCount -= 2U;
ARM GAS  /tmp/ccqUhOmw.s 			page 27


1456:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if (hspi->RxXferCount <= 1U)
1457:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
1458:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             /* Set RX Fifo threshold before to switch on 8 bit data size */
1459:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             SET_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
1460:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           }
1461:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
1462:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         else
1463:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
1464:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           (*(uint8_t *)hspi->pRxBuffPtr) = *(__IO uint8_t *)&hspi->Instance->DR;
1465:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pRxBuffPtr++;
1466:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->RxXferCount--;
1467:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
1468:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Next Data is a Transmission (Tx). Tx is allowed */
1469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         txallowed = 1U;
1470:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1471:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((((HAL_GetTick() - tickstart) >=  Timeout) && ((Timeout != HAL_MAX_DELAY))) || (Timeout =
1472:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1473:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         errorcode = HAL_TIMEOUT;
1474:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         goto error;
1475:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1476:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1477:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1478:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1479:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1480:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Read CRC from DR to close CRC calculation process */
1481:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
1482:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1483:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait until TXE flag */
1484:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_RXNE, SET, Timeout, tickstart) != HAL_OK)
1485:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1486:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Error on the CRC reception */
1487:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
1488:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       errorcode = HAL_TIMEOUT;
1489:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       goto error;
1490:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1491:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Read CRC */
1492:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.DataSize == SPI_DATASIZE_16BIT)
1493:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1494:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Read 16bit CRC */
1495:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       tmpreg = READ_REG(hspi->Instance->DR);
1496:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* To avoid GCC warning */
1497:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       UNUSED(tmpreg);
1498:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1499:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     else
1500:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1501:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Initialize the 8bit temporary pointer */
1502:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       ptmpreg8 = (__IO uint8_t *)&hspi->Instance->DR;
1503:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Read 8bit CRC */
1504:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       tmpreg8 = *ptmpreg8;
1505:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* To avoid GCC warning */
1506:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       UNUSED(tmpreg8);
1507:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1508:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (hspi->Init.CRCLength == SPI_CRC_LENGTH_16BIT)
1509:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
1510:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_RXNE, SET, Timeout, tickstart) != HAL_OK)
1511:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
1512:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Error on the CRC reception */
ARM GAS  /tmp/ccqUhOmw.s 			page 28


1513:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
1514:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           errorcode = HAL_TIMEOUT;
1515:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
1516:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
1517:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Read 8bit CRC again in case of 16bit CRC in 8bit Data mode */
1518:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         tmpreg8 = *ptmpreg8;
1519:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* To avoid GCC warning */
1520:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         UNUSED(tmpreg8);
1521:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
1522:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1523:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1524:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1525:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if CRC error occurred */
1526:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_CRCERR))
1527:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1528:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
1529:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Clear CRC Flag */
1530:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_CRCERRFLAG(hspi);
1531:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1532:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
1533:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1534:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1535:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1536:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the end of the transaction */
1537:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_EndRxTxTransaction(hspi, Timeout, tickstart) != HAL_OK)
1538:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1539:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
1540:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_FLAG;
1541:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1542:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1543:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** error :
1544:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
1545:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
1546:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
1547:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
1548:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1549:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
1550:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Transmit an amount of data in non-blocking mode with Interrupt.
1551:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
1552:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
1553:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pData pointer to data buffer
1554:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Size amount of data to be sent
1555:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
1556:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
1557:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Transmit_IT(SPI_HandleTypeDef *hspi, uint8_t *pData, uint16_t Size)
1558:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
1559:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
1560:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1561:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check Direction parameter */
1562:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION_2LINES_OR_1LINE(hspi->Init.Direction));
1563:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1564:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Locked */
1565:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
1566:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1567:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((pData == NULL) || (Size == 0U))
1568:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1569:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
ARM GAS  /tmp/ccqUhOmw.s 			page 29


1570:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1571:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1572:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1573:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_READY)
1574:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1575:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_BUSY;
1576:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1577:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1578:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1579:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the transaction information */
1580:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State       = HAL_SPI_STATE_BUSY_TX;
1581:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
1582:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pData;
1583:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
1584:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
1585:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1586:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init field not used in handle to zero */
1587:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)NULL;
1588:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = 0U;
1589:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
1590:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
1591:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1592:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the function for IT treatment */
1593:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
1594:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1595:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR = SPI_TxISR_16BIT;
1596:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1597:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
1598:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1599:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR = SPI_TxISR_8BIT;
1600:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1601:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1602:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Configure communication direction : 1Line */
1603:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.Direction == SPI_DIRECTION_1LINE)
1604:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1605:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable SPI Peripheral before set 1Line direction (BIDIOE bit) */
1606:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE(hspi);
1607:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_TX(hspi);
1608:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1609:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1610:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1611:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Reset CRC Calculation */
1612:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
1613:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1614:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_RESET_CRC(hspi);
1615:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1616:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1617:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1618:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable TXE and ERR interrupt */
1619:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_ENABLE_IT(hspi, (SPI_IT_TXE | SPI_IT_ERR));
1620:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1621:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1622:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if the SPI is already enabled */
1623:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Instance->CR1 & SPI_CR1_SPE) != SPI_CR1_SPE)
1624:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1625:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Enable SPI peripheral */
1626:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_ENABLE(hspi);
ARM GAS  /tmp/ccqUhOmw.s 			page 30


1627:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1628:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1629:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** error :
1630:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
1631:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
1632:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
1633:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1634:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
1635:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Receive an amount of data in non-blocking mode with Interrupt.
1636:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
1637:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
1638:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pData pointer to data buffer
1639:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Size amount of data to be sent
1640:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
1641:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
1642:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Receive_IT(SPI_HandleTypeDef *hspi, uint8_t *pData, uint16_t Size)
1643:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
1644:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
1645:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1646:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.Direction == SPI_DIRECTION_2LINES) && (hspi->Init.Mode == SPI_MODE_MASTER))
1647:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1648:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_BUSY_RX;
1649:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Call transmit-receive function to send Dummy data on Tx line and generate clock on CLK line 
1650:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_SPI_TransmitReceive_IT(hspi, pData, pData, Size);
1651:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1652:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1653:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Locked */
1654:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
1655:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1656:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_READY)
1657:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1658:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_BUSY;
1659:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1660:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1661:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1662:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((pData == NULL) || (Size == 0U))
1663:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1664:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
1665:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1666:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1667:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1668:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the transaction information */
1669:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State       = HAL_SPI_STATE_BUSY_RX;
1670:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
1671:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
1672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
1673:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
1674:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1675:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init field not used in handle to zero */
1676:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)NULL;
1677:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = 0U;
1678:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
1679:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
1680:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1681:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the data size to adapt Rx threshold and the set the function for IT treatment */
1682:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
1683:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/ccqUhOmw.s 			page 31


1684:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set RX Fifo threshold according the reception data length: 16 bit */
1685:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     CLEAR_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
1686:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxISR = SPI_RxISR_16BIT;
1687:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1688:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
1689:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1690:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set RX Fifo threshold according the reception data length: 8 bit */
1691:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
1692:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxISR = SPI_RxISR_8BIT;
1693:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1694:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1695:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Configure communication direction : 1Line */
1696:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.Direction == SPI_DIRECTION_1LINE)
1697:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1698:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable SPI Peripheral before set 1Line direction (BIDIOE bit) */
1699:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE(hspi);
1700:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_RX(hspi);
1701:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1702:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1703:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1704:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Reset CRC Calculation */
1705:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
1706:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1707:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->CRCSize = 1U;
1708:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if ((hspi->Init.DataSize <= SPI_DATASIZE_8BIT) && (hspi->Init.CRCLength == SPI_CRC_LENGTH_16BIT
1709:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1710:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->CRCSize = 2U;
1711:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1712:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_RESET_CRC(hspi);
1713:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1714:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
1715:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1716:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->CRCSize = 0U;
1717:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1718:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1719:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1720:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable TXE and ERR interrupt */
1721:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_ENABLE_IT(hspi, (SPI_IT_RXNE | SPI_IT_ERR));
1722:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1723:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Note : The SPI must be enabled after unlocking current process
1724:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             to avoid the risk of SPI interrupt handle execution before current
1725:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             process unlock */
1726:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1727:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if the SPI is already enabled */
1728:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Instance->CR1 & SPI_CR1_SPE) != SPI_CR1_SPE)
1729:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1730:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Enable SPI peripheral */
1731:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_ENABLE(hspi);
1732:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1733:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1734:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** error :
1735:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Unlocked */
1736:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
1737:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
1738:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
1739:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1740:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
ARM GAS  /tmp/ccqUhOmw.s 			page 32


1741:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Transmit and Receive an amount of data in non-blocking mode with Interrupt.
1742:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
1743:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
1744:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pTxData pointer to transmission data buffer
1745:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pRxData pointer to reception data buffer
1746:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Size amount of data to be sent and received
1747:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
1748:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
1749:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_TransmitReceive_IT(SPI_HandleTypeDef *hspi, uint8_t *pTxData, uint8_t *pR
1750:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
1751:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             tmp_mode;
1752:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_StateTypeDef tmp_state;
1753:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef    errorcode = HAL_OK;
1754:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1755:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check Direction parameter */
1756:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION_2LINES(hspi->Init.Direction));
1757:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1758:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process locked */
1759:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
1760:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1761:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init temporary variables */
1762:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_state           = hspi->State;
1763:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_mode            = hspi->Init.Mode;
1764:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1765:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (!((tmp_state == HAL_SPI_STATE_READY) || \
1766:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
1767:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1768:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_BUSY;
1769:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1770:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1771:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1772:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((pTxData == NULL) || (pRxData == NULL) || (Size == 0U))
1773:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
1775:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1776:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1777:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1778:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Don't overwrite in case of HAL_SPI_STATE_BUSY_RX */
1779:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_BUSY_RX)
1780:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1781:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_BUSY_TX_RX;
1782:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1783:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1784:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the transaction information */
1785:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
1786:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pTxData;
1787:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
1788:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
1789:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
1790:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
1791:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
1792:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1793:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the function for IT treatment */
1794:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
1795:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1796:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxISR     = SPI_2linesRxISR_16BIT;
1797:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR     = SPI_2linesTxISR_16BIT;
ARM GAS  /tmp/ccqUhOmw.s 			page 33


1798:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1799:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
1800:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1801:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxISR     = SPI_2linesRxISR_8BIT;
1802:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR     = SPI_2linesTxISR_8BIT;
1803:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1804:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1805:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1806:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Reset CRC Calculation */
1807:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
1808:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1809:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->CRCSize = 1U;
1810:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if ((hspi->Init.DataSize <= SPI_DATASIZE_8BIT) && (hspi->Init.CRCLength == SPI_CRC_LENGTH_16BIT
1811:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1812:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->CRCSize = 2U;
1813:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1814:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_RESET_CRC(hspi);
1815:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1816:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
1817:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1818:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->CRCSize = 0U;
1819:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1820:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
1821:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1822:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if packing mode is enabled and if there is more than 2 data to receive */
1823:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.DataSize > SPI_DATASIZE_8BIT) || (Size >= 2U))
1824:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1825:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set RX Fifo threshold according the reception data length: 16 bit */
1826:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     CLEAR_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
1827:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1828:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
1829:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1830:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set RX Fifo threshold according the reception data length: 8 bit */
1831:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
1832:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1833:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1834:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable TXE, RXNE and ERR interrupt */
1835:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_ENABLE_IT(hspi, (SPI_IT_TXE | SPI_IT_RXNE | SPI_IT_ERR));
1836:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1837:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if the SPI is already enabled */
1838:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Instance->CR1 & SPI_CR1_SPE) != SPI_CR1_SPE)
1839:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1840:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Enable SPI peripheral */
1841:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_ENABLE(hspi);
1842:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1843:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1844:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** error :
1845:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Unlocked */
1846:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
1847:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
1848:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
1849:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1850:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
1851:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Transmit an amount of data in non-blocking mode with DMA.
1852:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
1853:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
1854:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pData pointer to data buffer
ARM GAS  /tmp/ccqUhOmw.s 			page 34


1855:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Size amount of data to be sent
1856:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
1857:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
1858:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Transmit_DMA(SPI_HandleTypeDef *hspi, uint8_t *pData, uint16_t Size)
1859:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
1860:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
1861:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1862:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check tx dma handle */
1863:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DMA_HANDLE(hspi->hdmatx));
1864:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1865:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check Direction parameter */
1866:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION_2LINES_OR_1LINE(hspi->Init.Direction));
1867:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1868:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Locked */
1869:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
1870:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1871:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_READY)
1872:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1873:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_BUSY;
1874:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1875:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1876:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1877:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((pData == NULL) || (Size == 0U))
1878:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1879:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
1880:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1881:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1882:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1883:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the transaction information */
1884:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State       = HAL_SPI_STATE_BUSY_TX;
1885:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
1886:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pData;
1887:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
1888:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
1889:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1890:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init field not used in handle to zero */
1891:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)NULL;
1892:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
1893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
1894:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = 0U;
1895:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
1896:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1897:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Configure communication direction : 1Line */
1898:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.Direction == SPI_DIRECTION_1LINE)
1899:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1900:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable SPI Peripheral before set 1Line direction (BIDIOE bit) */
1901:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE(hspi);
1902:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_TX(hspi);
1903:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1904:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1905:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
1906:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Reset CRC Calculation */
1907:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
1908:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1909:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_RESET_CRC(hspi);
1910:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1911:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
ARM GAS  /tmp/ccqUhOmw.s 			page 35


1912:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1913:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the SPI TxDMA Half transfer complete callback */
1914:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferHalfCpltCallback = SPI_DMAHalfTransmitCplt;
1915:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1916:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the SPI TxDMA transfer complete callback */
1917:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferCpltCallback = SPI_DMATransmitCplt;
1918:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1919:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the DMA error callback */
1920:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferErrorCallback = SPI_DMAError;
1921:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1922:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the DMA AbortCpltCallback */
1923:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferAbortCallback = NULL;
1924:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1925:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_LDMATX);
1926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Packing mode is enabled only if the DMA setting is HALWORD */
1927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.DataSize <= SPI_DATASIZE_8BIT) && (hspi->hdmatx->Init.MemDataAlignment == DMA_MDA
1928:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1929:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Check the even/odd of the data size + crc if enabled */
1930:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if ((hspi->TxXferCount & 0x1U) == 0U)
1931:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1932:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_LDMATX);
1933:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount = (hspi->TxXferCount >> 1U);
1934:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1935:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     else
1936:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
1937:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->Instance->CR2, SPI_CR2_LDMATX);
1938:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount = (hspi->TxXferCount >> 1U) + 1U;
1939:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
1940:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1941:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1942:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable the Tx DMA Stream/Channel */
1943:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_OK != HAL_DMA_Start_IT(hspi->hdmatx, (uint32_t)hspi->pTxBuffPtr, (uint32_t)&hspi->Instanc
1944:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
1945:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1946:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Update SPI error code */
1947:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_DMA);
1948:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
1949:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1950:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
1951:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
1952:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1953:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1954:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if the SPI is already enabled */
1955:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Instance->CR1 & SPI_CR1_SPE) != SPI_CR1_SPE)
1956:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1957:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Enable SPI peripheral */
1958:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_ENABLE(hspi);
1959:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
1960:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1961:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable the SPI Error Interrupt Bit */
1962:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_ENABLE_IT(hspi, (SPI_IT_ERR));
1963:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1964:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable Tx DMA Request */
1965:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SET_BIT(hspi->Instance->CR2, SPI_CR2_TXDMAEN);
1966:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1967:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** error :
1968:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Unlocked */
ARM GAS  /tmp/ccqUhOmw.s 			page 36


1969:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
1970:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
1971:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
1972:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1973:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
1974:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Receive an amount of data in non-blocking mode with DMA.
1975:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @note   In case of MASTER mode and SPI_DIRECTION_2LINES direction, hdmatx shall be defined.
1976:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
1977:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
1978:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pData pointer to data buffer
1979:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @note   When the CRC feature is enabled the pData Length must be Size + 1.
1980:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Size amount of data to be sent
1981:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
1982:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
1983:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Receive_DMA(SPI_HandleTypeDef *hspi, uint8_t *pData, uint16_t Size)
1984:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
1985:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
1986:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1987:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check rx dma handle */
1988:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DMA_HANDLE(hspi->hdmarx));
1989:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1990:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.Direction == SPI_DIRECTION_2LINES) && (hspi->Init.Mode == SPI_MODE_MASTER))
1991:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
1992:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_BUSY_RX;
1993:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1994:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Check tx dma handle */
1995:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     assert_param(IS_SPI_DMA_HANDLE(hspi->hdmatx));
1996:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
1997:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Call transmit-receive function to send Dummy data on Tx line and generate clock on CLK line 
1998:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_SPI_TransmitReceive_DMA(hspi, pData, pData, Size);
1999:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2000:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2001:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Locked */
2002:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
2003:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2004:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_READY)
2005:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2006:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_BUSY;
2007:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
2008:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2009:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2010:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((pData == NULL) || (Size == 0U))
2011:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2012:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
2013:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
2014:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2015:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2016:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the transaction information */
2017:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State       = HAL_SPI_STATE_BUSY_RX;
2018:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
2019:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
2020:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
2021:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
2022:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2023:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /*Init field not used in handle to zero */
2024:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
2025:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
ARM GAS  /tmp/ccqUhOmw.s 			page 37


2026:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = 0U;
2027:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
2028:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2029:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Configure communication direction : 1Line */
2030:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.Direction == SPI_DIRECTION_1LINE)
2031:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2032:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable SPI Peripheral before set 1Line direction (BIDIOE bit) */
2033:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE(hspi);
2034:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_RX(hspi);
2035:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2036:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2037:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
2038:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Reset CRC Calculation */
2039:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
2040:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2041:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_RESET_CRC(hspi);
2042:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2043:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
2044:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2045:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if defined (STM32F302xC) || defined (STM32F303xC) || defined (STM32F373xC) || defined (STM32F358xx
2046:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Packing mode management is enabled by the DMA settings */
2047:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.DataSize <= SPI_DATASIZE_8BIT) && (hspi->hdmarx->Init.MemDataAlignment == DMA_MDA
2048:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2049:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Restriction the DMA data received is not allowed in this mode */
2050:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
2051:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
2052:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2053:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* STM32F302xC || STM32F303xC || STM32F373xC || STM32F358xx || STM32F378xx */
2054:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2055:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_LDMARX);
2056:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
2057:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2058:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set RX Fifo threshold according the reception data length: 16bit */
2059:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     CLEAR_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
2060:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2061:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
2062:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2063:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set RX Fifo threshold according the reception data length: 8bit */
2064:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
2065:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2066:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->hdmarx->Init.MemDataAlignment == DMA_MDATAALIGN_HALFWORD)
2067:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2068:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Set RX Fifo threshold according the reception data length: 16bit */
2069:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       CLEAR_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
2070:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2071:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((hspi->RxXferCount & 0x1U) == 0x0U)
2072:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2073:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_LDMARX);
2074:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount = hspi->RxXferCount >> 1U;
2075:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2076:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
2077:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2078:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->Instance->CR2, SPI_CR2_LDMARX);
2079:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount = (hspi->RxXferCount >> 1U) + 1U;
2080:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2081:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2082:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
ARM GAS  /tmp/ccqUhOmw.s 			page 38


2083:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2084:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the SPI RxDMA Half transfer complete callback */
2085:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmarx->XferHalfCpltCallback = SPI_DMAHalfReceiveCplt;
2086:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2087:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the SPI Rx DMA transfer complete callback */
2088:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmarx->XferCpltCallback = SPI_DMAReceiveCplt;
2089:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2090:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the DMA error callback */
2091:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmarx->XferErrorCallback = SPI_DMAError;
2092:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2093:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the DMA AbortCpltCallback */
2094:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmarx->XferAbortCallback = NULL;
2095:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2096:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable the Rx DMA Stream/Channel  */
2097:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_OK != HAL_DMA_Start_IT(hspi->hdmarx, (uint32_t)&hspi->Instance->DR, (uint32_t)hspi->pRxBu
2098:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->RxXferCount))
2099:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2100:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Update SPI error code */
2101:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_DMA);
2102:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
2103:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
2105:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
2106:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2107:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2108:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if the SPI is already enabled */
2109:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Instance->CR1 & SPI_CR1_SPE) != SPI_CR1_SPE)
2110:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2111:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Enable SPI peripheral */
2112:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_ENABLE(hspi);
2113:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2114:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2115:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable the SPI Error Interrupt Bit */
2116:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_ENABLE_IT(hspi, (SPI_IT_ERR));
2117:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2118:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable Rx DMA Request */
2119:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SET_BIT(hspi->Instance->CR2, SPI_CR2_RXDMAEN);
2120:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2121:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** error:
2122:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Unlocked */
2123:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
2124:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
2125:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2126:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2127:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2128:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Transmit and Receive an amount of data in non-blocking mode with DMA.
2129:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2130:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
2131:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pTxData pointer to transmission data buffer
2132:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  pRxData pointer to reception data buffer
2133:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @note   When the CRC feature is enabled the pRxData Length must be Size + 1
2134:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Size amount of data to be sent
2135:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
2136:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2137:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_TransmitReceive_DMA(SPI_HandleTypeDef *hspi, uint8_t *pTxData, uint8_t *p
2138:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                               uint16_t Size)
2139:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
ARM GAS  /tmp/ccqUhOmw.s 			page 39


2140:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             tmp_mode;
2141:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_StateTypeDef tmp_state;
2142:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
2143:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2144:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check rx & tx dma handles */
2145:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DMA_HANDLE(hspi->hdmarx));
2146:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DMA_HANDLE(hspi->hdmatx));
2147:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2148:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check Direction parameter */
2149:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION_2LINES(hspi->Init.Direction));
2150:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2151:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process locked */
2152:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
2153:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2154:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init temporary variables */
2155:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_state           = hspi->State;
2156:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_mode            = hspi->Init.Mode;
2157:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2158:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (!((tmp_state == HAL_SPI_STATE_READY) ||
2159:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
2160:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2161:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_BUSY;
2162:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
2163:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2164:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2165:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((pTxData == NULL) || (pRxData == NULL) || (Size == 0U))
2166:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2167:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
2168:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
2169:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2170:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2171:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Don't overwrite in case of HAL_SPI_STATE_BUSY_RX */
2172:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->State != HAL_SPI_STATE_BUSY_RX)
2173:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2174:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_BUSY_TX_RX;
2175:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2176:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2177:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the transaction information */
2178:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
2179:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pTxData;
2180:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
2181:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
2182:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
2183:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
2184:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
2185:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2186:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init field not used in handle to zero */
2187:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
2188:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
2189:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2190:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
2191:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Reset CRC Calculation */
2192:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
2193:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2194:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_RESET_CRC(hspi);
2195:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2196:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
ARM GAS  /tmp/ccqUhOmw.s 			page 40


2197:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2198:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if defined (STM32F302xC) || defined (STM32F303xC) || defined (STM32F373xC) || defined (STM32F358xx
2199:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Packing mode management is enabled by the DMA settings */
2200:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.DataSize <= SPI_DATASIZE_8BIT) && (hspi->hdmarx->Init.MemDataAlignment == DMA_MDA
2201:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2202:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Restriction the DMA data received is not allowed in this mode */
2203:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
2204:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
2205:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2206:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* STM32F302xC || STM32F303xC || STM32F373xC || STM32F358xx || STM32F378xx */
2207:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2208:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Reset the threshold bit */
2209:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_LDMATX | SPI_CR2_LDMARX);
2210:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2211:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* The packing mode management is enabled by the DMA settings according the spi data size */
2212:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
2213:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2214:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set fiforxthreshold according the reception data length: 16bit */
2215:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     CLEAR_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
2216:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2217:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
2218:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2219:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set RX Fifo threshold according the reception data length: 8bit */
2220:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
2221:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2222:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->hdmatx->Init.MemDataAlignment == DMA_MDATAALIGN_HALFWORD)
2223:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2224:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((hspi->TxXferSize & 0x1U) == 0x0U)
2225:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2226:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_LDMATX);
2227:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount = hspi->TxXferCount >> 1U;
2228:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2229:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
2230:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2231:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->Instance->CR2, SPI_CR2_LDMATX);
2232:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount = (hspi->TxXferCount >> 1U) + 1U;
2233:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2234:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2235:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2236:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->hdmarx->Init.MemDataAlignment == DMA_MDATAALIGN_HALFWORD)
2237:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2238:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Set RX Fifo threshold according the reception data length: 16bit */
2239:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       CLEAR_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
2240:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2241:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((hspi->RxXferCount & 0x1U) == 0x0U)
2242:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2243:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_LDMARX);
2244:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount = hspi->RxXferCount >> 1U;
2245:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2246:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
2247:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2248:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->Instance->CR2, SPI_CR2_LDMARX);
2249:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount = (hspi->RxXferCount >> 1U) + 1U;
2250:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2251:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2252:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2253:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/ccqUhOmw.s 			page 41


2254:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if we are in Rx only or in Rx/Tx Mode and configure the DMA transfer complete callback *
2255:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->State == HAL_SPI_STATE_BUSY_RX)
2256:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2257:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set the SPI Rx DMA Half transfer complete callback */
2258:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->hdmarx->XferHalfCpltCallback = SPI_DMAHalfReceiveCplt;
2259:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->hdmarx->XferCpltCallback     = SPI_DMAReceiveCplt;
2260:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2261:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
2262:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2263:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set the SPI Tx/Rx DMA Half transfer complete callback */
2264:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->hdmarx->XferHalfCpltCallback = SPI_DMAHalfTransmitReceiveCplt;
2265:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->hdmarx->XferCpltCallback     = SPI_DMATransmitReceiveCplt;
2266:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2267:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2268:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the DMA error callback */
2269:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmarx->XferErrorCallback = SPI_DMAError;
2270:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2271:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the DMA AbortCpltCallback */
2272:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmarx->XferAbortCallback = NULL;
2273:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2274:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable the Rx DMA Stream/Channel  */
2275:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_OK != HAL_DMA_Start_IT(hspi->hdmarx, (uint32_t)&hspi->Instance->DR, (uint32_t)hspi->pRxBu
2276:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->RxXferCount))
2277:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2278:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Update SPI error code */
2279:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_DMA);
2280:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
2281:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2282:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
2283:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
2284:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2285:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2286:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable Rx DMA Request */
2287:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SET_BIT(hspi->Instance->CR2, SPI_CR2_RXDMAEN);
2288:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2289:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Set the SPI Tx DMA transfer complete callback as NULL because the communication closing
2290:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   is performed in DMA reception complete callback  */
2291:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferHalfCpltCallback = NULL;
2292:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferCpltCallback     = NULL;
2293:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferErrorCallback    = NULL;
2294:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferAbortCallback    = NULL;
2295:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable the Tx DMA Stream/Channel  */
2297:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_OK != HAL_DMA_Start_IT(hspi->hdmatx, (uint32_t)hspi->pTxBuffPtr, (uint32_t)&hspi->Instanc
2298:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
2299:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2300:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Update SPI error code */
2301:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_DMA);
2302:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
2303:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
2305:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
2306:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2307:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2308:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if the SPI is already enabled */
2309:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Instance->CR1 & SPI_CR1_SPE) != SPI_CR1_SPE)
2310:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/ccqUhOmw.s 			page 42


2311:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Enable SPI peripheral */
2312:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_ENABLE(hspi);
2313:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2314:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable the SPI Error Interrupt Bit */
2315:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_ENABLE_IT(hspi, (SPI_IT_ERR));
2316:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2317:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable Tx DMA Request */
2318:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SET_BIT(hspi->Instance->CR2, SPI_CR2_TXDMAEN);
2319:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2320:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** error :
2321:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Unlocked */
2322:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
2323:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
2324:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2325:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2326:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2327:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Abort ongoing transfer (blocking mode).
2328:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi SPI handle.
2329:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @note   This procedure could be used for aborting any ongoing transfer (Tx and Rx),
2330:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         started in Interrupt or DMA mode.
2331:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         This procedure performs following operations :
2332:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           - Disable SPI Interrupts (depending of transfer direction)
2333:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           - Disable the DMA transfer in the peripheral register (if enabled)
2334:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           - Abort DMA transfer by calling HAL_DMA_Abort (in case of transfer in DMA mode)
2335:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           - Set handle State to READY
2336:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @note   This procedure is executed in blocking mode : when exiting function, Abort is considere
2337:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
2338:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2339:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Abort(SPI_HandleTypeDef *hspi)
2340:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2341:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode;
2342:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t count;
2343:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t resetcount;
2344:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2345:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Initialized local variable  */
2346:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   errorcode = HAL_OK;
2347:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   resetcount = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24U / 1000U);
2348:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = resetcount;
2349:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2350:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Clear ERRIE interrupt to avoid error interrupts generation during Abort procedure */
2351:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_ERRIE);
2352:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2353:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable TXEIE, RXNEIE and ERRIE(mode fault event, overrun error, TI frame error) interrupts */
2354:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_TXEIE))
2355:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2356:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR = SPI_AbortTx_ISR;
2357:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
2358:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     do
2359:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (count == 0U)
2361:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2362:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
2363:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
2364:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2365:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       count--;
2366:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
2367:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
ARM GAS  /tmp/ccqUhOmw.s 			page 43


2368:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     count = resetcount;
2369:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2370:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2371:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_RXNEIE))
2372:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2373:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxISR = SPI_AbortRx_ISR;
2374:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
2375:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     do
2376:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2377:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (count == 0U)
2378:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2379:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
2380:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
2381:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2382:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       count--;
2383:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
2384:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
2385:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     count = resetcount;
2386:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2387:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2388:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable the SPI DMA Tx request if enabled */
2389:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_TXDMAEN))
2390:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2391:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Abort the SPI DMA Tx Stream/Channel : use blocking DMA Abort API (no callback) */
2392:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->hdmatx != NULL)
2393:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2394:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Set the SPI DMA Abort callback :
2395:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       will lead to call HAL_SPI_AbortCpltCallback() at end of DMA abort procedure */
2396:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->hdmatx->XferAbortCallback = NULL;
2397:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2398:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Abort DMA Tx Handle linked to SPI Peripheral */
2399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (HAL_DMA_Abort(hspi->hdmatx) != HAL_OK)
2400:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2401:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
2402:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2404:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Disable Tx DMA Request */
2405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       CLEAR_BIT(hspi->Instance->CR2, (SPI_CR2_TXDMAEN));
2406:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2407:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (SPI_EndRxTxTransaction(hspi, SPI_DEFAULT_TIMEOUT, HAL_GetTick()) != HAL_OK)
2408:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2409:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
2410:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2412:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Disable SPI Peripheral */
2413:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_DISABLE(hspi);
2414:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2415:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Empty the FRLVL fifo */
2416:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FRLVL, SPI_FRLVL_EMPTY, SPI_DEFAULT_TIMEOUT,
2417:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2418:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
2419:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2420:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2421:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2422:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2423:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable the SPI DMA Rx request if enabled */
2424:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_RXDMAEN))
ARM GAS  /tmp/ccqUhOmw.s 			page 44


2425:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2426:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Abort the SPI DMA Rx Stream/Channel : use blocking DMA Abort API (no callback) */
2427:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->hdmarx != NULL)
2428:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2429:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Set the SPI DMA Abort callback :
2430:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       will lead to call HAL_SPI_AbortCpltCallback() at end of DMA abort procedure */
2431:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->hdmarx->XferAbortCallback = NULL;
2432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2433:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Abort DMA Rx Handle linked to SPI Peripheral */
2434:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (HAL_DMA_Abort(hspi->hdmarx) != HAL_OK)
2435:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2436:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
2437:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2438:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2439:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Disable peripheral */
2440:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_DISABLE(hspi);
2441:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2442:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Control the BSY flag */
2443:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_BSY, RESET, SPI_DEFAULT_TIMEOUT, HAL_GetTick
2444:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2445:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
2446:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2447:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2448:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Empty the FRLVL fifo */
2449:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FRLVL, SPI_FRLVL_EMPTY, SPI_DEFAULT_TIMEOUT,
2450:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2451:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
2452:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2453:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2454:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Disable Rx DMA Request */
2455:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       CLEAR_BIT(hspi->Instance->CR2, (SPI_CR2_RXDMAEN));
2456:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2457:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2458:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Reset Tx and Rx transfer counters */
2459:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
2460:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
2461:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2462:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check error during Abort procedure */
2463:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->ErrorCode == HAL_SPI_ERROR_ABORT)
2464:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2465:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* return HAL_Error in case of error during Abort procedure */
2466:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
2467:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2468:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
2469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2470:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset errorCode */
2471:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_NONE;
2472:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2473:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2474:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Clear the Error flags in the SR register */
2475:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_OVRFLAG(hspi);
2476:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
2477:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2478:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Restore hspi->state to ready */
2479:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
2480:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2481:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
ARM GAS  /tmp/ccqUhOmw.s 			page 45


2482:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2483:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2484:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2485:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Abort ongoing transfer (Interrupt mode).
2486:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi SPI handle.
2487:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @note   This procedure could be used for aborting any ongoing transfer (Tx and Rx),
2488:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         started in Interrupt or DMA mode.
2489:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         This procedure performs following operations :
2490:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           - Disable SPI Interrupts (depending of transfer direction)
2491:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           - Disable the DMA transfer in the peripheral register (if enabled)
2492:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           - Abort DMA transfer by calling HAL_DMA_Abort_IT (in case of transfer in DMA mode)
2493:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           - Set handle State to READY
2494:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *           - At abort completion, call user abort complete callback
2495:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @note   This procedure is executed in Interrupt mode, meaning that abort procedure could be
2496:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         considered as completed only when user abort complete callback is executed (not when ex
2497:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
2498:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2499:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_Abort_IT(SPI_HandleTypeDef *hspi)
2500:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2501:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode;
2502:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t abortcplt ;
2503:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t count;
2504:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t resetcount;
2505:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2506:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Initialized local variable  */
2507:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   errorcode = HAL_OK;
2508:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   abortcplt = 1U;
2509:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   resetcount = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24U / 1000U);
2510:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = resetcount;
2511:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2512:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Clear ERRIE interrupt to avoid error interrupts generation during Abort procedure */
2513:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_ERRIE);
2514:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2515:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Change Rx and Tx Irq Handler to Disable TXEIE, RXNEIE and ERRIE interrupts */
2516:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_TXEIE))
2517:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2518:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR = SPI_AbortTx_ISR;
2519:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
2520:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     do
2521:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2522:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (count == 0U)
2523:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2524:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
2525:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
2526:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2527:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       count--;
2528:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
2529:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
2530:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     count = resetcount;
2531:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2532:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2533:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_RXNEIE))
2534:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2535:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxISR = SPI_AbortRx_ISR;
2536:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
2537:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     do
2538:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
ARM GAS  /tmp/ccqUhOmw.s 			page 46


2539:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (count == 0U)
2540:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2541:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
2542:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
2543:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2544:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       count--;
2545:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
2546:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
2547:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     count = resetcount;
2548:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2549:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2550:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* If DMA Tx and/or DMA Rx Handles are associated to SPI Handle, DMA Abort complete callbacks sho
2551:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****      before any call to DMA Abort functions */
2552:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* DMA Tx Handle is valid */
2553:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->hdmatx != NULL)
2554:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2555:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set DMA Abort Complete callback if UART DMA Tx request if enabled.
2556:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        Otherwise, set it to NULL */
2557:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_TXDMAEN))
2558:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2559:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->hdmatx->XferAbortCallback = SPI_DMATxAbortCallback;
2560:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2561:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     else
2562:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2563:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->hdmatx->XferAbortCallback = NULL;
2564:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2565:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2566:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* DMA Rx Handle is valid */
2567:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->hdmarx != NULL)
2568:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2569:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Set DMA Abort Complete callback if UART DMA Rx request if enabled.
2570:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        Otherwise, set it to NULL */
2571:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_RXDMAEN))
2572:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2573:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->hdmarx->XferAbortCallback = SPI_DMARxAbortCallback;
2574:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2575:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     else
2576:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2577:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->hdmarx->XferAbortCallback = NULL;
2578:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2579:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2580:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2581:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable the SPI DMA Tx request if enabled */
2582:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_TXDMAEN))
2583:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2584:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Abort the SPI DMA Tx Stream/Channel */
2585:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->hdmatx != NULL)
2586:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2587:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Abort DMA Tx Handle linked to SPI Peripheral */
2588:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (HAL_DMA_Abort_IT(hspi->hdmatx) != HAL_OK)
2589:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2590:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->hdmatx->XferAbortCallback = NULL;
2591:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
2592:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2593:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
2594:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2595:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         abortcplt = 0U;
ARM GAS  /tmp/ccqUhOmw.s 			page 47


2596:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2597:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2598:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2599:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable the SPI DMA Rx request if enabled */
2600:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_RXDMAEN))
2601:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2602:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Abort the SPI DMA Rx Stream/Channel */
2603:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->hdmarx != NULL)
2604:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2605:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Abort DMA Rx Handle linked to SPI Peripheral */
2606:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (HAL_DMA_Abort_IT(hspi->hdmarx) !=  HAL_OK)
2607:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2608:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->hdmarx->XferAbortCallback = NULL;
2609:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
2610:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2611:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
2612:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2613:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         abortcplt = 0U;
2614:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2615:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2616:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2617:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2618:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (abortcplt == 1U)
2619:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2620:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Tx and Rx transfer counters */
2621:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount = 0U;
2622:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount = 0U;
2623:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2624:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Check error during Abort procedure */
2625:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->ErrorCode == HAL_SPI_ERROR_ABORT)
2626:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2627:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* return HAL_Error in case of error during Abort procedure */
2628:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       errorcode = HAL_ERROR;
2629:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2630:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     else
2631:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2632:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Reset errorCode */
2633:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->ErrorCode = HAL_SPI_ERROR_NONE;
2634:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2635:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2636:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Clear the Error flags in the SR register */
2637:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_OVRFLAG(hspi);
2638:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_FREFLAG(hspi);
2639:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2640:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Restore hspi->State to Ready */
2641:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
2642:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2643:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* As no DMA to be aborted, call directly user Abort complete callback */
2644:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
2645:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->AbortCpltCallback(hspi);
2646:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
2647:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     HAL_SPI_AbortCpltCallback(hspi);
2648:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
2649:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2650:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2651:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
2652:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
ARM GAS  /tmp/ccqUhOmw.s 			page 48


2653:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2654:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2655:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Pause the DMA Transfer.
2656:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2657:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for the specified SPI module.
2658:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
2659:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2660:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_DMAPause(SPI_HandleTypeDef *hspi)
2661:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2662:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Locked */
2663:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
2664:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2665:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable the SPI DMA Tx & Rx requests */
2666:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_TXDMAEN | SPI_CR2_RXDMAEN);
2667:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2668:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Unlocked */
2669:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
2670:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2671:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return HAL_OK;
2672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2673:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2674:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2675:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Resume the DMA Transfer.
2676:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2677:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for the specified SPI module.
2678:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
2679:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2680:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_DMAResume(SPI_HandleTypeDef *hspi)
2681:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2682:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Locked */
2683:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_LOCK(hspi);
2684:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2685:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable the SPI DMA Tx & Rx requests */
2686:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SET_BIT(hspi->Instance->CR2, SPI_CR2_TXDMAEN | SPI_CR2_RXDMAEN);
2687:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2688:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Unlocked */
2689:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
2690:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2691:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return HAL_OK;
2692:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2693:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2694:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2695:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Stop the DMA Transfer.
2696:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2697:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for the specified SPI module.
2698:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
2699:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2700:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_StatusTypeDef HAL_SPI_DMAStop(SPI_HandleTypeDef *hspi)
2701:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2702:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
2703:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* The Lock is not implemented on this API to allow the user application
2704:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****      to call the HAL SPI API under callbacks HAL_SPI_TxCpltCallback() or HAL_SPI_RxCpltCallback() o
2705:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****      when calling HAL_DMA_Abort() API the DMA TX/RX Transfer complete interrupt is generated
2706:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****      and the correspond call back is executed HAL_SPI_TxCpltCallback() or HAL_SPI_RxCpltCallback() 
2707:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****      */
2708:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2709:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Abort the SPI DMA tx Stream/Channel  */
ARM GAS  /tmp/ccqUhOmw.s 			page 49


2710:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->hdmatx != NULL)
2711:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2712:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (HAL_OK != HAL_DMA_Abort(hspi->hdmatx))
2713:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2714:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_DMA);
2715:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       errorcode = HAL_ERROR;
2716:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2717:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2718:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Abort the SPI DMA rx Stream/Channel  */
2719:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->hdmarx != NULL)
2720:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2721:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (HAL_OK != HAL_DMA_Abort(hspi->hdmarx))
2722:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2723:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_DMA);
2724:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       errorcode = HAL_ERROR;
2725:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2726:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2727:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2728:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable the SPI DMA Tx & Rx requests */
2729:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_TXDMAEN | SPI_CR2_RXDMAEN);
2730:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
2731:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
2732:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2733:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2734:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2735:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle SPI interrupt request.
2736:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2737:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for the specified SPI module.
2738:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
2739:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2740:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** void HAL_SPI_IRQHandler(SPI_HandleTypeDef *hspi)
2741:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2742:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t itsource = hspi->Instance->CR2;
2743:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t itflag   = hspi->Instance->SR;
2744:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2745:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* SPI in mode Receiver ----------------------------------------------------*/
2746:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((SPI_CHECK_FLAG(itflag, SPI_FLAG_OVR) == RESET) &&
2747:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (SPI_CHECK_FLAG(itflag, SPI_FLAG_RXNE) != RESET) && (SPI_CHECK_IT_SOURCE(itsource, SPI_IT_RXN
2748:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2749:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxISR(hspi);
2750:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return;
2751:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2752:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2753:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* SPI in mode Transmitter -------------------------------------------------*/
2754:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((SPI_CHECK_FLAG(itflag, SPI_FLAG_TXE) != RESET) && (SPI_CHECK_IT_SOURCE(itsource, SPI_IT_TXE)
2755:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2756:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR(hspi);
2757:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return;
2758:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2759:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2760:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* SPI in Error Treatment --------------------------------------------------*/
2761:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (((SPI_CHECK_FLAG(itflag, SPI_FLAG_MODF) != RESET) || (SPI_CHECK_FLAG(itflag, SPI_FLAG_OVR) !=
2762:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        || (SPI_CHECK_FLAG(itflag, SPI_FLAG_FRE) != RESET)) && (SPI_CHECK_IT_SOURCE(itsource, SPI_IT
2763:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
2764:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* SPI Overrun error interrupt occurred ----------------------------------*/
2765:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_CHECK_FLAG(itflag, SPI_FLAG_OVR) != RESET)
2766:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
ARM GAS  /tmp/ccqUhOmw.s 			page 50


2767:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (hspi->State != HAL_SPI_STATE_BUSY_TX)
2768:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2769:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_OVR);
2770:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         __HAL_SPI_CLEAR_OVRFLAG(hspi);
2771:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2772:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
2773:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         __HAL_SPI_CLEAR_OVRFLAG(hspi);
2775:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         return;
2776:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2777:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2778:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2779:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* SPI Mode Fault error interrupt occurred -------------------------------*/
2780:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_CHECK_FLAG(itflag, SPI_FLAG_MODF) != RESET)
2781:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2782:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_MODF);
2783:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_CLEAR_MODFFLAG(hspi);
2784:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2785:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2786:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* SPI Frame error interrupt occurred ------------------------------------*/
2787:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_CHECK_FLAG(itflag, SPI_FLAG_FRE) != RESET)
2788:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2789:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FRE);
2790:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_CLEAR_FREFLAG(hspi);
2791:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2792:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2793:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
2794:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
2795:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Disable all interrupts */
2796:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_DISABLE_IT(hspi, SPI_IT_RXNE | SPI_IT_TXE | SPI_IT_ERR);
2797:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2798:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->State = HAL_SPI_STATE_READY;
2799:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Disable the SPI DMA requests if enabled */
2800:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((HAL_IS_BIT_SET(itsource, SPI_CR2_TXDMAEN)) || (HAL_IS_BIT_SET(itsource, SPI_CR2_RXDMAEN)
2801:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2802:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         CLEAR_BIT(hspi->Instance->CR2, (SPI_CR2_TXDMAEN | SPI_CR2_RXDMAEN));
2803:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2804:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Abort the SPI DMA Rx channel */
2805:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (hspi->hdmarx != NULL)
2806:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
2807:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Set the SPI DMA Abort callback :
2808:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           will lead to call HAL_SPI_ErrorCallback() at end of DMA abort procedure */
2809:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->hdmarx->XferAbortCallback = SPI_DMAAbortOnError;
2810:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if (HAL_OK != HAL_DMA_Abort_IT(hspi->hdmarx))
2811:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
2812:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
2813:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           }
2814:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
2815:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Abort the SPI DMA Tx channel */
2816:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (hspi->hdmatx != NULL)
2817:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
2818:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Set the SPI DMA Abort callback :
2819:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           will lead to call HAL_SPI_ErrorCallback() at end of DMA abort procedure */
2820:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->hdmatx->XferAbortCallback = SPI_DMAAbortOnError;
2821:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if (HAL_OK != HAL_DMA_Abort_IT(hspi->hdmatx))
2822:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
2823:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
ARM GAS  /tmp/ccqUhOmw.s 			page 51


2824:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           }
2825:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
2826:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2827:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
2828:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
2829:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Call user error callback */
2830:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
2831:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCallback(hspi);
2832:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
2833:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         HAL_SPI_ErrorCallback(hspi);
2834:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
2835:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
2836:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
2837:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return;
2838:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
2839:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2840:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2841:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2842:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Tx Transfer completed callback.
2843:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2844:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
2845:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
2846:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2847:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** __weak void HAL_SPI_TxCpltCallback(SPI_HandleTypeDef *hspi)
2848:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2849:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
2850:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(hspi);
2851:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2852:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
2853:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             the HAL_SPI_TxCpltCallback should be implemented in the user file
2854:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****    */
2855:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2856:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2857:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2858:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Rx Transfer completed callback.
2859:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2860:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
2861:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
2862:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2863:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** __weak void HAL_SPI_RxCpltCallback(SPI_HandleTypeDef *hspi)
2864:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2865:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
2866:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(hspi);
2867:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2868:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
2869:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             the HAL_SPI_RxCpltCallback should be implemented in the user file
2870:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****    */
2871:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2872:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2873:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2874:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Tx and Rx Transfer completed callback.
2875:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2876:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
2877:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
2878:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2879:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** __weak void HAL_SPI_TxRxCpltCallback(SPI_HandleTypeDef *hspi)
2880:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
ARM GAS  /tmp/ccqUhOmw.s 			page 52


2881:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
2882:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(hspi);
2883:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2884:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
2885:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             the HAL_SPI_TxRxCpltCallback should be implemented in the user file
2886:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****    */
2887:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2888:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2889:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2890:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Tx Half Transfer completed callback.
2891:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2892:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
2893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
2894:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2895:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** __weak void HAL_SPI_TxHalfCpltCallback(SPI_HandleTypeDef *hspi)
2896:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2897:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
2898:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(hspi);
2899:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2900:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
2901:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             the HAL_SPI_TxHalfCpltCallback should be implemented in the user file
2902:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****    */
2903:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2904:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2905:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2906:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Rx Half Transfer completed callback.
2907:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2908:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
2909:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
2910:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2911:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** __weak void HAL_SPI_RxHalfCpltCallback(SPI_HandleTypeDef *hspi)
2912:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2913:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
2914:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(hspi);
2915:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2916:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
2917:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             the HAL_SPI_RxHalfCpltCallback() should be implemented in the user file
2918:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****    */
2919:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2920:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2921:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2922:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Tx and Rx Half Transfer callback.
2923:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2924:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
2925:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
2926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** __weak void HAL_SPI_TxRxHalfCpltCallback(SPI_HandleTypeDef *hspi)
2928:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2929:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
2930:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(hspi);
2931:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2932:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
2933:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             the HAL_SPI_TxRxHalfCpltCallback() should be implemented in the user file
2934:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****    */
2935:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2936:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2937:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
ARM GAS  /tmp/ccqUhOmw.s 			page 53


2938:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  SPI error callback.
2939:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2940:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
2941:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
2942:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2943:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** __weak void HAL_SPI_ErrorCallback(SPI_HandleTypeDef *hspi)
2944:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2945:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
2946:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(hspi);
2947:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2948:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
2949:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             the HAL_SPI_ErrorCallback should be implemented in the user file
2950:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****    */
2951:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* NOTE : The ErrorCode parameter in the hspi handle is updated by the SPI processes
2952:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             and user can use HAL_SPI_GetError() API to check the latest error occurred
2953:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****    */
2954:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2955:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2956:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2957:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  SPI Abort Complete callback.
2958:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi SPI handle.
2959:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
2960:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2961:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** __weak void HAL_SPI_AbortCpltCallback(SPI_HandleTypeDef *hspi)
2962:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2963:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
2964:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(hspi);
2965:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2966:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* NOTE : This function should not be modified, when the callback is needed,
2967:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             the HAL_SPI_AbortCpltCallback can be implemented in the user file.
2968:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****    */
2969:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
2970:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2971:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2972:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @}
2973:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2974:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2975:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /** @defgroup SPI_Exported_Functions_Group3 Peripheral State and Errors functions
2976:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief   SPI control functions
2977:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *
2978:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** @verbatim
2979:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****  ===============================================================================
2980:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                       ##### Peripheral State and Errors functions #####
2981:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****  ===============================================================================
2982:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     [..]
2983:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     This subsection provides a set of functions allowing to control the SPI.
2984:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****      (+) HAL_SPI_GetState() API can be helpful to check in run-time the state of the SPI peripheral
2985:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****      (+) HAL_SPI_GetError() check in run-time Errors occurring during communication
2986:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** @endverbatim
2987:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @{
2988:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2989:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
2990:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
2991:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Return the SPI handle state.
2992:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
2993:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
2994:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval SPI state
ARM GAS  /tmp/ccqUhOmw.s 			page 54


2995:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
2996:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** HAL_SPI_StateTypeDef HAL_SPI_GetState(SPI_HandleTypeDef *hspi)
2997:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
2998:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Return SPI handle state */
2999:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return hspi->State;
3000:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3001:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3002:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3003:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Return the SPI error code.
3004:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3005:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3006:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval SPI error code in bitmap format
3007:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3008:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** uint32_t HAL_SPI_GetError(SPI_HandleTypeDef *hspi)
3009:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3010:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Return SPI ErrorCode */
3011:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return hspi->ErrorCode;
3012:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3013:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3014:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3015:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @}
3016:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3017:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3018:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3019:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @}
3020:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3021:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3022:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /** @addtogroup SPI_Private_Functions
3023:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief   Private functions
3024:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @{
3025:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3026:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3027:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3028:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  DMA SPI transmit process complete callback.
3029:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hdma pointer to a DMA_HandleTypeDef structure that contains
3030:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for the specified DMA module.
3031:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3032:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3033:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMATransmitCplt(DMA_HandleTypeDef *hdma)
3034:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3035:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
3036:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
3037:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3038:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init tickstart for timeout management*/
3039:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tickstart = HAL_GetTick();
3040:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3041:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* DMA Normal Mode */
3042:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hdma->Instance->CCR & DMA_CCR_CIRC) != DMA_CCR_CIRC)
3043:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3044:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable ERR interrupt */
3045:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, SPI_IT_ERR);
3046:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3047:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable Tx DMA Request */
3048:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_TXDMAEN);
3049:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3050:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Check the end of the transaction */
3051:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_EndRxTxTransaction(hspi, SPI_DEFAULT_TIMEOUT, tickstart) != HAL_OK)
ARM GAS  /tmp/ccqUhOmw.s 			page 55


3052:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3053:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
3054:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3055:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3056:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Clear overrun flag in 2 Lines communication mode because received data is not read */
3057:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.Direction == SPI_DIRECTION_2LINES)
3058:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3059:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_CLEAR_OVRFLAG(hspi);
3060:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3061:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3062:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount = 0U;
3063:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
3064:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3065:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
3066:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3067:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Call user error callback */
3068:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3069:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->ErrorCallback(hspi);
3070:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3071:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       HAL_SPI_ErrorCallback(hspi);
3072:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3073:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return;
3074:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3075:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3076:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user Tx complete callback */
3077:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3078:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxCpltCallback(hspi);
3079:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3080:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_TxCpltCallback(hspi);
3081:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3082:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3083:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3084:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3085:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  DMA SPI receive process complete callback.
3086:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hdma pointer to a DMA_HandleTypeDef structure that contains
3087:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for the specified DMA module.
3088:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3089:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3090:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAReceiveCplt(DMA_HandleTypeDef *hdma)
3091:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3092:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
3093:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
3094:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3095:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t tmpreg = 0U;
3096:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  * ptmpreg8;
3097:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  tmpreg8 = 0;
3098:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3099:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3100:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init tickstart for timeout management*/
3101:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tickstart = HAL_GetTick();
3102:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3103:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* DMA Normal Mode */
3104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hdma->Instance->CCR & DMA_CCR_CIRC) != DMA_CCR_CIRC)
3105:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3106:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable ERR interrupt */
3107:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, SPI_IT_ERR);
3108:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/ccqUhOmw.s 			page 56


3109:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3110:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* CRC handling */
3111:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
3112:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3113:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Wait until RXNE flag */
3114:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_RXNE, SET, SPI_DEFAULT_TIMEOUT, tickstart) !
3115:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
3116:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Error on the CRC reception */
3117:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
3118:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
3119:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Read CRC */
3120:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
3121:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
3122:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Read 16bit CRC */
3123:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         tmpreg = READ_REG(hspi->Instance->DR);
3124:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* To avoid GCC warning */
3125:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         UNUSED(tmpreg);
3126:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
3127:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
3128:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
3129:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Initialize the 8bit temporary pointer */
3130:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ptmpreg8 = (__IO uint8_t *)&hspi->Instance->DR;
3131:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Read 8bit CRC */
3132:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         tmpreg8 = *ptmpreg8;
3133:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* To avoid GCC warning */
3134:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         UNUSED(tmpreg8);
3135:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3136:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (hspi->Init.CRCLength == SPI_CRC_LENGTH_16BIT)
3137:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
3138:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_RXNE, SET, SPI_DEFAULT_TIMEOUT, tickstar
3139:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
3140:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             /* Error on the CRC reception */
3141:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****             SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
3142:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           }
3143:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Read 8bit CRC again in case of 16bit CRC in 8bit Data mode */
3144:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           tmpreg8 = *ptmpreg8;
3145:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* To avoid GCC warning */
3146:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           UNUSED(tmpreg8);
3147:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
3148:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
3149:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3150:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3151:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3152:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Check if we are in Master RX 2 line mode */
3153:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if ((hspi->Init.Direction == SPI_DIRECTION_2LINES) && (hspi->Init.Mode == SPI_MODE_MASTER))
3154:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3155:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Disable Rx/Tx DMA Request (done by default to handle the case master rx direction 2 lines)
3156:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_TXDMAEN | SPI_CR2_RXDMAEN);
3157:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3158:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     else
3159:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3160:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Normal case */
3161:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_RXDMAEN);
3162:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3163:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3164:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Check the end of the transaction */
3165:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_EndRxTransaction(hspi, SPI_DEFAULT_TIMEOUT, tickstart) != HAL_OK)
ARM GAS  /tmp/ccqUhOmw.s 			page 57


3166:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3167:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->ErrorCode = HAL_SPI_ERROR_FLAG;
3168:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3169:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3170:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount = 0U;
3171:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
3172:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3173:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3174:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Check if CRC error occurred */
3175:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_CRCERR))
3176:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3177:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
3178:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_CLEAR_CRCERRFLAG(hspi);
3179:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3180:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3181:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3182:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
3183:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3184:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Call user error callback */
3185:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3186:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->ErrorCallback(hspi);
3187:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3188:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       HAL_SPI_ErrorCallback(hspi);
3189:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3190:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return;
3191:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3192:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3193:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user Rx complete callback */
3194:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3195:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxCpltCallback(hspi);
3196:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3197:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_RxCpltCallback(hspi);
3198:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3199:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3200:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3201:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3202:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  DMA SPI transmit receive process complete callback.
3203:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hdma pointer to a DMA_HandleTypeDef structure that contains
3204:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for the specified DMA module.
3205:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3206:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3207:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMATransmitReceiveCplt(DMA_HandleTypeDef *hdma)
3208:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3209:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
3210:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
3211:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3212:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t tmpreg = 0U;
3213:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  * ptmpreg8;
3214:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  tmpreg8 = 0;
3215:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3216:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3217:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init tickstart for timeout management*/
3218:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tickstart = HAL_GetTick();
3219:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3220:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* DMA Normal Mode */
3221:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hdma->Instance->CCR & DMA_CCR_CIRC) != DMA_CCR_CIRC)
3222:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/ccqUhOmw.s 			page 58


3223:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable ERR interrupt */
3224:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, SPI_IT_ERR);
3225:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3226:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3227:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* CRC handling */
3228:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
3229:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3230:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if ((hspi->Init.DataSize == SPI_DATASIZE_8BIT) && (hspi->Init.CRCLength == SPI_CRC_LENGTH_8BI
3231:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
3232:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FRLVL, SPI_FRLVL_QUARTER_FULL, SPI_DEFAULT
3233:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                           tickstart) != HAL_OK)
3234:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
3235:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Error on the CRC reception */
3236:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
3237:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
3238:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Initialize the 8bit temporary pointer */
3239:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ptmpreg8 = (__IO uint8_t *)&hspi->Instance->DR;
3240:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Read 8bit CRC */
3241:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         tmpreg8 = *ptmpreg8;
3242:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* To avoid GCC warning */
3243:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         UNUSED(tmpreg8);
3244:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
3245:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
3246:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
3247:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FRLVL, SPI_FRLVL_HALF_FULL, SPI_DEFAULT_TI
3248:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
3249:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Error on the CRC reception */
3250:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
3251:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
3252:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Read CRC to Flush DR and RXNE flag */
3253:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         tmpreg = READ_REG(hspi->Instance->DR);
3254:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* To avoid GCC warning */
3255:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         UNUSED(tmpreg);
3256:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
3257:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3258:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3259:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3260:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Check the end of the transaction */
3261:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_EndRxTxTransaction(hspi, SPI_DEFAULT_TIMEOUT, tickstart) != HAL_OK)
3262:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3263:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
3264:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3265:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3266:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable Rx/Tx DMA Request */
3267:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_TXDMAEN | SPI_CR2_RXDMAEN);
3268:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3269:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount = 0U;
3270:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount = 0U;
3271:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
3272:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3273:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3274:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Check if CRC error occurred */
3275:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_CRCERR))
3276:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3277:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
3278:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_CLEAR_CRCERRFLAG(hspi);
3279:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
ARM GAS  /tmp/ccqUhOmw.s 			page 59


3280:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3281:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3282:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
3283:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3284:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Call user error callback */
3285:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3286:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->ErrorCallback(hspi);
3287:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3288:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       HAL_SPI_ErrorCallback(hspi);
3289:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3290:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return;
3291:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3292:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3293:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user TxRx complete callback */
3294:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3295:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxRxCpltCallback(hspi);
3296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3297:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_TxRxCpltCallback(hspi);
3298:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3299:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3300:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3301:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3302:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  DMA SPI half transmit process complete callback.
3303:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hdma pointer to a DMA_HandleTypeDef structure that contains
3304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for the specified DMA module.
3305:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3306:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3307:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAHalfTransmitCplt(DMA_HandleTypeDef *hdma)
3308:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3309:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
3310:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3311:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user Tx half complete callback */
3312:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3313:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxHalfCpltCallback(hspi);
3314:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3315:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_TxHalfCpltCallback(hspi);
3316:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3317:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3318:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3319:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3320:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  DMA SPI half receive process complete callback
3321:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hdma pointer to a DMA_HandleTypeDef structure that contains
3322:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for the specified DMA module.
3323:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3324:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3325:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAHalfReceiveCplt(DMA_HandleTypeDef *hdma)
3326:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3327:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
3328:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3329:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user Rx half complete callback */
3330:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3331:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxHalfCpltCallback(hspi);
3332:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3333:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_RxHalfCpltCallback(hspi);
3334:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3335:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3336:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/ccqUhOmw.s 			page 60


3337:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3338:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  DMA SPI half transmit receive process complete callback.
3339:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hdma pointer to a DMA_HandleTypeDef structure that contains
3340:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for the specified DMA module.
3341:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3342:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3343:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAHalfTransmitReceiveCplt(DMA_HandleTypeDef *hdma)
3344:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3345:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
3346:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3347:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user TxRx half complete callback */
3348:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3349:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxRxHalfCpltCallback(hspi);
3350:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3351:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_TxRxHalfCpltCallback(hspi);
3352:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3353:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3354:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3355:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3356:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  DMA SPI communication error callback.
3357:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hdma pointer to a DMA_HandleTypeDef structure that contains
3358:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for the specified DMA module.
3359:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3361:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAError(DMA_HandleTypeDef *hdma)
3362:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3363:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
3364:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3365:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Stop the disable DMA transfer on SPI side */
3366:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_TXDMAEN | SPI_CR2_RXDMAEN);
3367:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3368:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_DMA);
3369:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
3370:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user error callback */
3371:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3372:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCallback(hspi);
3373:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3374:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_ErrorCallback(hspi);
3375:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3376:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3377:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3378:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3379:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  DMA SPI communication abort callback, when initiated by HAL services on Error
3380:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         (To be called at end of DMA Abort procedure following error occurrence).
3381:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hdma DMA handle.
3382:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3383:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3384:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMAAbortOnError(DMA_HandleTypeDef *hdma)
3385:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3386:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
3387:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
3388:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
3389:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3390:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user error callback */
3391:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3392:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCallback(hspi);
3393:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
ARM GAS  /tmp/ccqUhOmw.s 			page 61


3394:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_ErrorCallback(hspi);
3395:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3396:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3397:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3398:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  DMA SPI Tx communication abort callback, when initiated by user
3400:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         (To be called at end of DMA Tx Abort procedure following user abort request).
3401:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @note   When this callback is executed, User Abort complete call back is called only if no
3402:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         Abort still ongoing for Rx DMA Handle.
3403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hdma DMA handle.
3404:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3406:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMATxAbortCallback(DMA_HandleTypeDef *hdma)
3407:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3408:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
3409:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3410:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferAbortCallback = NULL;
3411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3412:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable Tx DMA Request */
3413:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_TXDMAEN);
3414:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3415:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_EndRxTxTransaction(hspi, SPI_DEFAULT_TIMEOUT, HAL_GetTick()) != HAL_OK)
3416:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3417:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
3418:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3419:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3420:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable SPI Peripheral */
3421:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_DISABLE(hspi);
3422:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3423:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Empty the FRLVL fifo */
3424:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FRLVL, SPI_FRLVL_EMPTY, SPI_DEFAULT_TIMEOUT, HAL
3425:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3426:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
3427:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3428:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3429:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if an Abort process is still ongoing */
3430:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->hdmarx != NULL)
3431:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->hdmarx->XferAbortCallback != NULL)
3433:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3434:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return;
3435:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3436:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3437:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3438:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* No Abort process still ongoing : All DMA Stream/Channel are aborted, call user Abort Complete 
3439:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
3440:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
3441:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3442:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check no error during Abort procedure */
3443:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->ErrorCode != HAL_SPI_ERROR_ABORT)
3444:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3445:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset errorCode */
3446:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_NONE;
3447:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3448:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3449:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Clear the Error flags in the SR register */
3450:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_OVRFLAG(hspi);
ARM GAS  /tmp/ccqUhOmw.s 			page 62


3451:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
3452:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3453:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Restore hspi->State to Ready */
3454:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State  = HAL_SPI_STATE_READY;
3455:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3456:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user Abort complete callback */
3457:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3458:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->AbortCpltCallback(hspi);
3459:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3460:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_AbortCpltCallback(hspi);
3461:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3462:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3463:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3464:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3465:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  DMA SPI Rx communication abort callback, when initiated by user
3466:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         (To be called at end of DMA Rx Abort procedure following user abort request).
3467:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @note   When this callback is executed, User Abort complete call back is called only if no
3468:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *         Abort still ongoing for Tx DMA Handle.
3469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hdma DMA handle.
3470:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3471:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3472:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_DMARxAbortCallback(DMA_HandleTypeDef *hdma)
3473:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3474:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
3475:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3476:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable SPI Peripheral */
3477:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_DISABLE(hspi);
3478:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3479:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmarx->XferAbortCallback = NULL;
3480:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3481:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable Rx DMA Request */
3482:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, SPI_CR2_RXDMAEN);
3483:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3484:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Control the BSY flag */
3485:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_BSY, RESET, SPI_DEFAULT_TIMEOUT, HAL_GetTick()) 
3486:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3487:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
3488:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3489:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3490:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Empty the FRLVL fifo */
3491:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FRLVL, SPI_FRLVL_EMPTY, SPI_DEFAULT_TIMEOUT, HAL
3492:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3493:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
3494:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3495:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3496:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if an Abort process is still ongoing */
3497:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->hdmatx != NULL)
3498:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3499:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->hdmatx->XferAbortCallback != NULL)
3500:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3501:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return;
3502:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3503:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3504:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3505:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* No Abort process still ongoing : All DMA Stream/Channel are aborted, call user Abort Complete 
3506:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
3507:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
ARM GAS  /tmp/ccqUhOmw.s 			page 63


3508:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3509:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check no error during Abort procedure */
3510:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->ErrorCode != HAL_SPI_ERROR_ABORT)
3511:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3512:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset errorCode */
3513:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_NONE;
3514:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3515:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3516:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Clear the Error flags in the SR register */
3517:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_OVRFLAG(hspi);
3518:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
3519:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3520:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Restore hspi->State to Ready */
3521:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State  = HAL_SPI_STATE_READY;
3522:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3523:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user Abort complete callback */
3524:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
3525:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->AbortCpltCallback(hspi);
3526:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
3527:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_AbortCpltCallback(hspi);
3528:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
3529:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3530:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3531:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3532:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Rx 8-bit handler for Transmit and Receive in Interrupt mode.
3533:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3534:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3535:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3536:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3537:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesRxISR_8BIT(struct __SPI_HandleTypeDef *hspi)
3538:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3539:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Receive data in packing mode */
3540:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->RxXferCount > 1U)
3541:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3542:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     *((uint16_t *)hspi->pRxBuffPtr) = (uint16_t)(hspi->Instance->DR);
3543:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr += sizeof(uint16_t);
3544:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount -= 2U;
3545:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->RxXferCount == 1U)
3546:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3547:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Set RX Fifo threshold according the reception data length: 8bit */
3548:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
3549:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3550:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3551:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Receive data in 8 Bit mode */
3552:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
3553:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3554:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     *hspi->pRxBuffPtr = *((__IO uint8_t *)&hspi->Instance->DR);
3555:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr++;
3556:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount--;
3557:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3558:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3559:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check end of the reception */
3560:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->RxXferCount == 0U)
3561:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3562:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3563:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
3564:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
ARM GAS  /tmp/ccqUhOmw.s 			page 64


3565:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->Instance->CR2, SPI_RXFIFO_THRESHOLD);
3566:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->RxISR =  SPI_2linesRxISR_8BITCRC;
3567:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return;
3568:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3569:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3570:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3571:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable RXNE  and ERR interrupt */
3572:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, (SPI_IT_RXNE | SPI_IT_ERR));
3573:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3574:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->TxXferCount == 0U)
3575:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3576:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SPI_CloseRxTx_ISR(hspi);
3577:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3578:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3579:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3580:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3581:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3582:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3583:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Rx 8-bit handler for Transmit and Receive in Interrupt mode.
3584:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3585:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3586:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3587:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3588:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesRxISR_8BITCRC(struct __SPI_HandleTypeDef *hspi)
3589:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3590:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  * ptmpreg8;
3591:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  tmpreg8 = 0;
3592:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3593:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Initialize the 8bit temporary pointer */
3594:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   ptmpreg8 = (__IO uint8_t *)&hspi->Instance->DR;
3595:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Read 8bit CRC to flush Data Register */
3596:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmpreg8 = *ptmpreg8;
3597:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* To avoid GCC warning */
3598:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(tmpreg8);
3599:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3600:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->CRCSize--;
3601:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3602:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check end of the reception */
3603:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->CRCSize == 0U)
3604:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3605:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable RXNE and ERR interrupt */
3606:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, (SPI_IT_RXNE | SPI_IT_ERR));
3607:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3608:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->TxXferCount == 0U)
3609:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3610:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SPI_CloseRxTx_ISR(hspi);
3611:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3612:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3613:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3614:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3615:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3616:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3617:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Tx 8-bit handler for Transmit and Receive in Interrupt mode.
3618:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3619:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3620:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3621:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
ARM GAS  /tmp/ccqUhOmw.s 			page 65


3622:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesTxISR_8BIT(struct __SPI_HandleTypeDef *hspi)
3623:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3624:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in packing Bit mode */
3625:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->TxXferCount >= 2U)
3626:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3627:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->Instance->DR = *((uint16_t *)hspi->pTxBuffPtr);
3628:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr += sizeof(uint16_t);
3629:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount -= 2U;
3630:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3631:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in 8 Bit mode */
3632:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
3633:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3634:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     *(__IO uint8_t *)&hspi->Instance->DR = (*hspi->pTxBuffPtr);
3635:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr++;
3636:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount--;
3637:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3638:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3639:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the end of the transmission */
3640:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->TxXferCount == 0U)
3641:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3642:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3643:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
3644:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3645:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Set CRC Next Bit to send CRC */
3646:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCNEXT);
3647:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Disable TXE interrupt */
3648:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_DISABLE_IT(hspi, SPI_IT_TXE);
3649:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return;
3650:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3651:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3652:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3653:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable TXE interrupt */
3654:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, SPI_IT_TXE);
3655:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3656:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->RxXferCount == 0U)
3657:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3658:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SPI_CloseRxTx_ISR(hspi);
3659:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3660:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3661:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3662:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3663:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3664:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Rx 16-bit handler for Transmit and Receive in Interrupt mode.
3665:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3666:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3667:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3668:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3669:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesRxISR_16BIT(struct __SPI_HandleTypeDef *hspi)
3670:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3671:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Receive data in 16 Bit mode */
3672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *((uint16_t *)hspi->pRxBuffPtr) = (uint16_t)(hspi->Instance->DR);
3673:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
3674:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
3675:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3676:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->RxXferCount == 0U)
3677:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3678:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
ARM GAS  /tmp/ccqUhOmw.s 			page 66


3679:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
3680:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3681:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->RxISR =  SPI_2linesRxISR_16BITCRC;
3682:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return;
3683:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3684:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3685:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3686:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable RXNE interrupt */
3687:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, SPI_IT_RXNE);
3688:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3689:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->TxXferCount == 0U)
3690:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3691:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SPI_CloseRxTx_ISR(hspi);
3692:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3693:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3694:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3695:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3696:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3697:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3698:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Manage the CRC 16-bit receive for Transmit and Receive in Interrupt mode.
3699:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3700:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3701:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3702:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3703:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesRxISR_16BITCRC(struct __SPI_HandleTypeDef *hspi)
3704:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3705:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t tmpreg = 0U;
3706:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3707:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Read 16bit CRC to flush Data Register */
3708:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmpreg = READ_REG(hspi->Instance->DR);
3709:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* To avoid GCC warning */
3710:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(tmpreg);  
3711:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3712:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable RXNE interrupt */
3713:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_DISABLE_IT(hspi, SPI_IT_RXNE);
3714:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3715:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_CloseRxTx_ISR(hspi);
3716:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3717:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3718:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3719:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3720:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Tx 16-bit handler for Transmit and Receive in Interrupt mode.
3721:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3722:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3723:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3724:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3725:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_2linesTxISR_16BIT(struct __SPI_HandleTypeDef *hspi)
3726:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3727:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in 16 Bit mode */
3728:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->Instance->DR = *((uint16_t *)hspi->pTxBuffPtr);
3729:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
3730:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
3731:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3732:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable CRC Transmission */
3733:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->TxXferCount == 0U)
3734:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3735:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
ARM GAS  /tmp/ccqUhOmw.s 			page 67


3736:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
3737:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3738:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Set CRC Next Bit to send CRC */
3739:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCNEXT);
3740:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Disable TXE interrupt */
3741:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_DISABLE_IT(hspi, SPI_IT_TXE);
3742:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return;
3743:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3744:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3745:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3746:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable TXE interrupt */
3747:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE_IT(hspi, SPI_IT_TXE);
3748:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3749:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->RxXferCount == 0U)
3750:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3751:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SPI_CloseRxTx_ISR(hspi);
3752:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3753:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3754:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3755:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3756:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3757:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3758:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Manage the CRC 8-bit receive in Interrupt context.
3759:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3760:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3761:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3762:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3763:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_RxISR_8BITCRC(struct __SPI_HandleTypeDef *hspi)
3764:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3765:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  * ptmpreg8;
3766:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  tmpreg8 = 0;
3767:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3768:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Initialize the 8bit temporary pointer */
3769:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   ptmpreg8 = (__IO uint8_t *)&hspi->Instance->DR;
3770:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Read 8bit CRC to flush Data Register */
3771:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmpreg8 = *ptmpreg8;
3772:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* To avoid GCC warning */
3773:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(tmpreg8);
3774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3775:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->CRCSize--;
3776:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3777:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->CRCSize == 0U)
3778:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3779:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_CloseRx_ISR(hspi);
3780:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3781:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3782:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3783:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3784:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3785:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Manage the receive 8-bit in Interrupt context.
3786:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3787:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3788:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3789:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3790:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_RxISR_8BIT(struct __SPI_HandleTypeDef *hspi)
3791:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3792:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *hspi->pRxBuffPtr = (*(__IO uint8_t *)&hspi->Instance->DR);
ARM GAS  /tmp/ccqUhOmw.s 			page 68


3793:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr++;
3794:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
3795:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3796:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3797:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable CRC Transmission */
3798:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->RxXferCount == 1U) && (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE))
3799:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3800:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCNEXT);
3801:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3802:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3803:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3804:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->RxXferCount == 0U)
3805:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3806:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3807:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
3808:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3809:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->RxISR =  SPI_RxISR_8BITCRC;
3810:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return;
3811:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3812:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3813:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_CloseRx_ISR(hspi);
3814:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3815:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3816:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3817:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3818:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3819:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Manage the CRC 16-bit receive in Interrupt context.
3820:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3821:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3822:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3823:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3824:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_RxISR_16BITCRC(struct __SPI_HandleTypeDef *hspi)
3825:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3826:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t tmpreg = 0U;
3827:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3828:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Read 16bit CRC to flush Data Register */
3829:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmpreg = READ_REG(hspi->Instance->DR);
3830:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* To avoid GCC warning */
3831:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   UNUSED(tmpreg);
3832:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3833:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable RXNE and ERR interrupt */
3834:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_DISABLE_IT(hspi, (SPI_IT_RXNE | SPI_IT_ERR));
3835:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3836:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_CloseRx_ISR(hspi);
3837:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3838:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3839:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3840:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3841:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Manage the 16-bit receive in Interrupt context.
3842:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3843:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3844:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3845:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3846:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_RxISR_16BIT(struct __SPI_HandleTypeDef *hspi)
3847:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3848:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *((uint16_t *)hspi->pRxBuffPtr) = (uint16_t)(hspi->Instance->DR);
3849:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
ARM GAS  /tmp/ccqUhOmw.s 			page 69


3850:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
3851:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3852:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3853:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Enable CRC Transmission */
3854:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->RxXferCount == 1U) && (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE))
3855:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3856:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCNEXT);
3857:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3858:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3859:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3860:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->RxXferCount == 0U)
3861:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3862:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3863:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
3864:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3865:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->RxISR = SPI_RxISR_16BITCRC;
3866:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return;
3867:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3868:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3869:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_CloseRx_ISR(hspi);
3870:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3871:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3872:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3873:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3874:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle the data 8-bit transmit in Interrupt mode.
3875:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3876:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3877:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3878:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3879:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_TxISR_8BIT(struct __SPI_HandleTypeDef *hspi)
3880:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3881:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *(__IO uint8_t *)&hspi->Instance->DR = (*hspi->pTxBuffPtr);
3882:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr++;
3883:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
3884:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3885:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->TxXferCount == 0U)
3886:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3887:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3888:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
3889:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3890:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Enable CRC Transmission */
3891:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCNEXT);
3892:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3894:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_CloseTx_ISR(hspi);
3895:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3896:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3897:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3898:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3899:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle the data 16-bit transmit in Interrupt mode.
3900:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3901:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
3902:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
3903:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3904:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_TxISR_16BIT(struct __SPI_HandleTypeDef *hspi)
3905:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
3906:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in 16 Bit mode */
ARM GAS  /tmp/ccqUhOmw.s 			page 70


3907:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->Instance->DR = *((uint16_t *)hspi->pTxBuffPtr);
3908:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
3909:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
3910:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3911:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->TxXferCount == 0U)
3912:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3913:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
3914:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
3915:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
3916:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Enable CRC Transmission */
3917:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->Instance->CR1, SPI_CR1_CRCNEXT);
3918:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3919:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
3920:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_CloseTx_ISR(hspi);
3921:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3922:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
3923:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3924:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3925:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle SPI Communication Timeout.
3926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *              the configuration information for SPI module.
3928:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Flag SPI flag to check
3929:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  State flag state to check
3930:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Timeout Timeout duration
3931:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Tickstart tick start value
3932:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
3933:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
3934:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static HAL_StatusTypeDef SPI_WaitFlagStateUntilTimeout(SPI_HandleTypeDef *hspi, uint32_t Flag, Flag
3935:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                        uint32_t Timeout, uint32_t Tickstart)
3936:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
  29              		.loc 1 3936 1 view -0
  30              		.cfi_startproc
  31              		@ args = 4, pretend = 0, frame = 8
  32              		@ frame_needed = 0, uses_anonymous_args = 0
  33              		.loc 1 3936 1 is_stmt 0 view .LVU1
  34 0000 2DE9F047 		push	{r4, r5, r6, r7, r8, r9, r10, lr}
  35              		.cfi_def_cfa_offset 32
  36              		.cfi_offset 4, -32
  37              		.cfi_offset 5, -28
  38              		.cfi_offset 6, -24
  39              		.cfi_offset 7, -20
  40              		.cfi_offset 8, -16
  41              		.cfi_offset 9, -12
  42              		.cfi_offset 10, -8
  43              		.cfi_offset 14, -4
  44 0004 82B0     		sub	sp, sp, #8
  45              		.cfi_def_cfa_offset 40
  46 0006 0546     		mov	r5, r0
  47 0008 8846     		mov	r8, r1
  48 000a 1746     		mov	r7, r2
  49 000c 1E46     		mov	r6, r3
3937:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t count;
  50              		.loc 1 3937 3 is_stmt 1 view .LVU2
3938:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tmp_timeout;
  51              		.loc 1 3938 3 view .LVU3
3939:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tmp_tickstart;
  52              		.loc 1 3939 3 view .LVU4
ARM GAS  /tmp/ccqUhOmw.s 			page 71


3940:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3941:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Adjust Timeout value  in case of end of transfer */
3942:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_timeout   = Timeout - (HAL_GetTick() - Tickstart);
  53              		.loc 1 3942 3 view .LVU5
  54              		.loc 1 3942 30 is_stmt 0 view .LVU6
  55 000e FFF7FEFF 		bl	HAL_GetTick
  56              	.LVL1:
  57              		.loc 1 3942 44 view .LVU7
  58 0012 0A9B     		ldr	r3, [sp, #40]
  59 0014 1B1A     		subs	r3, r3, r0
  60              		.loc 1 3942 17 view .LVU8
  61 0016 03EB0609 		add	r9, r3, r6
  62              	.LVL2:
3943:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_tickstart = HAL_GetTick();
  63              		.loc 1 3943 3 is_stmt 1 view .LVU9
  64              		.loc 1 3943 19 is_stmt 0 view .LVU10
  65 001a FFF7FEFF 		bl	HAL_GetTick
  66              	.LVL3:
  67 001e 8246     		mov	r10, r0
  68              	.LVL4:
3944:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3945:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Calculate Timeout based on a software loop to avoid blocking issue if Systick is disabled */
3946:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = tmp_timeout * ((SystemCoreClock * 32U) >> 20U);
  69              		.loc 1 3946 3 is_stmt 1 view .LVU11
  70              		.loc 1 3946 43 is_stmt 0 view .LVU12
  71 0020 284B     		ldr	r3, .L16
  72 0022 1B68     		ldr	r3, [r3]
  73              		.loc 1 3946 50 view .LVU13
  74 0024 C3F3CB33 		ubfx	r3, r3, #15, #12
  75              		.loc 1 3946 23 view .LVU14
  76 0028 09FB03F3 		mul	r3, r9, r3
  77              		.loc 1 3946 9 view .LVU15
  78 002c 0193     		str	r3, [sp, #4]
3947:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3948:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   while ((__HAL_SPI_GET_FLAG(hspi, Flag) ? SET : RESET) != State)
  79              		.loc 1 3948 3 is_stmt 1 view .LVU16
  80              	.LVL5:
  81              	.L3:
  82              		.loc 1 3948 57 view .LVU17
  83              		.loc 1 3948 11 is_stmt 0 view .LVU18
  84 002e 2B68     		ldr	r3, [r5]
  85 0030 9C68     		ldr	r4, [r3, #8]
  86              		.loc 1 3948 48 view .LVU19
  87 0032 38EA0404 		bics	r4, r8, r4
  88 0036 0CBF     		ite	eq
  89 0038 0123     		moveq	r3, #1
  90 003a 0023     		movne	r3, #0
  91              		.loc 1 3948 57 view .LVU20
  92 003c BB42     		cmp	r3, r7
  93 003e 3DD0     		beq	.L12
3949:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
3950:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (Timeout != HAL_MAX_DELAY)
  94              		.loc 1 3950 5 is_stmt 1 view .LVU21
  95              		.loc 1 3950 8 is_stmt 0 view .LVU22
  96 0040 B6F1FF3F 		cmp	r6, #-1
  97 0044 F3D0     		beq	.L3
3951:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
ARM GAS  /tmp/ccqUhOmw.s 			page 72


3952:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (((HAL_GetTick() - tmp_tickstart) >= tmp_timeout) || (tmp_timeout == 0U))
  98              		.loc 1 3952 7 is_stmt 1 view .LVU23
  99              		.loc 1 3952 13 is_stmt 0 view .LVU24
 100 0046 FFF7FEFF 		bl	HAL_GetTick
 101              	.LVL6:
 102              		.loc 1 3952 27 view .LVU25
 103 004a A0EB0A00 		sub	r0, r0, r10
 104              		.loc 1 3952 10 view .LVU26
 105 004e 4845     		cmp	r0, r9
 106 0050 07D2     		bcs	.L13
3953:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
3954:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Disable the SPI and reset the CRC: the CRC value should be cleared
3955:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****            on both master and slave sides in order to resynchronize the master
3956:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****            and slave for their respective CRC calculation */
3957:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3958:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Disable TXE, RXNE and ERR interrupts for the interrupt process */
3959:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         __HAL_SPI_DISABLE_IT(hspi, (SPI_IT_TXE | SPI_IT_RXNE | SPI_IT_ERR));
3960:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3961:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if ((hspi->Init.Mode == SPI_MODE_MASTER) && ((hspi->Init.Direction == SPI_DIRECTION_1LINE)
3962:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
3963:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
3964:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Disable SPI peripheral */
3965:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           __HAL_SPI_DISABLE(hspi);
3966:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
3967:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3968:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Reset CRC Calculation */
3969:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
3970:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
3971:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           SPI_RESET_CRC(hspi);
3972:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
3973:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3974:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->State = HAL_SPI_STATE_READY;
3975:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3976:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Process Unlocked */
3977:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         __HAL_UNLOCK(hspi);
3978:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3979:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         return HAL_TIMEOUT;
3980:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
3981:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* If Systick is disabled or not incremented, deactivate timeout to go in disable loop proced
3982:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if(count == 0U)
 107              		.loc 1 3982 7 is_stmt 1 view .LVU27
 108              		.loc 1 3982 16 is_stmt 0 view .LVU28
 109 0052 019A     		ldr	r2, [sp, #4]
 110              		.loc 1 3982 9 view .LVU29
 111 0054 02B1     		cbz	r2, .L9
 112 0056 4A46     		mov	r2, r9
 113              	.L9:
 114              	.LVL7:
3983:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
3984:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         tmp_timeout = 0U;
3985:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
3986:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       count--;
 115              		.loc 1 3986 7 is_stmt 1 view .LVU30
 116              		.loc 1 3986 12 is_stmt 0 view .LVU31
 117 0058 019B     		ldr	r3, [sp, #4]
 118 005a 013B     		subs	r3, r3, #1
 119 005c 0193     		str	r3, [sp, #4]
ARM GAS  /tmp/ccqUhOmw.s 			page 73


 120 005e 9146     		mov	r9, r2
 121 0060 E5E7     		b	.L3
 122              	.LVL8:
 123              	.L13:
3959:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 124              		.loc 1 3959 9 is_stmt 1 view .LVU32
 125 0062 2A68     		ldr	r2, [r5]
 126 0064 5368     		ldr	r3, [r2, #4]
 127 0066 23F0E003 		bic	r3, r3, #224
 128 006a 5360     		str	r3, [r2, #4]
3961:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
 129              		.loc 1 3961 9 view .LVU33
3961:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
 130              		.loc 1 3961 24 is_stmt 0 view .LVU34
 131 006c 6B68     		ldr	r3, [r5, #4]
3961:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
 132              		.loc 1 3961 12 view .LVU35
 133 006e B3F5827F 		cmp	r3, #260
 134 0072 0BD0     		beq	.L14
 135              	.L5:
3969:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 136              		.loc 1 3969 9 is_stmt 1 view .LVU36
3969:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 137              		.loc 1 3969 23 is_stmt 0 view .LVU37
 138 0074 AB6A     		ldr	r3, [r5, #40]
3969:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 139              		.loc 1 3969 12 view .LVU38
 140 0076 B3F5005F 		cmp	r3, #8192
 141 007a 14D0     		beq	.L15
 142              	.L7:
3971:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 143              		.loc 1 3971 11 is_stmt 1 discriminator 1 view .LVU39
3974:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 144              		.loc 1 3974 9 discriminator 1 view .LVU40
3974:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 145              		.loc 1 3974 21 is_stmt 0 discriminator 1 view .LVU41
 146 007c 0123     		movs	r3, #1
 147 007e 85F85D30 		strb	r3, [r5, #93]
3977:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 148              		.loc 1 3977 9 is_stmt 1 discriminator 1 view .LVU42
3977:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 149              		.loc 1 3977 9 discriminator 1 view .LVU43
 150 0082 0023     		movs	r3, #0
 151 0084 85F85C30 		strb	r3, [r5, #92]
3977:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 152              		.loc 1 3977 9 discriminator 1 view .LVU44
3979:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 153              		.loc 1 3979 9 discriminator 1 view .LVU45
3979:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 154              		.loc 1 3979 16 is_stmt 0 discriminator 1 view .LVU46
 155 0088 0320     		movs	r0, #3
 156 008a 18E0     		b	.L8
 157              	.L14:
3961:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
 158              		.loc 1 3961 65 discriminator 1 view .LVU47
 159 008c AB68     		ldr	r3, [r5, #8]
3961:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
ARM GAS  /tmp/ccqUhOmw.s 			page 74


 160              		.loc 1 3961 50 discriminator 1 view .LVU48
 161 008e B3F5004F 		cmp	r3, #32768
 162 0092 02D0     		beq	.L6
3962:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 163              		.loc 1 3962 54 view .LVU49
 164 0094 B3F5806F 		cmp	r3, #1024
 165 0098 ECD1     		bne	.L5
 166              	.L6:
3965:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 167              		.loc 1 3965 11 is_stmt 1 view .LVU50
 168 009a 2A68     		ldr	r2, [r5]
 169 009c 1368     		ldr	r3, [r2]
 170 009e 23F04003 		bic	r3, r3, #64
 171 00a2 1360     		str	r3, [r2]
 172 00a4 E6E7     		b	.L5
 173              	.L15:
3971:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 174              		.loc 1 3971 11 view .LVU51
3971:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 175              		.loc 1 3971 11 view .LVU52
 176 00a6 2A68     		ldr	r2, [r5]
 177 00a8 1368     		ldr	r3, [r2]
 178 00aa 23F40053 		bic	r3, r3, #8192
 179 00ae 1360     		str	r3, [r2]
3971:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 180              		.loc 1 3971 11 view .LVU53
 181 00b0 2A68     		ldr	r2, [r5]
 182 00b2 1368     		ldr	r3, [r2]
 183 00b4 43F40053 		orr	r3, r3, #8192
 184 00b8 1360     		str	r3, [r2]
 185 00ba DFE7     		b	.L7
 186              	.L12:
3987:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
3988:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
3989:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3990:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return HAL_OK;
 187              		.loc 1 3990 10 is_stmt 0 view .LVU54
 188 00bc 0020     		movs	r0, #0
 189              	.L8:
3991:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 190              		.loc 1 3991 1 view .LVU55
 191 00be 02B0     		add	sp, sp, #8
 192              		.cfi_def_cfa_offset 32
 193              		@ sp needed
 194 00c0 BDE8F087 		pop	{r4, r5, r6, r7, r8, r9, r10, pc}
 195              	.LVL9:
 196              	.L17:
 197              		.loc 1 3991 1 view .LVU56
 198              		.align	2
 199              	.L16:
 200 00c4 00000000 		.word	SystemCoreClock
 201              		.cfi_endproc
 202              	.LFE177:
 204              		.section	.text.SPI_WaitFifoStateUntilTimeout,"ax",%progbits
 205              		.align	1
 206              		.syntax unified
 207              		.thumb
ARM GAS  /tmp/ccqUhOmw.s 			page 75


 208              		.thumb_func
 210              	SPI_WaitFifoStateUntilTimeout:
 211              	.LVL10:
 212              	.LFB178:
3992:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
3993:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
3994:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle SPI FIFO Communication Timeout.
3995:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
3996:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *              the configuration information for SPI module.
3997:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Fifo Fifo to check
3998:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  State Fifo state to check
3999:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Timeout Timeout duration
4000:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Tickstart tick start value
4001:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
4002:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
4003:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static HAL_StatusTypeDef SPI_WaitFifoStateUntilTimeout(SPI_HandleTypeDef *hspi, uint32_t Fifo, uint
4004:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                        uint32_t Timeout, uint32_t Tickstart)
4005:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
 213              		.loc 1 4005 1 is_stmt 1 view -0
 214              		.cfi_startproc
 215              		@ args = 4, pretend = 0, frame = 8
 216              		@ frame_needed = 0, uses_anonymous_args = 0
 217              		.loc 1 4005 1 is_stmt 0 view .LVU58
 218 0000 2DE9F047 		push	{r4, r5, r6, r7, r8, r9, r10, lr}
 219              		.cfi_def_cfa_offset 32
 220              		.cfi_offset 4, -32
 221              		.cfi_offset 5, -28
 222              		.cfi_offset 6, -24
 223              		.cfi_offset 7, -20
 224              		.cfi_offset 8, -16
 225              		.cfi_offset 9, -12
 226              		.cfi_offset 10, -8
 227              		.cfi_offset 14, -4
 228 0004 82B0     		sub	sp, sp, #8
 229              		.cfi_def_cfa_offset 40
 230 0006 0646     		mov	r6, r0
 231 0008 0C46     		mov	r4, r1
 232 000a 1546     		mov	r5, r2
 233 000c 1F46     		mov	r7, r3
4006:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t count;
 234              		.loc 1 4006 3 is_stmt 1 view .LVU59
4007:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tmp_timeout;
 235              		.loc 1 4007 3 view .LVU60
4008:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tmp_tickstart;
 236              		.loc 1 4008 3 view .LVU61
4009:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  * ptmpreg8;
 237              		.loc 1 4009 3 view .LVU62
4010:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint8_t  tmpreg8 = 0;
 238              		.loc 1 4010 3 view .LVU63
 239              		.loc 1 4010 17 is_stmt 0 view .LVU64
 240 000e 0023     		movs	r3, #0
 241              	.LVL11:
 242              		.loc 1 4010 17 view .LVU65
 243 0010 8DF80330 		strb	r3, [sp, #3]
4011:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4012:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Adjust Timeout value  in case of end of transfer */
4013:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_timeout = Timeout - (HAL_GetTick() - Tickstart);
ARM GAS  /tmp/ccqUhOmw.s 			page 76


 244              		.loc 1 4013 3 is_stmt 1 view .LVU66
 245              		.loc 1 4013 28 is_stmt 0 view .LVU67
 246 0014 FFF7FEFF 		bl	HAL_GetTick
 247              	.LVL12:
 248              		.loc 1 4013 42 view .LVU68
 249 0018 0A9B     		ldr	r3, [sp, #40]
 250 001a 1B1A     		subs	r3, r3, r0
 251              		.loc 1 4013 15 view .LVU69
 252 001c 03EB0708 		add	r8, r3, r7
 253              	.LVL13:
4014:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_tickstart = HAL_GetTick();
 254              		.loc 1 4014 3 is_stmt 1 view .LVU70
 255              		.loc 1 4014 19 is_stmt 0 view .LVU71
 256 0020 FFF7FEFF 		bl	HAL_GetTick
 257              	.LVL14:
 258 0024 8146     		mov	r9, r0
 259              	.LVL15:
4015:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4016:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Initialize the 8bit temporary pointer */
4017:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   ptmpreg8 = (__IO uint8_t *)&hspi->Instance->DR;
 260              		.loc 1 4017 3 is_stmt 1 view .LVU72
 261              		.loc 1 4017 35 is_stmt 0 view .LVU73
 262 0026 D6F800A0 		ldr	r10, [r6]
 263              	.LVL16:
4018:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4019:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Calculate Timeout based on a software loop to avoid blocking issue if Systick is disabled */
4020:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = tmp_timeout * ((SystemCoreClock * 35U) >> 20U);
 264              		.loc 1 4020 3 is_stmt 1 view .LVU74
 265              		.loc 1 4020 43 is_stmt 0 view .LVU75
 266 002a 304B     		ldr	r3, .L35
 267 002c 1B68     		ldr	r3, [r3]
 268 002e 03EB8303 		add	r3, r3, r3, lsl #2
 269 0032 C3EBC303 		rsb	r3, r3, r3, lsl #3
 270              		.loc 1 4020 50 view .LVU76
 271 0036 1B0D     		lsrs	r3, r3, #20
 272              		.loc 1 4020 23 view .LVU77
 273 0038 08FB03F3 		mul	r3, r8, r3
 274              		.loc 1 4020 9 view .LVU78
 275 003c 0193     		str	r3, [sp, #4]
4021:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4022:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   while ((hspi->Instance->SR & Fifo) != State)
 276              		.loc 1 4022 3 is_stmt 1 view .LVU79
 277              		.loc 1 4022 9 is_stmt 0 view .LVU80
 278 003e 02E0     		b	.L21
 279              	.LVL17:
 280              	.L20:
4023:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4024:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if ((Fifo == SPI_SR_FRLVL) && (State == SPI_FRLVL_EMPTY))
4025:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4026:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Flush Data Register by a blank read */
4027:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       tmpreg8 = *ptmpreg8;
4028:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* To avoid GCC warning */
4029:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       UNUSED(tmpreg8);
4030:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4031:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4032:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (Timeout != HAL_MAX_DELAY)
 281              		.loc 1 4032 5 is_stmt 1 view .LVU81
ARM GAS  /tmp/ccqUhOmw.s 			page 77


 282              		.loc 1 4032 8 is_stmt 0 view .LVU82
 283 0040 B7F1FF3F 		cmp	r7, #-1
 284 0044 12D1     		bne	.L30
 285              	.L21:
4022:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 286              		.loc 1 4022 38 is_stmt 1 view .LVU83
4022:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 287              		.loc 1 4022 15 is_stmt 0 view .LVU84
 288 0046 3368     		ldr	r3, [r6]
4022:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 289              		.loc 1 4022 25 view .LVU85
 290 0048 9B68     		ldr	r3, [r3, #8]
4022:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 291              		.loc 1 4022 30 view .LVU86
 292 004a 03EA040C 		and	ip, r3, r4
4022:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 293              		.loc 1 4022 38 view .LVU87
 294 004e AC45     		cmp	ip, r5
 295 0050 47D0     		beq	.L31
4024:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 296              		.loc 1 4024 5 is_stmt 1 view .LVU88
4024:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 297              		.loc 1 4024 8 is_stmt 0 view .LVU89
 298 0052 B4F5C06F 		cmp	r4, #1536
 299 0056 F3D1     		bne	.L20
4024:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 300              		.loc 1 4024 32 discriminator 1 view .LVU90
 301 0058 002D     		cmp	r5, #0
 302 005a F1D1     		bne	.L20
4027:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* To avoid GCC warning */
 303              		.loc 1 4027 7 is_stmt 1 view .LVU91
4027:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* To avoid GCC warning */
 304              		.loc 1 4027 17 is_stmt 0 view .LVU92
 305 005c 9AF80C30 		ldrb	r3, [r10, #12]	@ zero_extendqisi2
 306 0060 DBB2     		uxtb	r3, r3
4027:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* To avoid GCC warning */
 307              		.loc 1 4027 15 view .LVU93
 308 0062 8DF80330 		strb	r3, [sp, #3]
4029:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 309              		.loc 1 4029 7 is_stmt 1 view .LVU94
 310 0066 9DF80330 		ldrb	r3, [sp, #3]	@ zero_extendqisi2
 311 006a E9E7     		b	.L20
 312              	.L30:
4033:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4034:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (((HAL_GetTick() - tmp_tickstart) >= tmp_timeout) || (tmp_timeout == 0U))
 313              		.loc 1 4034 7 view .LVU95
 314              		.loc 1 4034 13 is_stmt 0 view .LVU96
 315 006c FFF7FEFF 		bl	HAL_GetTick
 316              	.LVL18:
 317              		.loc 1 4034 27 view .LVU97
 318 0070 A0EB0900 		sub	r0, r0, r9
 319              		.loc 1 4034 10 view .LVU98
 320 0074 4045     		cmp	r0, r8
 321 0076 07D2     		bcs	.L32
4035:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
4036:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Disable the SPI and reset the CRC: the CRC value should be cleared
4037:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****            on both master and slave sides in order to resynchronize the master
ARM GAS  /tmp/ccqUhOmw.s 			page 78


4038:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****            and slave for their respective CRC calculation */
4039:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4040:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Disable TXE, RXNE and ERR interrupts for the interrupt process */
4041:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         __HAL_SPI_DISABLE_IT(hspi, (SPI_IT_TXE | SPI_IT_RXNE | SPI_IT_ERR));
4042:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4043:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if ((hspi->Init.Mode == SPI_MODE_MASTER) && ((hspi->Init.Direction == SPI_DIRECTION_1LINE)
4044:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
4045:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
4046:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           /* Disable SPI peripheral */
4047:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           __HAL_SPI_DISABLE(hspi);
4048:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
4049:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4050:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Reset CRC Calculation */
4051:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         if (hspi->Init.CRCCalculation == SPI_CRCCALCULATION_ENABLE)
4052:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
4053:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           SPI_RESET_CRC(hspi);
4054:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
4055:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4056:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->State = HAL_SPI_STATE_READY;
4057:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4058:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Process Unlocked */
4059:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         __HAL_UNLOCK(hspi);
4060:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4061:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         return HAL_TIMEOUT;
4062:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
4063:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* If Systick is disabled or not incremented, deactivate timeout to go in disable loop proced
4064:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if(count == 0U)
 322              		.loc 1 4064 7 is_stmt 1 view .LVU99
 323              		.loc 1 4064 16 is_stmt 0 view .LVU100
 324 0078 019A     		ldr	r2, [sp, #4]
 325              		.loc 1 4064 9 view .LVU101
 326 007a 02B1     		cbz	r2, .L27
 327 007c 4246     		mov	r2, r8
 328              	.L27:
 329              	.LVL19:
4065:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
4066:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         tmp_timeout = 0U;
4067:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }      
4068:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       count--;
 330              		.loc 1 4068 7 is_stmt 1 view .LVU102
 331              		.loc 1 4068 12 is_stmt 0 view .LVU103
 332 007e 019B     		ldr	r3, [sp, #4]
 333 0080 013B     		subs	r3, r3, #1
 334 0082 0193     		str	r3, [sp, #4]
 335 0084 9046     		mov	r8, r2
 336 0086 DEE7     		b	.L21
 337              	.LVL20:
 338              	.L32:
4041:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 339              		.loc 1 4041 9 is_stmt 1 view .LVU104
 340 0088 3268     		ldr	r2, [r6]
 341 008a 5368     		ldr	r3, [r2, #4]
 342 008c 23F0E003 		bic	r3, r3, #224
 343 0090 5360     		str	r3, [r2, #4]
4043:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
 344              		.loc 1 4043 9 view .LVU105
4043:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
ARM GAS  /tmp/ccqUhOmw.s 			page 79


 345              		.loc 1 4043 24 is_stmt 0 view .LVU106
 346 0092 7368     		ldr	r3, [r6, #4]
4043:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
 347              		.loc 1 4043 12 view .LVU107
 348 0094 B3F5827F 		cmp	r3, #260
 349 0098 0BD0     		beq	.L33
 350              	.L23:
4051:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 351              		.loc 1 4051 9 is_stmt 1 view .LVU108
4051:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 352              		.loc 1 4051 23 is_stmt 0 view .LVU109
 353 009a B36A     		ldr	r3, [r6, #40]
4051:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 354              		.loc 1 4051 12 view .LVU110
 355 009c B3F5005F 		cmp	r3, #8192
 356 00a0 14D0     		beq	.L34
 357              	.L25:
4053:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 358              		.loc 1 4053 11 is_stmt 1 discriminator 1 view .LVU111
4056:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 359              		.loc 1 4056 9 discriminator 1 view .LVU112
4056:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 360              		.loc 1 4056 21 is_stmt 0 discriminator 1 view .LVU113
 361 00a2 0123     		movs	r3, #1
 362 00a4 86F85D30 		strb	r3, [r6, #93]
4059:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 363              		.loc 1 4059 9 is_stmt 1 discriminator 1 view .LVU114
4059:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 364              		.loc 1 4059 9 discriminator 1 view .LVU115
 365 00a8 0023     		movs	r3, #0
 366 00aa 86F85C30 		strb	r3, [r6, #92]
4059:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 367              		.loc 1 4059 9 discriminator 1 view .LVU116
4061:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 368              		.loc 1 4061 9 discriminator 1 view .LVU117
4061:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 369              		.loc 1 4061 16 is_stmt 0 discriminator 1 view .LVU118
 370 00ae 0320     		movs	r0, #3
 371 00b0 18E0     		b	.L26
 372              	.L33:
4043:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
 373              		.loc 1 4043 65 discriminator 1 view .LVU119
 374 00b2 B368     		ldr	r3, [r6, #8]
4043:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                      || (hspi->Init.Direction == SPI_DIRECTION_2LIN
 375              		.loc 1 4043 50 discriminator 1 view .LVU120
 376 00b4 B3F5004F 		cmp	r3, #32768
 377 00b8 02D0     		beq	.L24
4044:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 378              		.loc 1 4044 54 view .LVU121
 379 00ba B3F5806F 		cmp	r3, #1024
 380 00be ECD1     		bne	.L23
 381              	.L24:
4047:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 382              		.loc 1 4047 11 is_stmt 1 view .LVU122
 383 00c0 3268     		ldr	r2, [r6]
 384 00c2 1368     		ldr	r3, [r2]
 385 00c4 23F04003 		bic	r3, r3, #64
ARM GAS  /tmp/ccqUhOmw.s 			page 80


 386 00c8 1360     		str	r3, [r2]
 387 00ca E6E7     		b	.L23
 388              	.L34:
4053:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 389              		.loc 1 4053 11 view .LVU123
4053:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 390              		.loc 1 4053 11 view .LVU124
 391 00cc 3268     		ldr	r2, [r6]
 392 00ce 1368     		ldr	r3, [r2]
 393 00d0 23F40053 		bic	r3, r3, #8192
 394 00d4 1360     		str	r3, [r2]
4053:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 395              		.loc 1 4053 11 view .LVU125
 396 00d6 3268     		ldr	r2, [r6]
 397 00d8 1368     		ldr	r3, [r2]
 398 00da 43F40053 		orr	r3, r3, #8192
 399 00de 1360     		str	r3, [r2]
 400 00e0 DFE7     		b	.L25
 401              	.L31:
4069:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4070:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4071:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4072:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return HAL_OK;
 402              		.loc 1 4072 10 is_stmt 0 view .LVU126
 403 00e2 0020     		movs	r0, #0
 404              	.L26:
4073:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 405              		.loc 1 4073 1 view .LVU127
 406 00e4 02B0     		add	sp, sp, #8
 407              		.cfi_def_cfa_offset 32
 408              		@ sp needed
 409 00e6 BDE8F087 		pop	{r4, r5, r6, r7, r8, r9, r10, pc}
 410              	.LVL21:
 411              	.L36:
 412              		.loc 1 4073 1 view .LVU128
 413 00ea 00BF     		.align	2
 414              	.L35:
 415 00ec 00000000 		.word	SystemCoreClock
 416              		.cfi_endproc
 417              	.LFE178:
 419              		.section	.text.SPI_EndRxTxTransaction,"ax",%progbits
 420              		.align	1
 421              		.syntax unified
 422              		.thumb
 423              		.thumb_func
 425              	SPI_EndRxTxTransaction:
 426              	.LVL22:
 427              	.LFB180:
4074:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4075:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
4076:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle the check of the RX transaction complete.
4077:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
4078:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
4079:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Timeout Timeout duration
4080:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Tickstart tick start value
4081:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
4082:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
ARM GAS  /tmp/ccqUhOmw.s 			page 81


4083:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static HAL_StatusTypeDef SPI_EndRxTransaction(SPI_HandleTypeDef *hspi,  uint32_t Timeout, uint32_t 
4084:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
4085:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.Mode == SPI_MODE_MASTER) && ((hspi->Init.Direction == SPI_DIRECTION_1LINE)
4086:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
4087:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4088:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable SPI peripheral */
4089:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_DISABLE(hspi);
4090:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4091:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4092:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Control the BSY flag */
4093:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_BSY, RESET, Timeout, Tickstart) != HAL_OK)
4094:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4095:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
4096:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_TIMEOUT;
4097:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4098:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4099:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.Mode == SPI_MODE_MASTER) && ((hspi->Init.Direction == SPI_DIRECTION_1LINE)
4100:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
4101:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4102:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Empty the FRLVL fifo */
4103:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FRLVL, SPI_FRLVL_EMPTY, Timeout, Tickstart) !=
4104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4105:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
4106:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return HAL_TIMEOUT;
4107:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4108:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4109:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return HAL_OK;
4110:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
4111:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4112:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
4113:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle the check of the RXTX or TX transaction complete.
4114:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi SPI handle
4115:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Timeout Timeout duration
4116:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  Tickstart tick start value
4117:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval HAL status
4118:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
4119:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static HAL_StatusTypeDef SPI_EndRxTxTransaction(SPI_HandleTypeDef *hspi, uint32_t Timeout, uint32_t
4120:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
 428              		.loc 1 4120 1 is_stmt 1 view -0
 429              		.cfi_startproc
 430              		@ args = 0, pretend = 0, frame = 0
 431              		@ frame_needed = 0, uses_anonymous_args = 0
 432              		.loc 1 4120 1 is_stmt 0 view .LVU130
 433 0000 70B5     		push	{r4, r5, r6, lr}
 434              		.cfi_def_cfa_offset 16
 435              		.cfi_offset 4, -16
 436              		.cfi_offset 5, -12
 437              		.cfi_offset 6, -8
 438              		.cfi_offset 14, -4
 439 0002 82B0     		sub	sp, sp, #8
 440              		.cfi_def_cfa_offset 24
 441 0004 0446     		mov	r4, r0
 442 0006 0D46     		mov	r5, r1
 443 0008 1646     		mov	r6, r2
4121:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Control if the TX fifo is empty */
4122:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FTLVL, SPI_FTLVL_EMPTY, Timeout, Tickstart) != H
 444              		.loc 1 4122 3 is_stmt 1 view .LVU131
ARM GAS  /tmp/ccqUhOmw.s 			page 82


 445              		.loc 1 4122 7 is_stmt 0 view .LVU132
 446 000a 0092     		str	r2, [sp]
 447 000c 0B46     		mov	r3, r1
 448 000e 0022     		movs	r2, #0
 449              	.LVL23:
 450              		.loc 1 4122 7 view .LVU133
 451 0010 4FF4C051 		mov	r1, #6144
 452              	.LVL24:
 453              		.loc 1 4122 7 view .LVU134
 454 0014 FFF7FEFF 		bl	SPI_WaitFifoStateUntilTimeout
 455              	.LVL25:
 456              		.loc 1 4122 6 view .LVU135
 457 0018 B0B9     		cbnz	r0, .L42
4123:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4124:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
4125:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_TIMEOUT;
4126:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4127:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4128:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Control the BSY flag */
4129:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_BSY, RESET, Timeout, Tickstart) != HAL_OK)
 458              		.loc 1 4129 3 is_stmt 1 view .LVU136
 459              		.loc 1 4129 7 is_stmt 0 view .LVU137
 460 001a 0096     		str	r6, [sp]
 461 001c 2B46     		mov	r3, r5
 462 001e 0022     		movs	r2, #0
 463 0020 8021     		movs	r1, #128
 464 0022 2046     		mov	r0, r4
 465 0024 FFF7FEFF 		bl	SPI_WaitFlagStateUntilTimeout
 466              	.LVL26:
 467              		.loc 1 4129 6 view .LVU138
 468 0028 A8B9     		cbnz	r0, .L43
4130:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4131:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
4132:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_TIMEOUT;
4133:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4134:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4135:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Control if the RX fifo is empty */
4136:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FRLVL, SPI_FRLVL_EMPTY, Timeout, Tickstart) != H
 469              		.loc 1 4136 3 is_stmt 1 view .LVU139
 470              		.loc 1 4136 7 is_stmt 0 view .LVU140
 471 002a 0096     		str	r6, [sp]
 472 002c 2B46     		mov	r3, r5
 473 002e 0022     		movs	r2, #0
 474 0030 4FF4C061 		mov	r1, #1536
 475 0034 2046     		mov	r0, r4
 476 0036 FFF7FEFF 		bl	SPI_WaitFifoStateUntilTimeout
 477              	.LVL27:
 478              		.loc 1 4136 6 view .LVU141
 479 003a 50B1     		cbz	r0, .L39
4137:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4138:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
 480              		.loc 1 4138 5 is_stmt 1 view .LVU142
 481 003c 236E     		ldr	r3, [r4, #96]
 482 003e 43F02003 		orr	r3, r3, #32
 483 0042 2366     		str	r3, [r4, #96]
4139:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_TIMEOUT;
 484              		.loc 1 4139 5 view .LVU143
ARM GAS  /tmp/ccqUhOmw.s 			page 83


 485              		.loc 1 4139 12 is_stmt 0 view .LVU144
 486 0044 0320     		movs	r0, #3
 487 0046 04E0     		b	.L39
 488              	.L42:
4124:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_TIMEOUT;
 489              		.loc 1 4124 5 is_stmt 1 view .LVU145
 490 0048 236E     		ldr	r3, [r4, #96]
 491 004a 43F02003 		orr	r3, r3, #32
 492 004e 2366     		str	r3, [r4, #96]
4125:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 493              		.loc 1 4125 5 view .LVU146
4125:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 494              		.loc 1 4125 12 is_stmt 0 view .LVU147
 495 0050 0320     		movs	r0, #3
 496              	.L39:
4140:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4141:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4142:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return HAL_OK;
4143:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 497              		.loc 1 4143 1 view .LVU148
 498 0052 02B0     		add	sp, sp, #8
 499              		.cfi_remember_state
 500              		.cfi_def_cfa_offset 16
 501              		@ sp needed
 502 0054 70BD     		pop	{r4, r5, r6, pc}
 503              	.LVL28:
 504              	.L43:
 505              		.cfi_restore_state
4131:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_TIMEOUT;
 506              		.loc 1 4131 5 is_stmt 1 view .LVU149
 507 0056 236E     		ldr	r3, [r4, #96]
 508 0058 43F02003 		orr	r3, r3, #32
 509 005c 2366     		str	r3, [r4, #96]
4132:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 510              		.loc 1 4132 5 view .LVU150
4132:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 511              		.loc 1 4132 12 is_stmt 0 view .LVU151
 512 005e 0320     		movs	r0, #3
 513 0060 F7E7     		b	.L39
 514              		.cfi_endproc
 515              	.LFE180:
 517              		.section	.text.SPI_EndRxTransaction,"ax",%progbits
 518              		.align	1
 519              		.syntax unified
 520              		.thumb
 521              		.thumb_func
 523              	SPI_EndRxTransaction:
 524              	.LVL29:
 525              	.LFB179:
4084:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.Mode == SPI_MODE_MASTER) && ((hspi->Init.Direction == SPI_DIRECTION_1LINE)
 526              		.loc 1 4084 1 is_stmt 1 view -0
 527              		.cfi_startproc
 528              		@ args = 0, pretend = 0, frame = 0
 529              		@ frame_needed = 0, uses_anonymous_args = 0
4084:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if ((hspi->Init.Mode == SPI_MODE_MASTER) && ((hspi->Init.Direction == SPI_DIRECTION_1LINE)
 530              		.loc 1 4084 1 is_stmt 0 view .LVU153
 531 0000 70B5     		push	{r4, r5, r6, lr}
ARM GAS  /tmp/ccqUhOmw.s 			page 84


 532              		.cfi_def_cfa_offset 16
 533              		.cfi_offset 4, -16
 534              		.cfi_offset 5, -12
 535              		.cfi_offset 6, -8
 536              		.cfi_offset 14, -4
 537 0002 82B0     		sub	sp, sp, #8
 538              		.cfi_def_cfa_offset 24
 539 0004 0446     		mov	r4, r0
 540 0006 0D46     		mov	r5, r1
 541 0008 1646     		mov	r6, r2
4085:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
 542              		.loc 1 4085 3 is_stmt 1 view .LVU154
4085:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
 543              		.loc 1 4085 18 is_stmt 0 view .LVU155
 544 000a 4368     		ldr	r3, [r0, #4]
4085:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
 545              		.loc 1 4085 6 view .LVU156
 546 000c B3F5827F 		cmp	r3, #260
 547 0010 0DD0     		beq	.L51
 548              	.LVL30:
 549              	.L45:
4093:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 550              		.loc 1 4093 3 is_stmt 1 view .LVU157
4093:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 551              		.loc 1 4093 7 is_stmt 0 view .LVU158
 552 0012 0096     		str	r6, [sp]
 553 0014 2B46     		mov	r3, r5
 554 0016 0022     		movs	r2, #0
 555 0018 8021     		movs	r1, #128
 556              	.LVL31:
4093:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 557              		.loc 1 4093 7 view .LVU159
 558 001a 2046     		mov	r0, r4
 559              	.LVL32:
4093:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 560              		.loc 1 4093 7 view .LVU160
 561 001c FFF7FEFF 		bl	SPI_WaitFlagStateUntilTimeout
 562              	.LVL33:
4093:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 563              		.loc 1 4093 6 view .LVU161
 564 0020 90B9     		cbnz	r0, .L52
4099:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
 565              		.loc 1 4099 3 is_stmt 1 view .LVU162
4099:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
 566              		.loc 1 4099 18 is_stmt 0 view .LVU163
 567 0022 6368     		ldr	r3, [r4, #4]
4099:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
 568              		.loc 1 4099 6 view .LVU164
 569 0024 B3F5827F 		cmp	r3, #260
 570 0028 14D0     		beq	.L53
 571              	.L48:
4110:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 572              		.loc 1 4110 1 view .LVU165
 573 002a 02B0     		add	sp, sp, #8
 574              		.cfi_remember_state
 575              		.cfi_def_cfa_offset 16
 576              		@ sp needed
ARM GAS  /tmp/ccqUhOmw.s 			page 85


 577 002c 70BD     		pop	{r4, r5, r6, pc}
 578              	.LVL34:
 579              	.L51:
 580              		.cfi_restore_state
4085:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
 581              		.loc 1 4085 59 discriminator 1 view .LVU166
 582 002e 8368     		ldr	r3, [r0, #8]
4085:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
 583              		.loc 1 4085 44 discriminator 1 view .LVU167
 584 0030 B3F5004F 		cmp	r3, #32768
 585 0034 02D0     		beq	.L46
4086:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 586              		.loc 1 4086 48 view .LVU168
 587 0036 B3F5806F 		cmp	r3, #1024
 588 003a EAD1     		bne	.L45
 589              	.L46:
4089:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 590              		.loc 1 4089 5 is_stmt 1 view .LVU169
 591 003c 2268     		ldr	r2, [r4]
 592              	.LVL35:
4089:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 593              		.loc 1 4089 5 is_stmt 0 view .LVU170
 594 003e 1368     		ldr	r3, [r2]
 595 0040 23F04003 		bic	r3, r3, #64
 596 0044 1360     		str	r3, [r2]
 597 0046 E4E7     		b	.L45
 598              	.LVL36:
 599              	.L52:
4095:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return HAL_TIMEOUT;
 600              		.loc 1 4095 5 is_stmt 1 view .LVU171
 601 0048 236E     		ldr	r3, [r4, #96]
 602 004a 43F02003 		orr	r3, r3, #32
 603 004e 2366     		str	r3, [r4, #96]
4096:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 604              		.loc 1 4096 5 view .LVU172
4096:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 605              		.loc 1 4096 12 is_stmt 0 view .LVU173
 606 0050 0320     		movs	r0, #3
 607 0052 EAE7     		b	.L48
 608              	.L53:
4099:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
 609              		.loc 1 4099 59 discriminator 1 view .LVU174
 610 0054 A368     		ldr	r3, [r4, #8]
4099:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                                || (hspi->Init.Direction == SPI_DIRECTION_2LINES_RXO
 611              		.loc 1 4099 44 discriminator 1 view .LVU175
 612 0056 B3F5004F 		cmp	r3, #32768
 613 005a 02D0     		beq	.L49
4100:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 614              		.loc 1 4100 48 view .LVU176
 615 005c B3F5806F 		cmp	r3, #1024
 616 0060 E3D1     		bne	.L48
 617              	.L49:
4103:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 618              		.loc 1 4103 5 is_stmt 1 view .LVU177
4103:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 619              		.loc 1 4103 9 is_stmt 0 view .LVU178
 620 0062 0096     		str	r6, [sp]
ARM GAS  /tmp/ccqUhOmw.s 			page 86


 621 0064 2B46     		mov	r3, r5
 622 0066 0022     		movs	r2, #0
 623 0068 4FF4C061 		mov	r1, #1536
 624 006c 2046     		mov	r0, r4
 625 006e FFF7FEFF 		bl	SPI_WaitFifoStateUntilTimeout
 626              	.LVL37:
4103:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 627              		.loc 1 4103 8 view .LVU179
 628 0072 0028     		cmp	r0, #0
 629 0074 D9D0     		beq	.L48
4105:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       return HAL_TIMEOUT;
 630              		.loc 1 4105 7 is_stmt 1 view .LVU180
 631 0076 236E     		ldr	r3, [r4, #96]
 632 0078 43F02003 		orr	r3, r3, #32
 633 007c 2366     		str	r3, [r4, #96]
4106:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 634              		.loc 1 4106 7 view .LVU181
4106:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 635              		.loc 1 4106 14 is_stmt 0 view .LVU182
 636 007e 0320     		movs	r0, #3
 637 0080 D3E7     		b	.L48
 638              		.cfi_endproc
 639              	.LFE179:
 641              		.section	.text.SPI_AbortRx_ISR,"ax",%progbits
 642              		.align	1
 643              		.syntax unified
 644              		.thumb
 645              		.thumb_func
 647              	SPI_AbortRx_ISR:
 648              	.LVL38:
 649              	.LFB184:
4144:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4145:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
4146:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle the end of the RXTX transaction.
4147:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
4148:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
4149:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
4150:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
4151:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_CloseRxTx_ISR(SPI_HandleTypeDef *hspi)
4152:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
4153:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
4154:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4155:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init tickstart for timeout management */
4156:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tickstart = HAL_GetTick();
4157:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4158:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable ERR interrupt */
4159:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_DISABLE_IT(hspi, SPI_IT_ERR);
4160:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4161:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the end of the transaction */
4162:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_EndRxTxTransaction(hspi, SPI_DEFAULT_TIMEOUT, tickstart) != HAL_OK)
4163:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4164:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
4165:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4166:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4167:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
4168:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if CRC error occurred */
4169:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_CRCERR) != RESET)
ARM GAS  /tmp/ccqUhOmw.s 			page 87


4170:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4171:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
4172:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
4173:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_CRCERRFLAG(hspi);
4174:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Call user error callback */
4175:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
4176:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCallback(hspi);
4177:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
4178:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     HAL_SPI_ErrorCallback(hspi);
4179:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
4180:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4181:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
4182:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4183:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
4184:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->ErrorCode == HAL_SPI_ERROR_NONE)
4185:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4186:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (hspi->State == HAL_SPI_STATE_BUSY_RX)
4187:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
4188:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->State = HAL_SPI_STATE_READY;
4189:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Call user Rx complete callback */
4190:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
4191:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxCpltCallback(hspi);
4192:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
4193:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         HAL_SPI_RxCpltCallback(hspi);
4194:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
4195:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
4196:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       else
4197:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
4198:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->State = HAL_SPI_STATE_READY;
4199:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Call user TxRx complete callback */
4200:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
4201:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxRxCpltCallback(hspi);
4202:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
4203:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         HAL_SPI_TxRxCpltCallback(hspi);
4204:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
4205:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
4206:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4207:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     else
4208:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4209:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->State = HAL_SPI_STATE_READY;
4210:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Call user error callback */
4211:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
4212:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->ErrorCallback(hspi);
4213:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
4214:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       HAL_SPI_ErrorCallback(hspi);
4215:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
4216:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4217:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
4218:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4219:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
4220:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
4221:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4222:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
4223:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle the end of the RX transaction.
4224:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
4225:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
4226:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
ARM GAS  /tmp/ccqUhOmw.s 			page 88


4227:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
4228:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_CloseRx_ISR(SPI_HandleTypeDef *hspi)
4229:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
4230:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable RXNE and ERR interrupt */
4231:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_DISABLE_IT(hspi, (SPI_IT_RXNE | SPI_IT_ERR));
4232:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4233:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the end of the transaction */
4234:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_EndRxTransaction(hspi, SPI_DEFAULT_TIMEOUT, HAL_GetTick()) != HAL_OK)
4235:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4236:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
4237:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4238:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
4239:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4240:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
4241:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check if CRC error occurred */
4242:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (__HAL_SPI_GET_FLAG(hspi, SPI_FLAG_CRCERR) != RESET)
4243:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4244:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_CRC);
4245:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_CRCERRFLAG(hspi);
4246:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Call user error callback */
4247:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
4248:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCallback(hspi);
4249:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
4250:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     HAL_SPI_ErrorCallback(hspi);
4251:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
4252:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4253:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
4254:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4255:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
4256:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->ErrorCode == HAL_SPI_ERROR_NONE)
4257:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4258:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Call user Rx complete callback */
4259:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
4260:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->RxCpltCallback(hspi);
4261:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
4262:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       HAL_SPI_RxCpltCallback(hspi);
4263:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
4264:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4265:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     else
4266:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4267:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Call user error callback */
4268:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
4269:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->ErrorCallback(hspi);
4270:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
4271:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       HAL_SPI_ErrorCallback(hspi);
4272:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
4273:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4274:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
4275:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4276:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
4277:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
4278:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4279:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
4280:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle the end of the TX transaction.
4281:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
4282:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
4283:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
ARM GAS  /tmp/ccqUhOmw.s 			page 89


4284:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
4285:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_CloseTx_ISR(SPI_HandleTypeDef *hspi)
4286:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
4287:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
4288:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4289:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Init tickstart for timeout management*/
4290:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tickstart = HAL_GetTick();
4291:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4292:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable TXE and ERR interrupt */
4293:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_DISABLE_IT(hspi, (SPI_IT_TXE | SPI_IT_ERR));
4294:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4295:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the end of the transaction */
4296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_EndRxTxTransaction(hspi, SPI_DEFAULT_TIMEOUT, tickstart) != HAL_OK)
4297:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4298:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_FLAG);
4299:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4300:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4301:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Clear overrun flag in 2 Lines communication mode because received is not read */
4302:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.Direction == SPI_DIRECTION_2LINES)
4303:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_OVRFLAG(hspi);
4305:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4306:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4307:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
4308:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
4309:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4310:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Call user error callback */
4311:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
4312:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCallback(hspi);
4313:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
4314:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     HAL_SPI_ErrorCallback(hspi);
4315:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
4316:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4317:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   else
4318:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4319:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Call user Rx complete callback */
4320:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_HAL_SPI_REGISTER_CALLBACKS == 1U)
4321:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxCpltCallback(hspi);
4322:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #else
4323:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     HAL_SPI_TxCpltCallback(hspi);
4324:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
4325:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4326:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
4327:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4328:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
4329:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle abort a Rx transaction.
4330:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
4331:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
4332:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
4333:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
4334:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_AbortRx_ISR(SPI_HandleTypeDef *hspi)
4335:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
 650              		.loc 1 4335 1 is_stmt 1 view -0
 651              		.cfi_startproc
 652              		@ args = 0, pretend = 0, frame = 8
 653              		@ frame_needed = 0, uses_anonymous_args = 0
 654              		.loc 1 4335 1 is_stmt 0 view .LVU184
ARM GAS  /tmp/ccqUhOmw.s 			page 90


 655 0000 10B5     		push	{r4, lr}
 656              		.cfi_def_cfa_offset 8
 657              		.cfi_offset 4, -8
 658              		.cfi_offset 14, -4
 659 0002 84B0     		sub	sp, sp, #16
 660              		.cfi_def_cfa_offset 24
 661 0004 0446     		mov	r4, r0
4336:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t count;
 662              		.loc 1 4336 3 is_stmt 1 view .LVU185
4337:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4338:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable SPI Peripheral */
4339:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_DISABLE(hspi);
 663              		.loc 1 4339 3 view .LVU186
 664 0006 0268     		ldr	r2, [r0]
 665 0008 1368     		ldr	r3, [r2]
 666 000a 23F04003 		bic	r3, r3, #64
 667 000e 1360     		str	r3, [r2]
4340:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4341:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24U / 1000U);
 668              		.loc 1 4341 3 view .LVU187
 669              		.loc 1 4341 56 is_stmt 0 view .LVU188
 670 0010 1D4B     		ldr	r3, .L62
 671 0012 1B68     		ldr	r3, [r3]
 672 0014 1D4A     		ldr	r2, .L62+4
 673 0016 A2FB0323 		umull	r2, r3, r2, r3
 674 001a 5B0A     		lsrs	r3, r3, #9
 675              		.loc 1 4341 31 view .LVU189
 676 001c 6422     		movs	r2, #100
 677 001e 02FB03F3 		mul	r3, r2, r3
 678              		.loc 1 4341 9 view .LVU190
 679 0022 0393     		str	r3, [sp, #12]
4342:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4343:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable RXNEIE interrupt */
4344:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, (SPI_CR2_RXNEIE));
 680              		.loc 1 4344 3 is_stmt 1 view .LVU191
 681 0024 0268     		ldr	r2, [r0]
 682 0026 5368     		ldr	r3, [r2, #4]
 683 0028 23F04003 		bic	r3, r3, #64
 684 002c 5360     		str	r3, [r2, #4]
 685              	.L57:
4345:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4346:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check RXNEIE is disabled */
4347:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   do
 686              		.loc 1 4347 3 view .LVU192
4348:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4349:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (count == 0U)
 687              		.loc 1 4349 5 view .LVU193
 688              		.loc 1 4349 15 is_stmt 0 view .LVU194
 689 002e 039B     		ldr	r3, [sp, #12]
 690              		.loc 1 4349 8 view .LVU195
 691 0030 43B1     		cbz	r3, .L61
4350:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4351:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
4352:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       break;
4353:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4354:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     count--;
 692              		.loc 1 4354 5 is_stmt 1 view .LVU196
ARM GAS  /tmp/ccqUhOmw.s 			page 91


 693              		.loc 1 4354 10 is_stmt 0 view .LVU197
 694 0032 039B     		ldr	r3, [sp, #12]
 695 0034 013B     		subs	r3, r3, #1
 696 0036 0393     		str	r3, [sp, #12]
4355:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   } while (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_RXNEIE));
 697              		.loc 1 4355 12 is_stmt 1 view .LVU198
 698 0038 2368     		ldr	r3, [r4]
 699 003a 5B68     		ldr	r3, [r3, #4]
 700 003c 13F0400F 		tst	r3, #64
 701 0040 F5D1     		bne	.L57
 702 0042 03E0     		b	.L56
 703              	.L61:
4351:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       break;
 704              		.loc 1 4351 7 view .LVU199
 705 0044 236E     		ldr	r3, [r4, #96]
 706 0046 43F04003 		orr	r3, r3, #64
 707 004a 2366     		str	r3, [r4, #96]
4352:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 708              		.loc 1 4352 7 view .LVU200
 709              	.L56:
4356:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4357:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Control the BSY flag */
4358:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_BSY, RESET, SPI_DEFAULT_TIMEOUT, HAL_GetTick()) 
 710              		.loc 1 4358 3 view .LVU201
 711              		.loc 1 4358 7 is_stmt 0 view .LVU202
 712 004c FFF7FEFF 		bl	HAL_GetTick
 713              	.LVL39:
 714              		.loc 1 4358 7 view .LVU203
 715 0050 0090     		str	r0, [sp]
 716 0052 6423     		movs	r3, #100
 717 0054 0022     		movs	r2, #0
 718 0056 8021     		movs	r1, #128
 719 0058 2046     		mov	r0, r4
 720 005a FFF7FEFF 		bl	SPI_WaitFlagStateUntilTimeout
 721              	.LVL40:
 722              		.loc 1 4358 6 view .LVU204
 723 005e 08B1     		cbz	r0, .L58
4359:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 724              		.loc 1 4360 5 is_stmt 1 view .LVU205
 725              		.loc 1 4360 21 is_stmt 0 view .LVU206
 726 0060 4023     		movs	r3, #64
 727 0062 2366     		str	r3, [r4, #96]
 728              	.L58:
4361:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4362:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4363:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Empty the FRLVL fifo */
4364:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FRLVL, SPI_FRLVL_EMPTY, SPI_DEFAULT_TIMEOUT, HAL
 729              		.loc 1 4364 3 is_stmt 1 view .LVU207
 730              		.loc 1 4364 7 is_stmt 0 view .LVU208
 731 0064 FFF7FEFF 		bl	HAL_GetTick
 732              	.LVL41:
 733 0068 0090     		str	r0, [sp]
 734 006a 6423     		movs	r3, #100
 735 006c 0022     		movs	r2, #0
 736 006e 4FF4C061 		mov	r1, #1536
 737 0072 2046     		mov	r0, r4
ARM GAS  /tmp/ccqUhOmw.s 			page 92


 738 0074 FFF7FEFF 		bl	SPI_WaitFifoStateUntilTimeout
 739              	.LVL42:
 740              		.loc 1 4364 6 view .LVU209
 741 0078 08B1     		cbz	r0, .L59
4365:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4366:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 742              		.loc 1 4366 5 is_stmt 1 view .LVU210
 743              		.loc 1 4366 21 is_stmt 0 view .LVU211
 744 007a 4023     		movs	r3, #64
 745 007c 2366     		str	r3, [r4, #96]
 746              	.L59:
4367:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4368:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4369:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_ABORT;
 747              		.loc 1 4369 3 is_stmt 1 view .LVU212
 748              		.loc 1 4369 15 is_stmt 0 view .LVU213
 749 007e 0723     		movs	r3, #7
 750 0080 84F85D30 		strb	r3, [r4, #93]
4370:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 751              		.loc 1 4370 1 view .LVU214
 752 0084 04B0     		add	sp, sp, #16
 753              		.cfi_def_cfa_offset 8
 754              		@ sp needed
 755 0086 10BD     		pop	{r4, pc}
 756              	.LVL43:
 757              	.L63:
 758              		.loc 1 4370 1 view .LVU215
 759              		.align	2
 760              	.L62:
 761 0088 00000000 		.word	SystemCoreClock
 762 008c F1197605 		.word	91625969
 763              		.cfi_endproc
 764              	.LFE184:
 766              		.section	.text.SPI_AbortTx_ISR,"ax",%progbits
 767              		.align	1
 768              		.syntax unified
 769              		.thumb
 770              		.thumb_func
 772              	SPI_AbortTx_ISR:
 773              	.LVL44:
 774              	.LFB185:
4371:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4372:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** /**
4373:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @brief  Handle abort a Tx or Rx/Tx transaction.
4374:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @param  hspi pointer to a SPI_HandleTypeDef structure that contains
4375:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *               the configuration information for SPI module.
4376:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   * @retval None
4377:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   */
4378:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** static void SPI_AbortTx_ISR(SPI_HandleTypeDef *hspi)
4379:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** {
 775              		.loc 1 4379 1 is_stmt 1 view -0
 776              		.cfi_startproc
 777              		@ args = 0, pretend = 0, frame = 8
 778              		@ frame_needed = 0, uses_anonymous_args = 0
 779              		.loc 1 4379 1 is_stmt 0 view .LVU217
 780 0000 10B5     		push	{r4, lr}
 781              		.cfi_def_cfa_offset 8
ARM GAS  /tmp/ccqUhOmw.s 			page 93


 782              		.cfi_offset 4, -8
 783              		.cfi_offset 14, -4
 784 0002 84B0     		sub	sp, sp, #16
 785              		.cfi_def_cfa_offset 24
 786 0004 0446     		mov	r4, r0
4380:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t count;
 787              		.loc 1 4380 3 is_stmt 1 view .LVU218
4381:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4382:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24U / 1000U);
 788              		.loc 1 4382 3 view .LVU219
 789              		.loc 1 4382 56 is_stmt 0 view .LVU220
 790 0006 384B     		ldr	r3, .L78
 791 0008 1B68     		ldr	r3, [r3]
 792 000a 384A     		ldr	r2, .L78+4
 793 000c A2FB0323 		umull	r2, r3, r2, r3
 794 0010 5B0A     		lsrs	r3, r3, #9
 795              		.loc 1 4382 31 view .LVU221
 796 0012 6422     		movs	r2, #100
 797 0014 02FB03F3 		mul	r3, r2, r3
 798              		.loc 1 4382 9 view .LVU222
 799 0018 0393     		str	r3, [sp, #12]
4383:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4384:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable TXEIE interrupt */
4385:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   CLEAR_BIT(hspi->Instance->CR2, (SPI_CR2_TXEIE));
 800              		.loc 1 4385 3 is_stmt 1 view .LVU223
 801 001a 0268     		ldr	r2, [r0]
 802 001c 5368     		ldr	r3, [r2, #4]
 803 001e 23F08003 		bic	r3, r3, #128
 804 0022 5360     		str	r3, [r2, #4]
 805              	.L67:
4386:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4387:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check TXEIE is disabled */
4388:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   do
 806              		.loc 1 4388 3 view .LVU224
4389:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4390:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (count == 0U)
 807              		.loc 1 4390 5 view .LVU225
 808              		.loc 1 4390 15 is_stmt 0 view .LVU226
 809 0024 039B     		ldr	r3, [sp, #12]
 810              		.loc 1 4390 8 view .LVU227
 811 0026 43B1     		cbz	r3, .L76
4391:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4392:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
4393:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       break;
4394:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4395:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     count--;
 812              		.loc 1 4395 5 is_stmt 1 view .LVU228
 813              		.loc 1 4395 10 is_stmt 0 view .LVU229
 814 0028 039B     		ldr	r3, [sp, #12]
 815 002a 013B     		subs	r3, r3, #1
 816 002c 0393     		str	r3, [sp, #12]
4396:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   } while (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_TXEIE));
 817              		.loc 1 4396 12 is_stmt 1 view .LVU230
 818 002e 2368     		ldr	r3, [r4]
 819 0030 5B68     		ldr	r3, [r3, #4]
 820 0032 13F0800F 		tst	r3, #128
 821 0036 F5D1     		bne	.L67
ARM GAS  /tmp/ccqUhOmw.s 			page 94


 822 0038 03E0     		b	.L66
 823              	.L76:
4392:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       break;
 824              		.loc 1 4392 7 view .LVU231
 825 003a 236E     		ldr	r3, [r4, #96]
 826 003c 43F04003 		orr	r3, r3, #64
 827 0040 2366     		str	r3, [r4, #96]
4393:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 828              		.loc 1 4393 7 view .LVU232
 829              	.L66:
4397:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4398:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_EndRxTxTransaction(hspi, SPI_DEFAULT_TIMEOUT, HAL_GetTick()) != HAL_OK)
 830              		.loc 1 4398 3 view .LVU233
 831              		.loc 1 4398 7 is_stmt 0 view .LVU234
 832 0042 FFF7FEFF 		bl	HAL_GetTick
 833              	.LVL45:
 834              		.loc 1 4398 7 view .LVU235
 835 0046 0246     		mov	r2, r0
 836 0048 6421     		movs	r1, #100
 837 004a 2046     		mov	r0, r4
 838 004c FFF7FEFF 		bl	SPI_EndRxTxTransaction
 839              	.LVL46:
 840              		.loc 1 4398 6 view .LVU236
 841 0050 08B1     		cbz	r0, .L68
4399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4400:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 842              		.loc 1 4400 5 is_stmt 1 view .LVU237
 843              		.loc 1 4400 21 is_stmt 0 view .LVU238
 844 0052 4023     		movs	r3, #64
 845 0054 2366     		str	r3, [r4, #96]
 846              	.L68:
4401:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4402:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable SPI Peripheral */
4404:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_DISABLE(hspi);
 847              		.loc 1 4404 3 is_stmt 1 view .LVU239
 848 0056 2268     		ldr	r2, [r4]
 849 0058 1368     		ldr	r3, [r2]
 850 005a 23F04003 		bic	r3, r3, #64
 851 005e 1360     		str	r3, [r2]
4405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4406:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Empty the FRLVL fifo */
4407:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FRLVL, SPI_FRLVL_EMPTY, SPI_DEFAULT_TIMEOUT, HAL
 852              		.loc 1 4407 3 view .LVU240
 853              		.loc 1 4407 7 is_stmt 0 view .LVU241
 854 0060 FFF7FEFF 		bl	HAL_GetTick
 855              	.LVL47:
 856 0064 0090     		str	r0, [sp]
 857 0066 6423     		movs	r3, #100
 858 0068 0022     		movs	r2, #0
 859 006a 4FF4C061 		mov	r1, #1536
 860 006e 2046     		mov	r0, r4
 861 0070 FFF7FEFF 		bl	SPI_WaitFifoStateUntilTimeout
 862              	.LVL48:
 863              		.loc 1 4407 6 view .LVU242
 864 0074 08B1     		cbz	r0, .L69
4408:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/ccqUhOmw.s 			page 95


4409:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 865              		.loc 1 4409 5 is_stmt 1 view .LVU243
 866              		.loc 1 4409 21 is_stmt 0 view .LVU244
 867 0076 4023     		movs	r3, #64
 868 0078 2366     		str	r3, [r4, #96]
 869              	.L69:
4410:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4412:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check case of Full-Duplex Mode and disable directly RXNEIE interrupt */
4413:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_RXNEIE))
 870              		.loc 1 4413 3 is_stmt 1 view .LVU245
 871              		.loc 1 4413 7 is_stmt 0 view .LVU246
 872 007a 2368     		ldr	r3, [r4]
 873 007c 5A68     		ldr	r2, [r3, #4]
 874              		.loc 1 4413 6 view .LVU247
 875 007e 12F0400F 		tst	r2, #64
 876 0082 2BD0     		beq	.L70
4414:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
4415:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Disable RXNEIE interrupt */
4416:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     CLEAR_BIT(hspi->Instance->CR2, (SPI_CR2_RXNEIE));
 877              		.loc 1 4416 5 is_stmt 1 view .LVU248
 878 0084 5A68     		ldr	r2, [r3, #4]
 879 0086 22F04002 		bic	r2, r2, #64
 880 008a 5A60     		str	r2, [r3, #4]
 881              	.L73:
4417:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4418:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Check RXNEIE is disabled */
4419:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     do
 882              		.loc 1 4419 5 view .LVU249
4420:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4421:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       if (count == 0U)
 883              		.loc 1 4421 7 view .LVU250
 884              		.loc 1 4421 17 is_stmt 0 view .LVU251
 885 008c 039B     		ldr	r3, [sp, #12]
 886              		.loc 1 4421 10 view .LVU252
 887 008e 43B1     		cbz	r3, .L77
4422:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
4423:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         SET_BIT(hspi->ErrorCode, HAL_SPI_ERROR_ABORT);
4424:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
4425:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
4426:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       count--;
 888              		.loc 1 4426 7 is_stmt 1 view .LVU253
 889              		.loc 1 4426 12 is_stmt 0 view .LVU254
 890 0090 039B     		ldr	r3, [sp, #12]
 891 0092 013B     		subs	r3, r3, #1
 892 0094 0393     		str	r3, [sp, #12]
4427:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (HAL_IS_BIT_SET(hspi->Instance->CR2, SPI_CR2_RXNEIE));
 893              		.loc 1 4427 14 is_stmt 1 view .LVU255
 894 0096 2368     		ldr	r3, [r4]
 895 0098 5B68     		ldr	r3, [r3, #4]
 896 009a 13F0400F 		tst	r3, #64
 897 009e F5D1     		bne	.L73
 898 00a0 03E0     		b	.L72
 899              	.L77:
4423:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 900              		.loc 1 4423 9 view .LVU256
 901 00a2 236E     		ldr	r3, [r4, #96]
ARM GAS  /tmp/ccqUhOmw.s 			page 96


 902 00a4 43F04003 		orr	r3, r3, #64
 903 00a8 2366     		str	r3, [r4, #96]
4424:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 904              		.loc 1 4424 9 view .LVU257
 905              	.L72:
4428:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4429:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Control the BSY flag */
4430:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_WaitFlagStateUntilTimeout(hspi, SPI_FLAG_BSY, RESET, SPI_DEFAULT_TIMEOUT, HAL_GetTick()
 906              		.loc 1 4430 5 view .LVU258
 907              		.loc 1 4430 9 is_stmt 0 view .LVU259
 908 00aa FFF7FEFF 		bl	HAL_GetTick
 909              	.LVL49:
 910 00ae 0090     		str	r0, [sp]
 911 00b0 6423     		movs	r3, #100
 912 00b2 0022     		movs	r2, #0
 913 00b4 8021     		movs	r1, #128
 914 00b6 2046     		mov	r0, r4
 915 00b8 FFF7FEFF 		bl	SPI_WaitFlagStateUntilTimeout
 916              	.LVL50:
 917              		.loc 1 4430 8 view .LVU260
 918 00bc 08B1     		cbz	r0, .L74
4431:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 919              		.loc 1 4432 7 is_stmt 1 view .LVU261
 920              		.loc 1 4432 23 is_stmt 0 view .LVU262
 921 00be 4023     		movs	r3, #64
 922 00c0 2366     		str	r3, [r4, #96]
 923              	.L74:
4433:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4434:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
4435:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Empty the FRLVL fifo */
4436:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (SPI_WaitFifoStateUntilTimeout(hspi, SPI_FLAG_FRLVL, SPI_FRLVL_EMPTY, SPI_DEFAULT_TIMEOUT, H
 924              		.loc 1 4436 5 is_stmt 1 view .LVU263
 925              		.loc 1 4436 9 is_stmt 0 view .LVU264
 926 00c2 FFF7FEFF 		bl	HAL_GetTick
 927              	.LVL51:
 928 00c6 0090     		str	r0, [sp]
 929 00c8 6423     		movs	r3, #100
 930 00ca 0022     		movs	r2, #0
 931 00cc 4FF4C061 		mov	r1, #1536
 932 00d0 2046     		mov	r0, r4
 933 00d2 FFF7FEFF 		bl	SPI_WaitFifoStateUntilTimeout
 934              	.LVL52:
 935              		.loc 1 4436 8 view .LVU265
 936 00d6 08B1     		cbz	r0, .L70
4437:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
4438:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 937              		.loc 1 4438 7 is_stmt 1 view .LVU266
 938              		.loc 1 4438 23 is_stmt 0 view .LVU267
 939 00d8 4023     		movs	r3, #64
 940 00da 2366     		str	r3, [r4, #96]
 941              	.L70:
4439:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
4440:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
4441:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_ABORT;
 942              		.loc 1 4441 3 is_stmt 1 view .LVU268
 943              		.loc 1 4441 15 is_stmt 0 view .LVU269
ARM GAS  /tmp/ccqUhOmw.s 			page 97


 944 00dc 0723     		movs	r3, #7
 945 00de 84F85D30 		strb	r3, [r4, #93]
4442:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 946              		.loc 1 4442 1 view .LVU270
 947 00e2 04B0     		add	sp, sp, #16
 948              		.cfi_def_cfa_offset 8
 949              		@ sp needed
 950 00e4 10BD     		pop	{r4, pc}
 951              	.LVL53:
 952              	.L79:
 953              		.loc 1 4442 1 view .LVU271
 954 00e6 00BF     		.align	2
 955              	.L78:
 956 00e8 00000000 		.word	SystemCoreClock
 957 00ec F1197605 		.word	91625969
 958              		.cfi_endproc
 959              	.LFE185:
 961              		.section	.text.HAL_SPI_MspInit,"ax",%progbits
 962              		.align	1
 963              		.weak	HAL_SPI_MspInit
 964              		.syntax unified
 965              		.thumb
 966              		.thumb_func
 968              	HAL_SPI_MspInit:
 969              	.LVL54:
 970              	.LFB132:
 536:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 971              		.loc 1 536 1 is_stmt 1 view -0
 972              		.cfi_startproc
 973              		@ args = 0, pretend = 0, frame = 0
 974              		@ frame_needed = 0, uses_anonymous_args = 0
 975              		@ link register save eliminated.
 538:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 976              		.loc 1 538 3 view .LVU273
 543:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 977              		.loc 1 543 1 is_stmt 0 view .LVU274
 978 0000 7047     		bx	lr
 979              		.cfi_endproc
 980              	.LFE132:
 982              		.section	.text.HAL_SPI_Init,"ax",%progbits
 983              		.align	1
 984              		.global	HAL_SPI_Init
 985              		.syntax unified
 986              		.thumb
 987              		.thumb_func
 989              	HAL_SPI_Init:
 990              	.LVL55:
 991              	.LFB130:
 317:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t frxth;
 992              		.loc 1 317 1 is_stmt 1 view -0
 993              		.cfi_startproc
 994              		@ args = 0, pretend = 0, frame = 0
 995              		@ frame_needed = 0, uses_anonymous_args = 0
 318:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 996              		.loc 1 318 3 view .LVU276
 321:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 997              		.loc 1 321 3 view .LVU277
ARM GAS  /tmp/ccqUhOmw.s 			page 98


 321:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 998              		.loc 1 321 6 is_stmt 0 view .LVU278
 999 0000 0028     		cmp	r0, #0
 1000 0002 6FD0     		beq	.L88
 317:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t frxth;
 1001              		.loc 1 317 1 view .LVU279
 1002 0004 10B5     		push	{r4, lr}
 1003              		.cfi_def_cfa_offset 8
 1004              		.cfi_offset 4, -8
 1005              		.cfi_offset 14, -4
 1006 0006 0446     		mov	r4, r0
 327:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_MODE(hspi->Init.Mode));
 1007              		.loc 1 327 3 is_stmt 1 view .LVU280
 328:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DIRECTION(hspi->Init.Direction));
 1008              		.loc 1 328 3 view .LVU281
 329:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DATASIZE(hspi->Init.DataSize));
 1009              		.loc 1 329 3 view .LVU282
 330:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_NSS(hspi->Init.NSS));
 1010              		.loc 1 330 3 view .LVU283
 331:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_NSSP(hspi->Init.NSSPMode));
 1011              		.loc 1 331 3 view .LVU284
 332:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_BAUDRATE_PRESCALER(hspi->Init.BaudRatePrescaler));
 1012              		.loc 1 332 3 view .LVU285
 333:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_FIRST_BIT(hspi->Init.FirstBit));
 1013              		.loc 1 333 3 view .LVU286
 334:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_TIMODE(hspi->Init.TIMode));
 1014              		.loc 1 334 3 view .LVU287
 335:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.TIMode == SPI_TIMODE_DISABLE)
 1015              		.loc 1 335 3 view .LVU288
 336:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1016              		.loc 1 336 3 view .LVU289
 336:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1017              		.loc 1 336 17 is_stmt 0 view .LVU290
 1018 0008 436A     		ldr	r3, [r0, #36]
 336:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1019              		.loc 1 336 6 view .LVU291
 1020 000a 33B9     		cbnz	r3, .L83
 338:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     assert_param(IS_SPI_CPHA(hspi->Init.CLKPhase));
 1021              		.loc 1 338 5 is_stmt 1 view .LVU292
 339:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1022              		.loc 1 339 5 view .LVU293
 341:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1023              		.loc 1 341 5 view .LVU294
 341:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1024              		.loc 1 341 19 is_stmt 0 view .LVU295
 1025 000c 4368     		ldr	r3, [r0, #4]
 341:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1026              		.loc 1 341 8 view .LVU296
 1027 000e B3F5827F 		cmp	r3, #260
 1028 0012 05D0     		beq	.L84
 348:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 1029              		.loc 1 348 7 is_stmt 1 view .LVU297
 348:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 1030              		.loc 1 348 36 is_stmt 0 view .LVU298
 1031 0014 0023     		movs	r3, #0
 1032 0016 C361     		str	r3, [r0, #28]
 1033 0018 02E0     		b	.L84
ARM GAS  /tmp/ccqUhOmw.s 			page 99


 1034              	.L83:
 353:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1035              		.loc 1 353 5 is_stmt 1 view .LVU299
 356:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->Init.CLKPhase    = SPI_PHASE_1EDGE;
 1036              		.loc 1 356 5 view .LVU300
 356:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->Init.CLKPhase    = SPI_PHASE_1EDGE;
 1037              		.loc 1 356 28 is_stmt 0 view .LVU301
 1038 001a 0023     		movs	r3, #0
 1039 001c 0361     		str	r3, [r0, #16]
 357:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1040              		.loc 1 357 5 is_stmt 1 view .LVU302
 357:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1041              		.loc 1 357 28 is_stmt 0 view .LVU303
 1042 001e 4361     		str	r3, [r0, #20]
 1043              	.L84:
 367:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 1044              		.loc 1 367 3 is_stmt 1 view .LVU304
 367:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_SPI_CRC */
 1045              		.loc 1 367 29 is_stmt 0 view .LVU305
 1046 0020 0023     		movs	r3, #0
 1047 0022 A362     		str	r3, [r4, #40]
 370:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1048              		.loc 1 370 3 is_stmt 1 view .LVU306
 370:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1049              		.loc 1 370 11 is_stmt 0 view .LVU307
 1050 0024 94F85D30 		ldrb	r3, [r4, #93]	@ zero_extendqisi2
 370:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1051              		.loc 1 370 6 view .LVU308
 1052 0028 002B     		cmp	r3, #0
 1053 002a 52D0     		beq	.L94
 1054              	.LVL56:
 1055              	.L85:
 399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1056              		.loc 1 399 3 is_stmt 1 view .LVU309
 399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1057              		.loc 1 399 15 is_stmt 0 view .LVU310
 1058 002c 0223     		movs	r3, #2
 1059 002e 84F85D30 		strb	r3, [r4, #93]
 402:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1060              		.loc 1 402 3 is_stmt 1 view .LVU311
 1061 0032 2268     		ldr	r2, [r4]
 1062 0034 1368     		ldr	r3, [r2]
 1063 0036 23F04003 		bic	r3, r3, #64
 1064 003a 1360     		str	r3, [r2]
 405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1065              		.loc 1 405 3 view .LVU312
 405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1066              		.loc 1 405 17 is_stmt 0 view .LVU313
 1067 003c E368     		ldr	r3, [r4, #12]
 405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1068              		.loc 1 405 6 view .LVU314
 1069 003e B3F5E06F 		cmp	r3, #1792
 1070 0042 4CD9     		bls	.L89
 407:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1071              		.loc 1 407 11 view .LVU315
 1072 0044 0022     		movs	r2, #0
 1073              	.L86:
ARM GAS  /tmp/ccqUhOmw.s 			page 100


 1074              	.LVL57:
 415:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1075              		.loc 1 415 3 is_stmt 1 view .LVU316
 415:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1076              		.loc 1 415 6 is_stmt 0 view .LVU317
 1077 0046 B3F5706F 		cmp	r3, #3840
 1078 004a 04D0     		beq	.L87
 415:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1079              		.loc 1 415 51 discriminator 1 view .LVU318
 1080 004c B3F5E06F 		cmp	r3, #1792
 1081 0050 01D0     		beq	.L87
 418:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1082              		.loc 1 418 5 is_stmt 1 view .LVU319
 418:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1083              		.loc 1 418 31 is_stmt 0 view .LVU320
 1084 0052 0023     		movs	r3, #0
 1085 0054 A362     		str	r3, [r4, #40]
 1086              	.L87:
 424:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.Direction & (SPI_CR1_RXONLY | SPI_CR1_BIDIMODE)) |
 1087              		.loc 1 424 3 is_stmt 1 view .LVU321
 1088 0056 6368     		ldr	r3, [r4, #4]
 1089 0058 03F48273 		and	r3, r3, #260
 1090 005c A168     		ldr	r1, [r4, #8]
 1091 005e 01F40441 		and	r1, r1, #33792
 1092 0062 0B43     		orrs	r3, r3, r1
 1093 0064 2169     		ldr	r1, [r4, #16]
 1094 0066 01F00201 		and	r1, r1, #2
 1095 006a 0B43     		orrs	r3, r3, r1
 1096 006c 6169     		ldr	r1, [r4, #20]
 1097 006e 01F00101 		and	r1, r1, #1
 1098 0072 0B43     		orrs	r3, r3, r1
 1099 0074 A169     		ldr	r1, [r4, #24]
 1100 0076 01F40071 		and	r1, r1, #512
 1101 007a 0B43     		orrs	r3, r3, r1
 1102 007c E169     		ldr	r1, [r4, #28]
 1103 007e 01F03801 		and	r1, r1, #56
 1104 0082 0B43     		orrs	r3, r3, r1
 1105 0084 216A     		ldr	r1, [r4, #32]
 1106 0086 01F08001 		and	r1, r1, #128
 1107 008a 0B43     		orrs	r3, r3, r1
 1108 008c A16A     		ldr	r1, [r4, #40]
 1109 008e 01F40051 		and	r1, r1, #8192
 1110 0092 2068     		ldr	r0, [r4]
 1111 0094 0B43     		orrs	r3, r3, r1
 1112 0096 0360     		str	r3, [r0]
 459:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.TIMode & SPI_CR2_FRF) |
 1113              		.loc 1 459 3 view .LVU322
 1114 0098 638B     		ldrh	r3, [r4, #26]
 1115 009a 03F00403 		and	r3, r3, #4
 1116 009e 616A     		ldr	r1, [r4, #36]
 1117 00a0 01F01001 		and	r1, r1, #16
 1118 00a4 0B43     		orrs	r3, r3, r1
 1119 00a6 616B     		ldr	r1, [r4, #52]
 1120 00a8 01F00801 		and	r1, r1, #8
 1121 00ac 0B43     		orrs	r3, r3, r1
 1122 00ae E168     		ldr	r1, [r4, #12]
 1123 00b0 01F47061 		and	r1, r1, #3840
ARM GAS  /tmp/ccqUhOmw.s 			page 101


 1124 00b4 0B43     		orrs	r3, r3, r1
 1125 00b6 2168     		ldr	r1, [r4]
 1126 00b8 1A43     		orrs	r2, r2, r3
 1127              	.LVL58:
 459:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                   (hspi->Init.TIMode & SPI_CR2_FRF) |
 1128              		.loc 1 459 3 is_stmt 0 view .LVU323
 1129 00ba 4A60     		str	r2, [r1, #4]
 476:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* SPI_I2SCFGR_I2SMOD */
 1130              		.loc 1 476 3 is_stmt 1 view .LVU324
 1131 00bc 2268     		ldr	r2, [r4]
 1132 00be D369     		ldr	r3, [r2, #28]
 1133 00c0 23F40063 		bic	r3, r3, #2048
 1134 00c4 D361     		str	r3, [r2, #28]
 479:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State     = HAL_SPI_STATE_READY;
 1135              		.loc 1 479 3 view .LVU325
 479:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State     = HAL_SPI_STATE_READY;
 1136              		.loc 1 479 19 is_stmt 0 view .LVU326
 1137 00c6 0020     		movs	r0, #0
 1138 00c8 2066     		str	r0, [r4, #96]
 480:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1139              		.loc 1 480 3 is_stmt 1 view .LVU327
 480:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1140              		.loc 1 480 19 is_stmt 0 view .LVU328
 1141 00ca 0123     		movs	r3, #1
 1142 00cc 84F85D30 		strb	r3, [r4, #93]
 482:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 1143              		.loc 1 482 3 is_stmt 1 view .LVU329
 483:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1144              		.loc 1 483 1 is_stmt 0 view .LVU330
 1145 00d0 10BD     		pop	{r4, pc}
 1146              	.LVL59:
 1147              	.L94:
 373:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1148              		.loc 1 373 5 is_stmt 1 view .LVU331
 373:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1149              		.loc 1 373 16 is_stmt 0 view .LVU332
 1150 00d2 84F85C30 		strb	r3, [r4, #92]
 395:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 1151              		.loc 1 395 5 is_stmt 1 view .LVU333
 1152 00d6 2046     		mov	r0, r4
 1153              	.LVL60:
 395:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 1154              		.loc 1 395 5 is_stmt 0 view .LVU334
 1155 00d8 FFF7FEFF 		bl	HAL_SPI_MspInit
 1156              	.LVL61:
 1157 00dc A6E7     		b	.L85
 1158              	.L89:
 411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1159              		.loc 1 411 11 view .LVU335
 1160 00de 4FF48052 		mov	r2, #4096
 1161 00e2 B0E7     		b	.L86
 1162              	.LVL62:
 1163              	.L88:
 1164              		.cfi_def_cfa_offset 0
 1165              		.cfi_restore 4
 1166              		.cfi_restore 14
 323:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
ARM GAS  /tmp/ccqUhOmw.s 			page 102


 1167              		.loc 1 323 12 view .LVU336
 1168 00e4 0120     		movs	r0, #1
 1169              	.LVL63:
 483:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1170              		.loc 1 483 1 view .LVU337
 1171 00e6 7047     		bx	lr
 1172              		.cfi_endproc
 1173              	.LFE130:
 1175              		.section	.text.HAL_SPI_MspDeInit,"ax",%progbits
 1176              		.align	1
 1177              		.weak	HAL_SPI_MspDeInit
 1178              		.syntax unified
 1179              		.thumb
 1180              		.thumb_func
 1182              	HAL_SPI_MspDeInit:
 1183              	.LVL64:
 1184              	.LFB133:
 552:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 1185              		.loc 1 552 1 is_stmt 1 view -0
 1186              		.cfi_startproc
 1187              		@ args = 0, pretend = 0, frame = 0
 1188              		@ frame_needed = 0, uses_anonymous_args = 0
 1189              		@ link register save eliminated.
 554:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1190              		.loc 1 554 3 view .LVU339
 559:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1191              		.loc 1 559 1 is_stmt 0 view .LVU340
 1192 0000 7047     		bx	lr
 1193              		.cfi_endproc
 1194              	.LFE133:
 1196              		.section	.text.HAL_SPI_DeInit,"ax",%progbits
 1197              		.align	1
 1198              		.global	HAL_SPI_DeInit
 1199              		.syntax unified
 1200              		.thumb
 1201              		.thumb_func
 1203              	HAL_SPI_DeInit:
 1204              	.LVL65:
 1205              	.LFB131:
 492:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the SPI handle allocation */
 1206              		.loc 1 492 1 is_stmt 1 view -0
 1207              		.cfi_startproc
 1208              		@ args = 0, pretend = 0, frame = 0
 1209              		@ frame_needed = 0, uses_anonymous_args = 0
 494:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1210              		.loc 1 494 3 view .LVU342
 494:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1211              		.loc 1 494 6 is_stmt 0 view .LVU343
 1212 0000 90B1     		cbz	r0, .L98
 492:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Check the SPI handle allocation */
 1213              		.loc 1 492 1 view .LVU344
 1214 0002 10B5     		push	{r4, lr}
 1215              		.cfi_def_cfa_offset 8
 1216              		.cfi_offset 4, -8
 1217              		.cfi_offset 14, -4
 1218 0004 0446     		mov	r4, r0
 500:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/ccqUhOmw.s 			page 103


 1219              		.loc 1 500 3 is_stmt 1 view .LVU345
 502:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1220              		.loc 1 502 3 view .LVU346
 502:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1221              		.loc 1 502 15 is_stmt 0 view .LVU347
 1222 0006 0223     		movs	r3, #2
 1223 0008 80F85D30 		strb	r3, [r0, #93]
 505:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1224              		.loc 1 505 3 is_stmt 1 view .LVU348
 1225 000c 0268     		ldr	r2, [r0]
 1226 000e 1368     		ldr	r3, [r2]
 1227 0010 23F04003 		bic	r3, r3, #64
 1228 0014 1360     		str	r3, [r2]
 517:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 1229              		.loc 1 517 3 view .LVU349
 1230 0016 FFF7FEFF 		bl	HAL_SPI_MspDeInit
 1231              	.LVL66:
 520:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_RESET;
 1232              		.loc 1 520 3 view .LVU350
 520:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_RESET;
 1233              		.loc 1 520 19 is_stmt 0 view .LVU351
 1234 001a 0020     		movs	r0, #0
 1235 001c 2066     		str	r0, [r4, #96]
 521:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1236              		.loc 1 521 3 is_stmt 1 view .LVU352
 521:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1237              		.loc 1 521 15 is_stmt 0 view .LVU353
 1238 001e 84F85D00 		strb	r0, [r4, #93]
 524:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1239              		.loc 1 524 3 is_stmt 1 view .LVU354
 524:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1240              		.loc 1 524 3 view .LVU355
 1241 0022 84F85C00 		strb	r0, [r4, #92]
 524:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1242              		.loc 1 524 3 view .LVU356
 526:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 1243              		.loc 1 526 3 view .LVU357
 527:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1244              		.loc 1 527 1 is_stmt 0 view .LVU358
 1245 0026 10BD     		pop	{r4, pc}
 1246              	.LVL67:
 1247              	.L98:
 1248              		.cfi_def_cfa_offset 0
 1249              		.cfi_restore 4
 1250              		.cfi_restore 14
 496:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1251              		.loc 1 496 12 view .LVU359
 1252 0028 0120     		movs	r0, #1
 1253              	.LVL68:
 527:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1254              		.loc 1 527 1 view .LVU360
 1255 002a 7047     		bx	lr
 1256              		.cfi_endproc
 1257              	.LFE131:
 1259              		.section	.text.HAL_SPI_Transmit,"ax",%progbits
 1260              		.align	1
 1261              		.global	HAL_SPI_Transmit
ARM GAS  /tmp/ccqUhOmw.s 			page 104


 1262              		.syntax unified
 1263              		.thumb
 1264              		.thumb_func
 1266              	HAL_SPI_Transmit:
 1267              	.LVL69:
 1268              	.LFB134:
 824:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 1269              		.loc 1 824 1 is_stmt 1 view -0
 1270              		.cfi_startproc
 1271              		@ args = 0, pretend = 0, frame = 8
 1272              		@ frame_needed = 0, uses_anonymous_args = 0
 824:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 1273              		.loc 1 824 1 is_stmt 0 view .LVU362
 1274 0000 2DE9F043 		push	{r4, r5, r6, r7, r8, r9, lr}
 1275              		.cfi_def_cfa_offset 28
 1276              		.cfi_offset 4, -28
 1277              		.cfi_offset 5, -24
 1278              		.cfi_offset 6, -20
 1279              		.cfi_offset 7, -16
 1280              		.cfi_offset 8, -12
 1281              		.cfi_offset 9, -8
 1282              		.cfi_offset 14, -4
 1283 0004 83B0     		sub	sp, sp, #12
 1284              		.cfi_def_cfa_offset 40
 1285 0006 1D46     		mov	r5, r3
 825:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 1286              		.loc 1 825 3 is_stmt 1 view .LVU363
 826:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint16_t initial_TxXferCount;
 1287              		.loc 1 826 3 view .LVU364
 1288              	.LVL70:
 827:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1289              		.loc 1 827 3 view .LVU365
 830:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1290              		.loc 1 830 3 view .LVU366
 833:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1291              		.loc 1 833 3 view .LVU367
 833:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1292              		.loc 1 833 3 view .LVU368
 1293 0008 90F85C30 		ldrb	r3, [r0, #92]	@ zero_extendqisi2
 1294              	.LVL71:
 833:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1295              		.loc 1 833 3 is_stmt 0 view .LVU369
 1296 000c 012B     		cmp	r3, #1
 1297 000e 00F0F680 		beq	.L128
 1298 0012 0446     		mov	r4, r0
 1299 0014 8846     		mov	r8, r1
 1300 0016 9146     		mov	r9, r2
 833:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1301              		.loc 1 833 3 is_stmt 1 discriminator 2 view .LVU370
 1302 0018 0123     		movs	r3, #1
 1303 001a 80F85C30 		strb	r3, [r0, #92]
 833:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1304              		.loc 1 833 3 discriminator 2 view .LVU371
 836:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   initial_TxXferCount = Size;
 1305              		.loc 1 836 3 discriminator 2 view .LVU372
 836:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   initial_TxXferCount = Size;
 1306              		.loc 1 836 15 is_stmt 0 discriminator 2 view .LVU373
ARM GAS  /tmp/ccqUhOmw.s 			page 105


 1307 001e FFF7FEFF 		bl	HAL_GetTick
 1308              	.LVL72:
 836:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   initial_TxXferCount = Size;
 1309              		.loc 1 836 15 discriminator 2 view .LVU374
 1310 0022 0746     		mov	r7, r0
 1311              	.LVL73:
 837:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1312              		.loc 1 837 3 is_stmt 1 discriminator 2 view .LVU375
 839:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1313              		.loc 1 839 3 discriminator 2 view .LVU376
 839:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1314              		.loc 1 839 11 is_stmt 0 discriminator 2 view .LVU377
 1315 0024 94F85D60 		ldrb	r6, [r4, #93]	@ zero_extendqisi2
 1316 0028 F6B2     		uxtb	r6, r6
 839:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1317              		.loc 1 839 6 discriminator 2 view .LVU378
 1318 002a 012E     		cmp	r6, #1
 1319 002c 40F0D480 		bne	.L129
 845:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1320              		.loc 1 845 3 is_stmt 1 view .LVU379
 845:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1321              		.loc 1 845 6 is_stmt 0 view .LVU380
 1322 0030 B8F1000F 		cmp	r8, #0
 1323 0034 00F0D180 		beq	.L105
 845:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1324              		.loc 1 845 23 discriminator 1 view .LVU381
 1325 0038 B9F1000F 		cmp	r9, #0
 1326 003c 00F0CD80 		beq	.L105
 852:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 1327              		.loc 1 852 3 is_stmt 1 view .LVU382
 852:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 1328              		.loc 1 852 21 is_stmt 0 view .LVU383
 1329 0040 0323     		movs	r3, #3
 1330 0042 84F85D30 		strb	r3, [r4, #93]
 853:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pData;
 1331              		.loc 1 853 3 is_stmt 1 view .LVU384
 853:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pData;
 1332              		.loc 1 853 21 is_stmt 0 view .LVU385
 1333 0046 0023     		movs	r3, #0
 1334 0048 2366     		str	r3, [r4, #96]
 854:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 1335              		.loc 1 854 3 is_stmt 1 view .LVU386
 854:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 1336              		.loc 1 854 21 is_stmt 0 view .LVU387
 1337 004a C4F83880 		str	r8, [r4, #56]
 855:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 1338              		.loc 1 855 3 is_stmt 1 view .LVU388
 855:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 1339              		.loc 1 855 21 is_stmt 0 view .LVU389
 1340 004e A4F83C90 		strh	r9, [r4, #60]	@ movhi
 856:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1341              		.loc 1 856 3 is_stmt 1 view .LVU390
 856:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1342              		.loc 1 856 21 is_stmt 0 view .LVU391
 1343 0052 A4F83E90 		strh	r9, [r4, #62]	@ movhi
 859:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = 0U;
 1344              		.loc 1 859 3 is_stmt 1 view .LVU392
ARM GAS  /tmp/ccqUhOmw.s 			page 106


 859:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = 0U;
 1345              		.loc 1 859 21 is_stmt 0 view .LVU393
 1346 0056 2364     		str	r3, [r4, #64]
 860:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
 1347              		.loc 1 860 3 is_stmt 1 view .LVU394
 860:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
 1348              		.loc 1 860 21 is_stmt 0 view .LVU395
 1349 0058 A4F84430 		strh	r3, [r4, #68]	@ movhi
 861:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 1350              		.loc 1 861 3 is_stmt 1 view .LVU396
 861:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 1351              		.loc 1 861 21 is_stmt 0 view .LVU397
 1352 005c A4F84630 		strh	r3, [r4, #70]	@ movhi
 862:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
 1353              		.loc 1 862 3 is_stmt 1 view .LVU398
 862:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
 1354              		.loc 1 862 21 is_stmt 0 view .LVU399
 1355 0060 2365     		str	r3, [r4, #80]
 863:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1356              		.loc 1 863 3 is_stmt 1 view .LVU400
 863:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1357              		.loc 1 863 21 is_stmt 0 view .LVU401
 1358 0062 E364     		str	r3, [r4, #76]
 866:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1359              		.loc 1 866 3 is_stmt 1 view .LVU402
 866:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1360              		.loc 1 866 17 is_stmt 0 view .LVU403
 1361 0064 A368     		ldr	r3, [r4, #8]
 866:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1362              		.loc 1 866 6 view .LVU404
 1363 0066 B3F5004F 		cmp	r3, #32768
 1364 006a 1ED0     		beq	.L135
 1365              	.L106:
 882:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1366              		.loc 1 882 3 is_stmt 1 view .LVU405
 882:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1367              		.loc 1 882 12 is_stmt 0 view .LVU406
 1368 006c 2368     		ldr	r3, [r4]
 882:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1369              		.loc 1 882 22 view .LVU407
 1370 006e 1A68     		ldr	r2, [r3]
 882:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1371              		.loc 1 882 6 view .LVU408
 1372 0070 12F0400F 		tst	r2, #64
 1373 0074 03D1     		bne	.L107
 885:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1374              		.loc 1 885 5 is_stmt 1 view .LVU409
 1375 0076 1A68     		ldr	r2, [r3]
 1376 0078 42F04002 		orr	r2, r2, #64
 1377 007c 1A60     		str	r2, [r3]
 1378              	.L107:
 889:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1379              		.loc 1 889 3 view .LVU410
 889:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1380              		.loc 1 889 17 is_stmt 0 view .LVU411
 1381 007e E368     		ldr	r3, [r4, #12]
 889:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/ccqUhOmw.s 			page 107


 1382              		.loc 1 889 6 view .LVU412
 1383 0080 B3F5E06F 		cmp	r3, #1792
 1384 0084 42D9     		bls	.L108
 891:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1385              		.loc 1 891 5 is_stmt 1 view .LVU413
 891:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1386              		.loc 1 891 20 is_stmt 0 view .LVU414
 1387 0086 6368     		ldr	r3, [r4, #4]
 891:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1388              		.loc 1 891 8 view .LVU415
 1389 0088 13B1     		cbz	r3, .L109
 891:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1390              		.loc 1 891 45 discriminator 1 view .LVU416
 1391 008a B9F1010F 		cmp	r9, #1
 1392 008e 23D1     		bne	.L111
 1393              	.L109:
 893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
 1394              		.loc 1 893 7 is_stmt 1 view .LVU417
 893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
 1395              		.loc 1 893 46 is_stmt 0 view .LVU418
 1396 0090 A26B     		ldr	r2, [r4, #56]
 893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
 1397              		.loc 1 893 11 view .LVU419
 1398 0092 2368     		ldr	r3, [r4]
 893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
 1399              		.loc 1 893 28 view .LVU420
 1400 0094 1288     		ldrh	r2, [r2]
 893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
 1401              		.loc 1 893 26 view .LVU421
 1402 0096 DA60     		str	r2, [r3, #12]
 894:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount--;
 1403              		.loc 1 894 7 is_stmt 1 view .LVU422
 894:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount--;
 1404              		.loc 1 894 11 is_stmt 0 view .LVU423
 1405 0098 A36B     		ldr	r3, [r4, #56]
 894:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount--;
 1406              		.loc 1 894 24 view .LVU424
 1407 009a 0233     		adds	r3, r3, #2
 1408 009c A363     		str	r3, [r4, #56]
 895:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 1409              		.loc 1 895 7 is_stmt 1 view .LVU425
 895:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 1410              		.loc 1 895 11 is_stmt 0 view .LVU426
 1411 009e E38F     		ldrh	r3, [r4, #62]
 1412 00a0 9BB2     		uxth	r3, r3
 895:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 1413              		.loc 1 895 24 view .LVU427
 1414 00a2 013B     		subs	r3, r3, #1
 1415 00a4 9BB2     		uxth	r3, r3
 1416 00a6 E387     		strh	r3, [r4, #62]	@ movhi
 1417 00a8 16E0     		b	.L111
 1418              	.L135:
 869:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_TX(hspi);
 1419              		.loc 1 869 5 is_stmt 1 view .LVU428
 1420 00aa 2268     		ldr	r2, [r4]
 1421 00ac 1368     		ldr	r3, [r2]
 1422 00ae 23F04003 		bic	r3, r3, #64
ARM GAS  /tmp/ccqUhOmw.s 			page 108


 1423 00b2 1360     		str	r3, [r2]
 870:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1424              		.loc 1 870 5 view .LVU429
 1425 00b4 2268     		ldr	r2, [r4]
 1426 00b6 1368     		ldr	r3, [r2]
 1427 00b8 43F48043 		orr	r3, r3, #16384
 1428 00bc 1360     		str	r3, [r2]
 1429 00be D5E7     		b	.L106
 1430              	.LVL74:
 1431              	.L112:
 910:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1432              		.loc 1 910 9 view .LVU430
 910:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1433              		.loc 1 910 16 is_stmt 0 view .LVU431
 1434 00c0 FFF7FEFF 		bl	HAL_GetTick
 1435              	.LVL75:
 910:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1436              		.loc 1 910 30 view .LVU432
 1437 00c4 C01B     		subs	r0, r0, r7
 910:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1438              		.loc 1 910 12 view .LVU433
 1439 00c6 A842     		cmp	r0, r5
 1440 00c8 03D3     		bcc	.L114
 910:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1441              		.loc 1 910 56 discriminator 1 view .LVU434
 1442 00ca B5F1FF3F 		cmp	r5, #-1
 1443 00ce 40F08E80 		bne	.L130
 1444              	.L114:
 910:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1445              		.loc 1 910 87 discriminator 3 view .LVU435
 1446 00d2 002D     		cmp	r5, #0
 1447 00d4 00F08D80 		beq	.L131
 1448              	.L111:
 898:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1449              		.loc 1 898 30 is_stmt 1 view .LVU436
 898:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1450              		.loc 1 898 16 is_stmt 0 view .LVU437
 1451 00d8 E38F     		ldrh	r3, [r4, #62]
 1452 00da 9BB2     		uxth	r3, r3
 898:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1453              		.loc 1 898 30 view .LVU438
 1454 00dc 002B     		cmp	r3, #0
 1455 00de 66D0     		beq	.L116
 901:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1456              		.loc 1 901 7 is_stmt 1 view .LVU439
 901:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1457              		.loc 1 901 11 is_stmt 0 view .LVU440
 1458 00e0 2368     		ldr	r3, [r4]
 1459 00e2 9A68     		ldr	r2, [r3, #8]
 901:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1460              		.loc 1 901 10 view .LVU441
 1461 00e4 12F0020F 		tst	r2, #2
 1462 00e8 EAD0     		beq	.L112
 903:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1463              		.loc 1 903 9 is_stmt 1 view .LVU442
 903:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1464              		.loc 1 903 48 is_stmt 0 view .LVU443
ARM GAS  /tmp/ccqUhOmw.s 			page 109


 1465 00ea A26B     		ldr	r2, [r4, #56]
 903:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1466              		.loc 1 903 30 view .LVU444
 1467 00ec 1288     		ldrh	r2, [r2]
 903:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1468              		.loc 1 903 28 view .LVU445
 1469 00ee DA60     		str	r2, [r3, #12]
 904:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 1470              		.loc 1 904 9 is_stmt 1 view .LVU446
 904:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 1471              		.loc 1 904 13 is_stmt 0 view .LVU447
 1472 00f0 A36B     		ldr	r3, [r4, #56]
 904:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 1473              		.loc 1 904 26 view .LVU448
 1474 00f2 0233     		adds	r3, r3, #2
 1475 00f4 A363     		str	r3, [r4, #56]
 905:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 1476              		.loc 1 905 9 is_stmt 1 view .LVU449
 905:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 1477              		.loc 1 905 13 is_stmt 0 view .LVU450
 1478 00f6 B4F83EC0 		ldrh	ip, [r4, #62]
 1479 00fa 1FFA8CFC 		uxth	ip, ip
 905:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 1480              		.loc 1 905 26 view .LVU451
 1481 00fe 0CF1FF3C 		add	ip, ip, #-1
 1482 0102 1FFA8CFC 		uxth	ip, ip
 1483 0106 A4F83EC0 		strh	ip, [r4, #62]	@ movhi
 1484 010a E5E7     		b	.L111
 1485              	.LVL76:
 1486              	.L108:
 921:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1487              		.loc 1 921 5 is_stmt 1 view .LVU452
 921:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1488              		.loc 1 921 20 is_stmt 0 view .LVU453
 1489 010c 6368     		ldr	r3, [r4, #4]
 921:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1490              		.loc 1 921 8 view .LVU454
 1491 010e 13B1     		cbz	r3, .L117
 921:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1492              		.loc 1 921 45 discriminator 1 view .LVU455
 1493 0110 B9F1010F 		cmp	r9, #1
 1494 0114 33D1     		bne	.L120
 1495              	.L117:
 923:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1496              		.loc 1 923 7 is_stmt 1 view .LVU456
 923:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1497              		.loc 1 923 15 is_stmt 0 view .LVU457
 1498 0116 E38F     		ldrh	r3, [r4, #62]
 1499 0118 9BB2     		uxth	r3, r3
 923:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1500              		.loc 1 923 10 view .LVU458
 1501 011a 012B     		cmp	r3, #1
 1502 011c 0CD9     		bls	.L119
 926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1503              		.loc 1 926 9 is_stmt 1 view .LVU459
 926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1504              		.loc 1 926 48 is_stmt 0 view .LVU460
ARM GAS  /tmp/ccqUhOmw.s 			page 110


 1505 011e A26B     		ldr	r2, [r4, #56]
 926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1506              		.loc 1 926 13 view .LVU461
 1507 0120 2368     		ldr	r3, [r4]
 926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1508              		.loc 1 926 30 view .LVU462
 1509 0122 1288     		ldrh	r2, [r2]
 926:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1510              		.loc 1 926 28 view .LVU463
 1511 0124 DA60     		str	r2, [r3, #12]
 927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount -= 2U;
 1512              		.loc 1 927 9 is_stmt 1 view .LVU464
 927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount -= 2U;
 1513              		.loc 1 927 13 is_stmt 0 view .LVU465
 1514 0126 A36B     		ldr	r3, [r4, #56]
 927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount -= 2U;
 1515              		.loc 1 927 26 view .LVU466
 1516 0128 0233     		adds	r3, r3, #2
 1517 012a A363     		str	r3, [r4, #56]
 928:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 1518              		.loc 1 928 9 is_stmt 1 view .LVU467
 928:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 1519              		.loc 1 928 13 is_stmt 0 view .LVU468
 1520 012c E38F     		ldrh	r3, [r4, #62]
 1521 012e 9BB2     		uxth	r3, r3
 928:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 1522              		.loc 1 928 27 view .LVU469
 1523 0130 023B     		subs	r3, r3, #2
 1524 0132 9BB2     		uxth	r3, r3
 1525 0134 E387     		strh	r3, [r4, #62]	@ movhi
 1526 0136 22E0     		b	.L120
 1527              	.L119:
 932:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr ++;
 1528              		.loc 1 932 9 is_stmt 1 view .LVU470
 932:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr ++;
 1529              		.loc 1 932 56 is_stmt 0 view .LVU471
 1530 0138 A26B     		ldr	r2, [r4, #56]
 932:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr ++;
 1531              		.loc 1 932 32 view .LVU472
 1532 013a 2368     		ldr	r3, [r4]
 932:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr ++;
 1533              		.loc 1 932 51 view .LVU473
 1534 013c 1278     		ldrb	r2, [r2]	@ zero_extendqisi2
 932:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr ++;
 1535              		.loc 1 932 48 view .LVU474
 1536 013e 1A73     		strb	r2, [r3, #12]
 933:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 1537              		.loc 1 933 9 is_stmt 1 view .LVU475
 933:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 1538              		.loc 1 933 13 is_stmt 0 view .LVU476
 1539 0140 A36B     		ldr	r3, [r4, #56]
 933:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 1540              		.loc 1 933 26 view .LVU477
 1541 0142 0133     		adds	r3, r3, #1
 1542 0144 A363     		str	r3, [r4, #56]
 934:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 1543              		.loc 1 934 9 is_stmt 1 view .LVU478
ARM GAS  /tmp/ccqUhOmw.s 			page 111


 934:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 1544              		.loc 1 934 13 is_stmt 0 view .LVU479
 1545 0146 E38F     		ldrh	r3, [r4, #62]
 1546 0148 9BB2     		uxth	r3, r3
 934:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 1547              		.loc 1 934 26 view .LVU480
 1548 014a 013B     		subs	r3, r3, #1
 1549 014c 9BB2     		uxth	r3, r3
 1550 014e E387     		strh	r3, [r4, #62]	@ movhi
 1551 0150 15E0     		b	.L120
 1552              	.LVL77:
 1553              	.L122:
 951:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr++;
 1554              		.loc 1 951 11 is_stmt 1 view .LVU481
 951:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr++;
 1555              		.loc 1 951 58 is_stmt 0 view .LVU482
 1556 0152 A36B     		ldr	r3, [r4, #56]
 951:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr++;
 1557              		.loc 1 951 53 view .LVU483
 1558 0154 1B78     		ldrb	r3, [r3]	@ zero_extendqisi2
 951:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr++;
 1559              		.loc 1 951 50 view .LVU484
 1560 0156 1373     		strb	r3, [r2, #12]
 952:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount--;
 1561              		.loc 1 952 11 is_stmt 1 view .LVU485
 952:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount--;
 1562              		.loc 1 952 15 is_stmt 0 view .LVU486
 1563 0158 A36B     		ldr	r3, [r4, #56]
 952:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount--;
 1564              		.loc 1 952 27 view .LVU487
 1565 015a 0133     		adds	r3, r3, #1
 1566 015c A363     		str	r3, [r4, #56]
 953:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 1567              		.loc 1 953 11 is_stmt 1 view .LVU488
 953:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 1568              		.loc 1 953 15 is_stmt 0 view .LVU489
 1569 015e E38F     		ldrh	r3, [r4, #62]
 1570 0160 9BB2     		uxth	r3, r3
 953:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 1571              		.loc 1 953 28 view .LVU490
 1572 0162 013B     		subs	r3, r3, #1
 1573 0164 9BB2     		uxth	r3, r3
 1574 0166 E387     		strh	r3, [r4, #62]	@ movhi
 1575 0168 09E0     		b	.L120
 1576              	.L121:
 959:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1577              		.loc 1 959 9 is_stmt 1 view .LVU491
 959:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1578              		.loc 1 959 16 is_stmt 0 view .LVU492
 1579 016a FFF7FEFF 		bl	HAL_GetTick
 1580              	.LVL78:
 959:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1581              		.loc 1 959 30 view .LVU493
 1582 016e C01B     		subs	r0, r0, r7
 959:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1583              		.loc 1 959 12 view .LVU494
 1584 0170 A842     		cmp	r0, r5
ARM GAS  /tmp/ccqUhOmw.s 			page 112


 1585 0172 02D3     		bcc	.L124
 959:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1586              		.loc 1 959 56 discriminator 1 view .LVU495
 1587 0174 B5F1FF3F 		cmp	r5, #-1
 1588 0178 3DD1     		bne	.L132
 1589              	.L124:
 959:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1590              		.loc 1 959 87 discriminator 3 view .LVU496
 1591 017a 002D     		cmp	r5, #0
 1592 017c 3DD0     		beq	.L133
 1593              	.L120:
 937:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1594              		.loc 1 937 30 is_stmt 1 view .LVU497
 937:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1595              		.loc 1 937 16 is_stmt 0 view .LVU498
 1596 017e E38F     		ldrh	r3, [r4, #62]
 1597 0180 9BB2     		uxth	r3, r3
 937:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1598              		.loc 1 937 30 view .LVU499
 1599 0182 A3B1     		cbz	r3, .L116
 940:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1600              		.loc 1 940 7 is_stmt 1 view .LVU500
 940:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1601              		.loc 1 940 11 is_stmt 0 view .LVU501
 1602 0184 2268     		ldr	r2, [r4]
 1603 0186 9368     		ldr	r3, [r2, #8]
 940:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1604              		.loc 1 940 10 view .LVU502
 1605 0188 13F0020F 		tst	r3, #2
 1606 018c EDD0     		beq	.L121
 942:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1607              		.loc 1 942 9 is_stmt 1 view .LVU503
 942:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1608              		.loc 1 942 17 is_stmt 0 view .LVU504
 1609 018e E38F     		ldrh	r3, [r4, #62]
 1610 0190 9BB2     		uxth	r3, r3
 942:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 1611              		.loc 1 942 12 view .LVU505
 1612 0192 012B     		cmp	r3, #1
 1613 0194 DDD9     		bls	.L122
 945:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint16_t);
 1614              		.loc 1 945 11 is_stmt 1 view .LVU506
 945:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint16_t);
 1615              		.loc 1 945 50 is_stmt 0 view .LVU507
 1616 0196 A36B     		ldr	r3, [r4, #56]
 945:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint16_t);
 1617              		.loc 1 945 32 view .LVU508
 1618 0198 1B88     		ldrh	r3, [r3]
 945:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint16_t);
 1619              		.loc 1 945 30 view .LVU509
 1620 019a D360     		str	r3, [r2, #12]
 946:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount -= 2U;
 1621              		.loc 1 946 11 is_stmt 1 view .LVU510
 946:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount -= 2U;
 1622              		.loc 1 946 15 is_stmt 0 view .LVU511
 1623 019c A36B     		ldr	r3, [r4, #56]
 946:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount -= 2U;
ARM GAS  /tmp/ccqUhOmw.s 			page 113


 1624              		.loc 1 946 28 view .LVU512
 1625 019e 0233     		adds	r3, r3, #2
 1626 01a0 A363     		str	r3, [r4, #56]
 947:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 1627              		.loc 1 947 11 is_stmt 1 view .LVU513
 947:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 1628              		.loc 1 947 15 is_stmt 0 view .LVU514
 1629 01a2 E38F     		ldrh	r3, [r4, #62]
 1630 01a4 9BB2     		uxth	r3, r3
 947:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 1631              		.loc 1 947 29 view .LVU515
 1632 01a6 023B     		subs	r3, r3, #2
 1633 01a8 9BB2     		uxth	r3, r3
 1634 01aa E387     		strh	r3, [r4, #62]	@ movhi
 1635 01ac E7E7     		b	.L120
 1636              	.L116:
 976:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1637              		.loc 1 976 3 is_stmt 1 view .LVU516
 976:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1638              		.loc 1 976 7 is_stmt 0 view .LVU517
 1639 01ae 3A46     		mov	r2, r7
 1640 01b0 2946     		mov	r1, r5
 1641 01b2 2046     		mov	r0, r4
 1642 01b4 FFF7FEFF 		bl	SPI_EndRxTxTransaction
 1643              	.LVL79:
 976:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1644              		.loc 1 976 6 view .LVU518
 1645 01b8 08B1     		cbz	r0, .L126
 978:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1646              		.loc 1 978 5 is_stmt 1 view .LVU519
 978:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1647              		.loc 1 978 21 is_stmt 0 view .LVU520
 1648 01ba 2023     		movs	r3, #32
 1649 01bc 2366     		str	r3, [r4, #96]
 1650              	.L126:
 982:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1651              		.loc 1 982 3 is_stmt 1 view .LVU521
 982:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1652              		.loc 1 982 17 is_stmt 0 view .LVU522
 1653 01be A368     		ldr	r3, [r4, #8]
 982:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1654              		.loc 1 982 6 view .LVU523
 1655 01c0 33B9     		cbnz	r3, .L127
 984:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1656              		.loc 1 984 5 is_stmt 1 view .LVU524
 1657              	.LBB2:
 984:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1658              		.loc 1 984 5 view .LVU525
 1659 01c2 0193     		str	r3, [sp, #4]
 984:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1660              		.loc 1 984 5 view .LVU526
 1661 01c4 2368     		ldr	r3, [r4]
 1662 01c6 DA68     		ldr	r2, [r3, #12]
 1663 01c8 0192     		str	r2, [sp, #4]
 984:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1664              		.loc 1 984 5 view .LVU527
 1665 01ca 9B68     		ldr	r3, [r3, #8]
ARM GAS  /tmp/ccqUhOmw.s 			page 114


 1666 01cc 0193     		str	r3, [sp, #4]
 984:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1667              		.loc 1 984 5 view .LVU528
 1668 01ce 019B     		ldr	r3, [sp, #4]
 1669              	.L127:
 1670              	.LBE2:
 984:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1671              		.loc 1 984 5 discriminator 1 view .LVU529
 987:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1672              		.loc 1 987 3 discriminator 1 view .LVU530
 987:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1673              		.loc 1 987 11 is_stmt 0 discriminator 1 view .LVU531
 1674 01d0 236E     		ldr	r3, [r4, #96]
 987:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1675              		.loc 1 987 6 discriminator 1 view .LVU532
 1676 01d2 13B9     		cbnz	r3, .L105
 826:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint16_t initial_TxXferCount;
 1677              		.loc 1 826 21 view .LVU533
 1678 01d4 0026     		movs	r6, #0
 1679 01d6 00E0     		b	.L105
 1680              	.LVL80:
 1681              	.L129:
 841:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 1682              		.loc 1 841 15 view .LVU534
 1683 01d8 0226     		movs	r6, #2
 1684              	.LVL81:
 1685              	.L105:
 993:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Unlocked */
 1686              		.loc 1 993 3 is_stmt 1 view .LVU535
 993:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Unlocked */
 1687              		.loc 1 993 15 is_stmt 0 view .LVU536
 1688 01da 0123     		movs	r3, #1
 1689 01dc 84F85D30 		strb	r3, [r4, #93]
 995:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 1690              		.loc 1 995 3 is_stmt 1 view .LVU537
 995:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 1691              		.loc 1 995 3 view .LVU538
 1692 01e0 0023     		movs	r3, #0
 1693 01e2 84F85C30 		strb	r3, [r4, #92]
 995:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 1694              		.loc 1 995 3 view .LVU539
 996:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 1695              		.loc 1 996 3 view .LVU540
 1696              	.LVL82:
 1697              	.L104:
 997:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1698              		.loc 1 997 1 is_stmt 0 view .LVU541
 1699 01e6 3046     		mov	r0, r6
 1700 01e8 03B0     		add	sp, sp, #12
 1701              		.cfi_remember_state
 1702              		.cfi_def_cfa_offset 28
 1703              		@ sp needed
 1704 01ea BDE8F083 		pop	{r4, r5, r6, r7, r8, r9, pc}
 1705              	.LVL83:
 1706              	.L130:
 1707              		.cfi_restore_state
 912:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
ARM GAS  /tmp/ccqUhOmw.s 			page 115


 1708              		.loc 1 912 21 view .LVU542
 1709 01ee 0326     		movs	r6, #3
 1710 01f0 F3E7     		b	.L105
 1711              	.L131:
 1712 01f2 0326     		movs	r6, #3
 1713 01f4 F1E7     		b	.L105
 1714              	.L132:
 961:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
 1715              		.loc 1 961 21 view .LVU543
 1716 01f6 0326     		movs	r6, #3
 1717 01f8 EFE7     		b	.L105
 1718              	.L133:
 1719 01fa 0326     		movs	r6, #3
 1720 01fc EDE7     		b	.L105
 1721              	.LVL84:
 1722              	.L128:
 833:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1723              		.loc 1 833 3 view .LVU544
 1724 01fe 0226     		movs	r6, #2
 1725 0200 F1E7     		b	.L104
 1726              		.cfi_endproc
 1727              	.LFE134:
 1729              		.section	.text.HAL_SPI_TransmitReceive,"ax",%progbits
 1730              		.align	1
 1731              		.global	HAL_SPI_TransmitReceive
 1732              		.syntax unified
 1733              		.thumb
 1734              		.thumb_func
 1736              	HAL_SPI_TransmitReceive:
 1737              	.LVL85:
 1738              	.LFB136:
1250:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint16_t             initial_TxXferCount;
 1739              		.loc 1 1250 1 is_stmt 1 view -0
 1740              		.cfi_startproc
 1741              		@ args = 4, pretend = 0, frame = 0
 1742              		@ frame_needed = 0, uses_anonymous_args = 0
1250:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint16_t             initial_TxXferCount;
 1743              		.loc 1 1250 1 is_stmt 0 view .LVU546
 1744 0000 2DE9F843 		push	{r3, r4, r5, r6, r7, r8, r9, lr}
 1745              		.cfi_def_cfa_offset 32
 1746              		.cfi_offset 3, -32
 1747              		.cfi_offset 4, -28
 1748              		.cfi_offset 5, -24
 1749              		.cfi_offset 6, -20
 1750              		.cfi_offset 7, -16
 1751              		.cfi_offset 8, -12
 1752              		.cfi_offset 9, -8
 1753              		.cfi_offset 14, -4
 1754 0004 1F46     		mov	r7, r3
 1755 0006 089D     		ldr	r5, [sp, #32]
1251:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint16_t             initial_RxXferCount;
 1756              		.loc 1 1251 3 is_stmt 1 view .LVU547
1252:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             tmp_mode;
 1757              		.loc 1 1252 3 view .LVU548
1253:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_StateTypeDef tmp_state;
 1758              		.loc 1 1253 3 view .LVU549
1254:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             tickstart;
ARM GAS  /tmp/ccqUhOmw.s 			page 116


 1759              		.loc 1 1254 3 view .LVU550
1255:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 1760              		.loc 1 1255 3 view .LVU551
1265:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef    errorcode = HAL_OK;
 1761              		.loc 1 1265 3 view .LVU552
 1762              	.LVL86:
1266:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1763              		.loc 1 1266 3 view .LVU553
1269:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1764              		.loc 1 1269 3 view .LVU554
1272:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1765              		.loc 1 1272 3 view .LVU555
1272:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1766              		.loc 1 1272 3 view .LVU556
 1767 0008 90F85C30 		ldrb	r3, [r0, #92]	@ zero_extendqisi2
 1768              	.LVL87:
1272:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1769              		.loc 1 1272 3 is_stmt 0 view .LVU557
 1770 000c 012B     		cmp	r3, #1
 1771 000e 00F06481 		beq	.L163
 1772 0012 0446     		mov	r4, r0
 1773 0014 8846     		mov	r8, r1
 1774 0016 9146     		mov	r9, r2
1272:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1775              		.loc 1 1272 3 is_stmt 1 discriminator 2 view .LVU558
 1776 0018 0123     		movs	r3, #1
 1777 001a 80F85C30 		strb	r3, [r0, #92]
1272:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1778              		.loc 1 1272 3 discriminator 2 view .LVU559
1275:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1779              		.loc 1 1275 3 discriminator 2 view .LVU560
1275:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1780              		.loc 1 1275 15 is_stmt 0 discriminator 2 view .LVU561
 1781 001e FFF7FEFF 		bl	HAL_GetTick
 1782              	.LVL88:
1275:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1783              		.loc 1 1275 15 discriminator 2 view .LVU562
 1784 0022 0646     		mov	r6, r0
 1785              	.LVL89:
1278:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_mode            = hspi->Init.Mode;
 1786              		.loc 1 1278 3 is_stmt 1 discriminator 2 view .LVU563
1278:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_mode            = hspi->Init.Mode;
 1787              		.loc 1 1278 23 is_stmt 0 discriminator 2 view .LVU564
 1788 0024 94F85D30 		ldrb	r3, [r4, #93]	@ zero_extendqisi2
 1789 0028 DBB2     		uxtb	r3, r3
 1790              	.LVL90:
1279:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   initial_TxXferCount = Size;
 1791              		.loc 1 1279 3 is_stmt 1 discriminator 2 view .LVU565
1279:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   initial_TxXferCount = Size;
 1792              		.loc 1 1279 23 is_stmt 0 discriminator 2 view .LVU566
 1793 002a 6268     		ldr	r2, [r4, #4]
 1794              	.LVL91:
1280:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   initial_RxXferCount = Size;
 1795              		.loc 1 1280 3 is_stmt 1 discriminator 2 view .LVU567
1281:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 1796              		.loc 1 1281 3 discriminator 2 view .LVU568
1287:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
ARM GAS  /tmp/ccqUhOmw.s 			page 117


 1797              		.loc 1 1287 3 discriminator 2 view .LVU569
1287:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
 1798              		.loc 1 1287 6 is_stmt 0 discriminator 2 view .LVU570
 1799 002c 012B     		cmp	r3, #1
 1800 002e 0AD0     		beq	.L138
1287:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
 1801              		.loc 1 1287 7 discriminator 1 view .LVU571
 1802 0030 B2F5827F 		cmp	r2, #260
 1803 0034 40F03881 		bne	.L164
1288:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1804              		.loc 1 1288 54 view .LVU572
 1805 0038 A268     		ldr	r2, [r4, #8]
 1806              	.LVL92:
1288:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1807              		.loc 1 1288 40 view .LVU573
 1808 003a 002A     		cmp	r2, #0
 1809 003c 40F03D81 		bne	.L165
1288:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1810              		.loc 1 1288 90 discriminator 1 view .LVU574
 1811 0040 042B     		cmp	r3, #4
 1812 0042 40F03C81 		bne	.L166
 1813              	.L138:
1294:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1814              		.loc 1 1294 3 is_stmt 1 view .LVU575
1294:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1815              		.loc 1 1294 6 is_stmt 0 view .LVU576
 1816 0046 B8F1000F 		cmp	r8, #0
 1817 004a 00F03A81 		beq	.L167
1294:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1818              		.loc 1 1294 25 discriminator 1 view .LVU577
 1819 004e B9F1000F 		cmp	r9, #0
 1820 0052 00F03881 		beq	.L168
1294:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1821              		.loc 1 1294 46 discriminator 2 view .LVU578
 1822 0056 002F     		cmp	r7, #0
 1823 0058 00F03781 		beq	.L169
1301:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1824              		.loc 1 1301 3 is_stmt 1 view .LVU579
1301:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1825              		.loc 1 1301 11 is_stmt 0 view .LVU580
 1826 005c 94F85D30 		ldrb	r3, [r4, #93]	@ zero_extendqisi2
 1827              	.LVL93:
1301:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1828              		.loc 1 1301 11 view .LVU581
 1829 0060 DBB2     		uxtb	r3, r3
1301:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1830              		.loc 1 1301 6 view .LVU582
 1831 0062 042B     		cmp	r3, #4
 1832 0064 02D0     		beq	.L140
1303:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1833              		.loc 1 1303 5 is_stmt 1 view .LVU583
1303:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1834              		.loc 1 1303 17 is_stmt 0 view .LVU584
 1835 0066 0523     		movs	r3, #5
 1836 0068 84F85D30 		strb	r3, [r4, #93]
 1837              	.L140:
1307:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
ARM GAS  /tmp/ccqUhOmw.s 			page 118


 1838              		.loc 1 1307 3 is_stmt 1 view .LVU585
1307:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
 1839              		.loc 1 1307 21 is_stmt 0 view .LVU586
 1840 006c 0023     		movs	r3, #0
 1841 006e 2366     		str	r3, [r4, #96]
1308:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 1842              		.loc 1 1308 3 is_stmt 1 view .LVU587
1308:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 1843              		.loc 1 1308 21 is_stmt 0 view .LVU588
 1844 0070 C4F84090 		str	r9, [r4, #64]
1309:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 1845              		.loc 1 1309 3 is_stmt 1 view .LVU589
1309:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 1846              		.loc 1 1309 21 is_stmt 0 view .LVU590
 1847 0074 A4F84670 		strh	r7, [r4, #70]	@ movhi
1310:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pTxData;
 1848              		.loc 1 1310 3 is_stmt 1 view .LVU591
1310:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pTxData;
 1849              		.loc 1 1310 21 is_stmt 0 view .LVU592
 1850 0078 A4F84470 		strh	r7, [r4, #68]	@ movhi
1311:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 1851              		.loc 1 1311 3 is_stmt 1 view .LVU593
1311:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 1852              		.loc 1 1311 21 is_stmt 0 view .LVU594
 1853 007c C4F83880 		str	r8, [r4, #56]
1312:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 1854              		.loc 1 1312 3 is_stmt 1 view .LVU595
1312:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 1855              		.loc 1 1312 21 is_stmt 0 view .LVU596
 1856 0080 E787     		strh	r7, [r4, #62]	@ movhi
1313:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1857              		.loc 1 1313 3 is_stmt 1 view .LVU597
1313:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1858              		.loc 1 1313 21 is_stmt 0 view .LVU598
 1859 0082 A787     		strh	r7, [r4, #60]	@ movhi
1316:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 1860              		.loc 1 1316 3 is_stmt 1 view .LVU599
1316:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 1861              		.loc 1 1316 21 is_stmt 0 view .LVU600
 1862 0084 E364     		str	r3, [r4, #76]
1317:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1863              		.loc 1 1317 3 is_stmt 1 view .LVU601
1317:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1864              		.loc 1 1317 21 is_stmt 0 view .LVU602
 1865 0086 2365     		str	r3, [r4, #80]
1328:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1866              		.loc 1 1328 3 is_stmt 1 view .LVU603
1328:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1867              		.loc 1 1328 18 is_stmt 0 view .LVU604
 1868 0088 E368     		ldr	r3, [r4, #12]
1328:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1869              		.loc 1 1328 6 view .LVU605
 1870 008a B3F5E06F 		cmp	r3, #1792
 1871 008e 01D8     		bhi	.L141
1328:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1872              		.loc 1 1328 49 discriminator 1 view .LVU606
 1873 0090 012F     		cmp	r7, #1
ARM GAS  /tmp/ccqUhOmw.s 			page 119


 1874 0092 23D9     		bls	.L142
 1875              	.L141:
1331:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1876              		.loc 1 1331 5 is_stmt 1 view .LVU607
 1877 0094 2268     		ldr	r2, [r4]
 1878 0096 5368     		ldr	r3, [r2, #4]
 1879 0098 23F48053 		bic	r3, r3, #4096
 1880 009c 5360     		str	r3, [r2, #4]
 1881              	.LVL94:
 1882              	.L143:
1340:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1883              		.loc 1 1340 3 view .LVU608
1340:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1884              		.loc 1 1340 12 is_stmt 0 view .LVU609
 1885 009e 2368     		ldr	r3, [r4]
1340:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1886              		.loc 1 1340 22 view .LVU610
 1887 00a0 1A68     		ldr	r2, [r3]
1340:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1888              		.loc 1 1340 6 view .LVU611
 1889 00a2 12F0400F 		tst	r2, #64
 1890 00a6 03D1     		bne	.L144
1343:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1891              		.loc 1 1343 5 is_stmt 1 view .LVU612
 1892 00a8 1A68     		ldr	r2, [r3]
 1893 00aa 42F04002 		orr	r2, r2, #64
 1894 00ae 1A60     		str	r2, [r3]
 1895              	.L144:
1347:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1896              		.loc 1 1347 3 view .LVU613
1347:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1897              		.loc 1 1347 17 is_stmt 0 view .LVU614
 1898 00b0 E368     		ldr	r3, [r4, #12]
1347:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 1899              		.loc 1 1347 6 view .LVU615
 1900 00b2 B3F5E06F 		cmp	r3, #1792
 1901 00b6 58D9     		bls	.L145
1349:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1902              		.loc 1 1349 5 is_stmt 1 view .LVU616
1349:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1903              		.loc 1 1349 20 is_stmt 0 view .LVU617
 1904 00b8 6368     		ldr	r3, [r4, #4]
1349:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1905              		.loc 1 1349 8 view .LVU618
 1906 00ba 0BB1     		cbz	r3, .L146
1349:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 1907              		.loc 1 1349 45 discriminator 1 view .LVU619
 1908 00bc 012F     		cmp	r7, #1
 1909 00be 0BD1     		bne	.L147
 1910              	.L146:
1351:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
 1911              		.loc 1 1351 7 is_stmt 1 view .LVU620
1351:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
 1912              		.loc 1 1351 46 is_stmt 0 view .LVU621
 1913 00c0 A26B     		ldr	r2, [r4, #56]
1351:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
 1914              		.loc 1 1351 11 view .LVU622
ARM GAS  /tmp/ccqUhOmw.s 			page 120


 1915 00c2 2368     		ldr	r3, [r4]
1351:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
 1916              		.loc 1 1351 28 view .LVU623
 1917 00c4 1288     		ldrh	r2, [r2]
1351:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->pTxBuffPtr += sizeof(uint16_t);
 1918              		.loc 1 1351 26 view .LVU624
 1919 00c6 DA60     		str	r2, [r3, #12]
1352:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount--;
 1920              		.loc 1 1352 7 is_stmt 1 view .LVU625
1352:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount--;
 1921              		.loc 1 1352 11 is_stmt 0 view .LVU626
 1922 00c8 A36B     		ldr	r3, [r4, #56]
1352:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount--;
 1923              		.loc 1 1352 24 view .LVU627
 1924 00ca 0233     		adds	r3, r3, #2
 1925 00cc A363     		str	r3, [r4, #56]
1353:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 1926              		.loc 1 1353 7 is_stmt 1 view .LVU628
1353:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 1927              		.loc 1 1353 11 is_stmt 0 view .LVU629
 1928 00ce E38F     		ldrh	r3, [r4, #62]
 1929 00d0 9BB2     		uxth	r3, r3
1353:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 1930              		.loc 1 1353 24 view .LVU630
 1931 00d2 013B     		subs	r3, r3, #1
 1932 00d4 9BB2     		uxth	r3, r3
 1933 00d6 E387     		strh	r3, [r4, #62]	@ movhi
 1934              	.L147:
1387:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 1935              		.loc 1 1387 19 view .LVU631
 1936 00d8 0127     		movs	r7, #1
 1937              	.LVL95:
1387:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 1938              		.loc 1 1387 19 view .LVU632
 1939 00da 31E0     		b	.L148
 1940              	.LVL96:
 1941              	.L142:
1336:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1942              		.loc 1 1336 5 is_stmt 1 view .LVU633
 1943 00dc 2268     		ldr	r2, [r4]
 1944 00de 5368     		ldr	r3, [r2, #4]
 1945 00e0 43F48053 		orr	r3, r3, #4096
 1946 00e4 5360     		str	r3, [r2, #4]
 1947              	.LVL97:
1336:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 1948              		.loc 1 1336 5 is_stmt 0 view .LVU634
 1949 00e6 DAE7     		b	.L143
 1950              	.LVL98:
 1951              	.L175:
1360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1952              		.loc 1 1360 9 is_stmt 1 view .LVU635
1360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1953              		.loc 1 1360 48 is_stmt 0 view .LVU636
 1954 00e8 A26B     		ldr	r2, [r4, #56]
1360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1955              		.loc 1 1360 30 view .LVU637
 1956 00ea 1288     		ldrh	r2, [r2]
ARM GAS  /tmp/ccqUhOmw.s 			page 121


1360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 1957              		.loc 1 1360 28 view .LVU638
 1958 00ec DA60     		str	r2, [r3, #12]
1361:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 1959              		.loc 1 1361 9 is_stmt 1 view .LVU639
1361:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 1960              		.loc 1 1361 13 is_stmt 0 view .LVU640
 1961 00ee A36B     		ldr	r3, [r4, #56]
1361:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 1962              		.loc 1 1361 26 view .LVU641
 1963 00f0 0233     		adds	r3, r3, #2
 1964 00f2 A363     		str	r3, [r4, #56]
1362:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Next Data is a reception (Rx). Tx not allowed */
 1965              		.loc 1 1362 9 is_stmt 1 view .LVU642
1362:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Next Data is a reception (Rx). Tx not allowed */
 1966              		.loc 1 1362 13 is_stmt 0 view .LVU643
 1967 00f4 E38F     		ldrh	r3, [r4, #62]
 1968 00f6 9BB2     		uxth	r3, r3
1362:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Next Data is a reception (Rx). Tx not allowed */
 1969              		.loc 1 1362 26 view .LVU644
 1970 00f8 013B     		subs	r3, r3, #1
 1971 00fa 9BB2     		uxth	r3, r3
 1972 00fc E387     		strh	r3, [r4, #62]	@ movhi
1364:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1973              		.loc 1 1364 9 is_stmt 1 view .LVU645
 1974              	.LVL99:
1364:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 1975              		.loc 1 1364 19 is_stmt 0 view .LVU646
 1976 00fe 0027     		movs	r7, #0
 1977              	.LVL100:
 1978              	.L149:
1381:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1979              		.loc 1 1381 7 is_stmt 1 view .LVU647
1381:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1980              		.loc 1 1381 12 is_stmt 0 view .LVU648
 1981 0100 2368     		ldr	r3, [r4]
 1982 0102 9A68     		ldr	r2, [r3, #8]
1381:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1983              		.loc 1 1381 10 view .LVU649
 1984 0104 12F0010F 		tst	r2, #1
 1985 0108 11D0     		beq	.L150
1381:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1986              		.loc 1 1381 61 discriminator 1 view .LVU650
 1987 010a B4F84620 		ldrh	r2, [r4, #70]
 1988 010e 92B2     		uxth	r2, r2
1381:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 1989              		.loc 1 1381 53 discriminator 1 view .LVU651
 1990 0110 6AB1     		cbz	r2, .L150
1383:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
 1991              		.loc 1 1383 9 is_stmt 1 view .LVU652
1383:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
 1992              		.loc 1 1383 67 is_stmt 0 view .LVU653
 1993 0112 DA68     		ldr	r2, [r3, #12]
1383:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
 1994              		.loc 1 1383 27 view .LVU654
 1995 0114 236C     		ldr	r3, [r4, #64]
1383:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
ARM GAS  /tmp/ccqUhOmw.s 			page 122


 1996              		.loc 1 1383 41 view .LVU655
 1997 0116 1A80     		strh	r2, [r3]	@ movhi
1384:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
 1998              		.loc 1 1384 9 is_stmt 1 view .LVU656
1384:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
 1999              		.loc 1 1384 13 is_stmt 0 view .LVU657
 2000 0118 236C     		ldr	r3, [r4, #64]
1384:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
 2001              		.loc 1 1384 26 view .LVU658
 2002 011a 0233     		adds	r3, r3, #2
 2003 011c 2364     		str	r3, [r4, #64]
1385:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Next Data is a Transmission (Tx). Tx is allowed */
 2004              		.loc 1 1385 9 is_stmt 1 view .LVU659
1385:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Next Data is a Transmission (Tx). Tx is allowed */
 2005              		.loc 1 1385 13 is_stmt 0 view .LVU660
 2006 011e B4F84630 		ldrh	r3, [r4, #70]
 2007 0122 9BB2     		uxth	r3, r3
1385:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Next Data is a Transmission (Tx). Tx is allowed */
 2008              		.loc 1 1385 26 view .LVU661
 2009 0124 013B     		subs	r3, r3, #1
 2010 0126 9BB2     		uxth	r3, r3
 2011 0128 A4F84630 		strh	r3, [r4, #70]	@ movhi
1387:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2012              		.loc 1 1387 9 is_stmt 1 view .LVU662
 2013              	.LVL101:
1387:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2014              		.loc 1 1387 19 is_stmt 0 view .LVU663
 2015 012c 0127     		movs	r7, #1
 2016              	.LVL102:
 2017              	.L150:
1389:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2018              		.loc 1 1389 7 is_stmt 1 view .LVU664
1389:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2019              		.loc 1 1389 13 is_stmt 0 view .LVU665
 2020 012e FFF7FEFF 		bl	HAL_GetTick
 2021              	.LVL103:
1389:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2022              		.loc 1 1389 27 view .LVU666
 2023 0132 831B     		subs	r3, r0, r6
1389:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2024              		.loc 1 1389 10 view .LVU667
 2025 0134 AB42     		cmp	r3, r5
 2026 0136 03D3     		bcc	.L148
1389:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2027              		.loc 1 1389 53 discriminator 1 view .LVU668
 2028 0138 B5F1FF3F 		cmp	r5, #-1
 2029 013c 40F0C780 		bne	.L170
 2030              	.LVL104:
 2031              	.L148:
1355:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2032              		.loc 1 1355 37 is_stmt 1 view .LVU669
1355:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2033              		.loc 1 1355 17 is_stmt 0 view .LVU670
 2034 0140 E38F     		ldrh	r3, [r4, #62]
 2035 0142 9BB2     		uxth	r3, r3
1355:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2036              		.loc 1 1355 37 view .LVU671
ARM GAS  /tmp/ccqUhOmw.s 			page 123


 2037 0144 2BB9     		cbnz	r3, .L151
1355:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2038              		.loc 1 1355 45 discriminator 1 view .LVU672
 2039 0146 B4F84630 		ldrh	r3, [r4, #70]
 2040 014a 9BB2     		uxth	r3, r3
1355:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2041              		.loc 1 1355 37 discriminator 1 view .LVU673
 2042 014c 002B     		cmp	r3, #0
 2043 014e 00F0A180 		beq	.L152
 2044              	.L151:
1358:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2045              		.loc 1 1358 7 is_stmt 1 view .LVU674
1358:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2046              		.loc 1 1358 12 is_stmt 0 view .LVU675
 2047 0152 2368     		ldr	r3, [r4]
 2048 0154 9A68     		ldr	r2, [r3, #8]
1358:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2049              		.loc 1 1358 10 view .LVU676
 2050 0156 12F0020F 		tst	r2, #2
 2051 015a D1D0     		beq	.L149
1358:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2052              		.loc 1 1358 60 discriminator 1 view .LVU677
 2053 015c E28F     		ldrh	r2, [r4, #62]
 2054 015e 92B2     		uxth	r2, r2
1358:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2055              		.loc 1 1358 52 discriminator 1 view .LVU678
 2056 0160 002A     		cmp	r2, #0
 2057 0162 CDD0     		beq	.L149
1358:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2058              		.loc 1 1358 80 discriminator 2 view .LVU679
 2059 0164 002F     		cmp	r7, #0
 2060 0166 CBD0     		beq	.L149
 2061 0168 BEE7     		b	.L175
 2062              	.LVL105:
 2063              	.L145:
1399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2064              		.loc 1 1399 5 is_stmt 1 view .LVU680
1399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2065              		.loc 1 1399 20 is_stmt 0 view .LVU681
 2066 016a 6368     		ldr	r3, [r4, #4]
1399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2067              		.loc 1 1399 8 view .LVU682
 2068 016c 0BB1     		cbz	r3, .L153
1399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2069              		.loc 1 1399 45 discriminator 1 view .LVU683
 2070 016e 012F     		cmp	r7, #1
 2071 0170 0FD1     		bne	.L154
 2072              	.L153:
1401:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2073              		.loc 1 1401 7 is_stmt 1 view .LVU684
1401:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2074              		.loc 1 1401 15 is_stmt 0 view .LVU685
 2075 0172 E38F     		ldrh	r3, [r4, #62]
 2076 0174 9BB2     		uxth	r3, r3
1401:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2077              		.loc 1 1401 10 view .LVU686
 2078 0176 012B     		cmp	r3, #1
ARM GAS  /tmp/ccqUhOmw.s 			page 124


 2079 0178 0DD9     		bls	.L155
1403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 2080              		.loc 1 1403 9 is_stmt 1 view .LVU687
1403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 2081              		.loc 1 1403 48 is_stmt 0 view .LVU688
 2082 017a A26B     		ldr	r2, [r4, #56]
1403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 2083              		.loc 1 1403 13 view .LVU689
 2084 017c 2368     		ldr	r3, [r4]
1403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 2085              		.loc 1 1403 30 view .LVU690
 2086 017e 1288     		ldrh	r2, [r2]
1403:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr += sizeof(uint16_t);
 2087              		.loc 1 1403 28 view .LVU691
 2088 0180 DA60     		str	r2, [r3, #12]
1404:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount -= 2U;
 2089              		.loc 1 1404 9 is_stmt 1 view .LVU692
1404:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount -= 2U;
 2090              		.loc 1 1404 13 is_stmt 0 view .LVU693
 2091 0182 A36B     		ldr	r3, [r4, #56]
1404:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount -= 2U;
 2092              		.loc 1 1404 26 view .LVU694
 2093 0184 0233     		adds	r3, r3, #2
 2094 0186 A363     		str	r3, [r4, #56]
1405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2095              		.loc 1 1405 9 is_stmt 1 view .LVU695
1405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2096              		.loc 1 1405 13 is_stmt 0 view .LVU696
 2097 0188 E38F     		ldrh	r3, [r4, #62]
 2098 018a 9BB2     		uxth	r3, r3
1405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2099              		.loc 1 1405 27 view .LVU697
 2100 018c 023B     		subs	r3, r3, #2
 2101 018e 9BB2     		uxth	r3, r3
 2102 0190 E387     		strh	r3, [r4, #62]	@ movhi
 2103              	.L154:
1469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2104              		.loc 1 1469 19 view .LVU698
 2105 0192 0127     		movs	r7, #1
 2106              	.LVL106:
1469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2107              		.loc 1 1469 19 view .LVU699
 2108 0194 49E0     		b	.L161
 2109              	.LVL107:
 2110              	.L155:
1409:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr++;
 2111              		.loc 1 1409 9 is_stmt 1 view .LVU700
1409:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr++;
 2112              		.loc 1 1409 54 is_stmt 0 view .LVU701
 2113 0196 A26B     		ldr	r2, [r4, #56]
1409:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr++;
 2114              		.loc 1 1409 31 view .LVU702
 2115 0198 2368     		ldr	r3, [r4]
1409:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr++;
 2116              		.loc 1 1409 49 view .LVU703
 2117 019a 1278     		ldrb	r2, [r2]	@ zero_extendqisi2
1409:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pTxBuffPtr++;
ARM GAS  /tmp/ccqUhOmw.s 			page 125


 2118              		.loc 1 1409 46 view .LVU704
 2119 019c 1A73     		strb	r2, [r3, #12]
1410:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 2120              		.loc 1 1410 9 is_stmt 1 view .LVU705
1410:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 2121              		.loc 1 1410 13 is_stmt 0 view .LVU706
 2122 019e A36B     		ldr	r3, [r4, #56]
1410:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount--;
 2123              		.loc 1 1410 25 view .LVU707
 2124 01a0 0133     		adds	r3, r3, #1
 2125 01a2 A363     		str	r3, [r4, #56]
1411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2126              		.loc 1 1411 9 is_stmt 1 view .LVU708
1411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2127              		.loc 1 1411 13 is_stmt 0 view .LVU709
 2128 01a4 E38F     		ldrh	r3, [r4, #62]
 2129 01a6 9BB2     		uxth	r3, r3
1411:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2130              		.loc 1 1411 26 view .LVU710
 2131 01a8 013B     		subs	r3, r3, #1
 2132 01aa 9BB2     		uxth	r3, r3
 2133 01ac E387     		strh	r3, [r4, #62]	@ movhi
 2134 01ae F0E7     		b	.L154
 2135              	.LVL108:
 2136              	.L177:
1419:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2137              		.loc 1 1419 9 is_stmt 1 view .LVU711
1419:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2138              		.loc 1 1419 17 is_stmt 0 view .LVU712
 2139 01b0 E28F     		ldrh	r2, [r4, #62]
 2140 01b2 92B2     		uxth	r2, r2
1419:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2141              		.loc 1 1419 12 view .LVU713
 2142 01b4 012A     		cmp	r2, #1
 2143 01b6 0CD9     		bls	.L157
1421:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint16_t);
 2144              		.loc 1 1421 11 is_stmt 1 view .LVU714
1421:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint16_t);
 2145              		.loc 1 1421 50 is_stmt 0 view .LVU715
 2146 01b8 A26B     		ldr	r2, [r4, #56]
1421:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint16_t);
 2147              		.loc 1 1421 32 view .LVU716
 2148 01ba 1288     		ldrh	r2, [r2]
1421:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr += sizeof(uint16_t);
 2149              		.loc 1 1421 30 view .LVU717
 2150 01bc DA60     		str	r2, [r3, #12]
1422:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount -= 2U;
 2151              		.loc 1 1422 11 is_stmt 1 view .LVU718
1422:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount -= 2U;
 2152              		.loc 1 1422 15 is_stmt 0 view .LVU719
 2153 01be A36B     		ldr	r3, [r4, #56]
1422:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount -= 2U;
 2154              		.loc 1 1422 28 view .LVU720
 2155 01c0 0233     		adds	r3, r3, #2
 2156 01c2 A363     		str	r3, [r4, #56]
1423:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 2157              		.loc 1 1423 11 is_stmt 1 view .LVU721
ARM GAS  /tmp/ccqUhOmw.s 			page 126


1423:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 2158              		.loc 1 1423 15 is_stmt 0 view .LVU722
 2159 01c4 E38F     		ldrh	r3, [r4, #62]
 2160 01c6 9BB2     		uxth	r3, r3
1423:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 2161              		.loc 1 1423 29 view .LVU723
 2162 01c8 023B     		subs	r3, r3, #2
 2163 01ca 9BB2     		uxth	r3, r3
 2164 01cc E387     		strh	r3, [r4, #62]	@ movhi
1432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2165              		.loc 1 1432 19 view .LVU724
 2166 01ce 0027     		movs	r7, #0
 2167              	.LVL109:
1432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2168              		.loc 1 1432 19 view .LVU725
 2169 01d0 3DE0     		b	.L156
 2170              	.LVL110:
 2171              	.L157:
1427:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr++;
 2172              		.loc 1 1427 11 is_stmt 1 view .LVU726
1427:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr++;
 2173              		.loc 1 1427 56 is_stmt 0 view .LVU727
 2174 01d2 A26B     		ldr	r2, [r4, #56]
1427:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr++;
 2175              		.loc 1 1427 51 view .LVU728
 2176 01d4 1278     		ldrb	r2, [r2]	@ zero_extendqisi2
1427:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pTxBuffPtr++;
 2177              		.loc 1 1427 48 view .LVU729
 2178 01d6 1A73     		strb	r2, [r3, #12]
1428:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount--;
 2179              		.loc 1 1428 11 is_stmt 1 view .LVU730
1428:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount--;
 2180              		.loc 1 1428 15 is_stmt 0 view .LVU731
 2181 01d8 A36B     		ldr	r3, [r4, #56]
1428:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->TxXferCount--;
 2182              		.loc 1 1428 27 view .LVU732
 2183 01da 0133     		adds	r3, r3, #1
 2184 01dc A363     		str	r3, [r4, #56]
1429:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 2185              		.loc 1 1429 11 is_stmt 1 view .LVU733
1429:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 2186              		.loc 1 1429 15 is_stmt 0 view .LVU734
 2187 01de E38F     		ldrh	r3, [r4, #62]
 2188 01e0 9BB2     		uxth	r3, r3
1429:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 2189              		.loc 1 1429 28 view .LVU735
 2190 01e2 013B     		subs	r3, r3, #1
 2191 01e4 9BB2     		uxth	r3, r3
 2192 01e6 E387     		strh	r3, [r4, #62]	@ movhi
1432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2193              		.loc 1 1432 19 view .LVU736
 2194 01e8 0027     		movs	r7, #0
 2195              	.LVL111:
1432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2196              		.loc 1 1432 19 view .LVU737
 2197 01ea 30E0     		b	.L156
 2198              	.LVL112:
ARM GAS  /tmp/ccqUhOmw.s 			page 127


 2199              	.L178:
1459:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           }
 2200              		.loc 1 1459 13 is_stmt 1 view .LVU738
 2201 01ec 2268     		ldr	r2, [r4]
 2202 01ee 5368     		ldr	r3, [r2, #4]
 2203 01f0 43F48053 		orr	r3, r3, #4096
 2204 01f4 5360     		str	r3, [r2, #4]
1469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2205              		.loc 1 1469 19 is_stmt 0 view .LVU739
 2206 01f6 0127     		movs	r7, #1
 2207              	.LVL113:
1469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2208              		.loc 1 1469 19 view .LVU740
 2209 01f8 0DE0     		b	.L158
 2210              	.LVL114:
 2211              	.L159:
1464:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pRxBuffPtr++;
 2212              		.loc 1 1464 11 is_stmt 1 view .LVU741
1464:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pRxBuffPtr++;
 2213              		.loc 1 1464 28 is_stmt 0 view .LVU742
 2214 01fa 226C     		ldr	r2, [r4, #64]
1464:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pRxBuffPtr++;
 2215              		.loc 1 1464 44 view .LVU743
 2216 01fc 1B7B     		ldrb	r3, [r3, #12]	@ zero_extendqisi2
1464:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pRxBuffPtr++;
 2217              		.loc 1 1464 42 view .LVU744
 2218 01fe 1370     		strb	r3, [r2]
1465:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->RxXferCount--;
 2219              		.loc 1 1465 11 is_stmt 1 view .LVU745
1465:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->RxXferCount--;
 2220              		.loc 1 1465 15 is_stmt 0 view .LVU746
 2221 0200 236C     		ldr	r3, [r4, #64]
1465:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->RxXferCount--;
 2222              		.loc 1 1465 27 view .LVU747
 2223 0202 0133     		adds	r3, r3, #1
 2224 0204 2364     		str	r3, [r4, #64]
1466:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 2225              		.loc 1 1466 11 is_stmt 1 view .LVU748
1466:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 2226              		.loc 1 1466 15 is_stmt 0 view .LVU749
 2227 0206 B4F84630 		ldrh	r3, [r4, #70]
 2228 020a 9BB2     		uxth	r3, r3
1466:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         }
 2229              		.loc 1 1466 28 view .LVU750
 2230 020c 013B     		subs	r3, r3, #1
 2231 020e 9BB2     		uxth	r3, r3
 2232 0210 A4F84630 		strh	r3, [r4, #70]	@ movhi
1469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2233              		.loc 1 1469 19 view .LVU751
 2234 0214 0127     		movs	r7, #1
 2235              	.LVL115:
 2236              	.L158:
1471:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2237              		.loc 1 1471 7 is_stmt 1 view .LVU752
1471:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2238              		.loc 1 1471 14 is_stmt 0 view .LVU753
 2239 0216 FFF7FEFF 		bl	HAL_GetTick
ARM GAS  /tmp/ccqUhOmw.s 			page 128


 2240              	.LVL116:
1471:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2241              		.loc 1 1471 28 view .LVU754
 2242 021a 801B     		subs	r0, r0, r6
1471:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2243              		.loc 1 1471 10 view .LVU755
 2244 021c A842     		cmp	r0, r5
 2245 021e 02D3     		bcc	.L160
1471:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2246              		.loc 1 1471 54 discriminator 1 view .LVU756
 2247 0220 B5F1FF3F 		cmp	r5, #-1
 2248 0224 55D1     		bne	.L172
 2249              	.L160:
1471:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2250              		.loc 1 1471 87 discriminator 3 view .LVU757
 2251 0226 002D     		cmp	r5, #0
 2252 0228 55D0     		beq	.L176
 2253              	.LVL117:
 2254              	.L161:
1414:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2255              		.loc 1 1414 37 is_stmt 1 view .LVU758
1414:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2256              		.loc 1 1414 17 is_stmt 0 view .LVU759
 2257 022a E38F     		ldrh	r3, [r4, #62]
 2258 022c 9BB2     		uxth	r3, r3
1414:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2259              		.loc 1 1414 37 view .LVU760
 2260 022e 23B9     		cbnz	r3, .L162
1414:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2261              		.loc 1 1414 45 discriminator 1 view .LVU761
 2262 0230 B4F84630 		ldrh	r3, [r4, #70]
 2263 0234 9BB2     		uxth	r3, r3
1414:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2264              		.loc 1 1414 37 discriminator 1 view .LVU762
 2265 0236 002B     		cmp	r3, #0
 2266 0238 2CD0     		beq	.L152
 2267              	.L162:
1417:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2268              		.loc 1 1417 7 is_stmt 1 view .LVU763
1417:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2269              		.loc 1 1417 12 is_stmt 0 view .LVU764
 2270 023a 2368     		ldr	r3, [r4]
 2271 023c 9A68     		ldr	r2, [r3, #8]
1417:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2272              		.loc 1 1417 10 view .LVU765
 2273 023e 12F0020F 		tst	r2, #2
 2274 0242 04D0     		beq	.L156
1417:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2275              		.loc 1 1417 60 discriminator 1 view .LVU766
 2276 0244 E28F     		ldrh	r2, [r4, #62]
 2277 0246 92B2     		uxth	r2, r2
1417:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2278              		.loc 1 1417 52 discriminator 1 view .LVU767
 2279 0248 0AB1     		cbz	r2, .L156
1417:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2280              		.loc 1 1417 80 discriminator 2 view .LVU768
 2281 024a 002F     		cmp	r7, #0
ARM GAS  /tmp/ccqUhOmw.s 			page 129


 2282 024c B0D1     		bne	.L177
 2283              	.LVL118:
 2284              	.L156:
1449:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2285              		.loc 1 1449 7 is_stmt 1 view .LVU769
1449:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2286              		.loc 1 1449 12 is_stmt 0 view .LVU770
 2287 024e 2368     		ldr	r3, [r4]
 2288 0250 9A68     		ldr	r2, [r3, #8]
1449:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2289              		.loc 1 1449 10 view .LVU771
 2290 0252 12F0010F 		tst	r2, #1
 2291 0256 DED0     		beq	.L158
1449:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2292              		.loc 1 1449 61 discriminator 1 view .LVU772
 2293 0258 B4F84620 		ldrh	r2, [r4, #70]
 2294 025c 92B2     		uxth	r2, r2
1449:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2295              		.loc 1 1449 53 discriminator 1 view .LVU773
 2296 025e 002A     		cmp	r2, #0
 2297 0260 D9D0     		beq	.L158
1451:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2298              		.loc 1 1451 9 is_stmt 1 view .LVU774
1451:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2299              		.loc 1 1451 17 is_stmt 0 view .LVU775
 2300 0262 B4F84620 		ldrh	r2, [r4, #70]
 2301 0266 92B2     		uxth	r2, r2
1451:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2302              		.loc 1 1451 12 view .LVU776
 2303 0268 012A     		cmp	r2, #1
 2304 026a C6D9     		bls	.L159
1453:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint16_t);
 2305              		.loc 1 1453 11 is_stmt 1 view .LVU777
1453:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint16_t);
 2306              		.loc 1 1453 69 is_stmt 0 view .LVU778
 2307 026c DA68     		ldr	r2, [r3, #12]
1453:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint16_t);
 2308              		.loc 1 1453 29 view .LVU779
 2309 026e 236C     		ldr	r3, [r4, #64]
1453:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->pRxBuffPtr += sizeof(uint16_t);
 2310              		.loc 1 1453 43 view .LVU780
 2311 0270 1A80     		strh	r2, [r3]	@ movhi
1454:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->RxXferCount -= 2U;
 2312              		.loc 1 1454 11 is_stmt 1 view .LVU781
1454:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->RxXferCount -= 2U;
 2313              		.loc 1 1454 15 is_stmt 0 view .LVU782
 2314 0272 236C     		ldr	r3, [r4, #64]
1454:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           hspi->RxXferCount -= 2U;
 2315              		.loc 1 1454 28 view .LVU783
 2316 0274 0233     		adds	r3, r3, #2
 2317 0276 2364     		str	r3, [r4, #64]
1455:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if (hspi->RxXferCount <= 1U)
 2318              		.loc 1 1455 11 is_stmt 1 view .LVU784
1455:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if (hspi->RxXferCount <= 1U)
 2319              		.loc 1 1455 15 is_stmt 0 view .LVU785
 2320 0278 B4F84630 		ldrh	r3, [r4, #70]
 2321 027c 9BB2     		uxth	r3, r3
ARM GAS  /tmp/ccqUhOmw.s 			page 130


1455:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if (hspi->RxXferCount <= 1U)
 2322              		.loc 1 1455 29 view .LVU786
 2323 027e 023B     		subs	r3, r3, #2
 2324 0280 9BB2     		uxth	r3, r3
 2325 0282 A4F84630 		strh	r3, [r4, #70]	@ movhi
1456:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
 2326              		.loc 1 1456 11 is_stmt 1 view .LVU787
1456:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
 2327              		.loc 1 1456 19 is_stmt 0 view .LVU788
 2328 0286 B4F84630 		ldrh	r3, [r4, #70]
 2329 028a 9BB2     		uxth	r3, r3
1456:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
 2330              		.loc 1 1456 14 view .LVU789
 2331 028c 012B     		cmp	r3, #1
 2332 028e ADD9     		bls	.L178
1469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2333              		.loc 1 1469 19 view .LVU790
 2334 0290 0127     		movs	r7, #1
 2335              	.LVL119:
1469:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2336              		.loc 1 1469 19 view .LVU791
 2337 0292 C0E7     		b	.L158
 2338              	.LVL120:
 2339              	.L152:
1537:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2340              		.loc 1 1537 3 is_stmt 1 view .LVU792
1537:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2341              		.loc 1 1537 7 is_stmt 0 view .LVU793
 2342 0294 3246     		mov	r2, r6
 2343 0296 2946     		mov	r1, r5
 2344 0298 2046     		mov	r0, r4
 2345 029a FFF7FEFF 		bl	SPI_EndRxTxTransaction
 2346              	.LVL121:
1537:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2347              		.loc 1 1537 6 view .LVU794
 2348 029e 20B1     		cbz	r0, .L139
1539:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_FLAG;
 2349              		.loc 1 1539 5 is_stmt 1 view .LVU795
 2350              	.LVL122:
1540:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2351              		.loc 1 1540 5 view .LVU796
1540:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2352              		.loc 1 1540 21 is_stmt 0 view .LVU797
 2353 02a0 2023     		movs	r3, #32
 2354 02a2 2366     		str	r3, [r4, #96]
1539:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->ErrorCode = HAL_SPI_ERROR_FLAG;
 2355              		.loc 1 1539 15 view .LVU798
 2356 02a4 0120     		movs	r0, #1
 2357 02a6 00E0     		b	.L139
 2358              	.LVL123:
 2359              	.L164:
1290:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2360              		.loc 1 1290 15 view .LVU799
 2361 02a8 0220     		movs	r0, #2
 2362              	.LVL124:
 2363              	.L139:
1544:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
ARM GAS  /tmp/ccqUhOmw.s 			page 131


 2364              		.loc 1 1544 3 is_stmt 1 view .LVU800
1544:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
 2365              		.loc 1 1544 15 is_stmt 0 view .LVU801
 2366 02aa 0123     		movs	r3, #1
 2367 02ac 84F85D30 		strb	r3, [r4, #93]
1545:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 2368              		.loc 1 1545 3 is_stmt 1 view .LVU802
1545:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 2369              		.loc 1 1545 3 view .LVU803
 2370 02b0 0023     		movs	r3, #0
 2371 02b2 84F85C30 		strb	r3, [r4, #92]
1545:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 2372              		.loc 1 1545 3 view .LVU804
1546:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 2373              		.loc 1 1546 3 view .LVU805
 2374              	.LVL125:
 2375              	.L137:
1547:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2376              		.loc 1 1547 1 is_stmt 0 view .LVU806
 2377 02b6 BDE8F883 		pop	{r3, r4, r5, r6, r7, r8, r9, pc}
 2378              	.LVL126:
 2379              	.L165:
1290:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2380              		.loc 1 1290 15 view .LVU807
 2381 02ba 0220     		movs	r0, #2
 2382              	.LVL127:
1290:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2383              		.loc 1 1290 15 view .LVU808
 2384 02bc F5E7     		b	.L139
 2385              	.LVL128:
 2386              	.L166:
1290:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2387              		.loc 1 1290 15 view .LVU809
 2388 02be 0220     		movs	r0, #2
 2389              	.LVL129:
1290:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2390              		.loc 1 1290 15 view .LVU810
 2391 02c0 F3E7     		b	.L139
 2392              	.LVL130:
 2393              	.L167:
1296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2394              		.loc 1 1296 15 view .LVU811
 2395 02c2 0120     		movs	r0, #1
 2396              	.LVL131:
1296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2397              		.loc 1 1296 15 view .LVU812
 2398 02c4 F1E7     		b	.L139
 2399              	.LVL132:
 2400              	.L168:
1296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2401              		.loc 1 1296 15 view .LVU813
 2402 02c6 0120     		movs	r0, #1
 2403              	.LVL133:
1296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2404              		.loc 1 1296 15 view .LVU814
 2405 02c8 EFE7     		b	.L139
 2406              	.LVL134:
ARM GAS  /tmp/ccqUhOmw.s 			page 132


 2407              	.L169:
1296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2408              		.loc 1 1296 15 view .LVU815
 2409 02ca 0120     		movs	r0, #1
 2410              	.LVL135:
1296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2411              		.loc 1 1296 15 view .LVU816
 2412 02cc EDE7     		b	.L139
 2413              	.LVL136:
 2414              	.L170:
1391:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         goto error;
 2415              		.loc 1 1391 19 view .LVU817
 2416 02ce 0320     		movs	r0, #3
 2417 02d0 EBE7     		b	.L139
 2418              	.L172:
1473:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         goto error;
 2419              		.loc 1 1473 19 view .LVU818
 2420 02d2 0320     		movs	r0, #3
 2421 02d4 E9E7     		b	.L139
 2422              	.L176:
 2423 02d6 0320     		movs	r0, #3
 2424 02d8 E7E7     		b	.L139
 2425              	.LVL137:
 2426              	.L163:
1272:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2427              		.loc 1 1272 3 view .LVU819
 2428 02da 0220     		movs	r0, #2
 2429              	.LVL138:
1272:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2430              		.loc 1 1272 3 view .LVU820
 2431 02dc EBE7     		b	.L137
 2432              		.cfi_endproc
 2433              	.LFE136:
 2435              		.section	.text.HAL_SPI_Receive,"ax",%progbits
 2436              		.align	1
 2437              		.global	HAL_SPI_Receive
 2438              		.syntax unified
 2439              		.thumb
 2440              		.thumb_func
 2442              	HAL_SPI_Receive:
 2443              	.LVL139:
 2444              	.LFB135:
1009:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 2445              		.loc 1 1009 1 is_stmt 1 view -0
 2446              		.cfi_startproc
 2447              		@ args = 0, pretend = 0, frame = 0
 2448              		@ frame_needed = 0, uses_anonymous_args = 0
1009:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 2449              		.loc 1 1009 1 is_stmt 0 view .LVU822
 2450 0000 2DE9F043 		push	{r4, r5, r6, r7, r8, r9, lr}
 2451              		.cfi_def_cfa_offset 28
 2452              		.cfi_offset 4, -28
 2453              		.cfi_offset 5, -24
 2454              		.cfi_offset 6, -20
 2455              		.cfi_offset 7, -16
 2456              		.cfi_offset 8, -12
 2457              		.cfi_offset 9, -8
ARM GAS  /tmp/ccqUhOmw.s 			page 133


 2458              		.cfi_offset 14, -4
 2459 0004 83B0     		sub	sp, sp, #12
 2460              		.cfi_def_cfa_offset 40
 2461 0006 0446     		mov	r4, r0
 2462 0008 8846     		mov	r8, r1
 2463 000a 9146     		mov	r9, r2
 2464 000c 1D46     		mov	r5, r3
1015:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 2465              		.loc 1 1015 3 is_stmt 1 view .LVU823
1016:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2466              		.loc 1 1016 3 view .LVU824
 2467              	.LVL140:
1018:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2468              		.loc 1 1018 3 view .LVU825
1018:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2469              		.loc 1 1018 18 is_stmt 0 view .LVU826
 2470 000e 4068     		ldr	r0, [r0, #4]
 2471              	.LVL141:
1018:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2472              		.loc 1 1018 6 view .LVU827
 2473 0010 B0F5827F 		cmp	r0, #260
 2474 0014 43D0     		beq	.L206
 2475              	.LVL142:
 2476              	.L180:
1026:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2477              		.loc 1 1026 3 is_stmt 1 view .LVU828
1026:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2478              		.loc 1 1026 3 view .LVU829
 2479 0016 94F85C30 		ldrb	r3, [r4, #92]	@ zero_extendqisi2
 2480 001a 012B     		cmp	r3, #1
 2481 001c 00F0C380 		beq	.L199
1026:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2482              		.loc 1 1026 3 discriminator 2 view .LVU830
 2483 0020 0123     		movs	r3, #1
 2484 0022 84F85C30 		strb	r3, [r4, #92]
1026:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2485              		.loc 1 1026 3 discriminator 2 view .LVU831
1029:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2486              		.loc 1 1029 3 discriminator 2 view .LVU832
1029:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2487              		.loc 1 1029 15 is_stmt 0 discriminator 2 view .LVU833
 2488 0026 FFF7FEFF 		bl	HAL_GetTick
 2489              	.LVL143:
1029:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2490              		.loc 1 1029 15 discriminator 2 view .LVU834
 2491 002a 0746     		mov	r7, r0
 2492              	.LVL144:
1031:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2493              		.loc 1 1031 3 is_stmt 1 discriminator 2 view .LVU835
1031:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2494              		.loc 1 1031 11 is_stmt 0 discriminator 2 view .LVU836
 2495 002c 94F85D60 		ldrb	r6, [r4, #93]	@ zero_extendqisi2
 2496 0030 F6B2     		uxtb	r6, r6
1031:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2497              		.loc 1 1031 6 discriminator 2 view .LVU837
 2498 0032 012E     		cmp	r6, #1
 2499 0034 40F0A480 		bne	.L200
ARM GAS  /tmp/ccqUhOmw.s 			page 134


1037:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2500              		.loc 1 1037 3 is_stmt 1 view .LVU838
1037:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2501              		.loc 1 1037 6 is_stmt 0 view .LVU839
 2502 0038 B8F1000F 		cmp	r8, #0
 2503 003c 00F0A180 		beq	.L182
1037:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2504              		.loc 1 1037 23 discriminator 1 view .LVU840
 2505 0040 B9F1000F 		cmp	r9, #0
 2506 0044 00F09D80 		beq	.L182
1044:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 2507              		.loc 1 1044 3 is_stmt 1 view .LVU841
1044:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 2508              		.loc 1 1044 21 is_stmt 0 view .LVU842
 2509 0048 0423     		movs	r3, #4
 2510 004a 84F85D30 		strb	r3, [r4, #93]
1045:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
 2511              		.loc 1 1045 3 is_stmt 1 view .LVU843
1045:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
 2512              		.loc 1 1045 21 is_stmt 0 view .LVU844
 2513 004e 0023     		movs	r3, #0
 2514 0050 2366     		str	r3, [r4, #96]
1046:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 2515              		.loc 1 1046 3 is_stmt 1 view .LVU845
1046:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 2516              		.loc 1 1046 21 is_stmt 0 view .LVU846
 2517 0052 C4F84080 		str	r8, [r4, #64]
1047:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 2518              		.loc 1 1047 3 is_stmt 1 view .LVU847
1047:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 2519              		.loc 1 1047 21 is_stmt 0 view .LVU848
 2520 0056 A4F84490 		strh	r9, [r4, #68]	@ movhi
1048:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2521              		.loc 1 1048 3 is_stmt 1 view .LVU849
1048:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2522              		.loc 1 1048 21 is_stmt 0 view .LVU850
 2523 005a A4F84690 		strh	r9, [r4, #70]	@ movhi
1051:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = 0U;
 2524              		.loc 1 1051 3 is_stmt 1 view .LVU851
1051:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = 0U;
 2525              		.loc 1 1051 21 is_stmt 0 view .LVU852
 2526 005e A363     		str	r3, [r4, #56]
1052:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 2527              		.loc 1 1052 3 is_stmt 1 view .LVU853
1052:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 2528              		.loc 1 1052 21 is_stmt 0 view .LVU854
 2529 0060 A387     		strh	r3, [r4, #60]	@ movhi
1053:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
 2530              		.loc 1 1053 3 is_stmt 1 view .LVU855
1053:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
 2531              		.loc 1 1053 21 is_stmt 0 view .LVU856
 2532 0062 E387     		strh	r3, [r4, #62]	@ movhi
1054:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 2533              		.loc 1 1054 3 is_stmt 1 view .LVU857
1054:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 2534              		.loc 1 1054 21 is_stmt 0 view .LVU858
 2535 0064 E364     		str	r3, [r4, #76]
ARM GAS  /tmp/ccqUhOmw.s 			page 135


1055:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2536              		.loc 1 1055 3 is_stmt 1 view .LVU859
1055:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2537              		.loc 1 1055 21 is_stmt 0 view .LVU860
 2538 0066 2365     		str	r3, [r4, #80]
1068:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2539              		.loc 1 1068 3 is_stmt 1 view .LVU861
1068:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2540              		.loc 1 1068 17 is_stmt 0 view .LVU862
 2541 0068 E368     		ldr	r3, [r4, #12]
1068:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2542              		.loc 1 1068 6 view .LVU863
 2543 006a B3F5E06F 		cmp	r3, #1792
 2544 006e 24D9     		bls	.L183
1071:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2545              		.loc 1 1071 5 is_stmt 1 view .LVU864
 2546 0070 2268     		ldr	r2, [r4]
 2547 0072 5368     		ldr	r3, [r2, #4]
 2548 0074 23F48053 		bic	r3, r3, #4096
 2549 0078 5360     		str	r3, [r2, #4]
 2550              	.L184:
1080:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2551              		.loc 1 1080 3 view .LVU865
1080:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2552              		.loc 1 1080 17 is_stmt 0 view .LVU866
 2553 007a A368     		ldr	r3, [r4, #8]
1080:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2554              		.loc 1 1080 6 view .LVU867
 2555 007c B3F5004F 		cmp	r3, #32768
 2556 0080 21D0     		beq	.L207
 2557              	.L185:
1088:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2558              		.loc 1 1088 3 is_stmt 1 view .LVU868
1088:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2559              		.loc 1 1088 12 is_stmt 0 view .LVU869
 2560 0082 2368     		ldr	r3, [r4]
1088:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2561              		.loc 1 1088 22 view .LVU870
 2562 0084 1A68     		ldr	r2, [r3]
1088:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2563              		.loc 1 1088 6 view .LVU871
 2564 0086 12F0400F 		tst	r2, #64
 2565 008a 03D1     		bne	.L186
1091:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2566              		.loc 1 1091 5 is_stmt 1 view .LVU872
 2567 008c 1A68     		ldr	r2, [r3]
 2568 008e 42F04002 		orr	r2, r2, #64
 2569 0092 1A60     		str	r2, [r3]
 2570              	.L186:
1095:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2571              		.loc 1 1095 3 view .LVU873
1095:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2572              		.loc 1 1095 17 is_stmt 0 view .LVU874
 2573 0094 E368     		ldr	r3, [r4, #12]
1095:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2574              		.loc 1 1095 6 view .LVU875
 2575 0096 B3F5E06F 		cmp	r3, #1792
ARM GAS  /tmp/ccqUhOmw.s 			page 136


 2576 009a 29D9     		bls	.L187
 2577 009c 4AE0     		b	.L188
 2578              	.LVL145:
 2579              	.L206:
1018:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2580              		.loc 1 1018 58 discriminator 1 view .LVU876
 2581 009e A368     		ldr	r3, [r4, #8]
 2582              	.LVL146:
1018:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2583              		.loc 1 1018 44 discriminator 1 view .LVU877
 2584 00a0 002B     		cmp	r3, #0
 2585 00a2 B8D1     		bne	.L180
1020:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Call transmit-receive function to send Dummy data on Tx line and generate clock on CLK line 
 2586              		.loc 1 1020 5 is_stmt 1 view .LVU878
1020:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Call transmit-receive function to send Dummy data on Tx line and generate clock on CLK line 
 2587              		.loc 1 1020 17 is_stmt 0 view .LVU879
 2588 00a4 0423     		movs	r3, #4
 2589 00a6 84F85D30 		strb	r3, [r4, #93]
1022:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2590              		.loc 1 1022 5 is_stmt 1 view .LVU880
1022:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2591              		.loc 1 1022 12 is_stmt 0 view .LVU881
 2592 00aa 0095     		str	r5, [sp]
 2593 00ac 1346     		mov	r3, r2
 2594 00ae 0A46     		mov	r2, r1
 2595              	.LVL147:
1022:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2596              		.loc 1 1022 12 view .LVU882
 2597 00b0 2046     		mov	r0, r4
 2598 00b2 FFF7FEFF 		bl	HAL_SPI_TransmitReceive
 2599              	.LVL148:
1022:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2600              		.loc 1 1022 12 view .LVU883
 2601 00b6 0646     		mov	r6, r0
 2602 00b8 69E0     		b	.L181
 2603              	.LVL149:
 2604              	.L183:
1076:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2605              		.loc 1 1076 5 is_stmt 1 view .LVU884
 2606 00ba 2268     		ldr	r2, [r4]
 2607 00bc 5368     		ldr	r3, [r2, #4]
 2608 00be 43F48053 		orr	r3, r3, #4096
 2609 00c2 5360     		str	r3, [r2, #4]
 2610 00c4 D9E7     		b	.L184
 2611              	.L207:
1083:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_RX(hspi);
 2612              		.loc 1 1083 5 view .LVU885
 2613 00c6 2268     		ldr	r2, [r4]
 2614 00c8 1368     		ldr	r3, [r2]
 2615 00ca 23F04003 		bic	r3, r3, #64
 2616 00ce 1360     		str	r3, [r2]
1084:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2617              		.loc 1 1084 5 view .LVU886
 2618 00d0 2268     		ldr	r2, [r4]
 2619 00d2 1368     		ldr	r3, [r2]
 2620 00d4 23F48043 		bic	r3, r3, #16384
 2621 00d8 1360     		str	r3, [r2]
ARM GAS  /tmp/ccqUhOmw.s 			page 137


 2622 00da D2E7     		b	.L185
 2623              	.LVL150:
 2624              	.L189:
1111:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2625              		.loc 1 1111 9 view .LVU887
1111:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2626              		.loc 1 1111 16 is_stmt 0 view .LVU888
 2627 00dc FFF7FEFF 		bl	HAL_GetTick
 2628              	.LVL151:
1111:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2629              		.loc 1 1111 30 view .LVU889
 2630 00e0 C01B     		subs	r0, r0, r7
1111:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2631              		.loc 1 1111 12 view .LVU890
 2632 00e2 A842     		cmp	r0, r5
 2633 00e4 02D3     		bcc	.L191
1111:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2634              		.loc 1 1111 56 discriminator 1 view .LVU891
 2635 00e6 B5F1FF3F 		cmp	r5, #-1
 2636 00ea 54D1     		bne	.L201
 2637              	.L191:
1111:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2638              		.loc 1 1111 87 discriminator 3 view .LVU892
 2639 00ec 002D     		cmp	r5, #0
 2640 00ee 54D0     		beq	.L202
 2641              	.L187:
1098:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2642              		.loc 1 1098 30 is_stmt 1 view .LVU893
1098:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2643              		.loc 1 1098 16 is_stmt 0 view .LVU894
 2644 00f0 B4F84630 		ldrh	r3, [r4, #70]
 2645 00f4 9BB2     		uxth	r3, r3
1098:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2646              		.loc 1 1098 30 view .LVU895
 2647 00f6 002B     		cmp	r3, #0
 2648 00f8 36D0     		beq	.L193
1101:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2649              		.loc 1 1101 7 is_stmt 1 view .LVU896
1101:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2650              		.loc 1 1101 11 is_stmt 0 view .LVU897
 2651 00fa 2368     		ldr	r3, [r4]
 2652 00fc 9A68     		ldr	r2, [r3, #8]
1101:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2653              		.loc 1 1101 10 view .LVU898
 2654 00fe 12F0010F 		tst	r2, #1
 2655 0102 EBD0     		beq	.L189
1104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2656              		.loc 1 1104 9 is_stmt 1 view .LVU899
1104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2657              		.loc 1 1104 27 is_stmt 0 view .LVU900
 2658 0104 226C     		ldr	r2, [r4, #64]
1104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2659              		.loc 1 1104 43 view .LVU901
 2660 0106 1B7B     		ldrb	r3, [r3, #12]	@ zero_extendqisi2
1104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint8_t);
 2661              		.loc 1 1104 41 view .LVU902
 2662 0108 1370     		strb	r3, [r2]
ARM GAS  /tmp/ccqUhOmw.s 			page 138


1105:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
 2663              		.loc 1 1105 9 is_stmt 1 view .LVU903
1105:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
 2664              		.loc 1 1105 13 is_stmt 0 view .LVU904
 2665 010a 236C     		ldr	r3, [r4, #64]
1105:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
 2666              		.loc 1 1105 26 view .LVU905
 2667 010c 0133     		adds	r3, r3, #1
 2668 010e 2364     		str	r3, [r4, #64]
1106:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2669              		.loc 1 1106 9 is_stmt 1 view .LVU906
1106:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2670              		.loc 1 1106 13 is_stmt 0 view .LVU907
 2671 0110 B4F84630 		ldrh	r3, [r4, #70]
 2672 0114 9BB2     		uxth	r3, r3
1106:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2673              		.loc 1 1106 26 view .LVU908
 2674 0116 013B     		subs	r3, r3, #1
 2675 0118 9BB2     		uxth	r3, r3
 2676 011a A4F84630 		strh	r3, [r4, #70]	@ movhi
 2677 011e E7E7     		b	.L187
 2678              	.L194:
1134:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2679              		.loc 1 1134 9 is_stmt 1 view .LVU909
1134:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2680              		.loc 1 1134 16 is_stmt 0 view .LVU910
 2681 0120 FFF7FEFF 		bl	HAL_GetTick
 2682              	.LVL152:
1134:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2683              		.loc 1 1134 30 view .LVU911
 2684 0124 C01B     		subs	r0, r0, r7
1134:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2685              		.loc 1 1134 12 view .LVU912
 2686 0126 A842     		cmp	r0, r5
 2687 0128 02D3     		bcc	.L196
1134:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2688              		.loc 1 1134 56 discriminator 1 view .LVU913
 2689 012a B5F1FF3F 		cmp	r5, #-1
 2690 012e 36D1     		bne	.L203
 2691              	.L196:
1134:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 2692              		.loc 1 1134 87 discriminator 3 view .LVU914
 2693 0130 002D     		cmp	r5, #0
 2694 0132 36D0     		beq	.L204
 2695              	.L188:
1122:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2696              		.loc 1 1122 30 is_stmt 1 view .LVU915
1122:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2697              		.loc 1 1122 16 is_stmt 0 view .LVU916
 2698 0134 B4F84630 		ldrh	r3, [r4, #70]
 2699 0138 9BB2     		uxth	r3, r3
1122:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 2700              		.loc 1 1122 30 view .LVU917
 2701 013a ABB1     		cbz	r3, .L193
1125:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2702              		.loc 1 1125 7 is_stmt 1 view .LVU918
1125:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
ARM GAS  /tmp/ccqUhOmw.s 			page 139


 2703              		.loc 1 1125 11 is_stmt 0 view .LVU919
 2704 013c 2368     		ldr	r3, [r4]
 2705 013e 9A68     		ldr	r2, [r3, #8]
1125:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 2706              		.loc 1 1125 10 view .LVU920
 2707 0140 12F0010F 		tst	r2, #1
 2708 0144 ECD0     		beq	.L194
1127:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
 2709              		.loc 1 1127 9 is_stmt 1 view .LVU921
1127:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
 2710              		.loc 1 1127 67 is_stmt 0 view .LVU922
 2711 0146 DA68     		ldr	r2, [r3, #12]
1127:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
 2712              		.loc 1 1127 27 view .LVU923
 2713 0148 236C     		ldr	r3, [r4, #64]
1127:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->pRxBuffPtr += sizeof(uint16_t);
 2714              		.loc 1 1127 41 view .LVU924
 2715 014a 1A80     		strh	r2, [r3]	@ movhi
1128:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
 2716              		.loc 1 1128 9 is_stmt 1 view .LVU925
1128:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
 2717              		.loc 1 1128 13 is_stmt 0 view .LVU926
 2718 014c 236C     		ldr	r3, [r4, #64]
1128:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount--;
 2719              		.loc 1 1128 26 view .LVU927
 2720 014e 0233     		adds	r3, r3, #2
 2721 0150 2364     		str	r3, [r4, #64]
1129:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2722              		.loc 1 1129 9 is_stmt 1 view .LVU928
1129:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2723              		.loc 1 1129 13 is_stmt 0 view .LVU929
 2724 0152 B4F846C0 		ldrh	ip, [r4, #70]
 2725 0156 1FFA8CFC 		uxth	ip, ip
1129:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 2726              		.loc 1 1129 26 view .LVU930
 2727 015a 0CF1FF3C 		add	ip, ip, #-1
 2728 015e 1FFA8CFC 		uxth	ip, ip
 2729 0162 A4F846C0 		strh	ip, [r4, #70]	@ movhi
 2730 0166 E5E7     		b	.L188
 2731              	.L193:
1213:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2732              		.loc 1 1213 3 is_stmt 1 view .LVU931
1213:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2733              		.loc 1 1213 7 is_stmt 0 view .LVU932
 2734 0168 3A46     		mov	r2, r7
 2735 016a 2946     		mov	r1, r5
 2736 016c 2046     		mov	r0, r4
 2737 016e FFF7FEFF 		bl	SPI_EndRxTransaction
 2738              	.LVL153:
1213:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2739              		.loc 1 1213 6 view .LVU933
 2740 0172 08B1     		cbz	r0, .L198
1215:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2741              		.loc 1 1215 5 is_stmt 1 view .LVU934
1215:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2742              		.loc 1 1215 21 is_stmt 0 view .LVU935
 2743 0174 2023     		movs	r3, #32
ARM GAS  /tmp/ccqUhOmw.s 			page 140


 2744 0176 2366     		str	r3, [r4, #96]
 2745              	.L198:
1227:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2746              		.loc 1 1227 3 is_stmt 1 view .LVU936
1227:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2747              		.loc 1 1227 11 is_stmt 0 view .LVU937
 2748 0178 236E     		ldr	r3, [r4, #96]
1227:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2749              		.loc 1 1227 6 view .LVU938
 2750 017a 13B9     		cbnz	r3, .L182
1016:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2751              		.loc 1 1016 21 view .LVU939
 2752 017c 0026     		movs	r6, #0
 2753 017e 00E0     		b	.L182
 2754              	.LVL154:
 2755              	.L200:
1033:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2756              		.loc 1 1033 15 view .LVU940
 2757 0180 0226     		movs	r6, #2
 2758              	.LVL155:
 2759              	.L182:
1233:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
 2760              		.loc 1 1233 3 is_stmt 1 view .LVU941
1233:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_UNLOCK(hspi);
 2761              		.loc 1 1233 15 is_stmt 0 view .LVU942
 2762 0182 0123     		movs	r3, #1
 2763 0184 84F85D30 		strb	r3, [r4, #93]
1234:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 2764              		.loc 1 1234 3 is_stmt 1 view .LVU943
1234:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 2765              		.loc 1 1234 3 view .LVU944
 2766 0188 0023     		movs	r3, #0
 2767 018a 84F85C30 		strb	r3, [r4, #92]
1234:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 2768              		.loc 1 1234 3 view .LVU945
1235:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 2769              		.loc 1 1235 3 view .LVU946
 2770              	.LVL156:
 2771              	.L181:
1236:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2772              		.loc 1 1236 1 is_stmt 0 view .LVU947
 2773 018e 3046     		mov	r0, r6
 2774 0190 03B0     		add	sp, sp, #12
 2775              		.cfi_remember_state
 2776              		.cfi_def_cfa_offset 28
 2777              		@ sp needed
 2778 0192 BDE8F083 		pop	{r4, r5, r6, r7, r8, r9, pc}
 2779              	.LVL157:
 2780              	.L201:
 2781              		.cfi_restore_state
1113:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
 2782              		.loc 1 1113 21 view .LVU948
 2783 0196 0326     		movs	r6, #3
 2784 0198 F3E7     		b	.L182
 2785              	.L202:
 2786 019a 0326     		movs	r6, #3
 2787 019c F1E7     		b	.L182
ARM GAS  /tmp/ccqUhOmw.s 			page 141


 2788              	.L203:
1136:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           goto error;
 2789              		.loc 1 1136 21 view .LVU949
 2790 019e 0326     		movs	r6, #3
 2791 01a0 EFE7     		b	.L182
 2792              	.L204:
 2793 01a2 0326     		movs	r6, #3
 2794 01a4 EDE7     		b	.L182
 2795              	.LVL158:
 2796              	.L199:
1026:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2797              		.loc 1 1026 3 view .LVU950
 2798 01a6 0226     		movs	r6, #2
 2799 01a8 F1E7     		b	.L181
 2800              		.cfi_endproc
 2801              	.LFE135:
 2803              		.section	.text.HAL_SPI_Transmit_IT,"ax",%progbits
 2804              		.align	1
 2805              		.global	HAL_SPI_Transmit_IT
 2806              		.syntax unified
 2807              		.thumb
 2808              		.thumb_func
 2810              	HAL_SPI_Transmit_IT:
 2811              	.LVL159:
 2812              	.LFB137:
1558:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 2813              		.loc 1 1558 1 is_stmt 1 view -0
 2814              		.cfi_startproc
 2815              		@ args = 0, pretend = 0, frame = 0
 2816              		@ frame_needed = 0, uses_anonymous_args = 0
 2817              		@ link register save eliminated.
1558:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 2818              		.loc 1 1558 1 is_stmt 0 view .LVU952
 2819 0000 0346     		mov	r3, r0
1559:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2820              		.loc 1 1559 3 is_stmt 1 view .LVU953
 2821              	.LVL160:
1562:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2822              		.loc 1 1562 3 view .LVU954
1565:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2823              		.loc 1 1565 3 view .LVU955
1565:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2824              		.loc 1 1565 3 view .LVU956
 2825 0002 90F85C00 		ldrb	r0, [r0, #92]	@ zero_extendqisi2
 2826              	.LVL161:
1565:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2827              		.loc 1 1565 3 is_stmt 0 view .LVU957
 2828 0006 0128     		cmp	r0, #1
 2829 0008 4CD0     		beq	.L214
1565:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2830              		.loc 1 1565 3 is_stmt 1 discriminator 2 view .LVU958
 2831 000a 0120     		movs	r0, #1
 2832 000c 83F85C00 		strb	r0, [r3, #92]
1565:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2833              		.loc 1 1565 3 discriminator 2 view .LVU959
1567:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2834              		.loc 1 1567 3 discriminator 2 view .LVU960
ARM GAS  /tmp/ccqUhOmw.s 			page 142


1567:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2835              		.loc 1 1567 6 is_stmt 0 discriminator 2 view .LVU961
 2836 0010 0029     		cmp	r1, #0
 2837 0012 3CD0     		beq	.L215
1567:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2838              		.loc 1 1567 23 discriminator 1 view .LVU962
 2839 0014 002A     		cmp	r2, #0
 2840 0016 3CD0     		beq	.L216
1573:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2841              		.loc 1 1573 3 is_stmt 1 view .LVU963
1573:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2842              		.loc 1 1573 11 is_stmt 0 view .LVU964
 2843 0018 93F85D00 		ldrb	r0, [r3, #93]	@ zero_extendqisi2
 2844 001c C0B2     		uxtb	r0, r0
1573:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2845              		.loc 1 1573 6 view .LVU965
 2846 001e 0128     		cmp	r0, #1
 2847 0020 3CD1     		bne	.L217
1580:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 2848              		.loc 1 1580 3 is_stmt 1 view .LVU966
1580:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 2849              		.loc 1 1580 21 is_stmt 0 view .LVU967
 2850 0022 0320     		movs	r0, #3
 2851 0024 83F85D00 		strb	r0, [r3, #93]
1581:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pData;
 2852              		.loc 1 1581 3 is_stmt 1 view .LVU968
1581:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pData;
 2853              		.loc 1 1581 21 is_stmt 0 view .LVU969
 2854 0028 0020     		movs	r0, #0
 2855 002a 1866     		str	r0, [r3, #96]
1582:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 2856              		.loc 1 1582 3 is_stmt 1 view .LVU970
1582:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 2857              		.loc 1 1582 21 is_stmt 0 view .LVU971
 2858 002c 9963     		str	r1, [r3, #56]
1583:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 2859              		.loc 1 1583 3 is_stmt 1 view .LVU972
1583:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 2860              		.loc 1 1583 21 is_stmt 0 view .LVU973
 2861 002e 9A87     		strh	r2, [r3, #60]	@ movhi
1584:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2862              		.loc 1 1584 3 is_stmt 1 view .LVU974
1584:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2863              		.loc 1 1584 21 is_stmt 0 view .LVU975
 2864 0030 DA87     		strh	r2, [r3, #62]	@ movhi
1587:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = 0U;
 2865              		.loc 1 1587 3 is_stmt 1 view .LVU976
1587:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = 0U;
 2866              		.loc 1 1587 21 is_stmt 0 view .LVU977
 2867 0032 1864     		str	r0, [r3, #64]
1588:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
 2868              		.loc 1 1588 3 is_stmt 1 view .LVU978
1588:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
 2869              		.loc 1 1588 21 is_stmt 0 view .LVU979
 2870 0034 A3F84400 		strh	r0, [r3, #68]	@ movhi
1589:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
 2871              		.loc 1 1589 3 is_stmt 1 view .LVU980
ARM GAS  /tmp/ccqUhOmw.s 			page 143


1589:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
 2872              		.loc 1 1589 21 is_stmt 0 view .LVU981
 2873 0038 A3F84600 		strh	r0, [r3, #70]	@ movhi
1590:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2874              		.loc 1 1590 3 is_stmt 1 view .LVU982
1590:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2875              		.loc 1 1590 21 is_stmt 0 view .LVU983
 2876 003c D864     		str	r0, [r3, #76]
1593:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2877              		.loc 1 1593 3 is_stmt 1 view .LVU984
1593:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2878              		.loc 1 1593 17 is_stmt 0 view .LVU985
 2879 003e DA68     		ldr	r2, [r3, #12]
 2880              	.LVL162:
1593:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2881              		.loc 1 1593 6 view .LVU986
 2882 0040 B2F5E06F 		cmp	r2, #1792
 2883 0044 15D9     		bls	.L211
1595:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2884              		.loc 1 1595 5 is_stmt 1 view .LVU987
1595:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2885              		.loc 1 1595 17 is_stmt 0 view .LVU988
 2886 0046 184A     		ldr	r2, .L220
 2887 0048 1A65     		str	r2, [r3, #80]
 2888              	.L212:
1603:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2889              		.loc 1 1603 3 is_stmt 1 view .LVU989
1603:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2890              		.loc 1 1603 17 is_stmt 0 view .LVU990
 2891 004a 9A68     		ldr	r2, [r3, #8]
1603:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2892              		.loc 1 1603 6 view .LVU991
 2893 004c B2F5004F 		cmp	r2, #32768
 2894 0050 12D0     		beq	.L219
 2895              	.LVL163:
 2896              	.L213:
1619:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2897              		.loc 1 1619 3 is_stmt 1 view .LVU992
 2898 0052 1968     		ldr	r1, [r3]
 2899 0054 4A68     		ldr	r2, [r1, #4]
 2900 0056 42F0A002 		orr	r2, r2, #160
 2901 005a 4A60     		str	r2, [r1, #4]
1623:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2902              		.loc 1 1623 3 view .LVU993
1623:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2903              		.loc 1 1623 12 is_stmt 0 view .LVU994
 2904 005c 1A68     		ldr	r2, [r3]
1623:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2905              		.loc 1 1623 22 view .LVU995
 2906 005e 1168     		ldr	r1, [r2]
1623:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 2907              		.loc 1 1623 6 view .LVU996
 2908 0060 11F0400F 		tst	r1, #64
 2909 0064 1CD1     		bne	.L218
1626:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2910              		.loc 1 1626 5 is_stmt 1 view .LVU997
 2911 0066 1168     		ldr	r1, [r2]
ARM GAS  /tmp/ccqUhOmw.s 			page 144


 2912 0068 41F04001 		orr	r1, r1, #64
 2913 006c 1160     		str	r1, [r2]
1559:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2914              		.loc 1 1559 21 is_stmt 0 view .LVU998
 2915 006e 0020     		movs	r0, #0
 2916 0070 10E0     		b	.L210
 2917              	.LVL164:
 2918              	.L211:
1599:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2919              		.loc 1 1599 5 is_stmt 1 view .LVU999
1599:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2920              		.loc 1 1599 17 is_stmt 0 view .LVU1000
 2921 0072 0E4A     		ldr	r2, .L220+4
 2922 0074 1A65     		str	r2, [r3, #80]
 2923 0076 E8E7     		b	.L212
 2924              	.L219:
1606:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_TX(hspi);
 2925              		.loc 1 1606 5 is_stmt 1 view .LVU1001
 2926 0078 1968     		ldr	r1, [r3]
 2927              	.LVL165:
1606:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_TX(hspi);
 2928              		.loc 1 1606 5 is_stmt 0 view .LVU1002
 2929 007a 0A68     		ldr	r2, [r1]
 2930 007c 22F04002 		bic	r2, r2, #64
 2931 0080 0A60     		str	r2, [r1]
 2932              	.LVL166:
1607:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 2933              		.loc 1 1607 5 is_stmt 1 view .LVU1003
 2934 0082 1968     		ldr	r1, [r3]
 2935 0084 0A68     		ldr	r2, [r1]
 2936 0086 42F48042 		orr	r2, r2, #16384
 2937 008a 0A60     		str	r2, [r1]
 2938 008c E1E7     		b	.L213
 2939              	.LVL167:
 2940              	.L215:
1569:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2941              		.loc 1 1569 15 is_stmt 0 view .LVU1004
 2942 008e 0120     		movs	r0, #1
 2943 0090 00E0     		b	.L210
 2944              	.L216:
 2945 0092 0120     		movs	r0, #1
 2946              	.LVL168:
 2947              	.L210:
1630:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 2948              		.loc 1 1630 3 is_stmt 1 view .LVU1005
1630:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 2949              		.loc 1 1630 3 view .LVU1006
 2950 0094 0022     		movs	r2, #0
 2951 0096 83F85C20 		strb	r2, [r3, #92]
1630:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 2952              		.loc 1 1630 3 view .LVU1007
1631:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 2953              		.loc 1 1631 3 view .LVU1008
1631:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 2954              		.loc 1 1631 10 is_stmt 0 view .LVU1009
 2955 009a 7047     		bx	lr
 2956              	.LVL169:
ARM GAS  /tmp/ccqUhOmw.s 			page 145


 2957              	.L217:
1575:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 2958              		.loc 1 1575 15 view .LVU1010
 2959 009c 0220     		movs	r0, #2
 2960 009e F9E7     		b	.L210
 2961              	.LVL170:
 2962              	.L218:
1559:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2963              		.loc 1 1559 21 view .LVU1011
 2964 00a0 0020     		movs	r0, #0
 2965 00a2 F7E7     		b	.L210
 2966              	.LVL171:
 2967              	.L214:
1565:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2968              		.loc 1 1565 3 view .LVU1012
 2969 00a4 0220     		movs	r0, #2
1632:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2970              		.loc 1 1632 1 view .LVU1013
 2971 00a6 7047     		bx	lr
 2972              	.L221:
 2973              		.align	2
 2974              	.L220:
 2975 00a8 00000000 		.word	SPI_TxISR_16BIT
 2976 00ac 00000000 		.word	SPI_TxISR_8BIT
 2977              		.cfi_endproc
 2978              	.LFE137:
 2980              		.section	.text.HAL_SPI_TransmitReceive_IT,"ax",%progbits
 2981              		.align	1
 2982              		.global	HAL_SPI_TransmitReceive_IT
 2983              		.syntax unified
 2984              		.thumb
 2985              		.thumb_func
 2987              	HAL_SPI_TransmitReceive_IT:
 2988              	.LVL172:
 2989              	.LFB139:
1750:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             tmp_mode;
 2990              		.loc 1 1750 1 is_stmt 1 view -0
 2991              		.cfi_startproc
 2992              		@ args = 0, pretend = 0, frame = 0
 2993              		@ frame_needed = 0, uses_anonymous_args = 0
 2994              		@ link register save eliminated.
1750:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             tmp_mode;
 2995              		.loc 1 1750 1 is_stmt 0 view .LVU1015
 2996 0000 8446     		mov	ip, r0
1751:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_StateTypeDef tmp_state;
 2997              		.loc 1 1751 3 is_stmt 1 view .LVU1016
1752:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef    errorcode = HAL_OK;
 2998              		.loc 1 1752 3 view .LVU1017
1753:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 2999              		.loc 1 1753 3 view .LVU1018
 3000              	.LVL173:
1756:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3001              		.loc 1 1756 3 view .LVU1019
1759:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3002              		.loc 1 1759 3 view .LVU1020
1759:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3003              		.loc 1 1759 3 view .LVU1021
ARM GAS  /tmp/ccqUhOmw.s 			page 146


 3004 0002 90F85C00 		ldrb	r0, [r0, #92]	@ zero_extendqisi2
 3005              	.LVL174:
1759:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3006              		.loc 1 1759 3 is_stmt 0 view .LVU1022
 3007 0006 0128     		cmp	r0, #1
 3008 0008 79D0     		beq	.L232
1750:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             tmp_mode;
 3009              		.loc 1 1750 1 discriminator 2 view .LVU1023
 3010 000a 10B4     		push	{r4}
 3011              		.cfi_def_cfa_offset 4
 3012              		.cfi_offset 4, -4
1759:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3013              		.loc 1 1759 3 is_stmt 1 discriminator 2 view .LVU1024
 3014 000c 0120     		movs	r0, #1
 3015 000e 8CF85C00 		strb	r0, [ip, #92]
1759:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3016              		.loc 1 1759 3 discriminator 2 view .LVU1025
1762:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_mode            = hspi->Init.Mode;
 3017              		.loc 1 1762 3 discriminator 2 view .LVU1026
1762:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_mode            = hspi->Init.Mode;
 3018              		.loc 1 1762 23 is_stmt 0 discriminator 2 view .LVU1027
 3019 0012 9CF85D00 		ldrb	r0, [ip, #93]	@ zero_extendqisi2
 3020 0016 C0B2     		uxtb	r0, r0
 3021              	.LVL175:
1763:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3022              		.loc 1 1763 3 is_stmt 1 discriminator 2 view .LVU1028
1763:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3023              		.loc 1 1763 23 is_stmt 0 discriminator 2 view .LVU1029
 3024 0018 DCF80440 		ldr	r4, [ip, #4]
 3025              	.LVL176:
1765:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
 3026              		.loc 1 1765 3 is_stmt 1 discriminator 2 view .LVU1030
1765:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
 3027              		.loc 1 1765 6 is_stmt 0 discriminator 2 view .LVU1031
 3028 001c 0128     		cmp	r0, #1
 3029 001e 08D0     		beq	.L224
1765:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
 3030              		.loc 1 1765 7 discriminator 1 view .LVU1032
 3031 0020 B4F5827F 		cmp	r4, #260
 3032 0024 58D1     		bne	.L233
1766:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3033              		.loc 1 1766 54 view .LVU1033
 3034 0026 DCF80840 		ldr	r4, [ip, #8]
 3035              	.LVL177:
1766:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3036              		.loc 1 1766 40 view .LVU1034
 3037 002a 002C     		cmp	r4, #0
 3038 002c 5BD1     		bne	.L234
1766:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3039              		.loc 1 1766 90 discriminator 1 view .LVU1035
 3040 002e 0428     		cmp	r0, #4
 3041 0030 5BD1     		bne	.L235
 3042              	.L224:
1772:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3043              		.loc 1 1772 3 is_stmt 1 view .LVU1036
1772:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3044              		.loc 1 1772 6 is_stmt 0 view .LVU1037
ARM GAS  /tmp/ccqUhOmw.s 			page 147


 3045 0032 0029     		cmp	r1, #0
 3046 0034 5BD0     		beq	.L236
1772:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3047              		.loc 1 1772 25 discriminator 1 view .LVU1038
 3048 0036 002A     		cmp	r2, #0
 3049 0038 5BD0     		beq	.L237
1772:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3050              		.loc 1 1772 46 discriminator 2 view .LVU1039
 3051 003a 002B     		cmp	r3, #0
 3052 003c 5BD0     		beq	.L238
1779:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3053              		.loc 1 1779 3 is_stmt 1 view .LVU1040
1779:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3054              		.loc 1 1779 11 is_stmt 0 view .LVU1041
 3055 003e 9CF85D00 		ldrb	r0, [ip, #93]	@ zero_extendqisi2
 3056              	.LVL178:
1779:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3057              		.loc 1 1779 11 view .LVU1042
 3058 0042 C0B2     		uxtb	r0, r0
1779:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3059              		.loc 1 1779 6 view .LVU1043
 3060 0044 0428     		cmp	r0, #4
 3061 0046 02D0     		beq	.L226
1781:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3062              		.loc 1 1781 5 is_stmt 1 view .LVU1044
1781:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3063              		.loc 1 1781 17 is_stmt 0 view .LVU1045
 3064 0048 0520     		movs	r0, #5
 3065 004a 8CF85D00 		strb	r0, [ip, #93]
 3066              	.L226:
1785:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pTxData;
 3067              		.loc 1 1785 3 is_stmt 1 view .LVU1046
1785:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pTxData;
 3068              		.loc 1 1785 21 is_stmt 0 view .LVU1047
 3069 004e 0020     		movs	r0, #0
 3070 0050 CCF86000 		str	r0, [ip, #96]
1786:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 3071              		.loc 1 1786 3 is_stmt 1 view .LVU1048
1786:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 3072              		.loc 1 1786 21 is_stmt 0 view .LVU1049
 3073 0054 CCF83810 		str	r1, [ip, #56]
1787:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 3074              		.loc 1 1787 3 is_stmt 1 view .LVU1050
1787:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 3075              		.loc 1 1787 21 is_stmt 0 view .LVU1051
 3076 0058 ACF83C30 		strh	r3, [ip, #60]	@ movhi
1788:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
 3077              		.loc 1 1788 3 is_stmt 1 view .LVU1052
1788:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
 3078              		.loc 1 1788 21 is_stmt 0 view .LVU1053
 3079 005c ACF83E30 		strh	r3, [ip, #62]	@ movhi
1789:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 3080              		.loc 1 1789 3 is_stmt 1 view .LVU1054
1789:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 3081              		.loc 1 1789 21 is_stmt 0 view .LVU1055
 3082 0060 CCF84020 		str	r2, [ip, #64]
1790:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
ARM GAS  /tmp/ccqUhOmw.s 			page 148


 3083              		.loc 1 1790 3 is_stmt 1 view .LVU1056
1790:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 3084              		.loc 1 1790 21 is_stmt 0 view .LVU1057
 3085 0064 ACF84430 		strh	r3, [ip, #68]	@ movhi
1791:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3086              		.loc 1 1791 3 is_stmt 1 view .LVU1058
1791:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3087              		.loc 1 1791 21 is_stmt 0 view .LVU1059
 3088 0068 ACF84630 		strh	r3, [ip, #70]	@ movhi
1794:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3089              		.loc 1 1794 3 is_stmt 1 view .LVU1060
1794:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3090              		.loc 1 1794 17 is_stmt 0 view .LVU1061
 3091 006c DCF80C20 		ldr	r2, [ip, #12]
 3092              	.LVL179:
1794:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3093              		.loc 1 1794 6 view .LVU1062
 3094 0070 B2F5E06F 		cmp	r2, #1792
 3095 0074 22D9     		bls	.L227
1796:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR     = SPI_2linesTxISR_16BIT;
 3096              		.loc 1 1796 5 is_stmt 1 view .LVU1063
1796:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR     = SPI_2linesTxISR_16BIT;
 3097              		.loc 1 1796 21 is_stmt 0 view .LVU1064
 3098 0076 2349     		ldr	r1, .L244
 3099              	.LVL180:
1796:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR     = SPI_2linesTxISR_16BIT;
 3100              		.loc 1 1796 21 view .LVU1065
 3101 0078 CCF84C10 		str	r1, [ip, #76]
1797:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3102              		.loc 1 1797 5 is_stmt 1 view .LVU1066
1797:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3103              		.loc 1 1797 21 is_stmt 0 view .LVU1067
 3104 007c 2249     		ldr	r1, .L244+4
 3105 007e CCF85010 		str	r1, [ip, #80]
 3106              	.L228:
1823:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3107              		.loc 1 1823 3 is_stmt 1 view .LVU1068
1823:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3108              		.loc 1 1823 6 is_stmt 0 view .LVU1069
 3109 0082 B2F5E06F 		cmp	r2, #1792
 3110 0086 01D8     		bhi	.L229
1823:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3111              		.loc 1 1823 49 discriminator 1 view .LVU1070
 3112 0088 012B     		cmp	r3, #1
 3113 008a 1ED9     		bls	.L230
 3114              	.L229:
1826:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3115              		.loc 1 1826 5 is_stmt 1 view .LVU1071
 3116 008c DCF80020 		ldr	r2, [ip]
 3117 0090 5368     		ldr	r3, [r2, #4]
 3118              	.LVL181:
1826:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3119              		.loc 1 1826 5 is_stmt 0 view .LVU1072
 3120 0092 23F48053 		bic	r3, r3, #4096
 3121 0096 5360     		str	r3, [r2, #4]
 3122              	.LVL182:
 3123              	.L231:
ARM GAS  /tmp/ccqUhOmw.s 			page 149


1835:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3124              		.loc 1 1835 3 is_stmt 1 view .LVU1073
 3125 0098 DCF80020 		ldr	r2, [ip]
 3126 009c 5368     		ldr	r3, [r2, #4]
 3127 009e 43F0E003 		orr	r3, r3, #224
 3128 00a2 5360     		str	r3, [r2, #4]
1838:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3129              		.loc 1 1838 3 view .LVU1074
1838:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3130              		.loc 1 1838 12 is_stmt 0 view .LVU1075
 3131 00a4 DCF80030 		ldr	r3, [ip]
1838:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3132              		.loc 1 1838 22 view .LVU1076
 3133 00a8 1A68     		ldr	r2, [r3]
1838:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3134              		.loc 1 1838 6 view .LVU1077
 3135 00aa 12F0400F 		tst	r2, #64
 3136 00ae 24D1     		bne	.L239
1841:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3137              		.loc 1 1841 5 is_stmt 1 view .LVU1078
 3138 00b0 1A68     		ldr	r2, [r3]
 3139 00b2 42F04002 		orr	r2, r2, #64
 3140 00b6 1A60     		str	r2, [r3]
1753:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3141              		.loc 1 1753 24 is_stmt 0 view .LVU1079
 3142 00b8 0020     		movs	r0, #0
 3143 00ba 0EE0     		b	.L225
 3144              	.LVL183:
 3145              	.L227:
1801:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR     = SPI_2linesTxISR_8BIT;
 3146              		.loc 1 1801 5 is_stmt 1 view .LVU1080
1801:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR     = SPI_2linesTxISR_8BIT;
 3147              		.loc 1 1801 21 is_stmt 0 view .LVU1081
 3148 00bc 1349     		ldr	r1, .L244+8
 3149              	.LVL184:
1801:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxISR     = SPI_2linesTxISR_8BIT;
 3150              		.loc 1 1801 21 view .LVU1082
 3151 00be CCF84C10 		str	r1, [ip, #76]
1802:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3152              		.loc 1 1802 5 is_stmt 1 view .LVU1083
1802:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3153              		.loc 1 1802 21 is_stmt 0 view .LVU1084
 3154 00c2 1349     		ldr	r1, .L244+12
 3155 00c4 CCF85010 		str	r1, [ip, #80]
 3156 00c8 DBE7     		b	.L228
 3157              	.L230:
1831:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3158              		.loc 1 1831 5 is_stmt 1 view .LVU1085
 3159 00ca DCF80020 		ldr	r2, [ip]
 3160 00ce 5368     		ldr	r3, [r2, #4]
 3161              	.LVL185:
1831:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3162              		.loc 1 1831 5 is_stmt 0 view .LVU1086
 3163 00d0 43F48053 		orr	r3, r3, #4096
 3164 00d4 5360     		str	r3, [r2, #4]
 3165              	.LVL186:
1831:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
ARM GAS  /tmp/ccqUhOmw.s 			page 150


 3166              		.loc 1 1831 5 view .LVU1087
 3167 00d6 DFE7     		b	.L231
 3168              	.LVL187:
 3169              	.L233:
1768:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3170              		.loc 1 1768 15 view .LVU1088
 3171 00d8 0220     		movs	r0, #2
 3172              	.LVL188:
 3173              	.L225:
1846:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 3174              		.loc 1 1846 3 is_stmt 1 view .LVU1089
1846:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 3175              		.loc 1 1846 3 view .LVU1090
 3176 00da 0023     		movs	r3, #0
 3177 00dc 8CF85C30 		strb	r3, [ip, #92]
1846:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 3178              		.loc 1 1846 3 view .LVU1091
1847:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 3179              		.loc 1 1847 3 view .LVU1092
1848:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3180              		.loc 1 1848 1 is_stmt 0 view .LVU1093
 3181 00e0 5DF8044B 		ldr	r4, [sp], #4
 3182              		.cfi_remember_state
 3183              		.cfi_restore 4
 3184              		.cfi_def_cfa_offset 0
 3185 00e4 7047     		bx	lr
 3186              	.LVL189:
 3187              	.L234:
 3188              		.cfi_restore_state
1768:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3189              		.loc 1 1768 15 view .LVU1094
 3190 00e6 0220     		movs	r0, #2
 3191              	.LVL190:
1768:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3192              		.loc 1 1768 15 view .LVU1095
 3193 00e8 F7E7     		b	.L225
 3194              	.LVL191:
 3195              	.L235:
1768:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3196              		.loc 1 1768 15 view .LVU1096
 3197 00ea 0220     		movs	r0, #2
 3198              	.LVL192:
1768:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3199              		.loc 1 1768 15 view .LVU1097
 3200 00ec F5E7     		b	.L225
 3201              	.LVL193:
 3202              	.L236:
1774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3203              		.loc 1 1774 15 view .LVU1098
 3204 00ee 0120     		movs	r0, #1
 3205              	.LVL194:
1774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3206              		.loc 1 1774 15 view .LVU1099
 3207 00f0 F3E7     		b	.L225
 3208              	.LVL195:
 3209              	.L237:
1774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
ARM GAS  /tmp/ccqUhOmw.s 			page 151


 3210              		.loc 1 1774 15 view .LVU1100
 3211 00f2 0120     		movs	r0, #1
 3212              	.LVL196:
1774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3213              		.loc 1 1774 15 view .LVU1101
 3214 00f4 F1E7     		b	.L225
 3215              	.LVL197:
 3216              	.L238:
1774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3217              		.loc 1 1774 15 view .LVU1102
 3218 00f6 0120     		movs	r0, #1
 3219              	.LVL198:
1774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3220              		.loc 1 1774 15 view .LVU1103
 3221 00f8 EFE7     		b	.L225
 3222              	.LVL199:
 3223              	.L239:
1753:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3224              		.loc 1 1753 24 view .LVU1104
 3225 00fa 0020     		movs	r0, #0
 3226 00fc EDE7     		b	.L225
 3227              	.LVL200:
 3228              	.L232:
 3229              		.cfi_def_cfa_offset 0
 3230              		.cfi_restore 4
1759:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3231              		.loc 1 1759 3 view .LVU1105
 3232 00fe 0220     		movs	r0, #2
1848:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3233              		.loc 1 1848 1 view .LVU1106
 3234 0100 7047     		bx	lr
 3235              	.L245:
 3236 0102 00BF     		.align	2
 3237              	.L244:
 3238 0104 00000000 		.word	SPI_2linesRxISR_16BIT
 3239 0108 00000000 		.word	SPI_2linesTxISR_16BIT
 3240 010c 00000000 		.word	SPI_2linesRxISR_8BIT
 3241 0110 00000000 		.word	SPI_2linesTxISR_8BIT
 3242              		.cfi_endproc
 3243              	.LFE139:
 3245              		.section	.text.HAL_SPI_Receive_IT,"ax",%progbits
 3246              		.align	1
 3247              		.global	HAL_SPI_Receive_IT
 3248              		.syntax unified
 3249              		.thumb
 3250              		.thumb_func
 3252              	HAL_SPI_Receive_IT:
 3253              	.LVL201:
 3254              	.LFB138:
1643:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 3255              		.loc 1 1643 1 is_stmt 1 view -0
 3256              		.cfi_startproc
 3257              		@ args = 0, pretend = 0, frame = 0
 3258              		@ frame_needed = 0, uses_anonymous_args = 0
1643:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 3259              		.loc 1 1643 1 is_stmt 0 view .LVU1108
 3260 0000 08B5     		push	{r3, lr}
ARM GAS  /tmp/ccqUhOmw.s 			page 152


 3261              		.cfi_def_cfa_offset 8
 3262              		.cfi_offset 3, -8
 3263              		.cfi_offset 14, -4
 3264 0002 8446     		mov	ip, r0
1644:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3265              		.loc 1 1644 3 is_stmt 1 view .LVU1109
 3266              	.LVL202:
1646:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3267              		.loc 1 1646 3 view .LVU1110
1646:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3268              		.loc 1 1646 18 is_stmt 0 view .LVU1111
 3269 0004 8368     		ldr	r3, [r0, #8]
1646:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3270              		.loc 1 1646 6 view .LVU1112
 3271 0006 1BB9     		cbnz	r3, .L247
1646:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3272              		.loc 1 1646 68 discriminator 1 view .LVU1113
 3273 0008 4368     		ldr	r3, [r0, #4]
1646:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3274              		.loc 1 1646 54 discriminator 1 view .LVU1114
 3275 000a B3F5827F 		cmp	r3, #260
 3276 000e 48D0     		beq	.L257
 3277              	.L247:
1654:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3278              		.loc 1 1654 3 is_stmt 1 view .LVU1115
1654:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3279              		.loc 1 1654 3 view .LVU1116
 3280 0010 9CF85C30 		ldrb	r3, [ip, #92]	@ zero_extendqisi2
 3281 0014 012B     		cmp	r3, #1
 3282 0016 6AD0     		beq	.L253
1654:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3283              		.loc 1 1654 3 discriminator 2 view .LVU1117
 3284 0018 0123     		movs	r3, #1
 3285 001a 8CF85C30 		strb	r3, [ip, #92]
1654:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3286              		.loc 1 1654 3 discriminator 2 view .LVU1118
1656:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3287              		.loc 1 1656 3 discriminator 2 view .LVU1119
1656:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3288              		.loc 1 1656 11 is_stmt 0 discriminator 2 view .LVU1120
 3289 001e 9CF85D00 		ldrb	r0, [ip, #93]	@ zero_extendqisi2
 3290              	.LVL203:
1656:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3291              		.loc 1 1656 11 discriminator 2 view .LVU1121
 3292 0022 C0B2     		uxtb	r0, r0
1656:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3293              		.loc 1 1656 6 discriminator 2 view .LVU1122
 3294 0024 9842     		cmp	r0, r3
 3295 0026 5BD1     		bne	.L254
1662:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3296              		.loc 1 1662 3 is_stmt 1 view .LVU1123
1662:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3297              		.loc 1 1662 6 is_stmt 0 view .LVU1124
 3298 0028 0029     		cmp	r1, #0
 3299 002a 5AD0     		beq	.L249
1662:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3300              		.loc 1 1662 23 discriminator 1 view .LVU1125
ARM GAS  /tmp/ccqUhOmw.s 			page 153


 3301 002c 002A     		cmp	r2, #0
 3302 002e 58D0     		beq	.L249
1669:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 3303              		.loc 1 1669 3 is_stmt 1 view .LVU1126
1669:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 3304              		.loc 1 1669 21 is_stmt 0 view .LVU1127
 3305 0030 0423     		movs	r3, #4
 3306 0032 8CF85D30 		strb	r3, [ip, #93]
1670:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
 3307              		.loc 1 1670 3 is_stmt 1 view .LVU1128
1670:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
 3308              		.loc 1 1670 21 is_stmt 0 view .LVU1129
 3309 0036 0023     		movs	r3, #0
 3310 0038 CCF86030 		str	r3, [ip, #96]
1671:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 3311              		.loc 1 1671 3 is_stmt 1 view .LVU1130
1671:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 3312              		.loc 1 1671 21 is_stmt 0 view .LVU1131
 3313 003c CCF84010 		str	r1, [ip, #64]
1672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 3314              		.loc 1 1672 3 is_stmt 1 view .LVU1132
1672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 3315              		.loc 1 1672 21 is_stmt 0 view .LVU1133
 3316 0040 ACF84420 		strh	r2, [ip, #68]	@ movhi
1673:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3317              		.loc 1 1673 3 is_stmt 1 view .LVU1134
1673:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3318              		.loc 1 1673 21 is_stmt 0 view .LVU1135
 3319 0044 ACF84620 		strh	r2, [ip, #70]	@ movhi
1676:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = 0U;
 3320              		.loc 1 1676 3 is_stmt 1 view .LVU1136
1676:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = 0U;
 3321              		.loc 1 1676 21 is_stmt 0 view .LVU1137
 3322 0048 CCF83830 		str	r3, [ip, #56]
1677:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 3323              		.loc 1 1677 3 is_stmt 1 view .LVU1138
1677:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 3324              		.loc 1 1677 21 is_stmt 0 view .LVU1139
 3325 004c ACF83C30 		strh	r3, [ip, #60]	@ movhi
1678:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 3326              		.loc 1 1678 3 is_stmt 1 view .LVU1140
1678:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 3327              		.loc 1 1678 21 is_stmt 0 view .LVU1141
 3328 0050 ACF83E30 		strh	r3, [ip, #62]	@ movhi
1679:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3329              		.loc 1 1679 3 is_stmt 1 view .LVU1142
1679:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3330              		.loc 1 1679 21 is_stmt 0 view .LVU1143
 3331 0054 CCF85030 		str	r3, [ip, #80]
1682:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3332              		.loc 1 1682 3 is_stmt 1 view .LVU1144
1682:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3333              		.loc 1 1682 17 is_stmt 0 view .LVU1145
 3334 0058 DCF80C30 		ldr	r3, [ip, #12]
1682:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3335              		.loc 1 1682 6 view .LVU1146
 3336 005c B3F5E06F 		cmp	r3, #1792
ARM GAS  /tmp/ccqUhOmw.s 			page 154


 3337 0060 27D9     		bls	.L250
1685:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxISR = SPI_RxISR_16BIT;
 3338              		.loc 1 1685 5 is_stmt 1 view .LVU1147
 3339 0062 DCF80020 		ldr	r2, [ip]
 3340              	.LVL204:
1685:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxISR = SPI_RxISR_16BIT;
 3341              		.loc 1 1685 5 is_stmt 0 view .LVU1148
 3342 0066 5368     		ldr	r3, [r2, #4]
 3343 0068 23F48053 		bic	r3, r3, #4096
 3344 006c 5360     		str	r3, [r2, #4]
 3345              	.LVL205:
1686:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3346              		.loc 1 1686 5 is_stmt 1 view .LVU1149
1686:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3347              		.loc 1 1686 17 is_stmt 0 view .LVU1150
 3348 006e 214B     		ldr	r3, .L259
 3349 0070 CCF84C30 		str	r3, [ip, #76]
 3350              	.L251:
1696:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3351              		.loc 1 1696 3 is_stmt 1 view .LVU1151
1696:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3352              		.loc 1 1696 17 is_stmt 0 view .LVU1152
 3353 0074 DCF80830 		ldr	r3, [ip, #8]
1696:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3354              		.loc 1 1696 6 view .LVU1153
 3355 0078 B3F5004F 		cmp	r3, #32768
 3356 007c 23D0     		beq	.L258
 3357              	.L252:
1721:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3358              		.loc 1 1721 3 is_stmt 1 view .LVU1154
 3359 007e DCF80020 		ldr	r2, [ip]
 3360 0082 5368     		ldr	r3, [r2, #4]
 3361 0084 43F06003 		orr	r3, r3, #96
 3362 0088 5360     		str	r3, [r2, #4]
1728:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3363              		.loc 1 1728 3 view .LVU1155
1728:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3364              		.loc 1 1728 12 is_stmt 0 view .LVU1156
 3365 008a DCF80030 		ldr	r3, [ip]
1728:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3366              		.loc 1 1728 22 view .LVU1157
 3367 008e 1A68     		ldr	r2, [r3]
1728:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3368              		.loc 1 1728 6 view .LVU1158
 3369 0090 12F0400F 		tst	r2, #64
 3370 0094 29D1     		bne	.L255
1731:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3371              		.loc 1 1731 5 is_stmt 1 view .LVU1159
 3372 0096 1A68     		ldr	r2, [r3]
 3373 0098 42F04002 		orr	r2, r2, #64
 3374 009c 1A60     		str	r2, [r3]
1644:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3375              		.loc 1 1644 21 is_stmt 0 view .LVU1160
 3376 009e 0020     		movs	r0, #0
 3377 00a0 1FE0     		b	.L249
 3378              	.LVL206:
 3379              	.L257:
ARM GAS  /tmp/ccqUhOmw.s 			page 155


1648:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Call transmit-receive function to send Dummy data on Tx line and generate clock on CLK line 
 3380              		.loc 1 1648 5 is_stmt 1 view .LVU1161
1648:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Call transmit-receive function to send Dummy data on Tx line and generate clock on CLK line 
 3381              		.loc 1 1648 17 is_stmt 0 view .LVU1162
 3382 00a2 0423     		movs	r3, #4
 3383 00a4 80F85D30 		strb	r3, [r0, #93]
1650:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3384              		.loc 1 1650 5 is_stmt 1 view .LVU1163
1650:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3385              		.loc 1 1650 12 is_stmt 0 view .LVU1164
 3386 00a8 1346     		mov	r3, r2
 3387 00aa 0A46     		mov	r2, r1
 3388              	.LVL207:
1650:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3389              		.loc 1 1650 12 view .LVU1165
 3390 00ac FFF7FEFF 		bl	HAL_SPI_TransmitReceive_IT
 3391              	.LVL208:
1650:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3392              		.loc 1 1650 12 view .LVU1166
 3393 00b0 1AE0     		b	.L248
 3394              	.LVL209:
 3395              	.L250:
1691:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxISR = SPI_RxISR_8BIT;
 3396              		.loc 1 1691 5 is_stmt 1 view .LVU1167
 3397 00b2 DCF80020 		ldr	r2, [ip]
 3398              	.LVL210:
1691:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxISR = SPI_RxISR_8BIT;
 3399              		.loc 1 1691 5 is_stmt 0 view .LVU1168
 3400 00b6 5368     		ldr	r3, [r2, #4]
 3401 00b8 43F48053 		orr	r3, r3, #4096
 3402 00bc 5360     		str	r3, [r2, #4]
 3403              	.LVL211:
1692:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3404              		.loc 1 1692 5 is_stmt 1 view .LVU1169
1692:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3405              		.loc 1 1692 17 is_stmt 0 view .LVU1170
 3406 00be 0E4B     		ldr	r3, .L259+4
 3407 00c0 CCF84C30 		str	r3, [ip, #76]
 3408 00c4 D6E7     		b	.L251
 3409              	.L258:
1699:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_RX(hspi);
 3410              		.loc 1 1699 5 is_stmt 1 view .LVU1171
 3411 00c6 DCF80020 		ldr	r2, [ip]
 3412 00ca 1368     		ldr	r3, [r2]
 3413 00cc 23F04003 		bic	r3, r3, #64
 3414 00d0 1360     		str	r3, [r2]
1700:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3415              		.loc 1 1700 5 view .LVU1172
 3416 00d2 DCF80020 		ldr	r2, [ip]
 3417 00d6 1368     		ldr	r3, [r2]
 3418 00d8 23F48043 		bic	r3, r3, #16384
 3419 00dc 1360     		str	r3, [r2]
 3420 00de CEE7     		b	.L252
 3421              	.LVL212:
 3422              	.L254:
1658:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3423              		.loc 1 1658 15 is_stmt 0 view .LVU1173
ARM GAS  /tmp/ccqUhOmw.s 			page 156


 3424 00e0 0220     		movs	r0, #2
 3425              	.LVL213:
 3426              	.L249:
1736:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 3427              		.loc 1 1736 3 is_stmt 1 view .LVU1174
1736:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 3428              		.loc 1 1736 3 view .LVU1175
 3429 00e2 0023     		movs	r3, #0
 3430 00e4 8CF85C30 		strb	r3, [ip, #92]
1736:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 3431              		.loc 1 1736 3 view .LVU1176
1737:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 3432              		.loc 1 1737 3 view .LVU1177
 3433              	.LVL214:
 3434              	.L248:
1738:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3435              		.loc 1 1738 1 is_stmt 0 view .LVU1178
 3436 00e8 08BD     		pop	{r3, pc}
 3437              	.LVL215:
 3438              	.L255:
1644:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3439              		.loc 1 1644 21 view .LVU1179
 3440 00ea 0020     		movs	r0, #0
 3441 00ec F9E7     		b	.L249
 3442              	.LVL216:
 3443              	.L253:
1654:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3444              		.loc 1 1654 3 view .LVU1180
 3445 00ee 0220     		movs	r0, #2
 3446              	.LVL217:
1654:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3447              		.loc 1 1654 3 view .LVU1181
 3448 00f0 FAE7     		b	.L248
 3449              	.L260:
 3450 00f2 00BF     		.align	2
 3451              	.L259:
 3452 00f4 00000000 		.word	SPI_RxISR_16BIT
 3453 00f8 00000000 		.word	SPI_RxISR_8BIT
 3454              		.cfi_endproc
 3455              	.LFE138:
 3457              		.section	.text.HAL_SPI_Transmit_DMA,"ax",%progbits
 3458              		.align	1
 3459              		.global	HAL_SPI_Transmit_DMA
 3460              		.syntax unified
 3461              		.thumb
 3462              		.thumb_func
 3464              	HAL_SPI_Transmit_DMA:
 3465              	.LVL218:
 3466              	.LFB140:
1859:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 3467              		.loc 1 1859 1 is_stmt 1 view -0
 3468              		.cfi_startproc
 3469              		@ args = 0, pretend = 0, frame = 0
 3470              		@ frame_needed = 0, uses_anonymous_args = 0
1859:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 3471              		.loc 1 1859 1 is_stmt 0 view .LVU1183
 3472 0000 38B5     		push	{r3, r4, r5, lr}
ARM GAS  /tmp/ccqUhOmw.s 			page 157


 3473              		.cfi_def_cfa_offset 16
 3474              		.cfi_offset 3, -16
 3475              		.cfi_offset 4, -12
 3476              		.cfi_offset 5, -8
 3477              		.cfi_offset 14, -4
1860:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3478              		.loc 1 1860 3 is_stmt 1 view .LVU1184
 3479              	.LVL219:
1863:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3480              		.loc 1 1863 3 view .LVU1185
1866:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3481              		.loc 1 1866 3 view .LVU1186
1869:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3482              		.loc 1 1869 3 view .LVU1187
1869:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3483              		.loc 1 1869 3 view .LVU1188
 3484 0002 90F85C30 		ldrb	r3, [r0, #92]	@ zero_extendqisi2
 3485 0006 012B     		cmp	r3, #1
 3486 0008 00F08C80 		beq	.L269
 3487 000c 0446     		mov	r4, r0
1869:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3488              		.loc 1 1869 3 discriminator 2 view .LVU1189
 3489 000e 0123     		movs	r3, #1
 3490 0010 80F85C30 		strb	r3, [r0, #92]
1869:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3491              		.loc 1 1869 3 discriminator 2 view .LVU1190
1871:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3492              		.loc 1 1871 3 discriminator 2 view .LVU1191
1871:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3493              		.loc 1 1871 11 is_stmt 0 discriminator 2 view .LVU1192
 3494 0014 90F85D50 		ldrb	r5, [r0, #93]	@ zero_extendqisi2
 3495 0018 EDB2     		uxtb	r5, r5
1871:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3496              		.loc 1 1871 6 discriminator 2 view .LVU1193
 3497 001a 9D42     		cmp	r5, r3
 3498 001c 7CD1     		bne	.L270
1877:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3499              		.loc 1 1877 3 is_stmt 1 view .LVU1194
1877:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3500              		.loc 1 1877 6 is_stmt 0 view .LVU1195
 3501 001e 0029     		cmp	r1, #0
 3502 0020 7BD0     		beq	.L263
1877:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3503              		.loc 1 1877 23 discriminator 1 view .LVU1196
 3504 0022 002A     		cmp	r2, #0
 3505 0024 79D0     		beq	.L263
1884:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 3506              		.loc 1 1884 3 is_stmt 1 view .LVU1197
1884:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 3507              		.loc 1 1884 21 is_stmt 0 view .LVU1198
 3508 0026 0323     		movs	r3, #3
 3509 0028 80F85D30 		strb	r3, [r0, #93]
1885:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pData;
 3510              		.loc 1 1885 3 is_stmt 1 view .LVU1199
1885:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pData;
 3511              		.loc 1 1885 21 is_stmt 0 view .LVU1200
 3512 002c 0023     		movs	r3, #0
ARM GAS  /tmp/ccqUhOmw.s 			page 158


 3513 002e 0366     		str	r3, [r0, #96]
1886:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 3514              		.loc 1 1886 3 is_stmt 1 view .LVU1201
1886:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 3515              		.loc 1 1886 21 is_stmt 0 view .LVU1202
 3516 0030 8163     		str	r1, [r0, #56]
1887:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 3517              		.loc 1 1887 3 is_stmt 1 view .LVU1203
1887:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 3518              		.loc 1 1887 21 is_stmt 0 view .LVU1204
 3519 0032 8287     		strh	r2, [r0, #60]	@ movhi
1888:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3520              		.loc 1 1888 3 is_stmt 1 view .LVU1205
1888:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3521              		.loc 1 1888 21 is_stmt 0 view .LVU1206
 3522 0034 C287     		strh	r2, [r0, #62]	@ movhi
1891:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 3523              		.loc 1 1891 3 is_stmt 1 view .LVU1207
1891:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 3524              		.loc 1 1891 21 is_stmt 0 view .LVU1208
 3525 0036 0364     		str	r3, [r0, #64]
1892:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
 3526              		.loc 1 1892 3 is_stmt 1 view .LVU1209
1892:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxISR       = NULL;
 3527              		.loc 1 1892 21 is_stmt 0 view .LVU1210
 3528 0038 0365     		str	r3, [r0, #80]
1893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = 0U;
 3529              		.loc 1 1893 3 is_stmt 1 view .LVU1211
1893:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = 0U;
 3530              		.loc 1 1893 21 is_stmt 0 view .LVU1212
 3531 003a C364     		str	r3, [r0, #76]
1894:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
 3532              		.loc 1 1894 3 is_stmt 1 view .LVU1213
1894:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
 3533              		.loc 1 1894 21 is_stmt 0 view .LVU1214
 3534 003c A0F84430 		strh	r3, [r0, #68]	@ movhi
1895:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3535              		.loc 1 1895 3 is_stmt 1 view .LVU1215
1895:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3536              		.loc 1 1895 21 is_stmt 0 view .LVU1216
 3537 0040 A0F84630 		strh	r3, [r0, #70]	@ movhi
1898:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3538              		.loc 1 1898 3 is_stmt 1 view .LVU1217
1898:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3539              		.loc 1 1898 17 is_stmt 0 view .LVU1218
 3540 0044 8368     		ldr	r3, [r0, #8]
1898:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3541              		.loc 1 1898 6 view .LVU1219
 3542 0046 B3F5004F 		cmp	r3, #32768
 3543 004a 39D0     		beq	.L272
 3544              	.LVL220:
 3545              	.L264:
1914:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3546              		.loc 1 1914 3 is_stmt 1 view .LVU1220
1914:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3547              		.loc 1 1914 7 is_stmt 0 view .LVU1221
 3548 004c 636D     		ldr	r3, [r4, #84]
ARM GAS  /tmp/ccqUhOmw.s 			page 159


1914:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3549              		.loc 1 1914 38 view .LVU1222
 3550 004e 364A     		ldr	r2, .L275
 3551 0050 DA62     		str	r2, [r3, #44]
1917:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3552              		.loc 1 1917 3 is_stmt 1 view .LVU1223
1917:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3553              		.loc 1 1917 7 is_stmt 0 view .LVU1224
 3554 0052 636D     		ldr	r3, [r4, #84]
1917:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3555              		.loc 1 1917 34 view .LVU1225
 3556 0054 354A     		ldr	r2, .L275+4
 3557 0056 9A62     		str	r2, [r3, #40]
1920:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3558              		.loc 1 1920 3 is_stmt 1 view .LVU1226
1920:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3559              		.loc 1 1920 7 is_stmt 0 view .LVU1227
 3560 0058 636D     		ldr	r3, [r4, #84]
1920:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3561              		.loc 1 1920 35 view .LVU1228
 3562 005a 354A     		ldr	r2, .L275+8
 3563 005c 1A63     		str	r2, [r3, #48]
1923:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3564              		.loc 1 1923 3 is_stmt 1 view .LVU1229
1923:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3565              		.loc 1 1923 7 is_stmt 0 view .LVU1230
 3566 005e 636D     		ldr	r3, [r4, #84]
1923:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3567              		.loc 1 1923 35 view .LVU1231
 3568 0060 0022     		movs	r2, #0
 3569 0062 5A63     		str	r2, [r3, #52]
1925:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Packing mode is enabled only if the DMA setting is HALWORD */
 3570              		.loc 1 1925 3 is_stmt 1 view .LVU1232
 3571 0064 2268     		ldr	r2, [r4]
 3572 0066 5368     		ldr	r3, [r2, #4]
 3573 0068 23F48043 		bic	r3, r3, #16384
 3574 006c 5360     		str	r3, [r2, #4]
1927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3575              		.loc 1 1927 3 view .LVU1233
1927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3576              		.loc 1 1927 18 is_stmt 0 view .LVU1234
 3577 006e E368     		ldr	r3, [r4, #12]
1927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3578              		.loc 1 1927 6 view .LVU1235
 3579 0070 B3F5E06F 		cmp	r3, #1792
 3580 0074 04D8     		bhi	.L265
1927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3581              		.loc 1 1927 58 discriminator 1 view .LVU1236
 3582 0076 636D     		ldr	r3, [r4, #84]
1927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3583              		.loc 1 1927 72 discriminator 1 view .LVU1237
 3584 0078 5B69     		ldr	r3, [r3, #20]
1927:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3585              		.loc 1 1927 50 discriminator 1 view .LVU1238
 3586 007a B3F5806F 		cmp	r3, #1024
 3587 007e 2AD0     		beq	.L273
 3588              	.L265:
ARM GAS  /tmp/ccqUhOmw.s 			page 160


1943:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
 3589              		.loc 1 1943 3 is_stmt 1 view .LVU1239
1943:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
 3590              		.loc 1 1943 91 is_stmt 0 view .LVU1240
 3591 0080 2268     		ldr	r2, [r4]
1944:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3592              		.loc 1 1944 38 view .LVU1241
 3593 0082 E38F     		ldrh	r3, [r4, #62]
1943:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
 3594              		.loc 1 1943 17 view .LVU1242
 3595 0084 9BB2     		uxth	r3, r3
 3596 0086 0C32     		adds	r2, r2, #12
 3597 0088 A16B     		ldr	r1, [r4, #56]
 3598              	.LVL221:
1943:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
 3599              		.loc 1 1943 17 view .LVU1243
 3600 008a 606D     		ldr	r0, [r4, #84]
 3601              	.LVL222:
1943:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
 3602              		.loc 1 1943 17 view .LVU1244
 3603 008c FFF7FEFF 		bl	HAL_DMA_Start_IT
 3604              	.LVL223:
1943:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
 3605              		.loc 1 1943 6 view .LVU1245
 3606 0090 0146     		mov	r1, r0
 3607 0092 0028     		cmp	r0, #0
 3608 0094 38D1     		bne	.L274
1955:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3609              		.loc 1 1955 3 is_stmt 1 view .LVU1246
1955:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3610              		.loc 1 1955 12 is_stmt 0 view .LVU1247
 3611 0096 2368     		ldr	r3, [r4]
1955:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3612              		.loc 1 1955 22 view .LVU1248
 3613 0098 1A68     		ldr	r2, [r3]
1955:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3614              		.loc 1 1955 6 view .LVU1249
 3615 009a 12F0400F 		tst	r2, #64
 3616 009e 03D1     		bne	.L268
1958:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3617              		.loc 1 1958 5 is_stmt 1 view .LVU1250
 3618 00a0 1A68     		ldr	r2, [r3]
 3619 00a2 42F04002 		orr	r2, r2, #64
 3620 00a6 1A60     		str	r2, [r3]
 3621              	.L268:
1962:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3622              		.loc 1 1962 3 view .LVU1251
 3623 00a8 2268     		ldr	r2, [r4]
 3624 00aa 5368     		ldr	r3, [r2, #4]
 3625 00ac 43F02003 		orr	r3, r3, #32
 3626 00b0 5360     		str	r3, [r2, #4]
1965:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3627              		.loc 1 1965 3 view .LVU1252
 3628 00b2 2268     		ldr	r2, [r4]
 3629 00b4 5368     		ldr	r3, [r2, #4]
 3630 00b6 43F00203 		orr	r3, r3, #2
 3631 00ba 5360     		str	r3, [r2, #4]
ARM GAS  /tmp/ccqUhOmw.s 			page 161


1860:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3632              		.loc 1 1860 21 is_stmt 0 view .LVU1253
 3633 00bc 0D46     		mov	r5, r1
 3634 00be 2CE0     		b	.L263
 3635              	.LVL224:
 3636              	.L272:
1901:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_TX(hspi);
 3637              		.loc 1 1901 5 is_stmt 1 view .LVU1254
 3638 00c0 0268     		ldr	r2, [r0]
 3639              	.LVL225:
1901:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_TX(hspi);
 3640              		.loc 1 1901 5 is_stmt 0 view .LVU1255
 3641 00c2 1368     		ldr	r3, [r2]
 3642 00c4 23F04003 		bic	r3, r3, #64
 3643 00c8 1360     		str	r3, [r2]
 3644              	.LVL226:
1902:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3645              		.loc 1 1902 5 is_stmt 1 view .LVU1256
 3646 00ca 0268     		ldr	r2, [r0]
 3647 00cc 1368     		ldr	r3, [r2]
 3648 00ce 43F48043 		orr	r3, r3, #16384
 3649 00d2 1360     		str	r3, [r2]
 3650 00d4 BAE7     		b	.L264
 3651              	.L273:
1930:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 3652              		.loc 1 1930 5 view .LVU1257
1930:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 3653              		.loc 1 1930 14 is_stmt 0 view .LVU1258
 3654 00d6 E38F     		ldrh	r3, [r4, #62]
1930:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 3655              		.loc 1 1930 8 view .LVU1259
 3656 00d8 13F0010F 		tst	r3, #1
 3657 00dc 09D1     		bne	.L266
1932:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount = (hspi->TxXferCount >> 1U);
 3658              		.loc 1 1932 7 is_stmt 1 view .LVU1260
 3659 00de 2268     		ldr	r2, [r4]
 3660 00e0 5368     		ldr	r3, [r2, #4]
 3661 00e2 23F48043 		bic	r3, r3, #16384
 3662 00e6 5360     		str	r3, [r2, #4]
1933:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 3663              		.loc 1 1933 7 view .LVU1261
1933:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 3664              		.loc 1 1933 32 is_stmt 0 view .LVU1262
 3665 00e8 E38F     		ldrh	r3, [r4, #62]
1933:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 3666              		.loc 1 1933 25 view .LVU1263
 3667 00ea C3F34E03 		ubfx	r3, r3, #1, #15
 3668 00ee E387     		strh	r3, [r4, #62]	@ movhi
 3669 00f0 C6E7     		b	.L265
 3670              	.L266:
1937:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       hspi->TxXferCount = (hspi->TxXferCount >> 1U) + 1U;
 3671              		.loc 1 1937 7 is_stmt 1 view .LVU1264
 3672 00f2 2268     		ldr	r2, [r4]
 3673 00f4 5368     		ldr	r3, [r2, #4]
 3674 00f6 43F48043 		orr	r3, r3, #16384
 3675 00fa 5360     		str	r3, [r2, #4]
1938:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
ARM GAS  /tmp/ccqUhOmw.s 			page 162


 3676              		.loc 1 1938 7 view .LVU1265
1938:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 3677              		.loc 1 1938 32 is_stmt 0 view .LVU1266
 3678 00fc E38F     		ldrh	r3, [r4, #62]
1938:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 3679              		.loc 1 1938 53 view .LVU1267
 3680 00fe C3F34E03 		ubfx	r3, r3, #1, #15
 3681 0102 0133     		adds	r3, r3, #1
1938:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 3682              		.loc 1 1938 25 view .LVU1268
 3683 0104 E387     		strh	r3, [r4, #62]	@ movhi
 3684 0106 BBE7     		b	.L265
 3685              	.LVL227:
 3686              	.L274:
1947:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
 3687              		.loc 1 1947 5 is_stmt 1 view .LVU1269
 3688 0108 236E     		ldr	r3, [r4, #96]
 3689 010a 43F01003 		orr	r3, r3, #16
 3690 010e 2366     		str	r3, [r4, #96]
1948:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3691              		.loc 1 1948 5 view .LVU1270
 3692              	.LVL228:
1950:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3693              		.loc 1 1950 5 view .LVU1271
1950:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3694              		.loc 1 1950 17 is_stmt 0 view .LVU1272
 3695 0110 0123     		movs	r3, #1
 3696 0112 84F85D30 		strb	r3, [r4, #93]
1951:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3697              		.loc 1 1951 5 is_stmt 1 view .LVU1273
 3698 0116 00E0     		b	.L263
 3699              	.LVL229:
 3700              	.L270:
1873:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3701              		.loc 1 1873 15 is_stmt 0 view .LVU1274
 3702 0118 0225     		movs	r5, #2
 3703              	.LVL230:
 3704              	.L263:
1969:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 3705              		.loc 1 1969 3 is_stmt 1 view .LVU1275
1969:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 3706              		.loc 1 1969 3 view .LVU1276
 3707 011a 0023     		movs	r3, #0
 3708 011c 84F85C30 		strb	r3, [r4, #92]
1969:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 3709              		.loc 1 1969 3 view .LVU1277
1970:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 3710              		.loc 1 1970 3 view .LVU1278
 3711              	.LVL231:
 3712              	.L262:
1971:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3713              		.loc 1 1971 1 is_stmt 0 view .LVU1279
 3714 0120 2846     		mov	r0, r5
 3715 0122 38BD     		pop	{r3, r4, r5, pc}
 3716              	.LVL232:
 3717              	.L269:
1869:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/ccqUhOmw.s 			page 163


 3718              		.loc 1 1869 3 view .LVU1280
 3719 0124 0225     		movs	r5, #2
 3720 0126 FBE7     		b	.L262
 3721              	.L276:
 3722              		.align	2
 3723              	.L275:
 3724 0128 00000000 		.word	SPI_DMAHalfTransmitCplt
 3725 012c 00000000 		.word	SPI_DMATransmitCplt
 3726 0130 00000000 		.word	SPI_DMAError
 3727              		.cfi_endproc
 3728              	.LFE140:
 3730              		.section	.text.HAL_SPI_TransmitReceive_DMA,"ax",%progbits
 3731              		.align	1
 3732              		.global	HAL_SPI_TransmitReceive_DMA
 3733              		.syntax unified
 3734              		.thumb
 3735              		.thumb_func
 3737              	HAL_SPI_TransmitReceive_DMA:
 3738              	.LVL233:
 3739              	.LFB142:
2139:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             tmp_mode;
 3740              		.loc 1 2139 1 is_stmt 1 view -0
 3741              		.cfi_startproc
 3742              		@ args = 0, pretend = 0, frame = 0
 3743              		@ frame_needed = 0, uses_anonymous_args = 0
2139:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t             tmp_mode;
 3744              		.loc 1 2139 1 is_stmt 0 view .LVU1282
 3745 0000 38B5     		push	{r3, r4, r5, lr}
 3746              		.cfi_def_cfa_offset 16
 3747              		.cfi_offset 3, -16
 3748              		.cfi_offset 4, -12
 3749              		.cfi_offset 5, -8
 3750              		.cfi_offset 14, -4
 3751 0002 0446     		mov	r4, r0
2140:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_SPI_StateTypeDef tmp_state;
 3752              		.loc 1 2140 3 is_stmt 1 view .LVU1283
2141:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 3753              		.loc 1 2141 3 view .LVU1284
2142:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3754              		.loc 1 2142 3 view .LVU1285
 3755              	.LVL234:
2145:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   assert_param(IS_SPI_DMA_HANDLE(hspi->hdmatx));
 3756              		.loc 1 2145 3 view .LVU1286
2146:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3757              		.loc 1 2146 3 view .LVU1287
2149:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3758              		.loc 1 2149 3 view .LVU1288
2152:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3759              		.loc 1 2152 3 view .LVU1289
2152:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3760              		.loc 1 2152 3 view .LVU1290
 3761 0004 90F85C00 		ldrb	r0, [r0, #92]	@ zero_extendqisi2
 3762              	.LVL235:
2152:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3763              		.loc 1 2152 3 is_stmt 0 view .LVU1291
 3764 0008 0128     		cmp	r0, #1
 3765 000a 00F00381 		beq	.L293
ARM GAS  /tmp/ccqUhOmw.s 			page 164


2152:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3766              		.loc 1 2152 3 is_stmt 1 discriminator 2 view .LVU1292
 3767 000e 0120     		movs	r0, #1
 3768 0010 84F85C00 		strb	r0, [r4, #92]
2152:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3769              		.loc 1 2152 3 discriminator 2 view .LVU1293
2155:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_mode            = hspi->Init.Mode;
 3770              		.loc 1 2155 3 discriminator 2 view .LVU1294
2155:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   tmp_mode            = hspi->Init.Mode;
 3771              		.loc 1 2155 23 is_stmt 0 discriminator 2 view .LVU1295
 3772 0014 94F85D00 		ldrb	r0, [r4, #93]	@ zero_extendqisi2
 3773 0018 C0B2     		uxtb	r0, r0
 3774              	.LVL236:
2156:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3775              		.loc 1 2156 3 is_stmt 1 discriminator 2 view .LVU1296
2156:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3776              		.loc 1 2156 23 is_stmt 0 discriminator 2 view .LVU1297
 3777 001a 6568     		ldr	r5, [r4, #4]
 3778              	.LVL237:
2158:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
 3779              		.loc 1 2158 3 is_stmt 1 discriminator 2 view .LVU1298
2158:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
 3780              		.loc 1 2158 6 is_stmt 0 discriminator 2 view .LVU1299
 3781 001c 0128     		cmp	r0, #1
 3782 001e 0AD0     		beq	.L279
2158:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         ((tmp_mode == SPI_MODE_MASTER) && (hspi->Init.Direction == SPI_DIRECTION_2LINES) && (tmp_st
 3783              		.loc 1 2158 7 discriminator 1 view .LVU1300
 3784 0020 B5F5827F 		cmp	r5, #260
 3785 0024 40F0E580 		bne	.L294
2159:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3786              		.loc 1 2159 54 view .LVU1301
 3787 0028 A568     		ldr	r5, [r4, #8]
 3788              	.LVL238:
2159:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3789              		.loc 1 2159 40 view .LVU1302
 3790 002a 002D     		cmp	r5, #0
 3791 002c 40F0E680 		bne	.L295
2159:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3792              		.loc 1 2159 90 discriminator 1 view .LVU1303
 3793 0030 0428     		cmp	r0, #4
 3794 0032 40F0E580 		bne	.L296
 3795              	.L279:
2165:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3796              		.loc 1 2165 3 is_stmt 1 view .LVU1304
2165:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3797              		.loc 1 2165 6 is_stmt 0 view .LVU1305
 3798 0036 0029     		cmp	r1, #0
 3799 0038 00F0E480 		beq	.L297
2165:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3800              		.loc 1 2165 25 discriminator 1 view .LVU1306
 3801 003c 002A     		cmp	r2, #0
 3802 003e 00F0E380 		beq	.L298
2165:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3803              		.loc 1 2165 46 discriminator 2 view .LVU1307
 3804 0042 002B     		cmp	r3, #0
 3805 0044 00F0E280 		beq	.L299
2172:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/ccqUhOmw.s 			page 165


 3806              		.loc 1 2172 3 is_stmt 1 view .LVU1308
2172:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3807              		.loc 1 2172 11 is_stmt 0 view .LVU1309
 3808 0048 94F85D00 		ldrb	r0, [r4, #93]	@ zero_extendqisi2
 3809              	.LVL239:
2172:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3810              		.loc 1 2172 11 view .LVU1310
 3811 004c C0B2     		uxtb	r0, r0
2172:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3812              		.loc 1 2172 6 view .LVU1311
 3813 004e 0428     		cmp	r0, #4
 3814 0050 02D0     		beq	.L281
2174:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3815              		.loc 1 2174 5 is_stmt 1 view .LVU1312
2174:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3816              		.loc 1 2174 17 is_stmt 0 view .LVU1313
 3817 0052 0520     		movs	r0, #5
 3818 0054 84F85D00 		strb	r0, [r4, #93]
 3819              	.L281:
2178:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pTxData;
 3820              		.loc 1 2178 3 is_stmt 1 view .LVU1314
2178:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr  = (uint8_t *)pTxData;
 3821              		.loc 1 2178 21 is_stmt 0 view .LVU1315
 3822 0058 0020     		movs	r0, #0
 3823 005a 2066     		str	r0, [r4, #96]
2179:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 3824              		.loc 1 2179 3 is_stmt 1 view .LVU1316
2179:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = Size;
 3825              		.loc 1 2179 21 is_stmt 0 view .LVU1317
 3826 005c A163     		str	r1, [r4, #56]
2180:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 3827              		.loc 1 2180 3 is_stmt 1 view .LVU1318
2180:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = Size;
 3828              		.loc 1 2180 21 is_stmt 0 view .LVU1319
 3829 005e A387     		strh	r3, [r4, #60]	@ movhi
2181:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
 3830              		.loc 1 2181 3 is_stmt 1 view .LVU1320
2181:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pRxData;
 3831              		.loc 1 2181 21 is_stmt 0 view .LVU1321
 3832 0060 E387     		strh	r3, [r4, #62]	@ movhi
2182:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 3833              		.loc 1 2182 3 is_stmt 1 view .LVU1322
2182:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 3834              		.loc 1 2182 21 is_stmt 0 view .LVU1323
 3835 0062 2264     		str	r2, [r4, #64]
2183:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 3836              		.loc 1 2183 3 is_stmt 1 view .LVU1324
2183:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 3837              		.loc 1 2183 21 is_stmt 0 view .LVU1325
 3838 0064 A4F84430 		strh	r3, [r4, #68]	@ movhi
2184:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3839              		.loc 1 2184 3 is_stmt 1 view .LVU1326
2184:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3840              		.loc 1 2184 21 is_stmt 0 view .LVU1327
 3841 0068 A4F84630 		strh	r3, [r4, #70]	@ movhi
2187:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 3842              		.loc 1 2187 3 is_stmt 1 view .LVU1328
ARM GAS  /tmp/ccqUhOmw.s 			page 166


2187:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 3843              		.loc 1 2187 21 is_stmt 0 view .LVU1329
 3844 006c E064     		str	r0, [r4, #76]
2188:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3845              		.loc 1 2188 3 is_stmt 1 view .LVU1330
2188:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3846              		.loc 1 2188 21 is_stmt 0 view .LVU1331
 3847 006e 2065     		str	r0, [r4, #80]
2200:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3848              		.loc 1 2200 3 is_stmt 1 view .LVU1332
2200:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3849              		.loc 1 2200 18 is_stmt 0 view .LVU1333
 3850 0070 E368     		ldr	r3, [r4, #12]
 3851              	.LVL240:
2200:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3852              		.loc 1 2200 6 view .LVU1334
 3853 0072 B3F5E06F 		cmp	r3, #1792
 3854 0076 05D8     		bhi	.L282
2200:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3855              		.loc 1 2200 58 discriminator 1 view .LVU1335
 3856 0078 A36D     		ldr	r3, [r4, #88]
2200:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3857              		.loc 1 2200 72 discriminator 1 view .LVU1336
 3858 007a 5B69     		ldr	r3, [r3, #20]
2200:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3859              		.loc 1 2200 50 discriminator 1 view .LVU1337
 3860 007c B3F5806F 		cmp	r3, #1024
 3861 0080 00F0C680 		beq	.L300
 3862              	.L282:
2209:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3863              		.loc 1 2209 3 is_stmt 1 view .LVU1338
 3864 0084 2268     		ldr	r2, [r4]
 3865              	.LVL241:
2209:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3866              		.loc 1 2209 3 is_stmt 0 view .LVU1339
 3867 0086 5368     		ldr	r3, [r2, #4]
 3868 0088 23F4C043 		bic	r3, r3, #24576
 3869 008c 5360     		str	r3, [r2, #4]
 3870              	.LVL242:
2212:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3871              		.loc 1 2212 3 is_stmt 1 view .LVU1340
2212:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3872              		.loc 1 2212 17 is_stmt 0 view .LVU1341
 3873 008e E368     		ldr	r3, [r4, #12]
2212:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3874              		.loc 1 2212 6 view .LVU1342
 3875 0090 B3F5E06F 		cmp	r3, #1792
 3876 0094 28D9     		bls	.L283
2215:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3877              		.loc 1 2215 5 is_stmt 1 view .LVU1343
 3878 0096 2268     		ldr	r2, [r4]
 3879 0098 5368     		ldr	r3, [r2, #4]
 3880 009a 23F48053 		bic	r3, r3, #4096
 3881 009e 5360     		str	r3, [r2, #4]
 3882              	.L284:
2255:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3883              		.loc 1 2255 3 view .LVU1344
ARM GAS  /tmp/ccqUhOmw.s 			page 167


2255:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3884              		.loc 1 2255 11 is_stmt 0 view .LVU1345
 3885 00a0 94F85D30 		ldrb	r3, [r4, #93]	@ zero_extendqisi2
 3886 00a4 DBB2     		uxtb	r3, r3
2255:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3887              		.loc 1 2255 6 view .LVU1346
 3888 00a6 042B     		cmp	r3, #4
 3889 00a8 69D0     		beq	.L302
2264:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->hdmarx->XferCpltCallback     = SPI_DMATransmitReceiveCplt;
 3890              		.loc 1 2264 5 is_stmt 1 view .LVU1347
2264:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->hdmarx->XferCpltCallback     = SPI_DMATransmitReceiveCplt;
 3891              		.loc 1 2264 9 is_stmt 0 view .LVU1348
 3892 00aa A36D     		ldr	r3, [r4, #88]
2264:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->hdmarx->XferCpltCallback     = SPI_DMATransmitReceiveCplt;
 3893              		.loc 1 2264 40 view .LVU1349
 3894 00ac 5A4A     		ldr	r2, .L305
 3895 00ae DA62     		str	r2, [r3, #44]
2265:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3896              		.loc 1 2265 5 is_stmt 1 view .LVU1350
2265:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3897              		.loc 1 2265 9 is_stmt 0 view .LVU1351
 3898 00b0 A36D     		ldr	r3, [r4, #88]
2265:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3899              		.loc 1 2265 40 view .LVU1352
 3900 00b2 5A4A     		ldr	r2, .L305+4
 3901 00b4 9A62     		str	r2, [r3, #40]
 3902              	.L289:
2269:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3903              		.loc 1 2269 3 is_stmt 1 view .LVU1353
2269:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3904              		.loc 1 2269 7 is_stmt 0 view .LVU1354
 3905 00b6 A36D     		ldr	r3, [r4, #88]
2269:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3906              		.loc 1 2269 35 view .LVU1355
 3907 00b8 594A     		ldr	r2, .L305+8
 3908 00ba 1A63     		str	r2, [r3, #48]
2272:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3909              		.loc 1 2272 3 is_stmt 1 view .LVU1356
2272:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3910              		.loc 1 2272 7 is_stmt 0 view .LVU1357
 3911 00bc A36D     		ldr	r3, [r4, #88]
2272:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3912              		.loc 1 2272 35 view .LVU1358
 3913 00be 0022     		movs	r2, #0
 3914 00c0 5A63     		str	r2, [r3, #52]
2275:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->RxXferCount))
 3915              		.loc 1 2275 3 is_stmt 1 view .LVU1359
2275:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->RxXferCount))
 3916              		.loc 1 2275 63 is_stmt 0 view .LVU1360
 3917 00c2 2168     		ldr	r1, [r4]
 3918              	.LVL243:
2276:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 3919              		.loc 1 2276 38 view .LVU1361
 3920 00c4 B4F84630 		ldrh	r3, [r4, #70]
2275:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->RxXferCount))
 3921              		.loc 1 2275 17 view .LVU1362
 3922 00c8 9BB2     		uxth	r3, r3
ARM GAS  /tmp/ccqUhOmw.s 			page 168


 3923 00ca 226C     		ldr	r2, [r4, #64]
 3924 00cc 0C31     		adds	r1, r1, #12
 3925 00ce A06D     		ldr	r0, [r4, #88]
 3926 00d0 FFF7FEFF 		bl	HAL_DMA_Start_IT
 3927              	.LVL244:
2275:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->RxXferCount))
 3928              		.loc 1 2275 6 view .LVU1363
 3929 00d4 0028     		cmp	r0, #0
 3930 00d6 59D0     		beq	.L290
2279:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
 3931              		.loc 1 2279 5 is_stmt 1 view .LVU1364
 3932 00d8 236E     		ldr	r3, [r4, #96]
 3933 00da 43F01003 		orr	r3, r3, #16
 3934 00de 2366     		str	r3, [r4, #96]
2280:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3935              		.loc 1 2280 5 view .LVU1365
 3936              	.LVL245:
2282:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3937              		.loc 1 2282 5 view .LVU1366
2282:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 3938              		.loc 1 2282 17 is_stmt 0 view .LVU1367
 3939 00e0 0120     		movs	r0, #1
 3940 00e2 84F85D00 		strb	r0, [r4, #93]
2283:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 3941              		.loc 1 2283 5 is_stmt 1 view .LVU1368
 3942 00e6 85E0     		b	.L280
 3943              	.LVL246:
 3944              	.L283:
2220:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3945              		.loc 1 2220 5 view .LVU1369
 3946 00e8 2268     		ldr	r2, [r4]
 3947 00ea 5368     		ldr	r3, [r2, #4]
 3948 00ec 43F48053 		orr	r3, r3, #4096
 3949 00f0 5360     		str	r3, [r2, #4]
2222:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 3950              		.loc 1 2222 5 view .LVU1370
2222:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 3951              		.loc 1 2222 13 is_stmt 0 view .LVU1371
 3952 00f2 636D     		ldr	r3, [r4, #84]
2222:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 3953              		.loc 1 2222 27 view .LVU1372
 3954 00f4 5B69     		ldr	r3, [r3, #20]
2222:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 3955              		.loc 1 2222 8 view .LVU1373
 3956 00f6 B3F5806F 		cmp	r3, #1024
 3957 00fa 1AD0     		beq	.L303
 3958              	.L285:
2236:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 3959              		.loc 1 2236 5 is_stmt 1 view .LVU1374
2236:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 3960              		.loc 1 2236 13 is_stmt 0 view .LVU1375
 3961 00fc A36D     		ldr	r3, [r4, #88]
2236:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 3962              		.loc 1 2236 27 view .LVU1376
 3963 00fe 5B69     		ldr	r3, [r3, #20]
2236:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 3964              		.loc 1 2236 8 view .LVU1377
ARM GAS  /tmp/ccqUhOmw.s 			page 169


 3965 0100 B3F5806F 		cmp	r3, #1024
 3966 0104 CCD1     		bne	.L284
2239:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 3967              		.loc 1 2239 7 is_stmt 1 view .LVU1378
 3968 0106 2268     		ldr	r2, [r4]
 3969 0108 5368     		ldr	r3, [r2, #4]
 3970 010a 23F48053 		bic	r3, r3, #4096
 3971 010e 5360     		str	r3, [r2, #4]
2241:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 3972              		.loc 1 2241 7 view .LVU1379
2241:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 3973              		.loc 1 2241 16 is_stmt 0 view .LVU1380
 3974 0110 B4F84630 		ldrh	r3, [r4, #70]
2241:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 3975              		.loc 1 2241 10 view .LVU1381
 3976 0114 13F0010F 		tst	r3, #1
 3977 0118 24D1     		bne	.L287
2243:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount = hspi->RxXferCount >> 1U;
 3978              		.loc 1 2243 9 is_stmt 1 view .LVU1382
 3979 011a 2268     		ldr	r2, [r4]
 3980 011c 5368     		ldr	r3, [r2, #4]
 3981 011e 23F40053 		bic	r3, r3, #8192
 3982 0122 5360     		str	r3, [r2, #4]
2244:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 3983              		.loc 1 2244 9 view .LVU1383
2244:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 3984              		.loc 1 2244 33 is_stmt 0 view .LVU1384
 3985 0124 B4F84630 		ldrh	r3, [r4, #70]
2244:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 3986              		.loc 1 2244 27 view .LVU1385
 3987 0128 C3F34E03 		ubfx	r3, r3, #1, #15
 3988 012c A4F84630 		strh	r3, [r4, #70]	@ movhi
 3989 0130 B6E7     		b	.L284
 3990              	.L303:
2224:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 3991              		.loc 1 2224 7 is_stmt 1 view .LVU1386
2224:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 3992              		.loc 1 2224 16 is_stmt 0 view .LVU1387
 3993 0132 A38F     		ldrh	r3, [r4, #60]
2224:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 3994              		.loc 1 2224 10 view .LVU1388
 3995 0134 13F0010F 		tst	r3, #1
 3996 0138 09D1     		bne	.L286
2226:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount = hspi->TxXferCount >> 1U;
 3997              		.loc 1 2226 9 is_stmt 1 view .LVU1389
 3998 013a 2268     		ldr	r2, [r4]
 3999 013c 5368     		ldr	r3, [r2, #4]
 4000 013e 23F48043 		bic	r3, r3, #16384
 4001 0142 5360     		str	r3, [r2, #4]
2227:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4002              		.loc 1 2227 9 view .LVU1390
2227:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4003              		.loc 1 2227 33 is_stmt 0 view .LVU1391
 4004 0144 E38F     		ldrh	r3, [r4, #62]
2227:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4005              		.loc 1 2227 27 view .LVU1392
 4006 0146 C3F34E03 		ubfx	r3, r3, #1, #15
ARM GAS  /tmp/ccqUhOmw.s 			page 170


 4007 014a E387     		strh	r3, [r4, #62]	@ movhi
 4008 014c D6E7     		b	.L285
 4009              	.L286:
2231:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->TxXferCount = (hspi->TxXferCount >> 1U) + 1U;
 4010              		.loc 1 2231 9 is_stmt 1 view .LVU1393
 4011 014e 2268     		ldr	r2, [r4]
 4012 0150 5368     		ldr	r3, [r2, #4]
 4013 0152 43F48043 		orr	r3, r3, #16384
 4014 0156 5360     		str	r3, [r2, #4]
2232:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4015              		.loc 1 2232 9 view .LVU1394
2232:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4016              		.loc 1 2232 34 is_stmt 0 view .LVU1395
 4017 0158 E38F     		ldrh	r3, [r4, #62]
2232:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4018              		.loc 1 2232 55 view .LVU1396
 4019 015a C3F34E03 		ubfx	r3, r3, #1, #15
 4020 015e 0133     		adds	r3, r3, #1
2232:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4021              		.loc 1 2232 27 view .LVU1397
 4022 0160 E387     		strh	r3, [r4, #62]	@ movhi
 4023 0162 CBE7     		b	.L285
 4024              	.L287:
2248:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount = (hspi->RxXferCount >> 1U) + 1U;
 4025              		.loc 1 2248 9 is_stmt 1 view .LVU1398
 4026 0164 2268     		ldr	r2, [r4]
 4027 0166 5368     		ldr	r3, [r2, #4]
 4028 0168 43F40053 		orr	r3, r3, #8192
 4029 016c 5360     		str	r3, [r2, #4]
2249:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4030              		.loc 1 2249 9 view .LVU1399
2249:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4031              		.loc 1 2249 34 is_stmt 0 view .LVU1400
 4032 016e B4F84630 		ldrh	r3, [r4, #70]
2249:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4033              		.loc 1 2249 55 view .LVU1401
 4034 0172 C3F34E03 		ubfx	r3, r3, #1, #15
 4035 0176 0133     		adds	r3, r3, #1
2249:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4036              		.loc 1 2249 27 view .LVU1402
 4037 0178 A4F84630 		strh	r3, [r4, #70]	@ movhi
 4038 017c 90E7     		b	.L284
 4039              	.L302:
2258:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->hdmarx->XferCpltCallback     = SPI_DMAReceiveCplt;
 4040              		.loc 1 2258 5 is_stmt 1 view .LVU1403
2258:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->hdmarx->XferCpltCallback     = SPI_DMAReceiveCplt;
 4041              		.loc 1 2258 9 is_stmt 0 view .LVU1404
 4042 017e A36D     		ldr	r3, [r4, #88]
2258:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->hdmarx->XferCpltCallback     = SPI_DMAReceiveCplt;
 4043              		.loc 1 2258 40 view .LVU1405
 4044 0180 284A     		ldr	r2, .L305+12
 4045 0182 DA62     		str	r2, [r3, #44]
2259:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4046              		.loc 1 2259 5 is_stmt 1 view .LVU1406
2259:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4047              		.loc 1 2259 9 is_stmt 0 view .LVU1407
 4048 0184 A36D     		ldr	r3, [r4, #88]
ARM GAS  /tmp/ccqUhOmw.s 			page 171


2259:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4049              		.loc 1 2259 40 view .LVU1408
 4050 0186 284A     		ldr	r2, .L305+16
 4051 0188 9A62     		str	r2, [r3, #40]
 4052 018a 94E7     		b	.L289
 4053              	.LVL247:
 4054              	.L290:
2287:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4055              		.loc 1 2287 3 is_stmt 1 view .LVU1409
 4056 018c 2268     		ldr	r2, [r4]
 4057 018e 5368     		ldr	r3, [r2, #4]
 4058 0190 43F00103 		orr	r3, r3, #1
 4059 0194 5360     		str	r3, [r2, #4]
2291:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferCpltCallback     = NULL;
 4060              		.loc 1 2291 3 view .LVU1410
2291:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferCpltCallback     = NULL;
 4061              		.loc 1 2291 7 is_stmt 0 view .LVU1411
 4062 0196 626D     		ldr	r2, [r4, #84]
2291:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferCpltCallback     = NULL;
 4063              		.loc 1 2291 38 view .LVU1412
 4064 0198 0023     		movs	r3, #0
 4065 019a D362     		str	r3, [r2, #44]
2292:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferErrorCallback    = NULL;
 4066              		.loc 1 2292 3 is_stmt 1 view .LVU1413
2292:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferErrorCallback    = NULL;
 4067              		.loc 1 2292 7 is_stmt 0 view .LVU1414
 4068 019c 626D     		ldr	r2, [r4, #84]
2292:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferErrorCallback    = NULL;
 4069              		.loc 1 2292 38 view .LVU1415
 4070 019e 9362     		str	r3, [r2, #40]
2293:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferAbortCallback    = NULL;
 4071              		.loc 1 2293 3 is_stmt 1 view .LVU1416
2293:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferAbortCallback    = NULL;
 4072              		.loc 1 2293 7 is_stmt 0 view .LVU1417
 4073 01a0 626D     		ldr	r2, [r4, #84]
2293:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->hdmatx->XferAbortCallback    = NULL;
 4074              		.loc 1 2293 38 view .LVU1418
 4075 01a2 1363     		str	r3, [r2, #48]
2294:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4076              		.loc 1 2294 3 is_stmt 1 view .LVU1419
2294:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4077              		.loc 1 2294 7 is_stmt 0 view .LVU1420
 4078 01a4 626D     		ldr	r2, [r4, #84]
2294:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4079              		.loc 1 2294 38 view .LVU1421
 4080 01a6 5363     		str	r3, [r2, #52]
2297:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
 4081              		.loc 1 2297 3 is_stmt 1 view .LVU1422
2297:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
 4082              		.loc 1 2297 91 is_stmt 0 view .LVU1423
 4083 01a8 2268     		ldr	r2, [r4]
2298:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4084              		.loc 1 2298 38 view .LVU1424
 4085 01aa E38F     		ldrh	r3, [r4, #62]
2297:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
 4086              		.loc 1 2297 17 view .LVU1425
 4087 01ac 9BB2     		uxth	r3, r3
ARM GAS  /tmp/ccqUhOmw.s 			page 172


 4088 01ae 0C32     		adds	r2, r2, #12
 4089 01b0 A16B     		ldr	r1, [r4, #56]
 4090 01b2 606D     		ldr	r0, [r4, #84]
 4091 01b4 FFF7FEFF 		bl	HAL_DMA_Start_IT
 4092              	.LVL248:
2297:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->TxXferCount))
 4093              		.loc 1 2297 6 view .LVU1426
 4094 01b8 98B9     		cbnz	r0, .L304
2309:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4095              		.loc 1 2309 3 is_stmt 1 view .LVU1427
2309:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4096              		.loc 1 2309 12 is_stmt 0 view .LVU1428
 4097 01ba 2368     		ldr	r3, [r4]
2309:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4098              		.loc 1 2309 22 view .LVU1429
 4099 01bc 1A68     		ldr	r2, [r3]
2309:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4100              		.loc 1 2309 6 view .LVU1430
 4101 01be 12F0400F 		tst	r2, #64
 4102 01c2 03D1     		bne	.L292
2312:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4103              		.loc 1 2312 5 is_stmt 1 view .LVU1431
 4104 01c4 1A68     		ldr	r2, [r3]
 4105 01c6 42F04002 		orr	r2, r2, #64
 4106 01ca 1A60     		str	r2, [r3]
 4107              	.L292:
2315:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4108              		.loc 1 2315 3 view .LVU1432
 4109 01cc 2268     		ldr	r2, [r4]
 4110 01ce 5368     		ldr	r3, [r2, #4]
 4111 01d0 43F02003 		orr	r3, r3, #32
 4112 01d4 5360     		str	r3, [r2, #4]
2318:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4113              		.loc 1 2318 3 view .LVU1433
 4114 01d6 2268     		ldr	r2, [r4]
 4115 01d8 5368     		ldr	r3, [r2, #4]
 4116 01da 43F00203 		orr	r3, r3, #2
 4117 01de 5360     		str	r3, [r2, #4]
 4118 01e0 08E0     		b	.L280
 4119              	.L304:
2301:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
 4120              		.loc 1 2301 5 view .LVU1434
 4121 01e2 236E     		ldr	r3, [r4, #96]
 4122 01e4 43F01003 		orr	r3, r3, #16
 4123 01e8 2366     		str	r3, [r4, #96]
2302:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4124              		.loc 1 2302 5 view .LVU1435
 4125              	.LVL249:
2304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4126              		.loc 1 2304 5 view .LVU1436
2304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4127              		.loc 1 2304 17 is_stmt 0 view .LVU1437
 4128 01ea 0120     		movs	r0, #1
 4129 01ec 84F85D00 		strb	r0, [r4, #93]
2305:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4130              		.loc 1 2305 5 is_stmt 1 view .LVU1438
 4131 01f0 00E0     		b	.L280
ARM GAS  /tmp/ccqUhOmw.s 			page 173


 4132              	.LVL250:
 4133              	.L294:
2161:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4134              		.loc 1 2161 15 is_stmt 0 view .LVU1439
 4135 01f2 0220     		movs	r0, #2
 4136              	.LVL251:
 4137              	.L280:
2322:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 4138              		.loc 1 2322 3 is_stmt 1 view .LVU1440
2322:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 4139              		.loc 1 2322 3 view .LVU1441
 4140 01f4 0023     		movs	r3, #0
 4141 01f6 84F85C30 		strb	r3, [r4, #92]
2322:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 4142              		.loc 1 2322 3 view .LVU1442
2323:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 4143              		.loc 1 2323 3 view .LVU1443
 4144              	.LVL252:
 4145              	.L278:
2324:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4146              		.loc 1 2324 1 is_stmt 0 view .LVU1444
 4147 01fa 38BD     		pop	{r3, r4, r5, pc}
 4148              	.LVL253:
 4149              	.L295:
2161:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4150              		.loc 1 2161 15 view .LVU1445
 4151 01fc 0220     		movs	r0, #2
 4152              	.LVL254:
2161:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4153              		.loc 1 2161 15 view .LVU1446
 4154 01fe F9E7     		b	.L280
 4155              	.LVL255:
 4156              	.L296:
2161:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4157              		.loc 1 2161 15 view .LVU1447
 4158 0200 0220     		movs	r0, #2
 4159              	.LVL256:
2161:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4160              		.loc 1 2161 15 view .LVU1448
 4161 0202 F7E7     		b	.L280
 4162              	.LVL257:
 4163              	.L297:
2167:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4164              		.loc 1 2167 15 view .LVU1449
 4165 0204 0120     		movs	r0, #1
 4166              	.LVL258:
2167:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4167              		.loc 1 2167 15 view .LVU1450
 4168 0206 F5E7     		b	.L280
 4169              	.LVL259:
 4170              	.L298:
2167:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4171              		.loc 1 2167 15 view .LVU1451
 4172 0208 0120     		movs	r0, #1
 4173              	.LVL260:
2167:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4174              		.loc 1 2167 15 view .LVU1452
ARM GAS  /tmp/ccqUhOmw.s 			page 174


 4175 020a F3E7     		b	.L280
 4176              	.LVL261:
 4177              	.L299:
2167:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4178              		.loc 1 2167 15 view .LVU1453
 4179 020c 0120     		movs	r0, #1
 4180              	.LVL262:
2167:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4181              		.loc 1 2167 15 view .LVU1454
 4182 020e F1E7     		b	.L280
 4183              	.LVL263:
 4184              	.L300:
2203:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4185              		.loc 1 2203 15 view .LVU1455
 4186 0210 0120     		movs	r0, #1
 4187 0212 EFE7     		b	.L280
 4188              	.LVL264:
 4189              	.L293:
2152:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4190              		.loc 1 2152 3 view .LVU1456
 4191 0214 0220     		movs	r0, #2
 4192 0216 F0E7     		b	.L278
 4193              	.L306:
 4194              		.align	2
 4195              	.L305:
 4196 0218 00000000 		.word	SPI_DMAHalfTransmitReceiveCplt
 4197 021c 00000000 		.word	SPI_DMATransmitReceiveCplt
 4198 0220 00000000 		.word	SPI_DMAError
 4199 0224 00000000 		.word	SPI_DMAHalfReceiveCplt
 4200 0228 00000000 		.word	SPI_DMAReceiveCplt
 4201              		.cfi_endproc
 4202              	.LFE142:
 4204              		.section	.text.HAL_SPI_Receive_DMA,"ax",%progbits
 4205              		.align	1
 4206              		.global	HAL_SPI_Receive_DMA
 4207              		.syntax unified
 4208              		.thumb
 4209              		.thumb_func
 4211              	HAL_SPI_Receive_DMA:
 4212              	.LVL265:
 4213              	.LFB141:
1984:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 4214              		.loc 1 1984 1 is_stmt 1 view -0
 4215              		.cfi_startproc
 4216              		@ args = 0, pretend = 0, frame = 0
 4217              		@ frame_needed = 0, uses_anonymous_args = 0
1984:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 4218              		.loc 1 1984 1 is_stmt 0 view .LVU1458
 4219 0000 38B5     		push	{r3, r4, r5, lr}
 4220              		.cfi_def_cfa_offset 16
 4221              		.cfi_offset 3, -16
 4222              		.cfi_offset 4, -12
 4223              		.cfi_offset 5, -8
 4224              		.cfi_offset 14, -4
 4225 0002 0446     		mov	r4, r0
1985:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4226              		.loc 1 1985 3 is_stmt 1 view .LVU1459
ARM GAS  /tmp/ccqUhOmw.s 			page 175


 4227              	.LVL266:
1988:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4228              		.loc 1 1988 3 view .LVU1460
1990:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4229              		.loc 1 1990 3 view .LVU1461
1990:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4230              		.loc 1 1990 18 is_stmt 0 view .LVU1462
 4231 0004 8368     		ldr	r3, [r0, #8]
1990:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4232              		.loc 1 1990 6 view .LVU1463
 4233 0006 1BB9     		cbnz	r3, .L308
1990:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4234              		.loc 1 1990 68 discriminator 1 view .LVU1464
 4235 0008 4068     		ldr	r0, [r0, #4]
 4236              	.LVL267:
1990:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4237              		.loc 1 1990 54 discriminator 1 view .LVU1465
 4238 000a B0F5827F 		cmp	r0, #260
 4239 000e 69D0     		beq	.L321
 4240              	.L308:
2002:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4241              		.loc 1 2002 3 is_stmt 1 view .LVU1466
2002:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4242              		.loc 1 2002 3 view .LVU1467
 4243 0010 94F85C00 		ldrb	r0, [r4, #92]	@ zero_extendqisi2
 4244 0014 0128     		cmp	r0, #1
 4245 0016 00F0B580 		beq	.L318
2002:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4246              		.loc 1 2002 3 discriminator 2 view .LVU1468
 4247 001a 0120     		movs	r0, #1
 4248 001c 84F85C00 		strb	r0, [r4, #92]
2002:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4249              		.loc 1 2002 3 discriminator 2 view .LVU1469
2004:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4250              		.loc 1 2004 3 discriminator 2 view .LVU1470
2004:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4251              		.loc 1 2004 11 is_stmt 0 discriminator 2 view .LVU1471
 4252 0020 94F85D50 		ldrb	r5, [r4, #93]	@ zero_extendqisi2
 4253 0024 EDB2     		uxtb	r5, r5
2004:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4254              		.loc 1 2004 6 discriminator 2 view .LVU1472
 4255 0026 8542     		cmp	r5, r0
 4256 0028 40F0A680 		bne	.L319
2010:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4257              		.loc 1 2010 3 is_stmt 1 view .LVU1473
2010:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4258              		.loc 1 2010 6 is_stmt 0 view .LVU1474
 4259 002c 0029     		cmp	r1, #0
 4260 002e 00F0A480 		beq	.L310
2010:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4261              		.loc 1 2010 23 discriminator 1 view .LVU1475
 4262 0032 002A     		cmp	r2, #0
 4263 0034 00F0A180 		beq	.L310
2017:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 4264              		.loc 1 2017 3 is_stmt 1 view .LVU1476
2017:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->ErrorCode   = HAL_SPI_ERROR_NONE;
 4265              		.loc 1 2017 21 is_stmt 0 view .LVU1477
ARM GAS  /tmp/ccqUhOmw.s 			page 176


 4266 0038 0420     		movs	r0, #4
 4267 003a 84F85D00 		strb	r0, [r4, #93]
2018:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
 4268              		.loc 1 2018 3 is_stmt 1 view .LVU1478
2018:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr  = (uint8_t *)pData;
 4269              		.loc 1 2018 21 is_stmt 0 view .LVU1479
 4270 003e 0020     		movs	r0, #0
 4271 0040 2066     		str	r0, [r4, #96]
2019:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 4272              		.loc 1 2019 3 is_stmt 1 view .LVU1480
2019:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferSize  = Size;
 4273              		.loc 1 2019 21 is_stmt 0 view .LVU1481
 4274 0042 2164     		str	r1, [r4, #64]
2020:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 4275              		.loc 1 2020 3 is_stmt 1 view .LVU1482
2020:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = Size;
 4276              		.loc 1 2020 21 is_stmt 0 view .LVU1483
 4277 0044 A4F84420 		strh	r2, [r4, #68]	@ movhi
2021:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4278              		.loc 1 2021 3 is_stmt 1 view .LVU1484
2021:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4279              		.loc 1 2021 21 is_stmt 0 view .LVU1485
 4280 0048 A4F84620 		strh	r2, [r4, #70]	@ movhi
2024:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 4281              		.loc 1 2024 3 is_stmt 1 view .LVU1486
2024:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxISR       = NULL;
 4282              		.loc 1 2024 21 is_stmt 0 view .LVU1487
 4283 004c E064     		str	r0, [r4, #76]
2025:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = 0U;
 4284              		.loc 1 2025 3 is_stmt 1 view .LVU1488
2025:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferSize  = 0U;
 4285              		.loc 1 2025 21 is_stmt 0 view .LVU1489
 4286 004e 2065     		str	r0, [r4, #80]
2026:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 4287              		.loc 1 2026 3 is_stmt 1 view .LVU1490
2026:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 4288              		.loc 1 2026 21 is_stmt 0 view .LVU1491
 4289 0050 A087     		strh	r0, [r4, #60]	@ movhi
2027:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4290              		.loc 1 2027 3 is_stmt 1 view .LVU1492
2027:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4291              		.loc 1 2027 21 is_stmt 0 view .LVU1493
 4292 0052 E087     		strh	r0, [r4, #62]	@ movhi
2030:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4293              		.loc 1 2030 3 is_stmt 1 view .LVU1494
2030:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4294              		.loc 1 2030 6 is_stmt 0 view .LVU1495
 4295 0054 B3F5004F 		cmp	r3, #32768
 4296 0058 4ED0     		beq	.L322
 4297              	.LVL268:
 4298              	.L311:
2047:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4299              		.loc 1 2047 3 is_stmt 1 view .LVU1496
2047:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4300              		.loc 1 2047 18 is_stmt 0 view .LVU1497
 4301 005a E368     		ldr	r3, [r4, #12]
2047:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/ccqUhOmw.s 			page 177


 4302              		.loc 1 2047 6 view .LVU1498
 4303 005c B3F5E06F 		cmp	r3, #1792
 4304 0060 05D8     		bhi	.L312
2047:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4305              		.loc 1 2047 58 discriminator 1 view .LVU1499
 4306 0062 A36D     		ldr	r3, [r4, #88]
2047:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4307              		.loc 1 2047 72 discriminator 1 view .LVU1500
 4308 0064 5B69     		ldr	r3, [r3, #20]
2047:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4309              		.loc 1 2047 50 discriminator 1 view .LVU1501
 4310 0066 B3F5806F 		cmp	r3, #1024
 4311 006a 00F08680 		beq	.L310
 4312              	.L312:
2055:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->Init.DataSize > SPI_DATASIZE_8BIT)
 4313              		.loc 1 2055 3 is_stmt 1 view .LVU1502
 4314 006e 2268     		ldr	r2, [r4]
 4315 0070 5368     		ldr	r3, [r2, #4]
 4316 0072 23F40053 		bic	r3, r3, #8192
 4317 0076 5360     		str	r3, [r2, #4]
2056:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4318              		.loc 1 2056 3 view .LVU1503
2056:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4319              		.loc 1 2056 17 is_stmt 0 view .LVU1504
 4320 0078 E368     		ldr	r3, [r4, #12]
2056:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4321              		.loc 1 2056 6 view .LVU1505
 4322 007a B3F5E06F 		cmp	r3, #1792
 4323 007e 46D9     		bls	.L313
2059:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4324              		.loc 1 2059 5 is_stmt 1 view .LVU1506
 4325 0080 2268     		ldr	r2, [r4]
 4326 0082 5368     		ldr	r3, [r2, #4]
 4327 0084 23F48053 		bic	r3, r3, #4096
 4328 0088 5360     		str	r3, [r2, #4]
 4329              	.L314:
2085:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4330              		.loc 1 2085 3 view .LVU1507
2085:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4331              		.loc 1 2085 7 is_stmt 0 view .LVU1508
 4332 008a A36D     		ldr	r3, [r4, #88]
2085:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4333              		.loc 1 2085 38 view .LVU1509
 4334 008c 3E4A     		ldr	r2, .L324
 4335 008e DA62     		str	r2, [r3, #44]
2088:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4336              		.loc 1 2088 3 is_stmt 1 view .LVU1510
2088:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4337              		.loc 1 2088 7 is_stmt 0 view .LVU1511
 4338 0090 A36D     		ldr	r3, [r4, #88]
2088:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4339              		.loc 1 2088 34 view .LVU1512
 4340 0092 3E4A     		ldr	r2, .L324+4
 4341 0094 9A62     		str	r2, [r3, #40]
2091:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4342              		.loc 1 2091 3 is_stmt 1 view .LVU1513
2091:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/ccqUhOmw.s 			page 178


 4343              		.loc 1 2091 7 is_stmt 0 view .LVU1514
 4344 0096 A36D     		ldr	r3, [r4, #88]
2091:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4345              		.loc 1 2091 35 view .LVU1515
 4346 0098 3D4A     		ldr	r2, .L324+8
 4347 009a 1A63     		str	r2, [r3, #48]
2094:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4348              		.loc 1 2094 3 is_stmt 1 view .LVU1516
2094:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4349              		.loc 1 2094 7 is_stmt 0 view .LVU1517
 4350 009c A36D     		ldr	r3, [r4, #88]
2094:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4351              		.loc 1 2094 35 view .LVU1518
 4352 009e 0022     		movs	r2, #0
 4353 00a0 5A63     		str	r2, [r3, #52]
2097:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->RxXferCount))
 4354              		.loc 1 2097 3 is_stmt 1 view .LVU1519
2097:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->RxXferCount))
 4355              		.loc 1 2097 63 is_stmt 0 view .LVU1520
 4356 00a2 2168     		ldr	r1, [r4]
 4357              	.LVL269:
2098:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4358              		.loc 1 2098 38 view .LVU1521
 4359 00a4 B4F84630 		ldrh	r3, [r4, #70]
2097:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->RxXferCount))
 4360              		.loc 1 2097 17 view .LVU1522
 4361 00a8 9BB2     		uxth	r3, r3
 4362 00aa 226C     		ldr	r2, [r4, #64]
 4363 00ac 0C31     		adds	r1, r1, #12
 4364 00ae A06D     		ldr	r0, [r4, #88]
 4365 00b0 FFF7FEFF 		bl	HAL_DMA_Start_IT
 4366              	.LVL270:
2097:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****                                  hspi->RxXferCount))
 4367              		.loc 1 2097 6 view .LVU1523
 4368 00b4 0146     		mov	r1, r0
 4369 00b6 0028     		cmp	r0, #0
 4370 00b8 56D1     		bne	.L323
2109:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4371              		.loc 1 2109 3 is_stmt 1 view .LVU1524
2109:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4372              		.loc 1 2109 12 is_stmt 0 view .LVU1525
 4373 00ba 2368     		ldr	r3, [r4]
2109:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4374              		.loc 1 2109 22 view .LVU1526
 4375 00bc 1A68     		ldr	r2, [r3]
2109:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4376              		.loc 1 2109 6 view .LVU1527
 4377 00be 12F0400F 		tst	r2, #64
 4378 00c2 03D1     		bne	.L317
2112:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4379              		.loc 1 2112 5 is_stmt 1 view .LVU1528
 4380 00c4 1A68     		ldr	r2, [r3]
 4381 00c6 42F04002 		orr	r2, r2, #64
 4382 00ca 1A60     		str	r2, [r3]
 4383              	.L317:
2116:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4384              		.loc 1 2116 3 view .LVU1529
ARM GAS  /tmp/ccqUhOmw.s 			page 179


 4385 00cc 2268     		ldr	r2, [r4]
 4386 00ce 5368     		ldr	r3, [r2, #4]
 4387 00d0 43F02003 		orr	r3, r3, #32
 4388 00d4 5360     		str	r3, [r2, #4]
2119:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4389              		.loc 1 2119 3 view .LVU1530
 4390 00d6 2268     		ldr	r2, [r4]
 4391 00d8 5368     		ldr	r3, [r2, #4]
 4392 00da 43F00103 		orr	r3, r3, #1
 4393 00de 5360     		str	r3, [r2, #4]
1985:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4394              		.loc 1 1985 21 is_stmt 0 view .LVU1531
 4395 00e0 0D46     		mov	r5, r1
 4396 00e2 4AE0     		b	.L310
 4397              	.LVL271:
 4398              	.L321:
1992:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4399              		.loc 1 1992 5 is_stmt 1 view .LVU1532
1992:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4400              		.loc 1 1992 17 is_stmt 0 view .LVU1533
 4401 00e4 0423     		movs	r3, #4
 4402 00e6 84F85D30 		strb	r3, [r4, #93]
1995:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4403              		.loc 1 1995 5 is_stmt 1 view .LVU1534
1998:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4404              		.loc 1 1998 5 view .LVU1535
1998:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4405              		.loc 1 1998 12 is_stmt 0 view .LVU1536
 4406 00ea 1346     		mov	r3, r2
 4407 00ec 0A46     		mov	r2, r1
 4408              	.LVL272:
1998:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4409              		.loc 1 1998 12 view .LVU1537
 4410 00ee 2046     		mov	r0, r4
 4411 00f0 FFF7FEFF 		bl	HAL_SPI_TransmitReceive_DMA
 4412              	.LVL273:
1998:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4413              		.loc 1 1998 12 view .LVU1538
 4414 00f4 0546     		mov	r5, r0
 4415 00f6 43E0     		b	.L309
 4416              	.LVL274:
 4417              	.L322:
2033:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_RX(hspi);
 4418              		.loc 1 2033 5 is_stmt 1 view .LVU1539
 4419 00f8 2268     		ldr	r2, [r4]
 4420              	.LVL275:
2033:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     SPI_1LINE_RX(hspi);
 4421              		.loc 1 2033 5 is_stmt 0 view .LVU1540
 4422 00fa 1368     		ldr	r3, [r2]
 4423 00fc 23F04003 		bic	r3, r3, #64
 4424 0100 1360     		str	r3, [r2]
 4425              	.LVL276:
2034:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4426              		.loc 1 2034 5 is_stmt 1 view .LVU1541
 4427 0102 2268     		ldr	r2, [r4]
 4428 0104 1368     		ldr	r3, [r2]
 4429 0106 23F48043 		bic	r3, r3, #16384
ARM GAS  /tmp/ccqUhOmw.s 			page 180


 4430 010a 1360     		str	r3, [r2]
 4431 010c A5E7     		b	.L311
 4432              	.L313:
2064:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4433              		.loc 1 2064 5 view .LVU1542
 4434 010e 2268     		ldr	r2, [r4]
 4435 0110 5368     		ldr	r3, [r2, #4]
 4436 0112 43F48053 		orr	r3, r3, #4096
 4437 0116 5360     		str	r3, [r2, #4]
2066:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4438              		.loc 1 2066 5 view .LVU1543
2066:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4439              		.loc 1 2066 13 is_stmt 0 view .LVU1544
 4440 0118 A36D     		ldr	r3, [r4, #88]
2066:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4441              		.loc 1 2066 27 view .LVU1545
 4442 011a 5B69     		ldr	r3, [r3, #20]
2066:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4443              		.loc 1 2066 8 view .LVU1546
 4444 011c B3F5806F 		cmp	r3, #1024
 4445 0120 B3D1     		bne	.L314
2069:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4446              		.loc 1 2069 7 is_stmt 1 view .LVU1547
 4447 0122 2268     		ldr	r2, [r4]
 4448 0124 5368     		ldr	r3, [r2, #4]
 4449 0126 23F48053 		bic	r3, r3, #4096
 4450 012a 5360     		str	r3, [r2, #4]
2071:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4451              		.loc 1 2071 7 view .LVU1548
2071:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4452              		.loc 1 2071 16 is_stmt 0 view .LVU1549
 4453 012c B4F84630 		ldrh	r3, [r4, #70]
2071:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4454              		.loc 1 2071 10 view .LVU1550
 4455 0130 13F0010F 		tst	r3, #1
 4456 0134 0BD1     		bne	.L315
2073:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount = hspi->RxXferCount >> 1U;
 4457              		.loc 1 2073 9 is_stmt 1 view .LVU1551
 4458 0136 2268     		ldr	r2, [r4]
 4459 0138 5368     		ldr	r3, [r2, #4]
 4460 013a 23F40053 		bic	r3, r3, #8192
 4461 013e 5360     		str	r3, [r2, #4]
2074:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4462              		.loc 1 2074 9 view .LVU1552
2074:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4463              		.loc 1 2074 33 is_stmt 0 view .LVU1553
 4464 0140 B4F84630 		ldrh	r3, [r4, #70]
2074:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4465              		.loc 1 2074 27 view .LVU1554
 4466 0144 C3F34E03 		ubfx	r3, r3, #1, #15
 4467 0148 A4F84630 		strh	r3, [r4, #70]	@ movhi
 4468 014c 9DE7     		b	.L314
 4469              	.L315:
2078:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->RxXferCount = (hspi->RxXferCount >> 1U) + 1U;
 4470              		.loc 1 2078 9 is_stmt 1 view .LVU1555
 4471 014e 2268     		ldr	r2, [r4]
 4472 0150 5368     		ldr	r3, [r2, #4]
ARM GAS  /tmp/ccqUhOmw.s 			page 181


 4473 0152 43F40053 		orr	r3, r3, #8192
 4474 0156 5360     		str	r3, [r2, #4]
2079:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4475              		.loc 1 2079 9 view .LVU1556
2079:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4476              		.loc 1 2079 34 is_stmt 0 view .LVU1557
 4477 0158 B4F84630 		ldrh	r3, [r4, #70]
2079:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4478              		.loc 1 2079 55 view .LVU1558
 4479 015c C3F34E03 		ubfx	r3, r3, #1, #15
 4480 0160 0133     		adds	r3, r3, #1
2079:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4481              		.loc 1 2079 27 view .LVU1559
 4482 0162 A4F84630 		strh	r3, [r4, #70]	@ movhi
 4483 0166 90E7     		b	.L314
 4484              	.LVL277:
 4485              	.L323:
2101:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     errorcode = HAL_ERROR;
 4486              		.loc 1 2101 5 is_stmt 1 view .LVU1560
 4487 0168 236E     		ldr	r3, [r4, #96]
 4488 016a 43F01003 		orr	r3, r3, #16
 4489 016e 2366     		str	r3, [r4, #96]
2102:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4490              		.loc 1 2102 5 view .LVU1561
 4491              	.LVL278:
2104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4492              		.loc 1 2104 5 view .LVU1562
2104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4493              		.loc 1 2104 17 is_stmt 0 view .LVU1563
 4494 0170 0123     		movs	r3, #1
 4495 0172 84F85D30 		strb	r3, [r4, #93]
2105:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4496              		.loc 1 2105 5 is_stmt 1 view .LVU1564
 4497 0176 00E0     		b	.L310
 4498              	.LVL279:
 4499              	.L319:
2006:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     goto error;
 4500              		.loc 1 2006 15 is_stmt 0 view .LVU1565
 4501 0178 0225     		movs	r5, #2
 4502              	.LVL280:
 4503              	.L310:
2123:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 4504              		.loc 1 2123 3 is_stmt 1 view .LVU1566
2123:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 4505              		.loc 1 2123 3 view .LVU1567
 4506 017a 0023     		movs	r3, #0
 4507 017c 84F85C30 		strb	r3, [r4, #92]
2123:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 4508              		.loc 1 2123 3 view .LVU1568
2124:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 4509              		.loc 1 2124 3 view .LVU1569
 4510              	.LVL281:
 4511              	.L309:
2125:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4512              		.loc 1 2125 1 is_stmt 0 view .LVU1570
 4513 0180 2846     		mov	r0, r5
 4514 0182 38BD     		pop	{r3, r4, r5, pc}
ARM GAS  /tmp/ccqUhOmw.s 			page 182


 4515              	.LVL282:
 4516              	.L318:
2002:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4517              		.loc 1 2002 3 view .LVU1571
 4518 0184 0225     		movs	r5, #2
 4519 0186 FBE7     		b	.L309
 4520              	.L325:
 4521              		.align	2
 4522              	.L324:
 4523 0188 00000000 		.word	SPI_DMAHalfReceiveCplt
 4524 018c 00000000 		.word	SPI_DMAReceiveCplt
 4525 0190 00000000 		.word	SPI_DMAError
 4526              		.cfi_endproc
 4527              	.LFE141:
 4529              		.section	.text.HAL_SPI_Abort,"ax",%progbits
 4530              		.align	1
 4531              		.global	HAL_SPI_Abort
 4532              		.syntax unified
 4533              		.thumb
 4534              		.thumb_func
 4536              	HAL_SPI_Abort:
 4537              	.LVL283:
 4538              	.LFB143:
2340:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode;
 4539              		.loc 1 2340 1 is_stmt 1 view -0
 4540              		.cfi_startproc
 4541              		@ args = 0, pretend = 0, frame = 16
 4542              		@ frame_needed = 0, uses_anonymous_args = 0
2340:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode;
 4543              		.loc 1 2340 1 is_stmt 0 view .LVU1573
 4544 0000 10B5     		push	{r4, lr}
 4545              		.cfi_def_cfa_offset 8
 4546              		.cfi_offset 4, -8
 4547              		.cfi_offset 14, -4
 4548 0002 86B0     		sub	sp, sp, #24
 4549              		.cfi_def_cfa_offset 32
 4550 0004 0446     		mov	r4, r0
2341:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t count;
 4551              		.loc 1 2341 3 is_stmt 1 view .LVU1574
2342:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t resetcount;
 4552              		.loc 1 2342 3 view .LVU1575
2343:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4553              		.loc 1 2343 3 view .LVU1576
2346:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   resetcount = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24U / 1000U);
 4554              		.loc 1 2346 3 view .LVU1577
 4555              	.LVL284:
2347:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = resetcount;
 4556              		.loc 1 2347 3 view .LVU1578
2347:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = resetcount;
 4557              		.loc 1 2347 61 is_stmt 0 view .LVU1579
 4558 0006 5E4B     		ldr	r3, .L347
 4559 0008 1B68     		ldr	r3, [r3]
 4560 000a 5E4A     		ldr	r2, .L347+4
 4561 000c A2FB0323 		umull	r2, r3, r2, r3
 4562 0010 5B0A     		lsrs	r3, r3, #9
2347:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = resetcount;
 4563              		.loc 1 2347 36 view .LVU1580
ARM GAS  /tmp/ccqUhOmw.s 			page 183


 4564 0012 6422     		movs	r2, #100
 4565 0014 02FB03F3 		mul	r3, r2, r3
2347:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = resetcount;
 4566              		.loc 1 2347 14 view .LVU1581
 4567 0018 0493     		str	r3, [sp, #16]
2348:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4568              		.loc 1 2348 3 is_stmt 1 view .LVU1582
2348:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4569              		.loc 1 2348 9 is_stmt 0 view .LVU1583
 4570 001a 049B     		ldr	r3, [sp, #16]
 4571 001c 0593     		str	r3, [sp, #20]
2351:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4572              		.loc 1 2351 3 is_stmt 1 view .LVU1584
 4573 001e 0268     		ldr	r2, [r0]
 4574 0020 5368     		ldr	r3, [r2, #4]
 4575 0022 23F02003 		bic	r3, r3, #32
 4576 0026 5360     		str	r3, [r2, #4]
2354:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4577              		.loc 1 2354 3 view .LVU1585
2354:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4578              		.loc 1 2354 7 is_stmt 0 view .LVU1586
 4579 0028 0268     		ldr	r2, [r0]
 4580 002a 5368     		ldr	r3, [r2, #4]
2354:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4581              		.loc 1 2354 6 view .LVU1587
 4582 002c 13F0800F 		tst	r3, #128
 4583 0030 12D0     		beq	.L327
2356:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
 4584              		.loc 1 2356 5 is_stmt 1 view .LVU1588
2356:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
 4585              		.loc 1 2356 17 is_stmt 0 view .LVU1589
 4586 0032 554B     		ldr	r3, .L347+8
 4587 0034 0365     		str	r3, [r0, #80]
 4588              	.L330:
2358:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4589              		.loc 1 2358 5 is_stmt 1 view .LVU1590
2360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4590              		.loc 1 2360 7 view .LVU1591
2360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4591              		.loc 1 2360 17 is_stmt 0 view .LVU1592
 4592 0036 059B     		ldr	r3, [sp, #20]
2360:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4593              		.loc 1 2360 10 view .LVU1593
 4594 0038 43B1     		cbz	r3, .L345
2365:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
 4595              		.loc 1 2365 7 is_stmt 1 view .LVU1594
2365:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
 4596              		.loc 1 2365 12 is_stmt 0 view .LVU1595
 4597 003a 059B     		ldr	r3, [sp, #20]
 4598 003c 013B     		subs	r3, r3, #1
 4599 003e 0593     		str	r3, [sp, #20]
2366:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 4600              		.loc 1 2366 26 is_stmt 1 view .LVU1596
2366:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 4601              		.loc 1 2366 18 is_stmt 0 view .LVU1597
 4602 0040 94F85D30 		ldrb	r3, [r4, #93]	@ zero_extendqisi2
 4603 0044 DBB2     		uxtb	r3, r3
ARM GAS  /tmp/ccqUhOmw.s 			page 184


2366:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 4604              		.loc 1 2366 26 view .LVU1598
 4605 0046 072B     		cmp	r3, #7
 4606 0048 F5D1     		bne	.L330
 4607 004a 03E0     		b	.L329
 4608              	.L345:
2362:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 4609              		.loc 1 2362 9 is_stmt 1 view .LVU1599
 4610 004c 236E     		ldr	r3, [r4, #96]
 4611 004e 43F04003 		orr	r3, r3, #64
 4612 0052 2366     		str	r3, [r4, #96]
2363:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4613              		.loc 1 2363 9 view .LVU1600
 4614              	.L329:
2368:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4615              		.loc 1 2368 5 view .LVU1601
2368:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4616              		.loc 1 2368 11 is_stmt 0 view .LVU1602
 4617 0054 049B     		ldr	r3, [sp, #16]
 4618 0056 0593     		str	r3, [sp, #20]
 4619              	.L327:
2371:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4620              		.loc 1 2371 3 is_stmt 1 view .LVU1603
2371:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4621              		.loc 1 2371 7 is_stmt 0 view .LVU1604
 4622 0058 5368     		ldr	r3, [r2, #4]
2371:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4623              		.loc 1 2371 6 view .LVU1605
 4624 005a 13F0400F 		tst	r3, #64
 4625 005e 12D0     		beq	.L331
2373:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
 4626              		.loc 1 2373 5 is_stmt 1 view .LVU1606
2373:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
 4627              		.loc 1 2373 17 is_stmt 0 view .LVU1607
 4628 0060 4A4B     		ldr	r3, .L347+12
 4629 0062 E364     		str	r3, [r4, #76]
 4630              	.L334:
2375:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4631              		.loc 1 2375 5 is_stmt 1 view .LVU1608
2377:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4632              		.loc 1 2377 7 view .LVU1609
2377:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4633              		.loc 1 2377 17 is_stmt 0 view .LVU1610
 4634 0064 059B     		ldr	r3, [sp, #20]
2377:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4635              		.loc 1 2377 10 view .LVU1611
 4636 0066 43B1     		cbz	r3, .L346
2382:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
 4637              		.loc 1 2382 7 is_stmt 1 view .LVU1612
2382:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
 4638              		.loc 1 2382 12 is_stmt 0 view .LVU1613
 4639 0068 059B     		ldr	r3, [sp, #20]
 4640 006a 013B     		subs	r3, r3, #1
 4641 006c 0593     		str	r3, [sp, #20]
2383:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 4642              		.loc 1 2383 26 is_stmt 1 view .LVU1614
2383:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
ARM GAS  /tmp/ccqUhOmw.s 			page 185


 4643              		.loc 1 2383 18 is_stmt 0 view .LVU1615
 4644 006e 94F85D30 		ldrb	r3, [r4, #93]	@ zero_extendqisi2
 4645 0072 DBB2     		uxtb	r3, r3
2383:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 4646              		.loc 1 2383 26 view .LVU1616
 4647 0074 072B     		cmp	r3, #7
 4648 0076 F5D1     		bne	.L334
 4649 0078 03E0     		b	.L333
 4650              	.L346:
2379:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 4651              		.loc 1 2379 9 is_stmt 1 view .LVU1617
 4652 007a 236E     		ldr	r3, [r4, #96]
 4653 007c 43F04003 		orr	r3, r3, #64
 4654 0080 2366     		str	r3, [r4, #96]
2380:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4655              		.loc 1 2380 9 view .LVU1618
 4656              	.L333:
2385:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4657              		.loc 1 2385 5 view .LVU1619
2385:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4658              		.loc 1 2385 11 is_stmt 0 view .LVU1620
 4659 0082 049B     		ldr	r3, [sp, #16]
 4660 0084 0593     		str	r3, [sp, #20]
 4661              	.L331:
2389:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4662              		.loc 1 2389 3 is_stmt 1 view .LVU1621
2389:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4663              		.loc 1 2389 7 is_stmt 0 view .LVU1622
 4664 0086 5368     		ldr	r3, [r2, #4]
2389:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4665              		.loc 1 2389 6 view .LVU1623
 4666 0088 13F0020F 		tst	r3, #2
 4667 008c 2AD0     		beq	.L335
2392:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4668              		.loc 1 2392 5 is_stmt 1 view .LVU1624
2392:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4669              		.loc 1 2392 13 is_stmt 0 view .LVU1625
 4670 008e 636D     		ldr	r3, [r4, #84]
2392:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4671              		.loc 1 2392 8 view .LVU1626
 4672 0090 43B3     		cbz	r3, .L335
2396:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4673              		.loc 1 2396 7 is_stmt 1 view .LVU1627
2396:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4674              		.loc 1 2396 39 is_stmt 0 view .LVU1628
 4675 0092 0022     		movs	r2, #0
 4676 0094 5A63     		str	r2, [r3, #52]
2399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4677              		.loc 1 2399 7 is_stmt 1 view .LVU1629
2399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4678              		.loc 1 2399 11 is_stmt 0 view .LVU1630
 4679 0096 606D     		ldr	r0, [r4, #84]
 4680              	.LVL285:
2399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4681              		.loc 1 2399 11 view .LVU1631
 4682 0098 FFF7FEFF 		bl	HAL_DMA_Abort
 4683              	.LVL286:
ARM GAS  /tmp/ccqUhOmw.s 			page 186


2399:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4684              		.loc 1 2399 10 view .LVU1632
 4685 009c 08B1     		cbz	r0, .L336
2401:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4686              		.loc 1 2401 9 is_stmt 1 view .LVU1633
2401:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4687              		.loc 1 2401 25 is_stmt 0 view .LVU1634
 4688 009e 4023     		movs	r3, #64
 4689 00a0 2366     		str	r3, [r4, #96]
 4690              	.L336:
2405:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4691              		.loc 1 2405 7 is_stmt 1 view .LVU1635
 4692 00a2 2268     		ldr	r2, [r4]
 4693 00a4 5368     		ldr	r3, [r2, #4]
 4694 00a6 23F00203 		bic	r3, r3, #2
 4695 00aa 5360     		str	r3, [r2, #4]
2407:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4696              		.loc 1 2407 7 view .LVU1636
2407:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4697              		.loc 1 2407 11 is_stmt 0 view .LVU1637
 4698 00ac FFF7FEFF 		bl	HAL_GetTick
 4699              	.LVL287:
 4700 00b0 0246     		mov	r2, r0
 4701 00b2 6421     		movs	r1, #100
 4702 00b4 2046     		mov	r0, r4
 4703 00b6 FFF7FEFF 		bl	SPI_EndRxTxTransaction
 4704              	.LVL288:
2407:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4705              		.loc 1 2407 10 view .LVU1638
 4706 00ba 08B1     		cbz	r0, .L337
2409:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4707              		.loc 1 2409 9 is_stmt 1 view .LVU1639
2409:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4708              		.loc 1 2409 25 is_stmt 0 view .LVU1640
 4709 00bc 4023     		movs	r3, #64
 4710 00be 2366     		str	r3, [r4, #96]
 4711              	.L337:
2413:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4712              		.loc 1 2413 7 is_stmt 1 view .LVU1641
 4713 00c0 2268     		ldr	r2, [r4]
 4714 00c2 1368     		ldr	r3, [r2]
 4715 00c4 23F04003 		bic	r3, r3, #64
 4716 00c8 1360     		str	r3, [r2]
2416:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4717              		.loc 1 2416 7 view .LVU1642
2416:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4718              		.loc 1 2416 11 is_stmt 0 view .LVU1643
 4719 00ca FFF7FEFF 		bl	HAL_GetTick
 4720              	.LVL289:
 4721 00ce 0090     		str	r0, [sp]
 4722 00d0 6423     		movs	r3, #100
 4723 00d2 0022     		movs	r2, #0
 4724 00d4 4FF4C061 		mov	r1, #1536
 4725 00d8 2046     		mov	r0, r4
 4726 00da FFF7FEFF 		bl	SPI_WaitFifoStateUntilTimeout
 4727              	.LVL290:
2416:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
ARM GAS  /tmp/ccqUhOmw.s 			page 187


 4728              		.loc 1 2416 10 view .LVU1644
 4729 00de 08B1     		cbz	r0, .L335
2418:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4730              		.loc 1 2418 9 is_stmt 1 view .LVU1645
2418:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4731              		.loc 1 2418 25 is_stmt 0 view .LVU1646
 4732 00e0 4023     		movs	r3, #64
 4733 00e2 2366     		str	r3, [r4, #96]
 4734              	.L335:
2424:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4735              		.loc 1 2424 3 is_stmt 1 view .LVU1647
2424:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4736              		.loc 1 2424 7 is_stmt 0 view .LVU1648
 4737 00e4 2368     		ldr	r3, [r4]
 4738 00e6 5B68     		ldr	r3, [r3, #4]
2424:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4739              		.loc 1 2424 6 view .LVU1649
 4740 00e8 13F0010F 		tst	r3, #1
 4741 00ec 2CD0     		beq	.L338
2427:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4742              		.loc 1 2427 5 is_stmt 1 view .LVU1650
2427:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4743              		.loc 1 2427 13 is_stmt 0 view .LVU1651
 4744 00ee A36D     		ldr	r3, [r4, #88]
2427:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 4745              		.loc 1 2427 8 view .LVU1652
 4746 00f0 53B3     		cbz	r3, .L338
2431:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4747              		.loc 1 2431 7 is_stmt 1 view .LVU1653
2431:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4748              		.loc 1 2431 39 is_stmt 0 view .LVU1654
 4749 00f2 0022     		movs	r2, #0
 4750 00f4 5A63     		str	r2, [r3, #52]
2434:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4751              		.loc 1 2434 7 is_stmt 1 view .LVU1655
2434:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4752              		.loc 1 2434 11 is_stmt 0 view .LVU1656
 4753 00f6 A06D     		ldr	r0, [r4, #88]
 4754 00f8 FFF7FEFF 		bl	HAL_DMA_Abort
 4755              	.LVL291:
2434:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4756              		.loc 1 2434 10 view .LVU1657
 4757 00fc 08B1     		cbz	r0, .L339
2436:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4758              		.loc 1 2436 9 is_stmt 1 view .LVU1658
2436:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4759              		.loc 1 2436 25 is_stmt 0 view .LVU1659
 4760 00fe 4023     		movs	r3, #64
 4761 0100 2366     		str	r3, [r4, #96]
 4762              	.L339:
2440:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4763              		.loc 1 2440 7 is_stmt 1 view .LVU1660
 4764 0102 2268     		ldr	r2, [r4]
 4765 0104 1368     		ldr	r3, [r2]
 4766 0106 23F04003 		bic	r3, r3, #64
 4767 010a 1360     		str	r3, [r2]
2443:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
ARM GAS  /tmp/ccqUhOmw.s 			page 188


 4768              		.loc 1 2443 7 view .LVU1661
2443:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4769              		.loc 1 2443 11 is_stmt 0 view .LVU1662
 4770 010c FFF7FEFF 		bl	HAL_GetTick
 4771              	.LVL292:
 4772 0110 0090     		str	r0, [sp]
 4773 0112 6423     		movs	r3, #100
 4774 0114 0022     		movs	r2, #0
 4775 0116 8021     		movs	r1, #128
 4776 0118 2046     		mov	r0, r4
 4777 011a FFF7FEFF 		bl	SPI_WaitFlagStateUntilTimeout
 4778              	.LVL293:
2443:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4779              		.loc 1 2443 10 view .LVU1663
 4780 011e 08B1     		cbz	r0, .L340
2445:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4781              		.loc 1 2445 9 is_stmt 1 view .LVU1664
2445:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4782              		.loc 1 2445 25 is_stmt 0 view .LVU1665
 4783 0120 4023     		movs	r3, #64
 4784 0122 2366     		str	r3, [r4, #96]
 4785              	.L340:
2449:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4786              		.loc 1 2449 7 is_stmt 1 view .LVU1666
2449:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4787              		.loc 1 2449 11 is_stmt 0 view .LVU1667
 4788 0124 FFF7FEFF 		bl	HAL_GetTick
 4789              	.LVL294:
 4790 0128 0090     		str	r0, [sp]
 4791 012a 6423     		movs	r3, #100
 4792 012c 0022     		movs	r2, #0
 4793 012e 4FF4C061 		mov	r1, #1536
 4794 0132 2046     		mov	r0, r4
 4795 0134 FFF7FEFF 		bl	SPI_WaitFifoStateUntilTimeout
 4796              	.LVL295:
2449:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 4797              		.loc 1 2449 10 view .LVU1668
 4798 0138 08B1     		cbz	r0, .L341
2451:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4799              		.loc 1 2451 9 is_stmt 1 view .LVU1669
2451:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 4800              		.loc 1 2451 25 is_stmt 0 view .LVU1670
 4801 013a 4023     		movs	r3, #64
 4802 013c 2366     		str	r3, [r4, #96]
 4803              	.L341:
2455:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 4804              		.loc 1 2455 7 is_stmt 1 view .LVU1671
 4805 013e 2268     		ldr	r2, [r4]
 4806 0140 5368     		ldr	r3, [r2, #4]
 4807 0142 23F00103 		bic	r3, r3, #1
 4808 0146 5360     		str	r3, [r2, #4]
 4809              	.L338:
2459:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 4810              		.loc 1 2459 3 view .LVU1672
2459:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 4811              		.loc 1 2459 21 is_stmt 0 view .LVU1673
 4812 0148 0023     		movs	r3, #0
ARM GAS  /tmp/ccqUhOmw.s 			page 189


 4813 014a A4F84630 		strh	r3, [r4, #70]	@ movhi
2460:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4814              		.loc 1 2460 3 is_stmt 1 view .LVU1674
2460:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4815              		.loc 1 2460 21 is_stmt 0 view .LVU1675
 4816 014e E387     		strh	r3, [r4, #62]	@ movhi
2463:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4817              		.loc 1 2463 3 is_stmt 1 view .LVU1676
2463:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4818              		.loc 1 2463 11 is_stmt 0 view .LVU1677
 4819 0150 236E     		ldr	r3, [r4, #96]
2463:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 4820              		.loc 1 2463 6 view .LVU1678
 4821 0152 402B     		cmp	r3, #64
 4822 0154 12D0     		beq	.L343
2471:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4823              		.loc 1 2471 5 is_stmt 1 view .LVU1679
2471:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4824              		.loc 1 2471 21 is_stmt 0 view .LVU1680
 4825 0156 0020     		movs	r0, #0
 4826 0158 2066     		str	r0, [r4, #96]
 4827              	.L342:
 4828              	.LVL296:
2475:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 4829              		.loc 1 2475 3 is_stmt 1 view .LVU1681
 4830              	.LBB3:
2475:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 4831              		.loc 1 2475 3 view .LVU1682
 4832 015a 0022     		movs	r2, #0
 4833 015c 0292     		str	r2, [sp, #8]
2475:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 4834              		.loc 1 2475 3 view .LVU1683
 4835 015e 2368     		ldr	r3, [r4]
 4836 0160 D968     		ldr	r1, [r3, #12]
 4837 0162 0291     		str	r1, [sp, #8]
2475:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 4838              		.loc 1 2475 3 view .LVU1684
 4839 0164 9968     		ldr	r1, [r3, #8]
 4840 0166 0291     		str	r1, [sp, #8]
2475:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 4841              		.loc 1 2475 3 view .LVU1685
 4842 0168 0299     		ldr	r1, [sp, #8]
 4843              	.LBE3:
2475:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 4844              		.loc 1 2475 3 view .LVU1686
2476:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4845              		.loc 1 2476 3 view .LVU1687
 4846              	.LBB4:
2476:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4847              		.loc 1 2476 3 view .LVU1688
 4848 016a 0392     		str	r2, [sp, #12]
2476:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4849              		.loc 1 2476 3 view .LVU1689
 4850 016c 9B68     		ldr	r3, [r3, #8]
 4851 016e 0393     		str	r3, [sp, #12]
2476:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4852              		.loc 1 2476 3 view .LVU1690
ARM GAS  /tmp/ccqUhOmw.s 			page 190


 4853 0170 039B     		ldr	r3, [sp, #12]
 4854              	.LBE4:
2476:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4855              		.loc 1 2476 3 view .LVU1691
2479:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4856              		.loc 1 2479 3 view .LVU1692
2479:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4857              		.loc 1 2479 15 is_stmt 0 view .LVU1693
 4858 0172 0123     		movs	r3, #1
 4859 0174 84F85D30 		strb	r3, [r4, #93]
2481:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 4860              		.loc 1 2481 3 is_stmt 1 view .LVU1694
2482:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4861              		.loc 1 2482 1 is_stmt 0 view .LVU1695
 4862 0178 06B0     		add	sp, sp, #24
 4863              		.cfi_remember_state
 4864              		.cfi_def_cfa_offset 8
 4865              		@ sp needed
 4866 017a 10BD     		pop	{r4, pc}
 4867              	.LVL297:
 4868              	.L343:
 4869              		.cfi_restore_state
2466:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 4870              		.loc 1 2466 15 view .LVU1696
 4871 017c 0120     		movs	r0, #1
 4872 017e ECE7     		b	.L342
 4873              	.L348:
 4874              		.align	2
 4875              	.L347:
 4876 0180 00000000 		.word	SystemCoreClock
 4877 0184 F1197605 		.word	91625969
 4878 0188 00000000 		.word	SPI_AbortTx_ISR
 4879 018c 00000000 		.word	SPI_AbortRx_ISR
 4880              		.cfi_endproc
 4881              	.LFE143:
 4883              		.section	.text.HAL_SPI_DMAPause,"ax",%progbits
 4884              		.align	1
 4885              		.global	HAL_SPI_DMAPause
 4886              		.syntax unified
 4887              		.thumb
 4888              		.thumb_func
 4890              	HAL_SPI_DMAPause:
 4891              	.LVL298:
 4892              	.LFB145:
2661:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Locked */
 4893              		.loc 1 2661 1 is_stmt 1 view -0
 4894              		.cfi_startproc
 4895              		@ args = 0, pretend = 0, frame = 0
 4896              		@ frame_needed = 0, uses_anonymous_args = 0
 4897              		@ link register save eliminated.
2663:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4898              		.loc 1 2663 3 view .LVU1698
2663:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4899              		.loc 1 2663 3 view .LVU1699
 4900 0000 90F85C30 		ldrb	r3, [r0, #92]	@ zero_extendqisi2
 4901 0004 012B     		cmp	r3, #1
 4902 0006 0CD0     		beq	.L351
ARM GAS  /tmp/ccqUhOmw.s 			page 191


2663:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4903              		.loc 1 2663 3 discriminator 2 view .LVU1700
 4904 0008 0123     		movs	r3, #1
 4905 000a 80F85C30 		strb	r3, [r0, #92]
2663:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4906              		.loc 1 2663 3 discriminator 2 view .LVU1701
2666:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4907              		.loc 1 2666 3 discriminator 2 view .LVU1702
 4908 000e 0268     		ldr	r2, [r0]
 4909 0010 5368     		ldr	r3, [r2, #4]
 4910 0012 23F00303 		bic	r3, r3, #3
 4911 0016 5360     		str	r3, [r2, #4]
2669:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4912              		.loc 1 2669 3 discriminator 2 view .LVU1703
2669:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4913              		.loc 1 2669 3 discriminator 2 view .LVU1704
 4914 0018 0023     		movs	r3, #0
 4915 001a 80F85C30 		strb	r3, [r0, #92]
2669:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4916              		.loc 1 2669 3 discriminator 2 view .LVU1705
2671:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 4917              		.loc 1 2671 3 discriminator 2 view .LVU1706
2671:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 4918              		.loc 1 2671 10 is_stmt 0 discriminator 2 view .LVU1707
 4919 001e 1846     		mov	r0, r3
 4920              	.LVL299:
2671:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 4921              		.loc 1 2671 10 discriminator 2 view .LVU1708
 4922 0020 7047     		bx	lr
 4923              	.LVL300:
 4924              	.L351:
2663:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4925              		.loc 1 2663 3 view .LVU1709
 4926 0022 0220     		movs	r0, #2
 4927              	.LVL301:
2672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4928              		.loc 1 2672 1 view .LVU1710
 4929 0024 7047     		bx	lr
 4930              		.cfi_endproc
 4931              	.LFE145:
 4933              		.section	.text.HAL_SPI_DMAResume,"ax",%progbits
 4934              		.align	1
 4935              		.global	HAL_SPI_DMAResume
 4936              		.syntax unified
 4937              		.thumb
 4938              		.thumb_func
 4940              	HAL_SPI_DMAResume:
 4941              	.LVL302:
 4942              	.LFB146:
2681:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Process Locked */
 4943              		.loc 1 2681 1 is_stmt 1 view -0
 4944              		.cfi_startproc
 4945              		@ args = 0, pretend = 0, frame = 0
 4946              		@ frame_needed = 0, uses_anonymous_args = 0
 4947              		@ link register save eliminated.
2683:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4948              		.loc 1 2683 3 view .LVU1712
ARM GAS  /tmp/ccqUhOmw.s 			page 192


2683:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4949              		.loc 1 2683 3 view .LVU1713
 4950 0000 90F85C30 		ldrb	r3, [r0, #92]	@ zero_extendqisi2
 4951 0004 012B     		cmp	r3, #1
 4952 0006 0CD0     		beq	.L354
2683:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4953              		.loc 1 2683 3 discriminator 2 view .LVU1714
 4954 0008 0123     		movs	r3, #1
 4955 000a 80F85C30 		strb	r3, [r0, #92]
2683:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4956              		.loc 1 2683 3 discriminator 2 view .LVU1715
2686:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4957              		.loc 1 2686 3 discriminator 2 view .LVU1716
 4958 000e 0268     		ldr	r2, [r0]
 4959 0010 5368     		ldr	r3, [r2, #4]
 4960 0012 43F00303 		orr	r3, r3, #3
 4961 0016 5360     		str	r3, [r2, #4]
2689:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4962              		.loc 1 2689 3 discriminator 2 view .LVU1717
2689:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4963              		.loc 1 2689 3 discriminator 2 view .LVU1718
 4964 0018 0023     		movs	r3, #0
 4965 001a 80F85C30 		strb	r3, [r0, #92]
2689:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4966              		.loc 1 2689 3 discriminator 2 view .LVU1719
2691:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 4967              		.loc 1 2691 3 discriminator 2 view .LVU1720
2691:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 4968              		.loc 1 2691 10 is_stmt 0 discriminator 2 view .LVU1721
 4969 001e 1846     		mov	r0, r3
 4970              	.LVL303:
2691:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 4971              		.loc 1 2691 10 discriminator 2 view .LVU1722
 4972 0020 7047     		bx	lr
 4973              	.LVL304:
 4974              	.L354:
2683:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4975              		.loc 1 2683 3 view .LVU1723
 4976 0022 0220     		movs	r0, #2
 4977              	.LVL305:
2692:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 4978              		.loc 1 2692 1 view .LVU1724
 4979 0024 7047     		bx	lr
 4980              		.cfi_endproc
 4981              	.LFE146:
 4983              		.section	.text.HAL_SPI_DMAStop,"ax",%progbits
 4984              		.align	1
 4985              		.global	HAL_SPI_DMAStop
 4986              		.syntax unified
 4987              		.thumb
 4988              		.thumb_func
 4990              	HAL_SPI_DMAStop:
 4991              	.LVL306:
 4992              	.LFB147:
2701:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 4993              		.loc 1 2701 1 is_stmt 1 view -0
 4994              		.cfi_startproc
ARM GAS  /tmp/ccqUhOmw.s 			page 193


 4995              		@ args = 0, pretend = 0, frame = 0
 4996              		@ frame_needed = 0, uses_anonymous_args = 0
2701:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode = HAL_OK;
 4997              		.loc 1 2701 1 is_stmt 0 view .LVU1726
 4998 0000 38B5     		push	{r3, r4, r5, lr}
 4999              		.cfi_def_cfa_offset 16
 5000              		.cfi_offset 3, -16
 5001              		.cfi_offset 4, -12
 5002              		.cfi_offset 5, -8
 5003              		.cfi_offset 14, -4
 5004 0002 0446     		mov	r4, r0
2702:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* The Lock is not implemented on this API to allow the user application
 5005              		.loc 1 2702 3 is_stmt 1 view .LVU1727
 5006              	.LVL307:
2710:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5007              		.loc 1 2710 3 view .LVU1728
2710:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5008              		.loc 1 2710 11 is_stmt 0 view .LVU1729
 5009 0004 406D     		ldr	r0, [r0, #84]
 5010              	.LVL308:
2710:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5011              		.loc 1 2710 6 view .LVU1730
 5012 0006 48B1     		cbz	r0, .L358
2712:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5013              		.loc 1 2712 5 is_stmt 1 view .LVU1731
2712:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5014              		.loc 1 2712 19 is_stmt 0 view .LVU1732
 5015 0008 FFF7FEFF 		bl	HAL_DMA_Abort
 5016              	.LVL309:
2712:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5017              		.loc 1 2712 8 view .LVU1733
 5018 000c 0546     		mov	r5, r0
 5019 000e 30B1     		cbz	r0, .L356
2714:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       errorcode = HAL_ERROR;
 5020              		.loc 1 2714 7 is_stmt 1 view .LVU1734
 5021 0010 236E     		ldr	r3, [r4, #96]
 5022 0012 43F01003 		orr	r3, r3, #16
 5023 0016 2366     		str	r3, [r4, #96]
2715:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 5024              		.loc 1 2715 7 view .LVU1735
 5025              	.LVL310:
2715:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 5026              		.loc 1 2715 17 is_stmt 0 view .LVU1736
 5027 0018 0125     		movs	r5, #1
 5028 001a 00E0     		b	.L356
 5029              	.LVL311:
 5030              	.L358:
2702:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* The Lock is not implemented on this API to allow the user application
 5031              		.loc 1 2702 21 view .LVU1737
 5032 001c 0025     		movs	r5, #0
 5033              	.LVL312:
 5034              	.L356:
2719:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5035              		.loc 1 2719 3 is_stmt 1 view .LVU1738
2719:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5036              		.loc 1 2719 11 is_stmt 0 view .LVU1739
 5037 001e A06D     		ldr	r0, [r4, #88]
ARM GAS  /tmp/ccqUhOmw.s 			page 194


2719:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5038              		.loc 1 2719 6 view .LVU1740
 5039 0020 38B1     		cbz	r0, .L357
2721:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5040              		.loc 1 2721 5 is_stmt 1 view .LVU1741
2721:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5041              		.loc 1 2721 19 is_stmt 0 view .LVU1742
 5042 0022 FFF7FEFF 		bl	HAL_DMA_Abort
 5043              	.LVL313:
2721:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5044              		.loc 1 2721 8 view .LVU1743
 5045 0026 20B1     		cbz	r0, .L357
2723:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       errorcode = HAL_ERROR;
 5046              		.loc 1 2723 7 is_stmt 1 view .LVU1744
 5047 0028 236E     		ldr	r3, [r4, #96]
 5048 002a 43F01003 		orr	r3, r3, #16
 5049 002e 2366     		str	r3, [r4, #96]
2724:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 5050              		.loc 1 2724 7 view .LVU1745
 5051              	.LVL314:
2724:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 5052              		.loc 1 2724 17 is_stmt 0 view .LVU1746
 5053 0030 0125     		movs	r5, #1
 5054              	.LVL315:
 5055              	.L357:
2729:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
 5056              		.loc 1 2729 3 is_stmt 1 view .LVU1747
 5057 0032 2268     		ldr	r2, [r4]
 5058 0034 5368     		ldr	r3, [r2, #4]
 5059 0036 23F00303 		bic	r3, r3, #3
 5060 003a 5360     		str	r3, [r2, #4]
2730:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 5061              		.loc 1 2730 3 view .LVU1748
2730:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   return errorcode;
 5062              		.loc 1 2730 15 is_stmt 0 view .LVU1749
 5063 003c 0123     		movs	r3, #1
 5064 003e 84F85D30 		strb	r3, [r4, #93]
2731:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 5065              		.loc 1 2731 3 is_stmt 1 view .LVU1750
2732:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5066              		.loc 1 2732 1 is_stmt 0 view .LVU1751
 5067 0042 2846     		mov	r0, r5
 5068 0044 38BD     		pop	{r3, r4, r5, pc}
2732:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5069              		.loc 1 2732 1 view .LVU1752
 5070              		.cfi_endproc
 5071              	.LFE147:
 5073              		.section	.text.HAL_SPI_TxCpltCallback,"ax",%progbits
 5074              		.align	1
 5075              		.weak	HAL_SPI_TxCpltCallback
 5076              		.syntax unified
 5077              		.thumb
 5078              		.thumb_func
 5080              	HAL_SPI_TxCpltCallback:
 5081              	.LVL316:
 5082              	.LFB149:
2848:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
ARM GAS  /tmp/ccqUhOmw.s 			page 195


 5083              		.loc 1 2848 1 is_stmt 1 view -0
 5084              		.cfi_startproc
 5085              		@ args = 0, pretend = 0, frame = 0
 5086              		@ frame_needed = 0, uses_anonymous_args = 0
 5087              		@ link register save eliminated.
2850:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5088              		.loc 1 2850 3 view .LVU1754
2855:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5089              		.loc 1 2855 1 is_stmt 0 view .LVU1755
 5090 0000 7047     		bx	lr
 5091              		.cfi_endproc
 5092              	.LFE149:
 5094              		.section	.text.HAL_SPI_RxCpltCallback,"ax",%progbits
 5095              		.align	1
 5096              		.weak	HAL_SPI_RxCpltCallback
 5097              		.syntax unified
 5098              		.thumb
 5099              		.thumb_func
 5101              	HAL_SPI_RxCpltCallback:
 5102              	.LVL317:
 5103              	.LFB150:
2864:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 5104              		.loc 1 2864 1 is_stmt 1 view -0
 5105              		.cfi_startproc
 5106              		@ args = 0, pretend = 0, frame = 0
 5107              		@ frame_needed = 0, uses_anonymous_args = 0
 5108              		@ link register save eliminated.
2866:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5109              		.loc 1 2866 3 view .LVU1757
2871:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5110              		.loc 1 2871 1 is_stmt 0 view .LVU1758
 5111 0000 7047     		bx	lr
 5112              		.cfi_endproc
 5113              	.LFE150:
 5115              		.section	.text.HAL_SPI_TxRxCpltCallback,"ax",%progbits
 5116              		.align	1
 5117              		.weak	HAL_SPI_TxRxCpltCallback
 5118              		.syntax unified
 5119              		.thumb
 5120              		.thumb_func
 5122              	HAL_SPI_TxRxCpltCallback:
 5123              	.LVL318:
 5124              	.LFB151:
2880:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 5125              		.loc 1 2880 1 is_stmt 1 view -0
 5126              		.cfi_startproc
 5127              		@ args = 0, pretend = 0, frame = 0
 5128              		@ frame_needed = 0, uses_anonymous_args = 0
 5129              		@ link register save eliminated.
2882:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5130              		.loc 1 2882 3 view .LVU1760
2887:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5131              		.loc 1 2887 1 is_stmt 0 view .LVU1761
 5132 0000 7047     		bx	lr
 5133              		.cfi_endproc
 5134              	.LFE151:
 5136              		.section	.text.HAL_SPI_TxHalfCpltCallback,"ax",%progbits
ARM GAS  /tmp/ccqUhOmw.s 			page 196


 5137              		.align	1
 5138              		.weak	HAL_SPI_TxHalfCpltCallback
 5139              		.syntax unified
 5140              		.thumb
 5141              		.thumb_func
 5143              	HAL_SPI_TxHalfCpltCallback:
 5144              	.LVL319:
 5145              	.LFB152:
2896:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 5146              		.loc 1 2896 1 is_stmt 1 view -0
 5147              		.cfi_startproc
 5148              		@ args = 0, pretend = 0, frame = 0
 5149              		@ frame_needed = 0, uses_anonymous_args = 0
 5150              		@ link register save eliminated.
2898:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5151              		.loc 1 2898 3 view .LVU1763
2903:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5152              		.loc 1 2903 1 is_stmt 0 view .LVU1764
 5153 0000 7047     		bx	lr
 5154              		.cfi_endproc
 5155              	.LFE152:
 5157              		.section	.text.SPI_DMAHalfTransmitCplt,"ax",%progbits
 5158              		.align	1
 5159              		.syntax unified
 5160              		.thumb
 5161              		.thumb_func
 5163              	SPI_DMAHalfTransmitCplt:
 5164              	.LVL320:
 5165              	.LFB162:
3308:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 5166              		.loc 1 3308 1 is_stmt 1 view -0
 5167              		.cfi_startproc
 5168              		@ args = 0, pretend = 0, frame = 0
 5169              		@ frame_needed = 0, uses_anonymous_args = 0
3308:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 5170              		.loc 1 3308 1 is_stmt 0 view .LVU1766
 5171 0000 08B5     		push	{r3, lr}
 5172              		.cfi_def_cfa_offset 8
 5173              		.cfi_offset 3, -8
 5174              		.cfi_offset 14, -4
3309:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5175              		.loc 1 3309 3 is_stmt 1 view .LVU1767
 5176              	.LVL321:
3315:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5177              		.loc 1 3315 3 view .LVU1768
 5178 0002 406A     		ldr	r0, [r0, #36]
 5179              	.LVL322:
3315:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5180              		.loc 1 3315 3 is_stmt 0 view .LVU1769
 5181 0004 FFF7FEFF 		bl	HAL_SPI_TxHalfCpltCallback
 5182              	.LVL323:
3317:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5183              		.loc 1 3317 1 view .LVU1770
 5184 0008 08BD     		pop	{r3, pc}
 5185              		.cfi_endproc
 5186              	.LFE162:
 5188              		.section	.text.HAL_SPI_RxHalfCpltCallback,"ax",%progbits
ARM GAS  /tmp/ccqUhOmw.s 			page 197


 5189              		.align	1
 5190              		.weak	HAL_SPI_RxHalfCpltCallback
 5191              		.syntax unified
 5192              		.thumb
 5193              		.thumb_func
 5195              	HAL_SPI_RxHalfCpltCallback:
 5196              	.LVL324:
 5197              	.LFB153:
2912:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 5198              		.loc 1 2912 1 is_stmt 1 view -0
 5199              		.cfi_startproc
 5200              		@ args = 0, pretend = 0, frame = 0
 5201              		@ frame_needed = 0, uses_anonymous_args = 0
 5202              		@ link register save eliminated.
2914:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5203              		.loc 1 2914 3 view .LVU1772
2919:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5204              		.loc 1 2919 1 is_stmt 0 view .LVU1773
 5205 0000 7047     		bx	lr
 5206              		.cfi_endproc
 5207              	.LFE153:
 5209              		.section	.text.SPI_DMAHalfReceiveCplt,"ax",%progbits
 5210              		.align	1
 5211              		.syntax unified
 5212              		.thumb
 5213              		.thumb_func
 5215              	SPI_DMAHalfReceiveCplt:
 5216              	.LVL325:
 5217              	.LFB163:
3326:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 5218              		.loc 1 3326 1 is_stmt 1 view -0
 5219              		.cfi_startproc
 5220              		@ args = 0, pretend = 0, frame = 0
 5221              		@ frame_needed = 0, uses_anonymous_args = 0
3326:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 5222              		.loc 1 3326 1 is_stmt 0 view .LVU1775
 5223 0000 08B5     		push	{r3, lr}
 5224              		.cfi_def_cfa_offset 8
 5225              		.cfi_offset 3, -8
 5226              		.cfi_offset 14, -4
3327:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5227              		.loc 1 3327 3 is_stmt 1 view .LVU1776
 5228              	.LVL326:
3333:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5229              		.loc 1 3333 3 view .LVU1777
 5230 0002 406A     		ldr	r0, [r0, #36]
 5231              	.LVL327:
3333:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5232              		.loc 1 3333 3 is_stmt 0 view .LVU1778
 5233 0004 FFF7FEFF 		bl	HAL_SPI_RxHalfCpltCallback
 5234              	.LVL328:
3335:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5235              		.loc 1 3335 1 view .LVU1779
 5236 0008 08BD     		pop	{r3, pc}
 5237              		.cfi_endproc
 5238              	.LFE163:
 5240              		.section	.text.HAL_SPI_TxRxHalfCpltCallback,"ax",%progbits
ARM GAS  /tmp/ccqUhOmw.s 			page 198


 5241              		.align	1
 5242              		.weak	HAL_SPI_TxRxHalfCpltCallback
 5243              		.syntax unified
 5244              		.thumb
 5245              		.thumb_func
 5247              	HAL_SPI_TxRxHalfCpltCallback:
 5248              	.LVL329:
 5249              	.LFB154:
2928:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 5250              		.loc 1 2928 1 is_stmt 1 view -0
 5251              		.cfi_startproc
 5252              		@ args = 0, pretend = 0, frame = 0
 5253              		@ frame_needed = 0, uses_anonymous_args = 0
 5254              		@ link register save eliminated.
2930:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5255              		.loc 1 2930 3 view .LVU1781
2935:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5256              		.loc 1 2935 1 is_stmt 0 view .LVU1782
 5257 0000 7047     		bx	lr
 5258              		.cfi_endproc
 5259              	.LFE154:
 5261              		.section	.text.SPI_DMAHalfTransmitReceiveCplt,"ax",%progbits
 5262              		.align	1
 5263              		.syntax unified
 5264              		.thumb
 5265              		.thumb_func
 5267              	SPI_DMAHalfTransmitReceiveCplt:
 5268              	.LVL330:
 5269              	.LFB164:
3344:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 5270              		.loc 1 3344 1 is_stmt 1 view -0
 5271              		.cfi_startproc
 5272              		@ args = 0, pretend = 0, frame = 0
 5273              		@ frame_needed = 0, uses_anonymous_args = 0
3344:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 5274              		.loc 1 3344 1 is_stmt 0 view .LVU1784
 5275 0000 08B5     		push	{r3, lr}
 5276              		.cfi_def_cfa_offset 8
 5277              		.cfi_offset 3, -8
 5278              		.cfi_offset 14, -4
3345:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5279              		.loc 1 3345 3 is_stmt 1 view .LVU1785
 5280              	.LVL331:
3351:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5281              		.loc 1 3351 3 view .LVU1786
 5282 0002 406A     		ldr	r0, [r0, #36]
 5283              	.LVL332:
3351:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5284              		.loc 1 3351 3 is_stmt 0 view .LVU1787
 5285 0004 FFF7FEFF 		bl	HAL_SPI_TxRxHalfCpltCallback
 5286              	.LVL333:
3353:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5287              		.loc 1 3353 1 view .LVU1788
 5288 0008 08BD     		pop	{r3, pc}
 5289              		.cfi_endproc
 5290              	.LFE164:
 5292              		.section	.text.HAL_SPI_ErrorCallback,"ax",%progbits
ARM GAS  /tmp/ccqUhOmw.s 			page 199


 5293              		.align	1
 5294              		.weak	HAL_SPI_ErrorCallback
 5295              		.syntax unified
 5296              		.thumb
 5297              		.thumb_func
 5299              	HAL_SPI_ErrorCallback:
 5300              	.LVL334:
 5301              	.LFB155:
2944:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 5302              		.loc 1 2944 1 is_stmt 1 view -0
 5303              		.cfi_startproc
 5304              		@ args = 0, pretend = 0, frame = 0
 5305              		@ frame_needed = 0, uses_anonymous_args = 0
 5306              		@ link register save eliminated.
2946:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5307              		.loc 1 2946 3 view .LVU1790
2954:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5308              		.loc 1 2954 1 is_stmt 0 view .LVU1791
 5309 0000 7047     		bx	lr
 5310              		.cfi_endproc
 5311              	.LFE155:
 5313              		.section	.text.SPI_CloseTx_ISR,"ax",%progbits
 5314              		.align	1
 5315              		.syntax unified
 5316              		.thumb
 5317              		.thumb_func
 5319              	SPI_CloseTx_ISR:
 5320              	.LVL335:
 5321              	.LFB183:
4286:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 5322              		.loc 1 4286 1 is_stmt 1 view -0
 5323              		.cfi_startproc
 5324              		@ args = 0, pretend = 0, frame = 8
 5325              		@ frame_needed = 0, uses_anonymous_args = 0
4286:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 5326              		.loc 1 4286 1 is_stmt 0 view .LVU1793
 5327 0000 10B5     		push	{r4, lr}
 5328              		.cfi_def_cfa_offset 8
 5329              		.cfi_offset 4, -8
 5330              		.cfi_offset 14, -4
 5331 0002 82B0     		sub	sp, sp, #8
 5332              		.cfi_def_cfa_offset 16
 5333 0004 0446     		mov	r4, r0
4287:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5334              		.loc 1 4287 3 is_stmt 1 view .LVU1794
4290:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5335              		.loc 1 4290 3 view .LVU1795
4290:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5336              		.loc 1 4290 15 is_stmt 0 view .LVU1796
 5337 0006 FFF7FEFF 		bl	HAL_GetTick
 5338              	.LVL336:
4290:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5339              		.loc 1 4290 15 view .LVU1797
 5340 000a 0246     		mov	r2, r0
 5341              	.LVL337:
4293:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5342              		.loc 1 4293 3 is_stmt 1 view .LVU1798
ARM GAS  /tmp/ccqUhOmw.s 			page 200


 5343 000c 2168     		ldr	r1, [r4]
 5344 000e 4B68     		ldr	r3, [r1, #4]
 5345 0010 23F0A003 		bic	r3, r3, #160
 5346 0014 4B60     		str	r3, [r1, #4]
4296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5347              		.loc 1 4296 3 view .LVU1799
4296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5348              		.loc 1 4296 7 is_stmt 0 view .LVU1800
 5349 0016 6421     		movs	r1, #100
 5350 0018 2046     		mov	r0, r4
 5351              	.LVL338:
4296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5352              		.loc 1 4296 7 view .LVU1801
 5353 001a FFF7FEFF 		bl	SPI_EndRxTxTransaction
 5354              	.LVL339:
4296:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5355              		.loc 1 4296 6 view .LVU1802
 5356 001e 18B1     		cbz	r0, .L374
4298:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5357              		.loc 1 4298 5 is_stmt 1 view .LVU1803
 5358 0020 236E     		ldr	r3, [r4, #96]
 5359 0022 43F02003 		orr	r3, r3, #32
 5360 0026 2366     		str	r3, [r4, #96]
 5361              	.L374:
4302:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5362              		.loc 1 4302 3 view .LVU1804
4302:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5363              		.loc 1 4302 17 is_stmt 0 view .LVU1805
 5364 0028 A368     		ldr	r3, [r4, #8]
4302:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5365              		.loc 1 4302 6 view .LVU1806
 5366 002a 33B9     		cbnz	r3, .L375
4304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5367              		.loc 1 4304 5 is_stmt 1 view .LVU1807
 5368              	.LBB5:
4304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5369              		.loc 1 4304 5 view .LVU1808
 5370 002c 0193     		str	r3, [sp, #4]
4304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5371              		.loc 1 4304 5 view .LVU1809
 5372 002e 2368     		ldr	r3, [r4]
 5373 0030 DA68     		ldr	r2, [r3, #12]
 5374 0032 0192     		str	r2, [sp, #4]
4304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5375              		.loc 1 4304 5 view .LVU1810
 5376 0034 9B68     		ldr	r3, [r3, #8]
 5377 0036 0193     		str	r3, [sp, #4]
4304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5378              		.loc 1 4304 5 view .LVU1811
 5379 0038 019B     		ldr	r3, [sp, #4]
 5380              	.L375:
 5381              	.LBE5:
4304:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5382              		.loc 1 4304 5 discriminator 1 view .LVU1812
4307:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
 5383              		.loc 1 4307 3 discriminator 1 view .LVU1813
4307:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   if (hspi->ErrorCode != HAL_SPI_ERROR_NONE)
ARM GAS  /tmp/ccqUhOmw.s 			page 201


 5384              		.loc 1 4307 15 is_stmt 0 discriminator 1 view .LVU1814
 5385 003a 0123     		movs	r3, #1
 5386 003c 84F85D30 		strb	r3, [r4, #93]
4308:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5387              		.loc 1 4308 3 is_stmt 1 discriminator 1 view .LVU1815
4308:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5388              		.loc 1 4308 11 is_stmt 0 discriminator 1 view .LVU1816
 5389 0040 236E     		ldr	r3, [r4, #96]
4308:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5390              		.loc 1 4308 6 discriminator 1 view .LVU1817
 5391 0042 23B1     		cbz	r3, .L376
4314:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5392              		.loc 1 4314 5 is_stmt 1 view .LVU1818
 5393 0044 2046     		mov	r0, r4
 5394 0046 FFF7FEFF 		bl	HAL_SPI_ErrorCallback
 5395              	.LVL340:
 5396              	.L373:
4326:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5397              		.loc 1 4326 1 is_stmt 0 view .LVU1819
 5398 004a 02B0     		add	sp, sp, #8
 5399              		.cfi_remember_state
 5400              		.cfi_def_cfa_offset 8
 5401              		@ sp needed
 5402 004c 10BD     		pop	{r4, pc}
 5403              	.LVL341:
 5404              	.L376:
 5405              		.cfi_restore_state
4323:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5406              		.loc 1 4323 5 is_stmt 1 view .LVU1820
 5407 004e 2046     		mov	r0, r4
 5408 0050 FFF7FEFF 		bl	HAL_SPI_TxCpltCallback
 5409              	.LVL342:
4326:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5410              		.loc 1 4326 1 is_stmt 0 view .LVU1821
 5411 0054 F9E7     		b	.L373
 5412              		.cfi_endproc
 5413              	.LFE183:
 5415              		.section	.text.SPI_TxISR_8BIT,"ax",%progbits
 5416              		.align	1
 5417              		.syntax unified
 5418              		.thumb
 5419              		.thumb_func
 5421              	SPI_TxISR_8BIT:
 5422              	.LVL343:
 5423              	.LFB175:
3880:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *(__IO uint8_t *)&hspi->Instance->DR = (*hspi->pTxBuffPtr);
 5424              		.loc 1 3880 1 is_stmt 1 view -0
 5425              		.cfi_startproc
 5426              		@ args = 0, pretend = 0, frame = 0
 5427              		@ frame_needed = 0, uses_anonymous_args = 0
3880:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *(__IO uint8_t *)&hspi->Instance->DR = (*hspi->pTxBuffPtr);
 5428              		.loc 1 3880 1 is_stmt 0 view .LVU1823
 5429 0000 08B5     		push	{r3, lr}
 5430              		.cfi_def_cfa_offset 8
 5431              		.cfi_offset 3, -8
 5432              		.cfi_offset 14, -4
3881:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr++;
ARM GAS  /tmp/ccqUhOmw.s 			page 202


 5433              		.loc 1 3881 3 is_stmt 1 view .LVU1824
3881:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr++;
 5434              		.loc 1 3881 48 is_stmt 0 view .LVU1825
 5435 0002 826B     		ldr	r2, [r0, #56]
3881:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr++;
 5436              		.loc 1 3881 25 view .LVU1826
 5437 0004 0368     		ldr	r3, [r0]
3881:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr++;
 5438              		.loc 1 3881 43 view .LVU1827
 5439 0006 1278     		ldrb	r2, [r2]	@ zero_extendqisi2
3881:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr++;
 5440              		.loc 1 3881 40 view .LVU1828
 5441 0008 1A73     		strb	r2, [r3, #12]
3882:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
 5442              		.loc 1 3882 3 is_stmt 1 view .LVU1829
3882:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
 5443              		.loc 1 3882 7 is_stmt 0 view .LVU1830
 5444 000a 836B     		ldr	r3, [r0, #56]
3882:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
 5445              		.loc 1 3882 19 view .LVU1831
 5446 000c 0133     		adds	r3, r3, #1
 5447 000e 8363     		str	r3, [r0, #56]
3883:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5448              		.loc 1 3883 3 is_stmt 1 view .LVU1832
3883:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5449              		.loc 1 3883 7 is_stmt 0 view .LVU1833
 5450 0010 C38F     		ldrh	r3, [r0, #62]
 5451 0012 9BB2     		uxth	r3, r3
3883:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5452              		.loc 1 3883 20 view .LVU1834
 5453 0014 013B     		subs	r3, r3, #1
 5454 0016 9BB2     		uxth	r3, r3
 5455 0018 C387     		strh	r3, [r0, #62]	@ movhi
3885:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5456              		.loc 1 3885 3 is_stmt 1 view .LVU1835
3885:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5457              		.loc 1 3885 11 is_stmt 0 view .LVU1836
 5458 001a C38F     		ldrh	r3, [r0, #62]
 5459 001c 9BB2     		uxth	r3, r3
3885:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5460              		.loc 1 3885 6 view .LVU1837
 5461 001e 03B1     		cbz	r3, .L382
 5462              	.LVL344:
 5463              	.L379:
3896:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5464              		.loc 1 3896 1 view .LVU1838
 5465 0020 08BD     		pop	{r3, pc}
 5466              	.LVL345:
 5467              	.L382:
3894:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5468              		.loc 1 3894 5 is_stmt 1 view .LVU1839
 5469 0022 FFF7FEFF 		bl	SPI_CloseTx_ISR
 5470              	.LVL346:
3896:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5471              		.loc 1 3896 1 is_stmt 0 view .LVU1840
 5472 0026 FBE7     		b	.L379
 5473              		.cfi_endproc
ARM GAS  /tmp/ccqUhOmw.s 			page 203


 5474              	.LFE175:
 5476              		.section	.text.SPI_TxISR_16BIT,"ax",%progbits
 5477              		.align	1
 5478              		.syntax unified
 5479              		.thumb
 5480              		.thumb_func
 5482              	SPI_TxISR_16BIT:
 5483              	.LVL347:
 5484              	.LFB176:
3905:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in 16 Bit mode */
 5485              		.loc 1 3905 1 is_stmt 1 view -0
 5486              		.cfi_startproc
 5487              		@ args = 0, pretend = 0, frame = 0
 5488              		@ frame_needed = 0, uses_anonymous_args = 0
3905:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in 16 Bit mode */
 5489              		.loc 1 3905 1 is_stmt 0 view .LVU1842
 5490 0000 08B5     		push	{r3, lr}
 5491              		.cfi_def_cfa_offset 8
 5492              		.cfi_offset 3, -8
 5493              		.cfi_offset 14, -4
3907:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
 5494              		.loc 1 3907 3 is_stmt 1 view .LVU1843
3907:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
 5495              		.loc 1 3907 42 is_stmt 0 view .LVU1844
 5496 0002 826B     		ldr	r2, [r0, #56]
3907:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
 5497              		.loc 1 3907 7 view .LVU1845
 5498 0004 0368     		ldr	r3, [r0]
3907:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
 5499              		.loc 1 3907 24 view .LVU1846
 5500 0006 1288     		ldrh	r2, [r2]
3907:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
 5501              		.loc 1 3907 22 view .LVU1847
 5502 0008 DA60     		str	r2, [r3, #12]
3908:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
 5503              		.loc 1 3908 3 is_stmt 1 view .LVU1848
3908:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
 5504              		.loc 1 3908 7 is_stmt 0 view .LVU1849
 5505 000a 836B     		ldr	r3, [r0, #56]
3908:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
 5506              		.loc 1 3908 20 view .LVU1850
 5507 000c 0233     		adds	r3, r3, #2
 5508 000e 8363     		str	r3, [r0, #56]
3909:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5509              		.loc 1 3909 3 is_stmt 1 view .LVU1851
3909:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5510              		.loc 1 3909 7 is_stmt 0 view .LVU1852
 5511 0010 C38F     		ldrh	r3, [r0, #62]
 5512 0012 9BB2     		uxth	r3, r3
3909:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5513              		.loc 1 3909 20 view .LVU1853
 5514 0014 013B     		subs	r3, r3, #1
 5515 0016 9BB2     		uxth	r3, r3
 5516 0018 C387     		strh	r3, [r0, #62]	@ movhi
3911:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5517              		.loc 1 3911 3 is_stmt 1 view .LVU1854
3911:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/ccqUhOmw.s 			page 204


 5518              		.loc 1 3911 11 is_stmt 0 view .LVU1855
 5519 001a C38F     		ldrh	r3, [r0, #62]
 5520 001c 9BB2     		uxth	r3, r3
3911:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5521              		.loc 1 3911 6 view .LVU1856
 5522 001e 03B1     		cbz	r3, .L386
 5523              	.LVL348:
 5524              	.L383:
3922:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5525              		.loc 1 3922 1 view .LVU1857
 5526 0020 08BD     		pop	{r3, pc}
 5527              	.LVL349:
 5528              	.L386:
3920:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5529              		.loc 1 3920 5 is_stmt 1 view .LVU1858
 5530 0022 FFF7FEFF 		bl	SPI_CloseTx_ISR
 5531              	.LVL350:
3922:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5532              		.loc 1 3922 1 is_stmt 0 view .LVU1859
 5533 0026 FBE7     		b	.L383
 5534              		.cfi_endproc
 5535              	.LFE176:
 5537              		.section	.text.SPI_CloseRx_ISR,"ax",%progbits
 5538              		.align	1
 5539              		.syntax unified
 5540              		.thumb
 5541              		.thumb_func
 5543              	SPI_CloseRx_ISR:
 5544              	.LVL351:
 5545              	.LFB182:
4229:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable RXNE and ERR interrupt */
 5546              		.loc 1 4229 1 is_stmt 1 view -0
 5547              		.cfi_startproc
 5548              		@ args = 0, pretend = 0, frame = 0
 5549              		@ frame_needed = 0, uses_anonymous_args = 0
4229:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Disable RXNE and ERR interrupt */
 5550              		.loc 1 4229 1 is_stmt 0 view .LVU1861
 5551 0000 10B5     		push	{r4, lr}
 5552              		.cfi_def_cfa_offset 8
 5553              		.cfi_offset 4, -8
 5554              		.cfi_offset 14, -4
 5555 0002 0446     		mov	r4, r0
4231:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5556              		.loc 1 4231 3 is_stmt 1 view .LVU1862
 5557 0004 0268     		ldr	r2, [r0]
 5558 0006 5368     		ldr	r3, [r2, #4]
 5559 0008 23F06003 		bic	r3, r3, #96
 5560 000c 5360     		str	r3, [r2, #4]
4234:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5561              		.loc 1 4234 3 view .LVU1863
4234:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5562              		.loc 1 4234 7 is_stmt 0 view .LVU1864
 5563 000e FFF7FEFF 		bl	HAL_GetTick
 5564              	.LVL352:
4234:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5565              		.loc 1 4234 7 view .LVU1865
 5566 0012 0246     		mov	r2, r0
ARM GAS  /tmp/ccqUhOmw.s 			page 205


 5567 0014 6421     		movs	r1, #100
 5568 0016 2046     		mov	r0, r4
 5569 0018 FFF7FEFF 		bl	SPI_EndRxTransaction
 5570              	.LVL353:
4234:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5571              		.loc 1 4234 6 view .LVU1866
 5572 001c 18B1     		cbz	r0, .L388
4236:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5573              		.loc 1 4236 5 is_stmt 1 view .LVU1867
 5574 001e 236E     		ldr	r3, [r4, #96]
 5575 0020 43F02003 		orr	r3, r3, #32
 5576 0024 2366     		str	r3, [r4, #96]
 5577              	.L388:
4238:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5578              		.loc 1 4238 3 view .LVU1868
4238:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5579              		.loc 1 4238 15 is_stmt 0 view .LVU1869
 5580 0026 0123     		movs	r3, #1
 5581 0028 84F85D30 		strb	r3, [r4, #93]
4256:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5582              		.loc 1 4256 5 is_stmt 1 view .LVU1870
4256:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5583              		.loc 1 4256 13 is_stmt 0 view .LVU1871
 5584 002c 236E     		ldr	r3, [r4, #96]
4256:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5585              		.loc 1 4256 8 view .LVU1872
 5586 002e 1BB9     		cbnz	r3, .L389
4262:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5587              		.loc 1 4262 7 is_stmt 1 view .LVU1873
 5588 0030 2046     		mov	r0, r4
 5589 0032 FFF7FEFF 		bl	HAL_SPI_RxCpltCallback
 5590              	.LVL354:
 5591              	.L387:
4277:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5592              		.loc 1 4277 1 is_stmt 0 view .LVU1874
 5593 0036 10BD     		pop	{r4, pc}
 5594              	.LVL355:
 5595              	.L389:
4271:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5596              		.loc 1 4271 7 is_stmt 1 view .LVU1875
 5597 0038 2046     		mov	r0, r4
 5598 003a FFF7FEFF 		bl	HAL_SPI_ErrorCallback
 5599              	.LVL356:
4277:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5600              		.loc 1 4277 1 is_stmt 0 view .LVU1876
 5601 003e FAE7     		b	.L387
 5602              		.cfi_endproc
 5603              	.LFE182:
 5605              		.section	.text.SPI_RxISR_8BIT,"ax",%progbits
 5606              		.align	1
 5607              		.syntax unified
 5608              		.thumb
 5609              		.thumb_func
 5611              	SPI_RxISR_8BIT:
 5612              	.LVL357:
 5613              	.LFB173:
3791:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *hspi->pRxBuffPtr = (*(__IO uint8_t *)&hspi->Instance->DR);
ARM GAS  /tmp/ccqUhOmw.s 			page 206


 5614              		.loc 1 3791 1 is_stmt 1 view -0
 5615              		.cfi_startproc
 5616              		@ args = 0, pretend = 0, frame = 0
 5617              		@ frame_needed = 0, uses_anonymous_args = 0
3791:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *hspi->pRxBuffPtr = (*(__IO uint8_t *)&hspi->Instance->DR);
 5618              		.loc 1 3791 1 is_stmt 0 view .LVU1878
 5619 0000 08B5     		push	{r3, lr}
 5620              		.cfi_def_cfa_offset 8
 5621              		.cfi_offset 3, -8
 5622              		.cfi_offset 14, -4
3792:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr++;
 5623              		.loc 1 3792 3 is_stmt 1 view .LVU1879
3792:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr++;
 5624              		.loc 1 3792 46 is_stmt 0 view .LVU1880
 5625 0002 0268     		ldr	r2, [r0]
3792:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr++;
 5626              		.loc 1 3792 8 view .LVU1881
 5627 0004 036C     		ldr	r3, [r0, #64]
3792:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr++;
 5628              		.loc 1 3792 24 view .LVU1882
 5629 0006 127B     		ldrb	r2, [r2, #12]	@ zero_extendqisi2
3792:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr++;
 5630              		.loc 1 3792 21 view .LVU1883
 5631 0008 1A70     		strb	r2, [r3]
3793:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
 5632              		.loc 1 3793 3 is_stmt 1 view .LVU1884
3793:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
 5633              		.loc 1 3793 7 is_stmt 0 view .LVU1885
 5634 000a 036C     		ldr	r3, [r0, #64]
3793:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
 5635              		.loc 1 3793 19 view .LVU1886
 5636 000c 0133     		adds	r3, r3, #1
 5637 000e 0364     		str	r3, [r0, #64]
3794:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5638              		.loc 1 3794 3 is_stmt 1 view .LVU1887
3794:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5639              		.loc 1 3794 7 is_stmt 0 view .LVU1888
 5640 0010 B0F84630 		ldrh	r3, [r0, #70]
 5641 0014 9BB2     		uxth	r3, r3
3794:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5642              		.loc 1 3794 20 view .LVU1889
 5643 0016 013B     		subs	r3, r3, #1
 5644 0018 9BB2     		uxth	r3, r3
 5645 001a A0F84630 		strh	r3, [r0, #70]	@ movhi
3804:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5646              		.loc 1 3804 3 is_stmt 1 view .LVU1890
3804:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5647              		.loc 1 3804 11 is_stmt 0 view .LVU1891
 5648 001e B0F84630 		ldrh	r3, [r0, #70]
 5649 0022 9BB2     		uxth	r3, r3
3804:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5650              		.loc 1 3804 6 view .LVU1892
 5651 0024 03B1     		cbz	r3, .L395
 5652              	.LVL358:
 5653              	.L392:
3815:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5654              		.loc 1 3815 1 view .LVU1893
ARM GAS  /tmp/ccqUhOmw.s 			page 207


 5655 0026 08BD     		pop	{r3, pc}
 5656              	.LVL359:
 5657              	.L395:
3813:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5658              		.loc 1 3813 5 is_stmt 1 view .LVU1894
 5659 0028 FFF7FEFF 		bl	SPI_CloseRx_ISR
 5660              	.LVL360:
3815:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5661              		.loc 1 3815 1 is_stmt 0 view .LVU1895
 5662 002c FBE7     		b	.L392
 5663              		.cfi_endproc
 5664              	.LFE173:
 5666              		.section	.text.SPI_RxISR_16BIT,"ax",%progbits
 5667              		.align	1
 5668              		.syntax unified
 5669              		.thumb
 5670              		.thumb_func
 5672              	SPI_RxISR_16BIT:
 5673              	.LVL361:
 5674              	.LFB174:
3847:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *((uint16_t *)hspi->pRxBuffPtr) = (uint16_t)(hspi->Instance->DR);
 5675              		.loc 1 3847 1 is_stmt 1 view -0
 5676              		.cfi_startproc
 5677              		@ args = 0, pretend = 0, frame = 0
 5678              		@ frame_needed = 0, uses_anonymous_args = 0
3847:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   *((uint16_t *)hspi->pRxBuffPtr) = (uint16_t)(hspi->Instance->DR);
 5679              		.loc 1 3847 1 is_stmt 0 view .LVU1897
 5680 0000 08B5     		push	{r3, lr}
 5681              		.cfi_def_cfa_offset 8
 5682              		.cfi_offset 3, -8
 5683              		.cfi_offset 14, -4
3848:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
 5684              		.loc 1 3848 3 is_stmt 1 view .LVU1898
3848:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
 5685              		.loc 1 3848 52 is_stmt 0 view .LVU1899
 5686 0002 0368     		ldr	r3, [r0]
3848:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
 5687              		.loc 1 3848 62 view .LVU1900
 5688 0004 DA68     		ldr	r2, [r3, #12]
3848:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
 5689              		.loc 1 3848 21 view .LVU1901
 5690 0006 036C     		ldr	r3, [r0, #64]
3848:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
 5691              		.loc 1 3848 35 view .LVU1902
 5692 0008 1A80     		strh	r2, [r3]	@ movhi
3849:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
 5693              		.loc 1 3849 3 is_stmt 1 view .LVU1903
3849:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
 5694              		.loc 1 3849 7 is_stmt 0 view .LVU1904
 5695 000a 036C     		ldr	r3, [r0, #64]
3849:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
 5696              		.loc 1 3849 20 view .LVU1905
 5697 000c 0233     		adds	r3, r3, #2
 5698 000e 0364     		str	r3, [r0, #64]
3850:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5699              		.loc 1 3850 3 is_stmt 1 view .LVU1906
3850:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/ccqUhOmw.s 			page 208


 5700              		.loc 1 3850 7 is_stmt 0 view .LVU1907
 5701 0010 B0F84630 		ldrh	r3, [r0, #70]
 5702 0014 9BB2     		uxth	r3, r3
3850:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5703              		.loc 1 3850 20 view .LVU1908
 5704 0016 013B     		subs	r3, r3, #1
 5705 0018 9BB2     		uxth	r3, r3
 5706 001a A0F84630 		strh	r3, [r0, #70]	@ movhi
3860:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5707              		.loc 1 3860 3 is_stmt 1 view .LVU1909
3860:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5708              		.loc 1 3860 11 is_stmt 0 view .LVU1910
 5709 001e B0F84630 		ldrh	r3, [r0, #70]
 5710 0022 9BB2     		uxth	r3, r3
3860:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5711              		.loc 1 3860 6 view .LVU1911
 5712 0024 03B1     		cbz	r3, .L399
 5713              	.LVL362:
 5714              	.L396:
3871:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5715              		.loc 1 3871 1 view .LVU1912
 5716 0026 08BD     		pop	{r3, pc}
 5717              	.LVL363:
 5718              	.L399:
3869:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5719              		.loc 1 3869 5 is_stmt 1 view .LVU1913
 5720 0028 FFF7FEFF 		bl	SPI_CloseRx_ISR
 5721              	.LVL364:
3871:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5722              		.loc 1 3871 1 is_stmt 0 view .LVU1914
 5723 002c FBE7     		b	.L396
 5724              		.cfi_endproc
 5725              	.LFE174:
 5727              		.section	.text.SPI_CloseRxTx_ISR,"ax",%progbits
 5728              		.align	1
 5729              		.syntax unified
 5730              		.thumb
 5731              		.thumb_func
 5733              	SPI_CloseRxTx_ISR:
 5734              	.LVL365:
 5735              	.LFB181:
4152:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 5736              		.loc 1 4152 1 is_stmt 1 view -0
 5737              		.cfi_startproc
 5738              		@ args = 0, pretend = 0, frame = 0
 5739              		@ frame_needed = 0, uses_anonymous_args = 0
4152:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 5740              		.loc 1 4152 1 is_stmt 0 view .LVU1916
 5741 0000 10B5     		push	{r4, lr}
 5742              		.cfi_def_cfa_offset 8
 5743              		.cfi_offset 4, -8
 5744              		.cfi_offset 14, -4
 5745 0002 0446     		mov	r4, r0
4153:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5746              		.loc 1 4153 3 is_stmt 1 view .LVU1917
4156:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5747              		.loc 1 4156 3 view .LVU1918
ARM GAS  /tmp/ccqUhOmw.s 			page 209


4156:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5748              		.loc 1 4156 15 is_stmt 0 view .LVU1919
 5749 0004 FFF7FEFF 		bl	HAL_GetTick
 5750              	.LVL366:
4156:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5751              		.loc 1 4156 15 view .LVU1920
 5752 0008 0246     		mov	r2, r0
 5753              	.LVL367:
4159:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5754              		.loc 1 4159 3 is_stmt 1 view .LVU1921
 5755 000a 2168     		ldr	r1, [r4]
 5756 000c 4B68     		ldr	r3, [r1, #4]
 5757 000e 23F02003 		bic	r3, r3, #32
 5758 0012 4B60     		str	r3, [r1, #4]
4162:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5759              		.loc 1 4162 3 view .LVU1922
4162:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5760              		.loc 1 4162 7 is_stmt 0 view .LVU1923
 5761 0014 6421     		movs	r1, #100
 5762 0016 2046     		mov	r0, r4
 5763              	.LVL368:
4162:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5764              		.loc 1 4162 7 view .LVU1924
 5765 0018 FFF7FEFF 		bl	SPI_EndRxTxTransaction
 5766              	.LVL369:
4162:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5767              		.loc 1 4162 6 view .LVU1925
 5768 001c 18B1     		cbz	r0, .L401
4164:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5769              		.loc 1 4164 5 is_stmt 1 view .LVU1926
 5770 001e 236E     		ldr	r3, [r4, #96]
 5771 0020 43F02003 		orr	r3, r3, #32
 5772 0024 2366     		str	r3, [r4, #96]
 5773              	.L401:
4184:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5774              		.loc 1 4184 5 view .LVU1927
4184:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5775              		.loc 1 4184 13 is_stmt 0 view .LVU1928
 5776 0026 236E     		ldr	r3, [r4, #96]
4184:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5777              		.loc 1 4184 8 view .LVU1929
 5778 0028 93B9     		cbnz	r3, .L402
4186:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 5779              		.loc 1 4186 7 is_stmt 1 view .LVU1930
4186:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 5780              		.loc 1 4186 15 is_stmt 0 view .LVU1931
 5781 002a 94F85D30 		ldrb	r3, [r4, #93]	@ zero_extendqisi2
 5782 002e DBB2     		uxtb	r3, r3
4186:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 5783              		.loc 1 4186 10 view .LVU1932
 5784 0030 042B     		cmp	r3, #4
 5785 0032 06D0     		beq	.L406
4198:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Call user TxRx complete callback */
 5786              		.loc 1 4198 9 is_stmt 1 view .LVU1933
4198:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Call user TxRx complete callback */
 5787              		.loc 1 4198 21 is_stmt 0 view .LVU1934
 5788 0034 0123     		movs	r3, #1
ARM GAS  /tmp/ccqUhOmw.s 			page 210


 5789 0036 84F85D30 		strb	r3, [r4, #93]
4203:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5790              		.loc 1 4203 9 is_stmt 1 view .LVU1935
 5791 003a 2046     		mov	r0, r4
 5792 003c FFF7FEFF 		bl	HAL_SPI_TxRxCpltCallback
 5793              	.LVL370:
 5794              	.L400:
4220:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5795              		.loc 1 4220 1 is_stmt 0 view .LVU1936
 5796 0040 10BD     		pop	{r4, pc}
 5797              	.LVL371:
 5798              	.L406:
4188:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Call user Rx complete callback */
 5799              		.loc 1 4188 9 is_stmt 1 view .LVU1937
4188:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         /* Call user Rx complete callback */
 5800              		.loc 1 4188 21 is_stmt 0 view .LVU1938
 5801 0042 0123     		movs	r3, #1
 5802 0044 84F85D30 		strb	r3, [r4, #93]
4193:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5803              		.loc 1 4193 9 is_stmt 1 view .LVU1939
 5804 0048 2046     		mov	r0, r4
 5805 004a FFF7FEFF 		bl	HAL_SPI_RxCpltCallback
 5806              	.LVL372:
 5807 004e F7E7     		b	.L400
 5808              	.L402:
4209:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Call user error callback */
 5809              		.loc 1 4209 7 view .LVU1940
4209:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Call user error callback */
 5810              		.loc 1 4209 19 is_stmt 0 view .LVU1941
 5811 0050 0123     		movs	r3, #1
 5812 0052 84F85D30 		strb	r3, [r4, #93]
4214:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 5813              		.loc 1 4214 7 is_stmt 1 view .LVU1942
 5814 0056 2046     		mov	r0, r4
 5815 0058 FFF7FEFF 		bl	HAL_SPI_ErrorCallback
 5816              	.LVL373:
4220:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5817              		.loc 1 4220 1 is_stmt 0 view .LVU1943
 5818 005c F0E7     		b	.L400
 5819              		.cfi_endproc
 5820              	.LFE181:
 5822              		.section	.text.SPI_2linesTxISR_8BIT,"ax",%progbits
 5823              		.align	1
 5824              		.syntax unified
 5825              		.thumb
 5826              		.thumb_func
 5828              	SPI_2linesTxISR_8BIT:
 5829              	.LVL374:
 5830              	.LFB170:
3623:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in packing Bit mode */
 5831              		.loc 1 3623 1 is_stmt 1 view -0
 5832              		.cfi_startproc
 5833              		@ args = 0, pretend = 0, frame = 0
 5834              		@ frame_needed = 0, uses_anonymous_args = 0
3623:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in packing Bit mode */
 5835              		.loc 1 3623 1 is_stmt 0 view .LVU1945
 5836 0000 08B5     		push	{r3, lr}
ARM GAS  /tmp/ccqUhOmw.s 			page 211


 5837              		.cfi_def_cfa_offset 8
 5838              		.cfi_offset 3, -8
 5839              		.cfi_offset 14, -4
3625:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5840              		.loc 1 3625 3 is_stmt 1 view .LVU1946
3625:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5841              		.loc 1 3625 11 is_stmt 0 view .LVU1947
 5842 0002 C38F     		ldrh	r3, [r0, #62]
 5843 0004 9BB2     		uxth	r3, r3
3625:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5844              		.loc 1 3625 6 view .LVU1948
 5845 0006 012B     		cmp	r3, #1
 5846 0008 18D9     		bls	.L408
3627:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr += sizeof(uint16_t);
 5847              		.loc 1 3627 5 is_stmt 1 view .LVU1949
3627:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr += sizeof(uint16_t);
 5848              		.loc 1 3627 44 is_stmt 0 view .LVU1950
 5849 000a 826B     		ldr	r2, [r0, #56]
3627:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr += sizeof(uint16_t);
 5850              		.loc 1 3627 9 view .LVU1951
 5851 000c 0368     		ldr	r3, [r0]
3627:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr += sizeof(uint16_t);
 5852              		.loc 1 3627 26 view .LVU1952
 5853 000e 1288     		ldrh	r2, [r2]
3627:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr += sizeof(uint16_t);
 5854              		.loc 1 3627 24 view .LVU1953
 5855 0010 DA60     		str	r2, [r3, #12]
3628:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount -= 2U;
 5856              		.loc 1 3628 5 is_stmt 1 view .LVU1954
3628:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount -= 2U;
 5857              		.loc 1 3628 9 is_stmt 0 view .LVU1955
 5858 0012 836B     		ldr	r3, [r0, #56]
3628:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount -= 2U;
 5859              		.loc 1 3628 22 view .LVU1956
 5860 0014 0233     		adds	r3, r3, #2
 5861 0016 8363     		str	r3, [r0, #56]
3629:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5862              		.loc 1 3629 5 is_stmt 1 view .LVU1957
3629:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5863              		.loc 1 3629 9 is_stmt 0 view .LVU1958
 5864 0018 C38F     		ldrh	r3, [r0, #62]
 5865 001a 9BB2     		uxth	r3, r3
3629:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5866              		.loc 1 3629 23 view .LVU1959
 5867 001c 023B     		subs	r3, r3, #2
 5868 001e 9BB2     		uxth	r3, r3
 5869 0020 C387     		strh	r3, [r0, #62]	@ movhi
 5870              	.L409:
3640:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5871              		.loc 1 3640 3 is_stmt 1 view .LVU1960
3640:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5872              		.loc 1 3640 11 is_stmt 0 view .LVU1961
 5873 0022 C38F     		ldrh	r3, [r0, #62]
 5874 0024 9BB2     		uxth	r3, r3
3640:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5875              		.loc 1 3640 6 view .LVU1962
 5876 0026 43B9     		cbnz	r3, .L407
ARM GAS  /tmp/ccqUhOmw.s 			page 212


3654:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5877              		.loc 1 3654 5 is_stmt 1 view .LVU1963
 5878 0028 0268     		ldr	r2, [r0]
 5879 002a 5368     		ldr	r3, [r2, #4]
 5880 002c 23F08003 		bic	r3, r3, #128
 5881 0030 5360     		str	r3, [r2, #4]
3656:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5882              		.loc 1 3656 5 view .LVU1964
3656:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5883              		.loc 1 3656 13 is_stmt 0 view .LVU1965
 5884 0032 B0F84630 		ldrh	r3, [r0, #70]
 5885 0036 9BB2     		uxth	r3, r3
3656:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5886              		.loc 1 3656 8 view .LVU1966
 5887 0038 6BB1     		cbz	r3, .L412
 5888              	.LVL375:
 5889              	.L407:
3661:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5890              		.loc 1 3661 1 view .LVU1967
 5891 003a 08BD     		pop	{r3, pc}
 5892              	.LVL376:
 5893              	.L408:
3634:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr++;
 5894              		.loc 1 3634 5 is_stmt 1 view .LVU1968
3634:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr++;
 5895              		.loc 1 3634 50 is_stmt 0 view .LVU1969
 5896 003c 826B     		ldr	r2, [r0, #56]
3634:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr++;
 5897              		.loc 1 3634 27 view .LVU1970
 5898 003e 0368     		ldr	r3, [r0]
3634:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr++;
 5899              		.loc 1 3634 45 view .LVU1971
 5900 0040 1278     		ldrb	r2, [r2]	@ zero_extendqisi2
3634:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pTxBuffPtr++;
 5901              		.loc 1 3634 42 view .LVU1972
 5902 0042 1A73     		strb	r2, [r3, #12]
3635:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount--;
 5903              		.loc 1 3635 5 is_stmt 1 view .LVU1973
3635:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount--;
 5904              		.loc 1 3635 9 is_stmt 0 view .LVU1974
 5905 0044 836B     		ldr	r3, [r0, #56]
3635:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount--;
 5906              		.loc 1 3635 21 view .LVU1975
 5907 0046 0133     		adds	r3, r3, #1
 5908 0048 8363     		str	r3, [r0, #56]
3636:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5909              		.loc 1 3636 5 is_stmt 1 view .LVU1976
3636:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5910              		.loc 1 3636 9 is_stmt 0 view .LVU1977
 5911 004a C38F     		ldrh	r3, [r0, #62]
 5912 004c 9BB2     		uxth	r3, r3
3636:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 5913              		.loc 1 3636 22 view .LVU1978
 5914 004e 013B     		subs	r3, r3, #1
 5915 0050 9BB2     		uxth	r3, r3
 5916 0052 C387     		strh	r3, [r0, #62]	@ movhi
 5917 0054 E5E7     		b	.L409
ARM GAS  /tmp/ccqUhOmw.s 			page 213


 5918              	.L412:
3658:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 5919              		.loc 1 3658 7 is_stmt 1 view .LVU1979
 5920 0056 FFF7FEFF 		bl	SPI_CloseRxTx_ISR
 5921              	.LVL377:
3661:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 5922              		.loc 1 3661 1 is_stmt 0 view .LVU1980
 5923 005a EEE7     		b	.L407
 5924              		.cfi_endproc
 5925              	.LFE170:
 5927              		.section	.text.SPI_2linesRxISR_8BIT,"ax",%progbits
 5928              		.align	1
 5929              		.syntax unified
 5930              		.thumb
 5931              		.thumb_func
 5933              	SPI_2linesRxISR_8BIT:
 5934              	.LVL378:
 5935              	.LFB169:
3538:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Receive data in packing mode */
 5936              		.loc 1 3538 1 is_stmt 1 view -0
 5937              		.cfi_startproc
 5938              		@ args = 0, pretend = 0, frame = 0
 5939              		@ frame_needed = 0, uses_anonymous_args = 0
3538:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Receive data in packing mode */
 5940              		.loc 1 3538 1 is_stmt 0 view .LVU1982
 5941 0000 08B5     		push	{r3, lr}
 5942              		.cfi_def_cfa_offset 8
 5943              		.cfi_offset 3, -8
 5944              		.cfi_offset 14, -4
3540:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5945              		.loc 1 3540 3 is_stmt 1 view .LVU1983
3540:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5946              		.loc 1 3540 11 is_stmt 0 view .LVU1984
 5947 0002 B0F84630 		ldrh	r3, [r0, #70]
 5948 0006 9BB2     		uxth	r3, r3
3540:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 5949              		.loc 1 3540 6 view .LVU1985
 5950 0008 012B     		cmp	r3, #1
 5951 000a 18D9     		bls	.L414
3542:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr += sizeof(uint16_t);
 5952              		.loc 1 3542 5 is_stmt 1 view .LVU1986
3542:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr += sizeof(uint16_t);
 5953              		.loc 1 3542 54 is_stmt 0 view .LVU1987
 5954 000c 0368     		ldr	r3, [r0]
3542:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr += sizeof(uint16_t);
 5955              		.loc 1 3542 64 view .LVU1988
 5956 000e DA68     		ldr	r2, [r3, #12]
3542:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr += sizeof(uint16_t);
 5957              		.loc 1 3542 23 view .LVU1989
 5958 0010 036C     		ldr	r3, [r0, #64]
3542:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr += sizeof(uint16_t);
 5959              		.loc 1 3542 37 view .LVU1990
 5960 0012 1A80     		strh	r2, [r3]	@ movhi
3543:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount -= 2U;
 5961              		.loc 1 3543 5 is_stmt 1 view .LVU1991
3543:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount -= 2U;
 5962              		.loc 1 3543 9 is_stmt 0 view .LVU1992
ARM GAS  /tmp/ccqUhOmw.s 			page 214


 5963 0014 036C     		ldr	r3, [r0, #64]
3543:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount -= 2U;
 5964              		.loc 1 3543 22 view .LVU1993
 5965 0016 0233     		adds	r3, r3, #2
 5966 0018 0364     		str	r3, [r0, #64]
3544:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->RxXferCount == 1U)
 5967              		.loc 1 3544 5 is_stmt 1 view .LVU1994
3544:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->RxXferCount == 1U)
 5968              		.loc 1 3544 9 is_stmt 0 view .LVU1995
 5969 001a B0F84630 		ldrh	r3, [r0, #70]
 5970 001e 9BB2     		uxth	r3, r3
3544:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     if (hspi->RxXferCount == 1U)
 5971              		.loc 1 3544 23 view .LVU1996
 5972 0020 023B     		subs	r3, r3, #2
 5973 0022 9BB2     		uxth	r3, r3
 5974 0024 A0F84630 		strh	r3, [r0, #70]	@ movhi
3545:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5975              		.loc 1 3545 5 is_stmt 1 view .LVU1997
3545:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5976              		.loc 1 3545 13 is_stmt 0 view .LVU1998
 5977 0028 B0F84630 		ldrh	r3, [r0, #70]
 5978 002c 9BB2     		uxth	r3, r3
3545:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 5979              		.loc 1 3545 8 view .LVU1999
 5980 002e 012B     		cmp	r3, #1
 5981 0030 13D1     		bne	.L415
3548:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 5982              		.loc 1 3548 7 is_stmt 1 view .LVU2000
 5983 0032 0268     		ldr	r2, [r0]
 5984 0034 5368     		ldr	r3, [r2, #4]
 5985 0036 43F48053 		orr	r3, r3, #4096
 5986 003a 5360     		str	r3, [r2, #4]
 5987 003c 0DE0     		b	.L415
 5988              	.L414:
3554:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr++;
 5989              		.loc 1 3554 5 view .LVU2001
3554:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr++;
 5990              		.loc 1 3554 48 is_stmt 0 view .LVU2002
 5991 003e 0268     		ldr	r2, [r0]
3554:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr++;
 5992              		.loc 1 3554 10 view .LVU2003
 5993 0040 036C     		ldr	r3, [r0, #64]
3554:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr++;
 5994              		.loc 1 3554 25 view .LVU2004
 5995 0042 127B     		ldrb	r2, [r2, #12]	@ zero_extendqisi2
3554:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->pRxBuffPtr++;
 5996              		.loc 1 3554 23 view .LVU2005
 5997 0044 1A70     		strb	r2, [r3]
3555:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount--;
 5998              		.loc 1 3555 5 is_stmt 1 view .LVU2006
3555:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount--;
 5999              		.loc 1 3555 9 is_stmt 0 view .LVU2007
 6000 0046 036C     		ldr	r3, [r0, #64]
3555:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount--;
 6001              		.loc 1 3555 21 view .LVU2008
 6002 0048 0133     		adds	r3, r3, #1
 6003 004a 0364     		str	r3, [r0, #64]
ARM GAS  /tmp/ccqUhOmw.s 			page 215


3556:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 6004              		.loc 1 3556 5 is_stmt 1 view .LVU2009
3556:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 6005              		.loc 1 3556 9 is_stmt 0 view .LVU2010
 6006 004c B0F84630 		ldrh	r3, [r0, #70]
 6007 0050 9BB2     		uxth	r3, r3
3556:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 6008              		.loc 1 3556 22 view .LVU2011
 6009 0052 013B     		subs	r3, r3, #1
 6010 0054 9BB2     		uxth	r3, r3
 6011 0056 A0F84630 		strh	r3, [r0, #70]	@ movhi
 6012              	.L415:
3560:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6013              		.loc 1 3560 3 is_stmt 1 view .LVU2012
3560:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6014              		.loc 1 3560 11 is_stmt 0 view .LVU2013
 6015 005a B0F84630 		ldrh	r3, [r0, #70]
 6016 005e 9BB2     		uxth	r3, r3
3560:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6017              		.loc 1 3560 6 view .LVU2014
 6018 0060 3BB9     		cbnz	r3, .L413
3572:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6019              		.loc 1 3572 5 is_stmt 1 view .LVU2015
 6020 0062 0268     		ldr	r2, [r0]
 6021 0064 5368     		ldr	r3, [r2, #4]
 6022 0066 23F06003 		bic	r3, r3, #96
 6023 006a 5360     		str	r3, [r2, #4]
3574:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6024              		.loc 1 3574 5 view .LVU2016
3574:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6025              		.loc 1 3574 13 is_stmt 0 view .LVU2017
 6026 006c C38F     		ldrh	r3, [r0, #62]
 6027 006e 9BB2     		uxth	r3, r3
3574:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6028              		.loc 1 3574 8 view .LVU2018
 6029 0070 03B1     		cbz	r3, .L418
 6030              	.LVL379:
 6031              	.L413:
3579:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6032              		.loc 1 3579 1 view .LVU2019
 6033 0072 08BD     		pop	{r3, pc}
 6034              	.LVL380:
 6035              	.L418:
3576:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6036              		.loc 1 3576 7 is_stmt 1 view .LVU2020
 6037 0074 FFF7FEFF 		bl	SPI_CloseRxTx_ISR
 6038              	.LVL381:
3579:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6039              		.loc 1 3579 1 is_stmt 0 view .LVU2021
 6040 0078 FBE7     		b	.L413
 6041              		.cfi_endproc
 6042              	.LFE169:
 6044              		.section	.text.SPI_2linesTxISR_16BIT,"ax",%progbits
 6045              		.align	1
 6046              		.syntax unified
 6047              		.thumb
 6048              		.thumb_func
ARM GAS  /tmp/ccqUhOmw.s 			page 216


 6050              	SPI_2linesTxISR_16BIT:
 6051              	.LVL382:
 6052              	.LFB172:
3726:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in 16 Bit mode */
 6053              		.loc 1 3726 1 is_stmt 1 view -0
 6054              		.cfi_startproc
 6055              		@ args = 0, pretend = 0, frame = 0
 6056              		@ frame_needed = 0, uses_anonymous_args = 0
3726:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Transmit data in 16 Bit mode */
 6057              		.loc 1 3726 1 is_stmt 0 view .LVU2023
 6058 0000 08B5     		push	{r3, lr}
 6059              		.cfi_def_cfa_offset 8
 6060              		.cfi_offset 3, -8
 6061              		.cfi_offset 14, -4
3728:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
 6062              		.loc 1 3728 3 is_stmt 1 view .LVU2024
3728:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
 6063              		.loc 1 3728 42 is_stmt 0 view .LVU2025
 6064 0002 826B     		ldr	r2, [r0, #56]
3728:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
 6065              		.loc 1 3728 7 view .LVU2026
 6066 0004 0368     		ldr	r3, [r0]
3728:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
 6067              		.loc 1 3728 24 view .LVU2027
 6068 0006 1288     		ldrh	r2, [r2]
3728:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pTxBuffPtr += sizeof(uint16_t);
 6069              		.loc 1 3728 22 view .LVU2028
 6070 0008 DA60     		str	r2, [r3, #12]
3729:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
 6071              		.loc 1 3729 3 is_stmt 1 view .LVU2029
3729:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
 6072              		.loc 1 3729 7 is_stmt 0 view .LVU2030
 6073 000a 836B     		ldr	r3, [r0, #56]
3729:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount--;
 6074              		.loc 1 3729 20 view .LVU2031
 6075 000c 0233     		adds	r3, r3, #2
 6076 000e 8363     		str	r3, [r0, #56]
3730:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6077              		.loc 1 3730 3 is_stmt 1 view .LVU2032
3730:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6078              		.loc 1 3730 7 is_stmt 0 view .LVU2033
 6079 0010 C38F     		ldrh	r3, [r0, #62]
 6080 0012 9BB2     		uxth	r3, r3
3730:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6081              		.loc 1 3730 20 view .LVU2034
 6082 0014 013B     		subs	r3, r3, #1
 6083 0016 9BB2     		uxth	r3, r3
 6084 0018 C387     		strh	r3, [r0, #62]	@ movhi
3733:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6085              		.loc 1 3733 3 is_stmt 1 view .LVU2035
3733:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6086              		.loc 1 3733 11 is_stmt 0 view .LVU2036
 6087 001a C38F     		ldrh	r3, [r0, #62]
 6088 001c 9BB2     		uxth	r3, r3
3733:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6089              		.loc 1 3733 6 view .LVU2037
 6090 001e 43B9     		cbnz	r3, .L419
ARM GAS  /tmp/ccqUhOmw.s 			page 217


3747:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6091              		.loc 1 3747 5 is_stmt 1 view .LVU2038
 6092 0020 0268     		ldr	r2, [r0]
 6093 0022 5368     		ldr	r3, [r2, #4]
 6094 0024 23F08003 		bic	r3, r3, #128
 6095 0028 5360     		str	r3, [r2, #4]
3749:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6096              		.loc 1 3749 5 view .LVU2039
3749:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6097              		.loc 1 3749 13 is_stmt 0 view .LVU2040
 6098 002a B0F84630 		ldrh	r3, [r0, #70]
 6099 002e 9BB2     		uxth	r3, r3
3749:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6100              		.loc 1 3749 8 view .LVU2041
 6101 0030 03B1     		cbz	r3, .L422
 6102              	.LVL383:
 6103              	.L419:
3754:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6104              		.loc 1 3754 1 view .LVU2042
 6105 0032 08BD     		pop	{r3, pc}
 6106              	.LVL384:
 6107              	.L422:
3751:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6108              		.loc 1 3751 7 is_stmt 1 view .LVU2043
 6109 0034 FFF7FEFF 		bl	SPI_CloseRxTx_ISR
 6110              	.LVL385:
3754:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6111              		.loc 1 3754 1 is_stmt 0 view .LVU2044
 6112 0038 FBE7     		b	.L419
 6113              		.cfi_endproc
 6114              	.LFE172:
 6116              		.section	.text.SPI_2linesRxISR_16BIT,"ax",%progbits
 6117              		.align	1
 6118              		.syntax unified
 6119              		.thumb
 6120              		.thumb_func
 6122              	SPI_2linesRxISR_16BIT:
 6123              	.LVL386:
 6124              	.LFB171:
3670:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Receive data in 16 Bit mode */
 6125              		.loc 1 3670 1 is_stmt 1 view -0
 6126              		.cfi_startproc
 6127              		@ args = 0, pretend = 0, frame = 0
 6128              		@ frame_needed = 0, uses_anonymous_args = 0
3670:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Receive data in 16 Bit mode */
 6129              		.loc 1 3670 1 is_stmt 0 view .LVU2046
 6130 0000 08B5     		push	{r3, lr}
 6131              		.cfi_def_cfa_offset 8
 6132              		.cfi_offset 3, -8
 6133              		.cfi_offset 14, -4
3672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
 6134              		.loc 1 3672 3 is_stmt 1 view .LVU2047
3672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
 6135              		.loc 1 3672 52 is_stmt 0 view .LVU2048
 6136 0002 0368     		ldr	r3, [r0]
3672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
 6137              		.loc 1 3672 62 view .LVU2049
ARM GAS  /tmp/ccqUhOmw.s 			page 218


 6138 0004 DA68     		ldr	r2, [r3, #12]
3672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
 6139              		.loc 1 3672 21 view .LVU2050
 6140 0006 036C     		ldr	r3, [r0, #64]
3672:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->pRxBuffPtr += sizeof(uint16_t);
 6141              		.loc 1 3672 35 view .LVU2051
 6142 0008 1A80     		strh	r2, [r3]	@ movhi
3673:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
 6143              		.loc 1 3673 3 is_stmt 1 view .LVU2052
3673:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
 6144              		.loc 1 3673 7 is_stmt 0 view .LVU2053
 6145 000a 036C     		ldr	r3, [r0, #64]
3673:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount--;
 6146              		.loc 1 3673 20 view .LVU2054
 6147 000c 0233     		adds	r3, r3, #2
 6148 000e 0364     		str	r3, [r0, #64]
3674:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6149              		.loc 1 3674 3 is_stmt 1 view .LVU2055
3674:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6150              		.loc 1 3674 7 is_stmt 0 view .LVU2056
 6151 0010 B0F84630 		ldrh	r3, [r0, #70]
 6152 0014 9BB2     		uxth	r3, r3
3674:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6153              		.loc 1 3674 20 view .LVU2057
 6154 0016 013B     		subs	r3, r3, #1
 6155 0018 9BB2     		uxth	r3, r3
 6156 001a A0F84630 		strh	r3, [r0, #70]	@ movhi
3676:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6157              		.loc 1 3676 3 is_stmt 1 view .LVU2058
3676:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6158              		.loc 1 3676 11 is_stmt 0 view .LVU2059
 6159 001e B0F84630 		ldrh	r3, [r0, #70]
 6160 0022 9BB2     		uxth	r3, r3
3676:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6161              		.loc 1 3676 6 view .LVU2060
 6162 0024 3BB9     		cbnz	r3, .L423
3687:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6163              		.loc 1 3687 5 is_stmt 1 view .LVU2061
 6164 0026 0268     		ldr	r2, [r0]
 6165 0028 5368     		ldr	r3, [r2, #4]
 6166 002a 23F04003 		bic	r3, r3, #64
 6167 002e 5360     		str	r3, [r2, #4]
3689:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6168              		.loc 1 3689 5 view .LVU2062
3689:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6169              		.loc 1 3689 13 is_stmt 0 view .LVU2063
 6170 0030 C38F     		ldrh	r3, [r0, #62]
 6171 0032 9BB2     		uxth	r3, r3
3689:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6172              		.loc 1 3689 8 view .LVU2064
 6173 0034 03B1     		cbz	r3, .L426
 6174              	.LVL387:
 6175              	.L423:
3694:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6176              		.loc 1 3694 1 view .LVU2065
 6177 0036 08BD     		pop	{r3, pc}
 6178              	.LVL388:
ARM GAS  /tmp/ccqUhOmw.s 			page 219


 6179              	.L426:
3691:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6180              		.loc 1 3691 7 is_stmt 1 view .LVU2066
 6181 0038 FFF7FEFF 		bl	SPI_CloseRxTx_ISR
 6182              	.LVL389:
3694:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6183              		.loc 1 3694 1 is_stmt 0 view .LVU2067
 6184 003c FBE7     		b	.L423
 6185              		.cfi_endproc
 6186              	.LFE171:
 6188              		.section	.text.SPI_DMAError,"ax",%progbits
 6189              		.align	1
 6190              		.syntax unified
 6191              		.thumb
 6192              		.thumb_func
 6194              	SPI_DMAError:
 6195              	.LVL390:
 6196              	.LFB165:
3362:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 6197              		.loc 1 3362 1 is_stmt 1 view -0
 6198              		.cfi_startproc
 6199              		@ args = 0, pretend = 0, frame = 0
 6200              		@ frame_needed = 0, uses_anonymous_args = 0
3362:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 6201              		.loc 1 3362 1 is_stmt 0 view .LVU2069
 6202 0000 08B5     		push	{r3, lr}
 6203              		.cfi_def_cfa_offset 8
 6204              		.cfi_offset 3, -8
 6205              		.cfi_offset 14, -4
3363:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6206              		.loc 1 3363 3 is_stmt 1 view .LVU2070
3363:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6207              		.loc 1 3363 22 is_stmt 0 view .LVU2071
 6208 0002 406A     		ldr	r0, [r0, #36]
 6209              	.LVL391:
3366:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6210              		.loc 1 3366 3 is_stmt 1 view .LVU2072
 6211 0004 0268     		ldr	r2, [r0]
 6212 0006 5368     		ldr	r3, [r2, #4]
 6213 0008 23F00303 		bic	r3, r3, #3
 6214 000c 5360     		str	r3, [r2, #4]
3368:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->State = HAL_SPI_STATE_READY;
 6215              		.loc 1 3368 3 view .LVU2073
 6216 000e 036E     		ldr	r3, [r0, #96]
 6217 0010 43F01003 		orr	r3, r3, #16
 6218 0014 0366     		str	r3, [r0, #96]
3369:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user error callback */
 6219              		.loc 1 3369 3 view .LVU2074
3369:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Call user error callback */
 6220              		.loc 1 3369 15 is_stmt 0 view .LVU2075
 6221 0016 0123     		movs	r3, #1
 6222 0018 80F85D30 		strb	r3, [r0, #93]
3374:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6223              		.loc 1 3374 3 is_stmt 1 view .LVU2076
 6224 001c FFF7FEFF 		bl	HAL_SPI_ErrorCallback
 6225              	.LVL392:
3376:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/ccqUhOmw.s 			page 220


 6226              		.loc 1 3376 1 is_stmt 0 view .LVU2077
 6227 0020 08BD     		pop	{r3, pc}
 6228              		.cfi_endproc
 6229              	.LFE165:
 6231              		.section	.text.SPI_DMATransmitCplt,"ax",%progbits
 6232              		.align	1
 6233              		.syntax unified
 6234              		.thumb
 6235              		.thumb_func
 6237              	SPI_DMATransmitCplt:
 6238              	.LVL393:
 6239              	.LFB159:
3034:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 6240              		.loc 1 3034 1 is_stmt 1 view -0
 6241              		.cfi_startproc
 6242              		@ args = 0, pretend = 0, frame = 8
 6243              		@ frame_needed = 0, uses_anonymous_args = 0
3034:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 6244              		.loc 1 3034 1 is_stmt 0 view .LVU2079
 6245 0000 30B5     		push	{r4, r5, lr}
 6246              		.cfi_def_cfa_offset 12
 6247              		.cfi_offset 4, -12
 6248              		.cfi_offset 5, -8
 6249              		.cfi_offset 14, -4
 6250 0002 83B0     		sub	sp, sp, #12
 6251              		.cfi_def_cfa_offset 24
 6252 0004 0546     		mov	r5, r0
3035:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 6253              		.loc 1 3035 3 is_stmt 1 view .LVU2080
3035:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 6254              		.loc 1 3035 22 is_stmt 0 view .LVU2081
 6255 0006 446A     		ldr	r4, [r0, #36]
 6256              	.LVL394:
3036:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6257              		.loc 1 3036 3 is_stmt 1 view .LVU2082
3039:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6258              		.loc 1 3039 3 view .LVU2083
3039:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6259              		.loc 1 3039 15 is_stmt 0 view .LVU2084
 6260 0008 FFF7FEFF 		bl	HAL_GetTick
 6261              	.LVL395:
3042:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6262              		.loc 1 3042 3 is_stmt 1 view .LVU2085
3042:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6263              		.loc 1 3042 12 is_stmt 0 view .LVU2086
 6264 000c 2B68     		ldr	r3, [r5]
3042:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6265              		.loc 1 3042 22 view .LVU2087
 6266 000e 1B68     		ldr	r3, [r3]
3042:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6267              		.loc 1 3042 6 view .LVU2088
 6268 0010 13F0200F 		tst	r3, #32
 6269 0014 23D1     		bne	.L430
 6270 0016 0246     		mov	r2, r0
3045:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6271              		.loc 1 3045 5 is_stmt 1 view .LVU2089
 6272 0018 2168     		ldr	r1, [r4]
ARM GAS  /tmp/ccqUhOmw.s 			page 221


 6273 001a 4B68     		ldr	r3, [r1, #4]
 6274 001c 23F02003 		bic	r3, r3, #32
 6275 0020 4B60     		str	r3, [r1, #4]
3048:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6276              		.loc 1 3048 5 view .LVU2090
 6277 0022 2168     		ldr	r1, [r4]
 6278 0024 4B68     		ldr	r3, [r1, #4]
 6279 0026 23F00203 		bic	r3, r3, #2
 6280 002a 4B60     		str	r3, [r1, #4]
3051:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6281              		.loc 1 3051 5 view .LVU2091
3051:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6282              		.loc 1 3051 9 is_stmt 0 view .LVU2092
 6283 002c 6421     		movs	r1, #100
 6284 002e 2046     		mov	r0, r4
 6285              	.LVL396:
3051:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6286              		.loc 1 3051 9 view .LVU2093
 6287 0030 FFF7FEFF 		bl	SPI_EndRxTxTransaction
 6288              	.LVL397:
3051:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6289              		.loc 1 3051 8 view .LVU2094
 6290 0034 18B1     		cbz	r0, .L431
3053:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6291              		.loc 1 3053 7 is_stmt 1 view .LVU2095
 6292 0036 236E     		ldr	r3, [r4, #96]
 6293 0038 43F02003 		orr	r3, r3, #32
 6294 003c 2366     		str	r3, [r4, #96]
 6295              	.L431:
3057:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6296              		.loc 1 3057 5 view .LVU2096
3057:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6297              		.loc 1 3057 19 is_stmt 0 view .LVU2097
 6298 003e A368     		ldr	r3, [r4, #8]
3057:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6299              		.loc 1 3057 8 view .LVU2098
 6300 0040 33B9     		cbnz	r3, .L432
3059:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6301              		.loc 1 3059 7 is_stmt 1 view .LVU2099
 6302              	.LBB6:
3059:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6303              		.loc 1 3059 7 view .LVU2100
 6304 0042 0193     		str	r3, [sp, #4]
3059:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6305              		.loc 1 3059 7 view .LVU2101
 6306 0044 2368     		ldr	r3, [r4]
 6307 0046 DA68     		ldr	r2, [r3, #12]
 6308 0048 0192     		str	r2, [sp, #4]
3059:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6309              		.loc 1 3059 7 view .LVU2102
 6310 004a 9B68     		ldr	r3, [r3, #8]
 6311 004c 0193     		str	r3, [sp, #4]
3059:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6312              		.loc 1 3059 7 view .LVU2103
 6313 004e 019B     		ldr	r3, [sp, #4]
 6314              	.L432:
 6315              	.LBE6:
ARM GAS  /tmp/ccqUhOmw.s 			page 222


3059:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6316              		.loc 1 3059 7 discriminator 1 view .LVU2104
3062:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
 6317              		.loc 1 3062 5 discriminator 1 view .LVU2105
3062:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
 6318              		.loc 1 3062 23 is_stmt 0 discriminator 1 view .LVU2106
 6319 0050 0023     		movs	r3, #0
 6320 0052 E387     		strh	r3, [r4, #62]	@ movhi
3063:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6321              		.loc 1 3063 5 is_stmt 1 discriminator 1 view .LVU2107
3063:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6322              		.loc 1 3063 17 is_stmt 0 discriminator 1 view .LVU2108
 6323 0054 0123     		movs	r3, #1
 6324 0056 84F85D30 		strb	r3, [r4, #93]
3065:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6325              		.loc 1 3065 5 is_stmt 1 discriminator 1 view .LVU2109
3065:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6326              		.loc 1 3065 13 is_stmt 0 discriminator 1 view .LVU2110
 6327 005a 236E     		ldr	r3, [r4, #96]
3065:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6328              		.loc 1 3065 8 discriminator 1 view .LVU2111
 6329 005c 23B9     		cbnz	r3, .L435
 6330              	.L430:
3080:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6331              		.loc 1 3080 3 is_stmt 1 view .LVU2112
 6332 005e 2046     		mov	r0, r4
 6333 0060 FFF7FEFF 		bl	HAL_SPI_TxCpltCallback
 6334              	.LVL398:
 6335              	.L429:
3082:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6336              		.loc 1 3082 1 is_stmt 0 view .LVU2113
 6337 0064 03B0     		add	sp, sp, #12
 6338              		.cfi_remember_state
 6339              		.cfi_def_cfa_offset 12
 6340              		@ sp needed
 6341 0066 30BD     		pop	{r4, r5, pc}
 6342              	.LVL399:
 6343              	.L435:
 6344              		.cfi_restore_state
3071:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6345              		.loc 1 3071 7 is_stmt 1 view .LVU2114
 6346 0068 2046     		mov	r0, r4
 6347 006a FFF7FEFF 		bl	HAL_SPI_ErrorCallback
 6348              	.LVL400:
3073:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6349              		.loc 1 3073 7 view .LVU2115
 6350 006e F9E7     		b	.L429
 6351              		.cfi_endproc
 6352              	.LFE159:
 6354              		.section	.text.SPI_DMAReceiveCplt,"ax",%progbits
 6355              		.align	1
 6356              		.syntax unified
 6357              		.thumb
 6358              		.thumb_func
 6360              	SPI_DMAReceiveCplt:
 6361              	.LVL401:
 6362              	.LFB160:
ARM GAS  /tmp/ccqUhOmw.s 			page 223


3091:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 6363              		.loc 1 3091 1 view -0
 6364              		.cfi_startproc
 6365              		@ args = 0, pretend = 0, frame = 0
 6366              		@ frame_needed = 0, uses_anonymous_args = 0
3091:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 6367              		.loc 1 3091 1 is_stmt 0 view .LVU2117
 6368 0000 38B5     		push	{r3, r4, r5, lr}
 6369              		.cfi_def_cfa_offset 16
 6370              		.cfi_offset 3, -16
 6371              		.cfi_offset 4, -12
 6372              		.cfi_offset 5, -8
 6373              		.cfi_offset 14, -4
 6374 0002 0546     		mov	r5, r0
3092:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 6375              		.loc 1 3092 3 is_stmt 1 view .LVU2118
3092:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 6376              		.loc 1 3092 22 is_stmt 0 view .LVU2119
 6377 0004 446A     		ldr	r4, [r0, #36]
 6378              	.LVL402:
3093:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
 6379              		.loc 1 3093 3 is_stmt 1 view .LVU2120
3101:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6380              		.loc 1 3101 3 view .LVU2121
3101:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6381              		.loc 1 3101 15 is_stmt 0 view .LVU2122
 6382 0006 FFF7FEFF 		bl	HAL_GetTick
 6383              	.LVL403:
3104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6384              		.loc 1 3104 3 is_stmt 1 view .LVU2123
3104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6385              		.loc 1 3104 12 is_stmt 0 view .LVU2124
 6386 000a 2B68     		ldr	r3, [r5]
3104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6387              		.loc 1 3104 22 view .LVU2125
 6388 000c 1B68     		ldr	r3, [r3]
3104:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6389              		.loc 1 3104 6 view .LVU2126
 6390 000e 13F0200F 		tst	r3, #32
 6391 0012 1FD1     		bne	.L437
 6392 0014 0246     		mov	r2, r0
3107:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6393              		.loc 1 3107 5 is_stmt 1 view .LVU2127
 6394 0016 2168     		ldr	r1, [r4]
 6395 0018 4B68     		ldr	r3, [r1, #4]
 6396 001a 23F02003 		bic	r3, r3, #32
 6397 001e 4B60     		str	r3, [r1, #4]
3153:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6398              		.loc 1 3153 5 view .LVU2128
3153:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6399              		.loc 1 3153 20 is_stmt 0 view .LVU2129
 6400 0020 A368     		ldr	r3, [r4, #8]
3153:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6401              		.loc 1 3153 8 view .LVU2130
 6402 0022 1BB9     		cbnz	r3, .L438
3153:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6403              		.loc 1 3153 70 discriminator 1 view .LVU2131
ARM GAS  /tmp/ccqUhOmw.s 			page 224


 6404 0024 6368     		ldr	r3, [r4, #4]
3153:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6405              		.loc 1 3153 56 discriminator 1 view .LVU2132
 6406 0026 B3F5827F 		cmp	r3, #260
 6407 002a 17D0     		beq	.L443
 6408              	.L438:
3161:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6409              		.loc 1 3161 7 is_stmt 1 view .LVU2133
 6410 002c 2168     		ldr	r1, [r4]
 6411 002e 4B68     		ldr	r3, [r1, #4]
 6412 0030 23F00103 		bic	r3, r3, #1
 6413 0034 4B60     		str	r3, [r1, #4]
 6414              	.L439:
3165:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6415              		.loc 1 3165 5 view .LVU2134
3165:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6416              		.loc 1 3165 9 is_stmt 0 view .LVU2135
 6417 0036 6421     		movs	r1, #100
 6418 0038 2046     		mov	r0, r4
 6419              	.LVL404:
3165:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6420              		.loc 1 3165 9 view .LVU2136
 6421 003a FFF7FEFF 		bl	SPI_EndRxTransaction
 6422              	.LVL405:
3165:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6423              		.loc 1 3165 8 view .LVU2137
 6424 003e 08B1     		cbz	r0, .L440
3167:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6425              		.loc 1 3167 7 is_stmt 1 view .LVU2138
3167:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6426              		.loc 1 3167 23 is_stmt 0 view .LVU2139
 6427 0040 2023     		movs	r3, #32
 6428 0042 2366     		str	r3, [r4, #96]
 6429              	.L440:
3170:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
 6430              		.loc 1 3170 5 is_stmt 1 view .LVU2140
3170:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
 6431              		.loc 1 3170 23 is_stmt 0 view .LVU2141
 6432 0044 0023     		movs	r3, #0
 6433 0046 A4F84630 		strh	r3, [r4, #70]	@ movhi
3171:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6434              		.loc 1 3171 5 is_stmt 1 view .LVU2142
3171:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6435              		.loc 1 3171 17 is_stmt 0 view .LVU2143
 6436 004a 0123     		movs	r3, #1
 6437 004c 84F85D30 		strb	r3, [r4, #93]
3182:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6438              		.loc 1 3182 5 is_stmt 1 view .LVU2144
3182:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6439              		.loc 1 3182 13 is_stmt 0 view .LVU2145
 6440 0050 236E     		ldr	r3, [r4, #96]
3182:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6441              		.loc 1 3182 8 view .LVU2146
 6442 0052 4BB9     		cbnz	r3, .L444
 6443              	.L437:
3197:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6444              		.loc 1 3197 3 is_stmt 1 view .LVU2147
ARM GAS  /tmp/ccqUhOmw.s 			page 225


 6445 0054 2046     		mov	r0, r4
 6446 0056 FFF7FEFF 		bl	HAL_SPI_RxCpltCallback
 6447              	.LVL406:
 6448              	.L436:
3199:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6449              		.loc 1 3199 1 is_stmt 0 view .LVU2148
 6450 005a 38BD     		pop	{r3, r4, r5, pc}
 6451              	.LVL407:
 6452              	.L443:
3156:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6453              		.loc 1 3156 7 is_stmt 1 view .LVU2149
 6454 005c 2168     		ldr	r1, [r4]
 6455 005e 4B68     		ldr	r3, [r1, #4]
 6456 0060 23F00303 		bic	r3, r3, #3
 6457 0064 4B60     		str	r3, [r1, #4]
 6458 0066 E6E7     		b	.L439
 6459              	.LVL408:
 6460              	.L444:
3188:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6461              		.loc 1 3188 7 view .LVU2150
 6462 0068 2046     		mov	r0, r4
 6463 006a FFF7FEFF 		bl	HAL_SPI_ErrorCallback
 6464              	.LVL409:
3190:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6465              		.loc 1 3190 7 view .LVU2151
 6466 006e F4E7     		b	.L436
 6467              		.cfi_endproc
 6468              	.LFE160:
 6470              		.section	.text.SPI_DMATransmitReceiveCplt,"ax",%progbits
 6471              		.align	1
 6472              		.syntax unified
 6473              		.thumb
 6474              		.thumb_func
 6476              	SPI_DMATransmitReceiveCplt:
 6477              	.LVL410:
 6478              	.LFB161:
3208:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 6479              		.loc 1 3208 1 view -0
 6480              		.cfi_startproc
 6481              		@ args = 0, pretend = 0, frame = 0
 6482              		@ frame_needed = 0, uses_anonymous_args = 0
3208:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 6483              		.loc 1 3208 1 is_stmt 0 view .LVU2153
 6484 0000 38B5     		push	{r3, r4, r5, lr}
 6485              		.cfi_def_cfa_offset 16
 6486              		.cfi_offset 3, -16
 6487              		.cfi_offset 4, -12
 6488              		.cfi_offset 5, -8
 6489              		.cfi_offset 14, -4
 6490 0002 0546     		mov	r5, r0
3209:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 6491              		.loc 1 3209 3 is_stmt 1 view .LVU2154
3209:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t tickstart;
 6492              		.loc 1 3209 22 is_stmt 0 view .LVU2155
 6493 0004 446A     		ldr	r4, [r0, #36]
 6494              	.LVL411:
3210:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #if (USE_SPI_CRC != 0U)
ARM GAS  /tmp/ccqUhOmw.s 			page 226


 6495              		.loc 1 3210 3 is_stmt 1 view .LVU2156
3218:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6496              		.loc 1 3218 3 view .LVU2157
3218:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6497              		.loc 1 3218 15 is_stmt 0 view .LVU2158
 6498 0006 FFF7FEFF 		bl	HAL_GetTick
 6499              	.LVL412:
3221:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6500              		.loc 1 3221 3 is_stmt 1 view .LVU2159
3221:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6501              		.loc 1 3221 12 is_stmt 0 view .LVU2160
 6502 000a 2B68     		ldr	r3, [r5]
3221:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6503              		.loc 1 3221 22 view .LVU2161
 6504 000c 1B68     		ldr	r3, [r3]
3221:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6505              		.loc 1 3221 6 view .LVU2162
 6506 000e 13F0200F 		tst	r3, #32
 6507 0012 1CD1     		bne	.L446
 6508 0014 0246     		mov	r2, r0
3224:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6509              		.loc 1 3224 5 is_stmt 1 view .LVU2163
 6510 0016 2168     		ldr	r1, [r4]
 6511 0018 4B68     		ldr	r3, [r1, #4]
 6512 001a 23F02003 		bic	r3, r3, #32
 6513 001e 4B60     		str	r3, [r1, #4]
3261:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6514              		.loc 1 3261 5 view .LVU2164
3261:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6515              		.loc 1 3261 9 is_stmt 0 view .LVU2165
 6516 0020 6421     		movs	r1, #100
 6517 0022 2046     		mov	r0, r4
 6518              	.LVL413:
3261:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6519              		.loc 1 3261 9 view .LVU2166
 6520 0024 FFF7FEFF 		bl	SPI_EndRxTxTransaction
 6521              	.LVL414:
3261:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6522              		.loc 1 3261 8 view .LVU2167
 6523 0028 18B1     		cbz	r0, .L447
3263:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6524              		.loc 1 3263 7 is_stmt 1 view .LVU2168
 6525 002a 236E     		ldr	r3, [r4, #96]
 6526 002c 43F02003 		orr	r3, r3, #32
 6527 0030 2366     		str	r3, [r4, #96]
 6528              	.L447:
3267:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6529              		.loc 1 3267 5 view .LVU2169
 6530 0032 2268     		ldr	r2, [r4]
 6531 0034 5368     		ldr	r3, [r2, #4]
 6532 0036 23F00303 		bic	r3, r3, #3
 6533 003a 5360     		str	r3, [r2, #4]
3269:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount = 0U;
 6534              		.loc 1 3269 5 view .LVU2170
3269:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->RxXferCount = 0U;
 6535              		.loc 1 3269 23 is_stmt 0 view .LVU2171
 6536 003c 0023     		movs	r3, #0
ARM GAS  /tmp/ccqUhOmw.s 			page 227


 6537 003e E387     		strh	r3, [r4, #62]	@ movhi
3270:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
 6538              		.loc 1 3270 5 is_stmt 1 view .LVU2172
3270:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->State = HAL_SPI_STATE_READY;
 6539              		.loc 1 3270 23 is_stmt 0 view .LVU2173
 6540 0040 A4F84630 		strh	r3, [r4, #70]	@ movhi
3271:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6541              		.loc 1 3271 5 is_stmt 1 view .LVU2174
3271:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6542              		.loc 1 3271 17 is_stmt 0 view .LVU2175
 6543 0044 0123     		movs	r3, #1
 6544 0046 84F85D30 		strb	r3, [r4, #93]
3282:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6545              		.loc 1 3282 5 is_stmt 1 view .LVU2176
3282:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6546              		.loc 1 3282 13 is_stmt 0 view .LVU2177
 6547 004a 236E     		ldr	r3, [r4, #96]
3282:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6548              		.loc 1 3282 8 view .LVU2178
 6549 004c 1BB9     		cbnz	r3, .L450
 6550              	.L446:
3297:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6551              		.loc 1 3297 3 is_stmt 1 view .LVU2179
 6552 004e 2046     		mov	r0, r4
 6553 0050 FFF7FEFF 		bl	HAL_SPI_TxRxCpltCallback
 6554              	.LVL415:
 6555              	.L445:
3299:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6556              		.loc 1 3299 1 is_stmt 0 view .LVU2180
 6557 0054 38BD     		pop	{r3, r4, r5, pc}
 6558              	.LVL416:
 6559              	.L450:
3288:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6560              		.loc 1 3288 7 is_stmt 1 view .LVU2181
 6561 0056 2046     		mov	r0, r4
 6562 0058 FFF7FEFF 		bl	HAL_SPI_ErrorCallback
 6563              	.LVL417:
3290:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6564              		.loc 1 3290 7 view .LVU2182
 6565 005c FAE7     		b	.L445
 6566              		.cfi_endproc
 6567              	.LFE161:
 6569              		.section	.text.HAL_SPI_IRQHandler,"ax",%progbits
 6570              		.align	1
 6571              		.global	HAL_SPI_IRQHandler
 6572              		.syntax unified
 6573              		.thumb
 6574              		.thumb_func
 6576              	HAL_SPI_IRQHandler:
 6577              	.LVL418:
 6578              	.LFB148:
2741:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t itsource = hspi->Instance->CR2;
 6579              		.loc 1 2741 1 view -0
 6580              		.cfi_startproc
 6581              		@ args = 0, pretend = 0, frame = 16
 6582              		@ frame_needed = 0, uses_anonymous_args = 0
2741:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t itsource = hspi->Instance->CR2;
ARM GAS  /tmp/ccqUhOmw.s 			page 228


 6583              		.loc 1 2741 1 is_stmt 0 view .LVU2184
 6584 0000 10B5     		push	{r4, lr}
 6585              		.cfi_def_cfa_offset 8
 6586              		.cfi_offset 4, -8
 6587              		.cfi_offset 14, -4
 6588 0002 84B0     		sub	sp, sp, #16
 6589              		.cfi_def_cfa_offset 24
 6590 0004 0446     		mov	r4, r0
2742:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t itflag   = hspi->Instance->SR;
 6591              		.loc 1 2742 3 is_stmt 1 view .LVU2185
2742:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t itflag   = hspi->Instance->SR;
 6592              		.loc 1 2742 27 is_stmt 0 view .LVU2186
 6593 0006 0268     		ldr	r2, [r0]
2742:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t itflag   = hspi->Instance->SR;
 6594              		.loc 1 2742 12 view .LVU2187
 6595 0008 5168     		ldr	r1, [r2, #4]
 6596              	.LVL419:
2743:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6597              		.loc 1 2743 3 is_stmt 1 view .LVU2188
2743:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6598              		.loc 1 2743 12 is_stmt 0 view .LVU2189
 6599 000a 9368     		ldr	r3, [r2, #8]
 6600              	.LVL420:
2746:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (SPI_CHECK_FLAG(itflag, SPI_FLAG_RXNE) != RESET) && (SPI_CHECK_IT_SOURCE(itsource, SPI_IT_RXN
 6601              		.loc 1 2746 3 is_stmt 1 view .LVU2190
2746:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (SPI_CHECK_FLAG(itflag, SPI_FLAG_RXNE) != RESET) && (SPI_CHECK_IT_SOURCE(itsource, SPI_IT_RXN
 6602              		.loc 1 2746 55 is_stmt 0 view .LVU2191
 6603 000c 03F04100 		and	r0, r3, #65
 6604              	.LVL421:
2746:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       (SPI_CHECK_FLAG(itflag, SPI_FLAG_RXNE) != RESET) && (SPI_CHECK_IT_SOURCE(itsource, SPI_IT_RXN
 6605              		.loc 1 2746 6 view .LVU2192
 6606 0010 0128     		cmp	r0, #1
 6607 0012 67D0     		beq	.L463
 6608              	.L452:
2754:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6609              		.loc 1 2754 3 is_stmt 1 view .LVU2193
2754:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6610              		.loc 1 2754 6 is_stmt 0 view .LVU2194
 6611 0014 13F0020F 		tst	r3, #2
 6612 0018 02D0     		beq	.L454
2754:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6613              		.loc 1 2754 55 discriminator 1 view .LVU2195
 6614 001a 11F0800F 		tst	r1, #128
 6615 001e 68D1     		bne	.L464
 6616              	.L454:
2761:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        || (SPI_CHECK_FLAG(itflag, SPI_FLAG_FRE) != RESET)) && (SPI_CHECK_IT_SOURCE(itsource, SPI_IT
 6617              		.loc 1 2761 3 is_stmt 1 view .LVU2196
2761:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****        || (SPI_CHECK_FLAG(itflag, SPI_FLAG_FRE) != RESET)) && (SPI_CHECK_IT_SOURCE(itsource, SPI_IT
 6618              		.loc 1 2761 6 is_stmt 0 view .LVU2197
 6619 0020 13F4B07F 		tst	r3, #352
 6620 0024 68D0     		beq	.L451
2762:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6621              		.loc 1 2762 60 view .LVU2198
 6622 0026 11F0200F 		tst	r1, #32
 6623 002a 65D0     		beq	.L451
2765:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6624              		.loc 1 2765 5 is_stmt 1 view .LVU2199
ARM GAS  /tmp/ccqUhOmw.s 			page 229


2765:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6625              		.loc 1 2765 8 is_stmt 0 view .LVU2200
 6626 002c 13F0400F 		tst	r3, #64
 6627 0030 0FD0     		beq	.L455
2767:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 6628              		.loc 1 2767 7 is_stmt 1 view .LVU2201
2767:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 6629              		.loc 1 2767 15 is_stmt 0 view .LVU2202
 6630 0032 94F85D00 		ldrb	r0, [r4, #93]	@ zero_extendqisi2
 6631 0036 C0B2     		uxtb	r0, r0
2767:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 6632              		.loc 1 2767 10 view .LVU2203
 6633 0038 0328     		cmp	r0, #3
 6634 003a 5FD0     		beq	.L456
2769:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         __HAL_SPI_CLEAR_OVRFLAG(hspi);
 6635              		.loc 1 2769 9 is_stmt 1 view .LVU2204
 6636 003c 206E     		ldr	r0, [r4, #96]
 6637 003e 40F00400 		orr	r0, r0, #4
 6638 0042 2066     		str	r0, [r4, #96]
2770:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 6639              		.loc 1 2770 9 view .LVU2205
 6640              	.LBB7:
2770:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 6641              		.loc 1 2770 9 view .LVU2206
 6642 0044 0020     		movs	r0, #0
 6643 0046 0090     		str	r0, [sp]
2770:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 6644              		.loc 1 2770 9 view .LVU2207
 6645 0048 D068     		ldr	r0, [r2, #12]
 6646 004a 0090     		str	r0, [sp]
2770:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 6647              		.loc 1 2770 9 view .LVU2208
 6648 004c 9068     		ldr	r0, [r2, #8]
 6649 004e 0090     		str	r0, [sp]
2770:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 6650              		.loc 1 2770 9 view .LVU2209
 6651 0050 0098     		ldr	r0, [sp]
 6652              	.LBE7:
2770:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 6653              		.loc 1 2770 9 view .LVU2210
 6654              	.L455:
2780:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6655              		.loc 1 2780 5 view .LVU2211
2780:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6656              		.loc 1 2780 8 is_stmt 0 view .LVU2212
 6657 0052 13F0200F 		tst	r3, #32
 6658 0056 0CD0     		beq	.L457
2782:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_CLEAR_MODFFLAG(hspi);
 6659              		.loc 1 2782 7 is_stmt 1 view .LVU2213
 6660 0058 206E     		ldr	r0, [r4, #96]
 6661 005a 40F00100 		orr	r0, r0, #1
 6662 005e 2066     		str	r0, [r4, #96]
2783:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6663              		.loc 1 2783 7 view .LVU2214
 6664              	.LBB8:
2783:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6665              		.loc 1 2783 7 view .LVU2215
ARM GAS  /tmp/ccqUhOmw.s 			page 230


 6666 0060 0020     		movs	r0, #0
 6667 0062 0290     		str	r0, [sp, #8]
2783:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6668              		.loc 1 2783 7 view .LVU2216
 6669 0064 9068     		ldr	r0, [r2, #8]
 6670 0066 0290     		str	r0, [sp, #8]
2783:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6671              		.loc 1 2783 7 view .LVU2217
 6672 0068 1068     		ldr	r0, [r2]
 6673 006a 20F04000 		bic	r0, r0, #64
 6674 006e 1060     		str	r0, [r2]
2783:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6675              		.loc 1 2783 7 view .LVU2218
 6676 0070 029A     		ldr	r2, [sp, #8]
 6677              	.L457:
2783:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6678              		.loc 1 2783 7 is_stmt 0 view .LVU2219
 6679              	.LBE8:
2783:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6680              		.loc 1 2783 7 is_stmt 1 discriminator 1 view .LVU2220
2787:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6681              		.loc 1 2787 5 discriminator 1 view .LVU2221
2787:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6682              		.loc 1 2787 8 is_stmt 0 discriminator 1 view .LVU2222
 6683 0072 13F4807F 		tst	r3, #256
 6684 0076 09D0     		beq	.L458
2789:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_CLEAR_FREFLAG(hspi);
 6685              		.loc 1 2789 7 is_stmt 1 view .LVU2223
 6686 0078 236E     		ldr	r3, [r4, #96]
 6687              	.LVL422:
2789:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       __HAL_SPI_CLEAR_FREFLAG(hspi);
 6688              		.loc 1 2789 7 is_stmt 0 view .LVU2224
 6689 007a 43F00803 		orr	r3, r3, #8
 6690 007e 2366     		str	r3, [r4, #96]
2790:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6691              		.loc 1 2790 7 is_stmt 1 view .LVU2225
 6692              	.LBB9:
2790:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6693              		.loc 1 2790 7 view .LVU2226
 6694 0080 0023     		movs	r3, #0
 6695 0082 0393     		str	r3, [sp, #12]
2790:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6696              		.loc 1 2790 7 view .LVU2227
 6697 0084 2368     		ldr	r3, [r4]
 6698 0086 9B68     		ldr	r3, [r3, #8]
 6699 0088 0393     		str	r3, [sp, #12]
2790:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6700              		.loc 1 2790 7 view .LVU2228
 6701 008a 039B     		ldr	r3, [sp, #12]
 6702              	.L458:
2790:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6703              		.loc 1 2790 7 is_stmt 0 view .LVU2229
 6704              	.LBE9:
2790:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 6705              		.loc 1 2790 7 is_stmt 1 discriminator 1 view .LVU2230
2793:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6706              		.loc 1 2793 5 discriminator 1 view .LVU2231
ARM GAS  /tmp/ccqUhOmw.s 			page 231


2793:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6707              		.loc 1 2793 13 is_stmt 0 discriminator 1 view .LVU2232
 6708 008c 236E     		ldr	r3, [r4, #96]
2793:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6709              		.loc 1 2793 8 discriminator 1 view .LVU2233
 6710 008e 002B     		cmp	r3, #0
 6711 0090 32D0     		beq	.L451
2796:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6712              		.loc 1 2796 7 is_stmt 1 view .LVU2234
 6713 0092 2268     		ldr	r2, [r4]
 6714 0094 5368     		ldr	r3, [r2, #4]
 6715 0096 23F0E003 		bic	r3, r3, #224
 6716 009a 5360     		str	r3, [r2, #4]
2798:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Disable the SPI DMA requests if enabled */
 6717              		.loc 1 2798 7 view .LVU2235
2798:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       /* Disable the SPI DMA requests if enabled */
 6718              		.loc 1 2798 19 is_stmt 0 view .LVU2236
 6719 009c 0123     		movs	r3, #1
 6720 009e 84F85D30 		strb	r3, [r4, #93]
2800:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 6721              		.loc 1 2800 7 is_stmt 1 view .LVU2237
2800:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 6722              		.loc 1 2800 10 is_stmt 0 view .LVU2238
 6723 00a2 11F0030F 		tst	r1, #3
 6724 00a6 31D0     		beq	.L460
2802:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6725              		.loc 1 2802 9 is_stmt 1 view .LVU2239
 6726 00a8 2268     		ldr	r2, [r4]
 6727 00aa 5368     		ldr	r3, [r2, #4]
 6728 00ac 23F00303 		bic	r3, r3, #3
 6729 00b0 5360     		str	r3, [r2, #4]
2805:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 6730              		.loc 1 2805 9 view .LVU2240
2805:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 6731              		.loc 1 2805 17 is_stmt 0 view .LVU2241
 6732 00b2 A36D     		ldr	r3, [r4, #88]
2805:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 6733              		.loc 1 2805 12 view .LVU2242
 6734 00b4 4BB1     		cbz	r3, .L461
2809:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if (HAL_OK != HAL_DMA_Abort_IT(hspi->hdmarx))
 6735              		.loc 1 2809 11 is_stmt 1 view .LVU2243
2809:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if (HAL_OK != HAL_DMA_Abort_IT(hspi->hdmarx))
 6736              		.loc 1 2809 43 is_stmt 0 view .LVU2244
 6737 00b6 174A     		ldr	r2, .L465
 6738 00b8 5A63     		str	r2, [r3, #52]
2810:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
 6739              		.loc 1 2810 11 is_stmt 1 view .LVU2245
2810:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
 6740              		.loc 1 2810 25 is_stmt 0 view .LVU2246
 6741 00ba A06D     		ldr	r0, [r4, #88]
 6742 00bc FFF7FEFF 		bl	HAL_DMA_Abort_IT
 6743              	.LVL423:
2810:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
 6744              		.loc 1 2810 14 view .LVU2247
 6745 00c0 18B1     		cbz	r0, .L461
2812:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           }
 6746              		.loc 1 2812 13 is_stmt 1 view .LVU2248
ARM GAS  /tmp/ccqUhOmw.s 			page 232


 6747 00c2 236E     		ldr	r3, [r4, #96]
 6748 00c4 43F04003 		orr	r3, r3, #64
 6749 00c8 2366     		str	r3, [r4, #96]
 6750              	.L461:
2816:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 6751              		.loc 1 2816 9 view .LVU2249
2816:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 6752              		.loc 1 2816 17 is_stmt 0 view .LVU2250
 6753 00ca 636D     		ldr	r3, [r4, #84]
2816:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         {
 6754              		.loc 1 2816 12 view .LVU2251
 6755 00cc A3B1     		cbz	r3, .L451
2820:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if (HAL_OK != HAL_DMA_Abort_IT(hspi->hdmatx))
 6756              		.loc 1 2820 11 is_stmt 1 view .LVU2252
2820:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           if (HAL_OK != HAL_DMA_Abort_IT(hspi->hdmatx))
 6757              		.loc 1 2820 43 is_stmt 0 view .LVU2253
 6758 00ce 114A     		ldr	r2, .L465
 6759 00d0 5A63     		str	r2, [r3, #52]
2821:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
 6760              		.loc 1 2821 11 is_stmt 1 view .LVU2254
2821:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
 6761              		.loc 1 2821 25 is_stmt 0 view .LVU2255
 6762 00d2 606D     		ldr	r0, [r4, #84]
 6763 00d4 FFF7FEFF 		bl	HAL_DMA_Abort_IT
 6764              	.LVL424:
2821:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           {
 6765              		.loc 1 2821 14 view .LVU2256
 6766 00d8 70B1     		cbz	r0, .L451
2823:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****           }
 6767              		.loc 1 2823 13 is_stmt 1 view .LVU2257
 6768 00da 236E     		ldr	r3, [r4, #96]
 6769 00dc 43F04003 		orr	r3, r3, #64
 6770 00e0 2366     		str	r3, [r4, #96]
 6771 00e2 09E0     		b	.L451
 6772              	.LVL425:
 6773              	.L463:
2747:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6774              		.loc 1 2747 56 is_stmt 0 view .LVU2258
 6775 00e4 11F0400F 		tst	r1, #64
 6776 00e8 94D0     		beq	.L452
2749:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return;
 6777              		.loc 1 2749 5 is_stmt 1 view .LVU2259
2749:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return;
 6778              		.loc 1 2749 9 is_stmt 0 view .LVU2260
 6779 00ea E36C     		ldr	r3, [r4, #76]
 6780              	.LVL426:
2749:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return;
 6781              		.loc 1 2749 5 view .LVU2261
 6782 00ec 2046     		mov	r0, r4
 6783 00ee 9847     		blx	r3
 6784              	.LVL427:
2750:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 6785              		.loc 1 2750 5 is_stmt 1 view .LVU2262
 6786 00f0 02E0     		b	.L451
 6787              	.LVL428:
 6788              	.L464:
2756:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return;
ARM GAS  /tmp/ccqUhOmw.s 			page 233


 6789              		.loc 1 2756 5 view .LVU2263
2756:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return;
 6790              		.loc 1 2756 9 is_stmt 0 view .LVU2264
 6791 00f2 236D     		ldr	r3, [r4, #80]
 6792              	.LVL429:
2756:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     return;
 6793              		.loc 1 2756 5 view .LVU2265
 6794 00f4 2046     		mov	r0, r4
 6795 00f6 9847     		blx	r3
 6796              	.LVL430:
2757:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 6797              		.loc 1 2757 5 is_stmt 1 view .LVU2266
 6798              	.L451:
2839:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6799              		.loc 1 2839 1 is_stmt 0 view .LVU2267
 6800 00f8 04B0     		add	sp, sp, #16
 6801              		.cfi_remember_state
 6802              		.cfi_def_cfa_offset 8
 6803              		@ sp needed
 6804 00fa 10BD     		pop	{r4, pc}
 6805              	.LVL431:
 6806              	.L456:
 6807              		.cfi_restore_state
2774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         return;
 6808              		.loc 1 2774 9 is_stmt 1 view .LVU2268
 6809              	.LBB10:
2774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         return;
 6810              		.loc 1 2774 9 view .LVU2269
 6811 00fc 0023     		movs	r3, #0
 6812              	.LVL432:
2774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         return;
 6813              		.loc 1 2774 9 is_stmt 0 view .LVU2270
 6814 00fe 0193     		str	r3, [sp, #4]
2774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         return;
 6815              		.loc 1 2774 9 is_stmt 1 view .LVU2271
 6816 0100 D368     		ldr	r3, [r2, #12]
 6817 0102 0193     		str	r3, [sp, #4]
2774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         return;
 6818              		.loc 1 2774 9 view .LVU2272
 6819 0104 9368     		ldr	r3, [r2, #8]
 6820 0106 0193     		str	r3, [sp, #4]
2774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         return;
 6821              		.loc 1 2774 9 view .LVU2273
 6822 0108 019B     		ldr	r3, [sp, #4]
 6823              	.LBE10:
2774:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         return;
 6824              		.loc 1 2774 9 view .LVU2274
2775:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 6825              		.loc 1 2775 9 view .LVU2275
 6826 010a F5E7     		b	.L451
 6827              	.L460:
2833:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6828              		.loc 1 2833 9 view .LVU2276
 6829 010c 2046     		mov	r0, r4
 6830 010e FFF7FEFF 		bl	HAL_SPI_ErrorCallback
 6831              	.LVL433:
2837:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
ARM GAS  /tmp/ccqUhOmw.s 			page 234


 6832              		.loc 1 2837 5 view .LVU2277
 6833 0112 F1E7     		b	.L451
 6834              	.L466:
 6835              		.align	2
 6836              	.L465:
 6837 0114 00000000 		.word	SPI_DMAAbortOnError
 6838              		.cfi_endproc
 6839              	.LFE148:
 6841              		.section	.text.SPI_DMAAbortOnError,"ax",%progbits
 6842              		.align	1
 6843              		.syntax unified
 6844              		.thumb
 6845              		.thumb_func
 6847              	SPI_DMAAbortOnError:
 6848              	.LVL434:
 6849              	.LFB166:
3385:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 6850              		.loc 1 3385 1 view -0
 6851              		.cfi_startproc
 6852              		@ args = 0, pretend = 0, frame = 0
 6853              		@ frame_needed = 0, uses_anonymous_args = 0
3385:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 6854              		.loc 1 3385 1 is_stmt 0 view .LVU2279
 6855 0000 08B5     		push	{r3, lr}
 6856              		.cfi_def_cfa_offset 8
 6857              		.cfi_offset 3, -8
 6858              		.cfi_offset 14, -4
3386:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
 6859              		.loc 1 3386 3 is_stmt 1 view .LVU2280
3386:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->RxXferCount = 0U;
 6860              		.loc 1 3386 22 is_stmt 0 view .LVU2281
 6861 0002 406A     		ldr	r0, [r0, #36]
 6862              	.LVL435:
3387:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 6863              		.loc 1 3387 3 is_stmt 1 view .LVU2282
3387:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 6864              		.loc 1 3387 21 is_stmt 0 view .LVU2283
 6865 0004 0023     		movs	r3, #0
 6866 0006 A0F84630 		strh	r3, [r0, #70]	@ movhi
3388:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6867              		.loc 1 3388 3 is_stmt 1 view .LVU2284
3388:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6868              		.loc 1 3388 21 is_stmt 0 view .LVU2285
 6869 000a C387     		strh	r3, [r0, #62]	@ movhi
3394:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 6870              		.loc 1 3394 3 is_stmt 1 view .LVU2286
 6871 000c FFF7FEFF 		bl	HAL_SPI_ErrorCallback
 6872              	.LVL436:
3396:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6873              		.loc 1 3396 1 is_stmt 0 view .LVU2287
 6874 0010 08BD     		pop	{r3, pc}
 6875              		.cfi_endproc
 6876              	.LFE166:
 6878              		.section	.text.HAL_SPI_AbortCpltCallback,"ax",%progbits
 6879              		.align	1
 6880              		.weak	HAL_SPI_AbortCpltCallback
 6881              		.syntax unified
ARM GAS  /tmp/ccqUhOmw.s 			page 235


 6882              		.thumb
 6883              		.thumb_func
 6885              	HAL_SPI_AbortCpltCallback:
 6886              	.LVL437:
 6887              	.LFB156:
2962:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Prevent unused argument(s) compilation warning */
 6888              		.loc 1 2962 1 is_stmt 1 view -0
 6889              		.cfi_startproc
 6890              		@ args = 0, pretend = 0, frame = 0
 6891              		@ frame_needed = 0, uses_anonymous_args = 0
 6892              		@ link register save eliminated.
2964:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6893              		.loc 1 2964 3 view .LVU2289
2969:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6894              		.loc 1 2969 1 is_stmt 0 view .LVU2290
 6895 0000 7047     		bx	lr
 6896              		.cfi_endproc
 6897              	.LFE156:
 6899              		.section	.text.HAL_SPI_Abort_IT,"ax",%progbits
 6900              		.align	1
 6901              		.global	HAL_SPI_Abort_IT
 6902              		.syntax unified
 6903              		.thumb
 6904              		.thumb_func
 6906              	HAL_SPI_Abort_IT:
 6907              	.LVL438:
 6908              	.LFB144:
2500:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode;
 6909              		.loc 1 2500 1 is_stmt 1 view -0
 6910              		.cfi_startproc
 6911              		@ args = 0, pretend = 0, frame = 16
 6912              		@ frame_needed = 0, uses_anonymous_args = 0
2500:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   HAL_StatusTypeDef errorcode;
 6913              		.loc 1 2500 1 is_stmt 0 view .LVU2292
 6914 0000 70B5     		push	{r4, r5, r6, lr}
 6915              		.cfi_def_cfa_offset 16
 6916              		.cfi_offset 4, -16
 6917              		.cfi_offset 5, -12
 6918              		.cfi_offset 6, -8
 6919              		.cfi_offset 14, -4
 6920 0002 84B0     		sub	sp, sp, #16
 6921              		.cfi_def_cfa_offset 32
 6922 0004 0446     		mov	r4, r0
2501:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   uint32_t abortcplt ;
 6923              		.loc 1 2501 3 is_stmt 1 view .LVU2293
2502:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t count;
 6924              		.loc 1 2502 3 view .LVU2294
2503:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __IO uint32_t resetcount;
 6925              		.loc 1 2503 3 view .LVU2295
2504:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6926              		.loc 1 2504 3 view .LVU2296
2507:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   abortcplt = 1U;
 6927              		.loc 1 2507 3 view .LVU2297
 6928              	.LVL439:
2508:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   resetcount = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24U / 1000U);
 6929              		.loc 1 2508 3 view .LVU2298
2509:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = resetcount;
ARM GAS  /tmp/ccqUhOmw.s 			page 236


 6930              		.loc 1 2509 3 view .LVU2299
2509:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = resetcount;
 6931              		.loc 1 2509 61 is_stmt 0 view .LVU2300
 6932 0006 504B     		ldr	r3, .L496
 6933 0008 1B68     		ldr	r3, [r3]
 6934 000a 504A     		ldr	r2, .L496+4
 6935 000c A2FB0323 		umull	r2, r3, r2, r3
 6936 0010 5B0A     		lsrs	r3, r3, #9
2509:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = resetcount;
 6937              		.loc 1 2509 36 view .LVU2301
 6938 0012 6422     		movs	r2, #100
 6939 0014 02FB03F3 		mul	r3, r2, r3
2509:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   count = resetcount;
 6940              		.loc 1 2509 14 view .LVU2302
 6941 0018 0293     		str	r3, [sp, #8]
2510:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6942              		.loc 1 2510 3 is_stmt 1 view .LVU2303
2510:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6943              		.loc 1 2510 9 is_stmt 0 view .LVU2304
 6944 001a 029B     		ldr	r3, [sp, #8]
 6945 001c 0393     		str	r3, [sp, #12]
2513:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 6946              		.loc 1 2513 3 is_stmt 1 view .LVU2305
 6947 001e 0268     		ldr	r2, [r0]
 6948 0020 5368     		ldr	r3, [r2, #4]
 6949 0022 23F02003 		bic	r3, r3, #32
 6950 0026 5360     		str	r3, [r2, #4]
2516:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6951              		.loc 1 2516 3 view .LVU2306
2516:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6952              		.loc 1 2516 7 is_stmt 0 view .LVU2307
 6953 0028 0268     		ldr	r2, [r0]
 6954 002a 5368     		ldr	r3, [r2, #4]
2516:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6955              		.loc 1 2516 6 view .LVU2308
 6956 002c 13F0800F 		tst	r3, #128
 6957 0030 12D0     		beq	.L471
2518:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
 6958              		.loc 1 2518 5 is_stmt 1 view .LVU2309
2518:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
 6959              		.loc 1 2518 17 is_stmt 0 view .LVU2310
 6960 0032 474B     		ldr	r3, .L496+8
 6961 0034 0365     		str	r3, [r0, #80]
 6962              	.L474:
2520:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 6963              		.loc 1 2520 5 is_stmt 1 view .LVU2311
2522:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 6964              		.loc 1 2522 7 view .LVU2312
2522:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 6965              		.loc 1 2522 17 is_stmt 0 view .LVU2313
 6966 0036 039B     		ldr	r3, [sp, #12]
2522:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 6967              		.loc 1 2522 10 view .LVU2314
 6968 0038 43B1     		cbz	r3, .L493
2527:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
 6969              		.loc 1 2527 7 is_stmt 1 view .LVU2315
2527:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
ARM GAS  /tmp/ccqUhOmw.s 			page 237


 6970              		.loc 1 2527 12 is_stmt 0 view .LVU2316
 6971 003a 039B     		ldr	r3, [sp, #12]
 6972 003c 013B     		subs	r3, r3, #1
 6973 003e 0393     		str	r3, [sp, #12]
2528:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 6974              		.loc 1 2528 26 is_stmt 1 view .LVU2317
2528:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 6975              		.loc 1 2528 18 is_stmt 0 view .LVU2318
 6976 0040 94F85D30 		ldrb	r3, [r4, #93]	@ zero_extendqisi2
 6977 0044 DBB2     		uxtb	r3, r3
2528:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 6978              		.loc 1 2528 26 view .LVU2319
 6979 0046 072B     		cmp	r3, #7
 6980 0048 F5D1     		bne	.L474
 6981 004a 03E0     		b	.L473
 6982              	.L493:
2524:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 6983              		.loc 1 2524 9 is_stmt 1 view .LVU2320
 6984 004c 236E     		ldr	r3, [r4, #96]
 6985 004e 43F04003 		orr	r3, r3, #64
 6986 0052 2366     		str	r3, [r4, #96]
2525:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 6987              		.loc 1 2525 9 view .LVU2321
 6988              	.L473:
2530:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 6989              		.loc 1 2530 5 view .LVU2322
2530:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 6990              		.loc 1 2530 11 is_stmt 0 view .LVU2323
 6991 0054 029B     		ldr	r3, [sp, #8]
 6992 0056 0393     		str	r3, [sp, #12]
 6993              	.L471:
2533:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6994              		.loc 1 2533 3 is_stmt 1 view .LVU2324
2533:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6995              		.loc 1 2533 7 is_stmt 0 view .LVU2325
 6996 0058 5368     		ldr	r3, [r2, #4]
2533:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 6997              		.loc 1 2533 6 view .LVU2326
 6998 005a 13F0400F 		tst	r3, #64
 6999 005e 12D0     		beq	.L475
2535:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
 7000              		.loc 1 2535 5 is_stmt 1 view .LVU2327
2535:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Wait HAL_SPI_STATE_ABORT state */
 7001              		.loc 1 2535 17 is_stmt 0 view .LVU2328
 7002 0060 3C4B     		ldr	r3, .L496+12
 7003 0062 E364     		str	r3, [r4, #76]
 7004              	.L478:
2537:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7005              		.loc 1 2537 5 is_stmt 1 view .LVU2329
2539:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 7006              		.loc 1 2539 7 view .LVU2330
2539:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 7007              		.loc 1 2539 17 is_stmt 0 view .LVU2331
 7008 0064 039B     		ldr	r3, [sp, #12]
2539:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 7009              		.loc 1 2539 10 view .LVU2332
 7010 0066 43B1     		cbz	r3, .L494
ARM GAS  /tmp/ccqUhOmw.s 			page 238


2544:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
 7011              		.loc 1 2544 7 is_stmt 1 view .LVU2333
2544:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     } while (hspi->State != HAL_SPI_STATE_ABORT);
 7012              		.loc 1 2544 12 is_stmt 0 view .LVU2334
 7013 0068 039B     		ldr	r3, [sp, #12]
 7014 006a 013B     		subs	r3, r3, #1
 7015 006c 0393     		str	r3, [sp, #12]
2545:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 7016              		.loc 1 2545 26 is_stmt 1 view .LVU2335
2545:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 7017              		.loc 1 2545 18 is_stmt 0 view .LVU2336
 7018 006e 94F85D30 		ldrb	r3, [r4, #93]	@ zero_extendqisi2
 7019 0072 DBB2     		uxtb	r3, r3
2545:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     /* Reset Timeout Counter */
 7020              		.loc 1 2545 26 view .LVU2337
 7021 0074 072B     		cmp	r3, #7
 7022 0076 F5D1     		bne	.L478
 7023 0078 03E0     		b	.L477
 7024              	.L494:
2541:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         break;
 7025              		.loc 1 2541 9 is_stmt 1 view .LVU2338
 7026 007a 236E     		ldr	r3, [r4, #96]
 7027 007c 43F04003 		orr	r3, r3, #64
 7028 0080 2366     		str	r3, [r4, #96]
2542:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 7029              		.loc 1 2542 9 view .LVU2339
 7030              	.L477:
2547:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7031              		.loc 1 2547 5 view .LVU2340
2547:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7032              		.loc 1 2547 11 is_stmt 0 view .LVU2341
 7033 0082 029B     		ldr	r3, [sp, #8]
 7034 0084 0393     		str	r3, [sp, #12]
 7035              	.L475:
2553:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7036              		.loc 1 2553 3 is_stmt 1 view .LVU2342
2553:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7037              		.loc 1 2553 11 is_stmt 0 view .LVU2343
 7038 0086 636D     		ldr	r3, [r4, #84]
2553:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7039              		.loc 1 2553 6 view .LVU2344
 7040 0088 2BB1     		cbz	r3, .L479
2557:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7041              		.loc 1 2557 5 is_stmt 1 view .LVU2345
2557:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7042              		.loc 1 2557 9 is_stmt 0 view .LVU2346
 7043 008a 5268     		ldr	r2, [r2, #4]
2557:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7044              		.loc 1 2557 8 view .LVU2347
 7045 008c 12F0020F 		tst	r2, #2
 7046 0090 1BD0     		beq	.L480
2559:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 7047              		.loc 1 2559 7 is_stmt 1 view .LVU2348
2559:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 7048              		.loc 1 2559 39 is_stmt 0 view .LVU2349
 7049 0092 314A     		ldr	r2, .L496+16
 7050 0094 5A63     		str	r2, [r3, #52]
ARM GAS  /tmp/ccqUhOmw.s 			page 239


 7051              	.L479:
2567:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7052              		.loc 1 2567 3 is_stmt 1 view .LVU2350
2567:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7053              		.loc 1 2567 11 is_stmt 0 view .LVU2351
 7054 0096 A36D     		ldr	r3, [r4, #88]
2567:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7055              		.loc 1 2567 6 view .LVU2352
 7056 0098 33B1     		cbz	r3, .L481
2571:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7057              		.loc 1 2571 5 is_stmt 1 view .LVU2353
2571:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7058              		.loc 1 2571 9 is_stmt 0 view .LVU2354
 7059 009a 2268     		ldr	r2, [r4]
 7060 009c 5268     		ldr	r2, [r2, #4]
2571:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7061              		.loc 1 2571 8 view .LVU2355
 7062 009e 12F0010F 		tst	r2, #1
 7063 00a2 15D0     		beq	.L482
2573:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 7064              		.loc 1 2573 7 is_stmt 1 view .LVU2356
2573:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 7065              		.loc 1 2573 39 is_stmt 0 view .LVU2357
 7066 00a4 2D4A     		ldr	r2, .L496+20
 7067 00a6 5A63     		str	r2, [r3, #52]
 7068              	.L481:
2582:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7069              		.loc 1 2582 3 is_stmt 1 view .LVU2358
2582:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7070              		.loc 1 2582 7 is_stmt 0 view .LVU2359
 7071 00a8 2368     		ldr	r3, [r4]
 7072 00aa 5B68     		ldr	r3, [r3, #4]
2582:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7073              		.loc 1 2582 6 view .LVU2360
 7074 00ac 13F0020F 		tst	r3, #2
 7075 00b0 11D0     		beq	.L487
2585:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7076              		.loc 1 2585 5 is_stmt 1 view .LVU2361
2585:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7077              		.loc 1 2585 13 is_stmt 0 view .LVU2362
 7078 00b2 606D     		ldr	r0, [r4, #84]
 7079              	.LVL440:
2585:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7080              		.loc 1 2585 8 view .LVU2363
 7081 00b4 28B3     		cbz	r0, .L488
2588:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 7082              		.loc 1 2588 7 is_stmt 1 view .LVU2364
2588:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 7083              		.loc 1 2588 11 is_stmt 0 view .LVU2365
 7084 00b6 FFF7FEFF 		bl	HAL_DMA_Abort_IT
 7085              	.LVL441:
2588:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 7086              		.loc 1 2588 10 view .LVU2366
 7087 00ba 20B3     		cbz	r0, .L489
2590:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 7088              		.loc 1 2590 9 is_stmt 1 view .LVU2367
2590:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
ARM GAS  /tmp/ccqUhOmw.s 			page 240


 7089              		.loc 1 2590 13 is_stmt 0 view .LVU2368
 7090 00bc 636D     		ldr	r3, [r4, #84]
2590:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 7091              		.loc 1 2590 41 view .LVU2369
 7092 00be 0022     		movs	r2, #0
 7093 00c0 5A63     		str	r2, [r3, #52]
2591:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 7094              		.loc 1 2591 9 is_stmt 1 view .LVU2370
2591:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 7095              		.loc 1 2591 25 is_stmt 0 view .LVU2371
 7096 00c2 4023     		movs	r3, #64
 7097 00c4 2366     		str	r3, [r4, #96]
2508:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   resetcount = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24U / 1000U);
 7098              		.loc 1 2508 13 view .LVU2372
 7099 00c6 0126     		movs	r6, #1
 7100 00c8 06E0     		b	.L483
 7101              	.LVL442:
 7102              	.L480:
2563:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 7103              		.loc 1 2563 7 is_stmt 1 view .LVU2373
2563:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 7104              		.loc 1 2563 39 is_stmt 0 view .LVU2374
 7105 00ca 0022     		movs	r2, #0
 7106 00cc 5A63     		str	r2, [r3, #52]
 7107 00ce E2E7     		b	.L479
 7108              	.L482:
2577:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 7109              		.loc 1 2577 7 is_stmt 1 view .LVU2375
2577:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 7110              		.loc 1 2577 39 is_stmt 0 view .LVU2376
 7111 00d0 0022     		movs	r2, #0
 7112 00d2 5A63     		str	r2, [r3, #52]
 7113 00d4 E8E7     		b	.L481
 7114              	.L487:
2508:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   resetcount = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24U / 1000U);
 7115              		.loc 1 2508 13 view .LVU2377
 7116 00d6 0126     		movs	r6, #1
 7117              	.LVL443:
 7118              	.L483:
2600:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7119              		.loc 1 2600 3 is_stmt 1 view .LVU2378
2600:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7120              		.loc 1 2600 7 is_stmt 0 view .LVU2379
 7121 00d8 2368     		ldr	r3, [r4]
 7122 00da 5B68     		ldr	r3, [r3, #4]
2600:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7123              		.loc 1 2600 6 view .LVU2380
 7124 00dc 13F0010F 		tst	r3, #1
 7125 00e0 0AD0     		beq	.L484
2603:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7126              		.loc 1 2603 5 is_stmt 1 view .LVU2381
2603:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7127              		.loc 1 2603 13 is_stmt 0 view .LVU2382
 7128 00e2 A06D     		ldr	r0, [r4, #88]
2603:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7129              		.loc 1 2603 8 view .LVU2383
 7130 00e4 40B1     		cbz	r0, .L484
ARM GAS  /tmp/ccqUhOmw.s 			page 241


2606:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 7131              		.loc 1 2606 7 is_stmt 1 view .LVU2384
2606:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 7132              		.loc 1 2606 11 is_stmt 0 view .LVU2385
 7133 00e6 FFF7FEFF 		bl	HAL_DMA_Abort_IT
 7134              	.LVL444:
2606:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       {
 7135              		.loc 1 2606 10 view .LVU2386
 7136 00ea 0546     		mov	r5, r0
 7137 00ec 30B1     		cbz	r0, .L485
2608:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 7138              		.loc 1 2608 9 is_stmt 1 view .LVU2387
2608:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 7139              		.loc 1 2608 13 is_stmt 0 view .LVU2388
 7140 00ee A36D     		ldr	r3, [r4, #88]
2608:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****         hspi->ErrorCode = HAL_SPI_ERROR_ABORT;
 7141              		.loc 1 2608 41 view .LVU2389
 7142 00f0 0022     		movs	r2, #0
 7143 00f2 5A63     		str	r2, [r3, #52]
2609:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 7144              		.loc 1 2609 9 is_stmt 1 view .LVU2390
2609:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 7145              		.loc 1 2609 25 is_stmt 0 view .LVU2391
 7146 00f4 4023     		movs	r3, #64
 7147 00f6 2366     		str	r3, [r4, #96]
 7148              	.L484:
2618:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7149              		.loc 1 2618 3 is_stmt 1 view .LVU2392
2618:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7150              		.loc 1 2618 6 is_stmt 0 view .LVU2393
 7151 00f8 3EB9     		cbnz	r6, .L495
2507:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   abortcplt = 1U;
 7152              		.loc 1 2507 13 view .LVU2394
 7153 00fa 0025     		movs	r5, #0
 7154              	.LVL445:
 7155              	.L485:
2651:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 7156              		.loc 1 2651 3 is_stmt 1 view .LVU2395
2652:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7157              		.loc 1 2652 1 is_stmt 0 view .LVU2396
 7158 00fc 2846     		mov	r0, r5
 7159 00fe 04B0     		add	sp, sp, #16
 7160              		.cfi_remember_state
 7161              		.cfi_def_cfa_offset 16
 7162              		@ sp needed
 7163 0100 70BD     		pop	{r4, r5, r6, pc}
 7164              	.LVL446:
 7165              	.L488:
 7166              		.cfi_restore_state
2508:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   resetcount = SPI_DEFAULT_TIMEOUT * (SystemCoreClock / 24U / 1000U);
 7167              		.loc 1 2508 13 view .LVU2397
 7168 0102 0126     		movs	r6, #1
 7169 0104 E8E7     		b	.L483
 7170              	.L489:
2595:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****       }
 7171              		.loc 1 2595 19 view .LVU2398
 7172 0106 0026     		movs	r6, #0
ARM GAS  /tmp/ccqUhOmw.s 			page 242


 7173 0108 E6E7     		b	.L483
 7174              	.LVL447:
 7175              	.L495:
2621:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount = 0U;
 7176              		.loc 1 2621 5 is_stmt 1 view .LVU2399
2621:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     hspi->TxXferCount = 0U;
 7177              		.loc 1 2621 23 is_stmt 0 view .LVU2400
 7178 010a 0023     		movs	r3, #0
 7179 010c A4F84630 		strh	r3, [r4, #70]	@ movhi
2622:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7180              		.loc 1 2622 5 is_stmt 1 view .LVU2401
2622:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7181              		.loc 1 2622 23 is_stmt 0 view .LVU2402
 7182 0110 E387     		strh	r3, [r4, #62]	@ movhi
2625:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7183              		.loc 1 2625 5 is_stmt 1 view .LVU2403
2625:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7184              		.loc 1 2625 13 is_stmt 0 view .LVU2404
 7185 0112 236E     		ldr	r3, [r4, #96]
2625:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7186              		.loc 1 2625 8 view .LVU2405
 7187 0114 402B     		cmp	r3, #64
 7188 0116 14D0     		beq	.L491
2633:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 7189              		.loc 1 2633 7 is_stmt 1 view .LVU2406
2633:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 7190              		.loc 1 2633 23 is_stmt 0 view .LVU2407
 7191 0118 0025     		movs	r5, #0
 7192 011a 2566     		str	r5, [r4, #96]
 7193              	.L486:
 7194              	.LVL448:
2637:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_FREFLAG(hspi);
 7195              		.loc 1 2637 5 is_stmt 1 view .LVU2408
 7196              	.LBB11:
2637:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_FREFLAG(hspi);
 7197              		.loc 1 2637 5 view .LVU2409
 7198 011c 0022     		movs	r2, #0
 7199 011e 0092     		str	r2, [sp]
2637:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_FREFLAG(hspi);
 7200              		.loc 1 2637 5 view .LVU2410
 7201 0120 2368     		ldr	r3, [r4]
 7202 0122 D968     		ldr	r1, [r3, #12]
 7203 0124 0091     		str	r1, [sp]
2637:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_FREFLAG(hspi);
 7204              		.loc 1 2637 5 view .LVU2411
 7205 0126 9968     		ldr	r1, [r3, #8]
 7206 0128 0091     		str	r1, [sp]
2637:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_FREFLAG(hspi);
 7207              		.loc 1 2637 5 view .LVU2412
 7208 012a 0099     		ldr	r1, [sp]
 7209              	.LBE11:
2637:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     __HAL_SPI_CLEAR_FREFLAG(hspi);
 7210              		.loc 1 2637 5 view .LVU2413
2638:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7211              		.loc 1 2638 5 view .LVU2414
 7212              	.LBB12:
2638:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
ARM GAS  /tmp/ccqUhOmw.s 			page 243


 7213              		.loc 1 2638 5 view .LVU2415
 7214 012c 0192     		str	r2, [sp, #4]
2638:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7215              		.loc 1 2638 5 view .LVU2416
 7216 012e 9B68     		ldr	r3, [r3, #8]
 7217 0130 0193     		str	r3, [sp, #4]
2638:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7218              		.loc 1 2638 5 view .LVU2417
 7219 0132 019B     		ldr	r3, [sp, #4]
 7220              	.LBE12:
2638:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7221              		.loc 1 2638 5 view .LVU2418
2641:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7222              		.loc 1 2641 5 view .LVU2419
2641:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7223              		.loc 1 2641 17 is_stmt 0 view .LVU2420
 7224 0134 0123     		movs	r3, #1
 7225 0136 84F85D30 		strb	r3, [r4, #93]
2647:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 7226              		.loc 1 2647 5 is_stmt 1 view .LVU2421
 7227 013a 2046     		mov	r0, r4
 7228 013c FFF7FEFF 		bl	HAL_SPI_AbortCpltCallback
 7229              	.LVL449:
 7230 0140 DCE7     		b	.L485
 7231              	.LVL450:
 7232              	.L491:
2628:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     }
 7233              		.loc 1 2628 17 is_stmt 0 view .LVU2422
 7234 0142 0125     		movs	r5, #1
 7235 0144 EAE7     		b	.L486
 7236              	.L497:
 7237 0146 00BF     		.align	2
 7238              	.L496:
 7239 0148 00000000 		.word	SystemCoreClock
 7240 014c F1197605 		.word	91625969
 7241 0150 00000000 		.word	SPI_AbortTx_ISR
 7242 0154 00000000 		.word	SPI_AbortRx_ISR
 7243 0158 00000000 		.word	SPI_DMATxAbortCallback
 7244 015c 00000000 		.word	SPI_DMARxAbortCallback
 7245              		.cfi_endproc
 7246              	.LFE144:
 7248              		.section	.text.SPI_DMARxAbortCallback,"ax",%progbits
 7249              		.align	1
 7250              		.syntax unified
 7251              		.thumb
 7252              		.thumb_func
 7254              	SPI_DMARxAbortCallback:
 7255              	.LVL451:
 7256              	.LFB168:
3473:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 7257              		.loc 1 3473 1 is_stmt 1 view -0
 7258              		.cfi_startproc
 7259              		@ args = 0, pretend = 0, frame = 8
 7260              		@ frame_needed = 0, uses_anonymous_args = 0
3473:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 7261              		.loc 1 3473 1 is_stmt 0 view .LVU2424
 7262 0000 30B5     		push	{r4, r5, lr}
ARM GAS  /tmp/ccqUhOmw.s 			page 244


 7263              		.cfi_def_cfa_offset 12
 7264              		.cfi_offset 4, -12
 7265              		.cfi_offset 5, -8
 7266              		.cfi_offset 14, -4
 7267 0002 85B0     		sub	sp, sp, #20
 7268              		.cfi_def_cfa_offset 32
3474:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7269              		.loc 1 3474 3 is_stmt 1 view .LVU2425
3474:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7270              		.loc 1 3474 22 is_stmt 0 view .LVU2426
 7271 0004 446A     		ldr	r4, [r0, #36]
 7272              	.LVL452:
3477:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7273              		.loc 1 3477 3 is_stmt 1 view .LVU2427
 7274 0006 2268     		ldr	r2, [r4]
 7275 0008 1368     		ldr	r3, [r2]
 7276 000a 23F04003 		bic	r3, r3, #64
 7277 000e 1360     		str	r3, [r2]
3479:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7278              		.loc 1 3479 3 view .LVU2428
3479:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7279              		.loc 1 3479 7 is_stmt 0 view .LVU2429
 7280 0010 A36D     		ldr	r3, [r4, #88]
3479:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7281              		.loc 1 3479 35 view .LVU2430
 7282 0012 0025     		movs	r5, #0
 7283 0014 5D63     		str	r5, [r3, #52]
3482:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7284              		.loc 1 3482 3 is_stmt 1 view .LVU2431
 7285 0016 2268     		ldr	r2, [r4]
 7286 0018 5368     		ldr	r3, [r2, #4]
 7287 001a 23F00103 		bic	r3, r3, #1
 7288 001e 5360     		str	r3, [r2, #4]
3485:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7289              		.loc 1 3485 3 view .LVU2432
3485:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7290              		.loc 1 3485 7 is_stmt 0 view .LVU2433
 7291 0020 FFF7FEFF 		bl	HAL_GetTick
 7292              	.LVL453:
3485:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7293              		.loc 1 3485 7 view .LVU2434
 7294 0024 0090     		str	r0, [sp]
 7295 0026 6423     		movs	r3, #100
 7296 0028 2A46     		mov	r2, r5
 7297 002a 8021     		movs	r1, #128
 7298 002c 2046     		mov	r0, r4
 7299 002e FFF7FEFF 		bl	SPI_WaitFlagStateUntilTimeout
 7300              	.LVL454:
3485:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7301              		.loc 1 3485 6 view .LVU2435
 7302 0032 08B1     		cbz	r0, .L499
3487:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7303              		.loc 1 3487 5 is_stmt 1 view .LVU2436
3487:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7304              		.loc 1 3487 21 is_stmt 0 view .LVU2437
 7305 0034 4023     		movs	r3, #64
 7306 0036 2366     		str	r3, [r4, #96]
ARM GAS  /tmp/ccqUhOmw.s 			page 245


 7307              	.L499:
3491:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7308              		.loc 1 3491 3 is_stmt 1 view .LVU2438
3491:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7309              		.loc 1 3491 7 is_stmt 0 view .LVU2439
 7310 0038 FFF7FEFF 		bl	HAL_GetTick
 7311              	.LVL455:
 7312 003c 0090     		str	r0, [sp]
 7313 003e 6423     		movs	r3, #100
 7314 0040 0022     		movs	r2, #0
 7315 0042 4FF4C061 		mov	r1, #1536
 7316 0046 2046     		mov	r0, r4
 7317 0048 FFF7FEFF 		bl	SPI_WaitFifoStateUntilTimeout
 7318              	.LVL456:
3491:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7319              		.loc 1 3491 6 view .LVU2440
 7320 004c 08B1     		cbz	r0, .L500
3493:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7321              		.loc 1 3493 5 is_stmt 1 view .LVU2441
3493:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7322              		.loc 1 3493 21 is_stmt 0 view .LVU2442
 7323 004e 4023     		movs	r3, #64
 7324 0050 2366     		str	r3, [r4, #96]
 7325              	.L500:
3497:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7326              		.loc 1 3497 3 is_stmt 1 view .LVU2443
3497:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7327              		.loc 1 3497 11 is_stmt 0 view .LVU2444
 7328 0052 636D     		ldr	r3, [r4, #84]
3497:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7329              		.loc 1 3497 6 view .LVU2445
 7330 0054 0BB1     		cbz	r3, .L501
3499:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7331              		.loc 1 3499 5 is_stmt 1 view .LVU2446
3499:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7332              		.loc 1 3499 21 is_stmt 0 view .LVU2447
 7333 0056 5B6B     		ldr	r3, [r3, #52]
3499:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7334              		.loc 1 3499 8 view .LVU2448
 7335 0058 D3B9     		cbnz	r3, .L498
 7336              	.L501:
3506:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 7337              		.loc 1 3506 3 is_stmt 1 view .LVU2449
3506:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 7338              		.loc 1 3506 21 is_stmt 0 view .LVU2450
 7339 005a 0023     		movs	r3, #0
 7340 005c A4F84630 		strh	r3, [r4, #70]	@ movhi
3507:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7341              		.loc 1 3507 3 is_stmt 1 view .LVU2451
3507:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7342              		.loc 1 3507 21 is_stmt 0 view .LVU2452
 7343 0060 E387     		strh	r3, [r4, #62]	@ movhi
3510:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7344              		.loc 1 3510 3 is_stmt 1 view .LVU2453
3510:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7345              		.loc 1 3510 11 is_stmt 0 view .LVU2454
 7346 0062 236E     		ldr	r3, [r4, #96]
ARM GAS  /tmp/ccqUhOmw.s 			page 246


3510:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7347              		.loc 1 3510 6 view .LVU2455
 7348 0064 402B     		cmp	r3, #64
 7349 0066 01D0     		beq	.L503
3513:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7350              		.loc 1 3513 5 is_stmt 1 view .LVU2456
3513:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7351              		.loc 1 3513 21 is_stmt 0 view .LVU2457
 7352 0068 0023     		movs	r3, #0
 7353 006a 2366     		str	r3, [r4, #96]
 7354              	.L503:
3517:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7355              		.loc 1 3517 3 is_stmt 1 view .LVU2458
 7356              	.LBB13:
3517:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7357              		.loc 1 3517 3 view .LVU2459
 7358 006c 0022     		movs	r2, #0
 7359 006e 0292     		str	r2, [sp, #8]
3517:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7360              		.loc 1 3517 3 view .LVU2460
 7361 0070 2368     		ldr	r3, [r4]
 7362 0072 D968     		ldr	r1, [r3, #12]
 7363 0074 0291     		str	r1, [sp, #8]
3517:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7364              		.loc 1 3517 3 view .LVU2461
 7365 0076 9968     		ldr	r1, [r3, #8]
 7366 0078 0291     		str	r1, [sp, #8]
3517:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7367              		.loc 1 3517 3 view .LVU2462
 7368 007a 0299     		ldr	r1, [sp, #8]
 7369              	.LBE13:
3517:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7370              		.loc 1 3517 3 view .LVU2463
3518:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7371              		.loc 1 3518 3 view .LVU2464
 7372              	.LBB14:
3518:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7373              		.loc 1 3518 3 view .LVU2465
 7374 007c 0392     		str	r2, [sp, #12]
3518:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7375              		.loc 1 3518 3 view .LVU2466
 7376 007e 9B68     		ldr	r3, [r3, #8]
 7377 0080 0393     		str	r3, [sp, #12]
3518:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7378              		.loc 1 3518 3 view .LVU2467
 7379 0082 039B     		ldr	r3, [sp, #12]
 7380              	.LBE14:
3518:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7381              		.loc 1 3518 3 view .LVU2468
3521:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7382              		.loc 1 3521 3 view .LVU2469
3521:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7383              		.loc 1 3521 16 is_stmt 0 view .LVU2470
 7384 0084 0123     		movs	r3, #1
 7385 0086 84F85D30 		strb	r3, [r4, #93]
3527:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 7386              		.loc 1 3527 3 is_stmt 1 view .LVU2471
ARM GAS  /tmp/ccqUhOmw.s 			page 247


 7387 008a 2046     		mov	r0, r4
 7388 008c FFF7FEFF 		bl	HAL_SPI_AbortCpltCallback
 7389              	.LVL457:
 7390              	.L498:
3529:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7391              		.loc 1 3529 1 is_stmt 0 view .LVU2472
 7392 0090 05B0     		add	sp, sp, #20
 7393              		.cfi_def_cfa_offset 12
 7394              		@ sp needed
 7395 0092 30BD     		pop	{r4, r5, pc}
3529:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7396              		.loc 1 3529 1 view .LVU2473
 7397              		.cfi_endproc
 7398              	.LFE168:
 7400              		.section	.text.SPI_DMATxAbortCallback,"ax",%progbits
 7401              		.align	1
 7402              		.syntax unified
 7403              		.thumb
 7404              		.thumb_func
 7406              	SPI_DMATxAbortCallback:
 7407              	.LVL458:
 7408              	.LFB167:
3407:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 7409              		.loc 1 3407 1 is_stmt 1 view -0
 7410              		.cfi_startproc
 7411              		@ args = 0, pretend = 0, frame = 8
 7412              		@ frame_needed = 0, uses_anonymous_args = 0
3407:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   SPI_HandleTypeDef *hspi = (SPI_HandleTypeDef *)(((DMA_HandleTypeDef *)hdma)->Parent); /* Derogati
 7413              		.loc 1 3407 1 is_stmt 0 view .LVU2475
 7414 0000 10B5     		push	{r4, lr}
 7415              		.cfi_def_cfa_offset 8
 7416              		.cfi_offset 4, -8
 7417              		.cfi_offset 14, -4
 7418 0002 84B0     		sub	sp, sp, #16
 7419              		.cfi_def_cfa_offset 24
3408:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7420              		.loc 1 3408 3 is_stmt 1 view .LVU2476
3408:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7421              		.loc 1 3408 22 is_stmt 0 view .LVU2477
 7422 0004 446A     		ldr	r4, [r0, #36]
 7423              	.LVL459:
3410:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7424              		.loc 1 3410 3 is_stmt 1 view .LVU2478
3410:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7425              		.loc 1 3410 7 is_stmt 0 view .LVU2479
 7426 0006 636D     		ldr	r3, [r4, #84]
3410:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7427              		.loc 1 3410 35 view .LVU2480
 7428 0008 0022     		movs	r2, #0
 7429 000a 5A63     		str	r2, [r3, #52]
3413:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7430              		.loc 1 3413 3 is_stmt 1 view .LVU2481
 7431 000c 2268     		ldr	r2, [r4]
 7432 000e 5368     		ldr	r3, [r2, #4]
 7433 0010 23F00203 		bic	r3, r3, #2
 7434 0014 5360     		str	r3, [r2, #4]
3415:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/ccqUhOmw.s 			page 248


 7435              		.loc 1 3415 3 view .LVU2482
3415:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7436              		.loc 1 3415 7 is_stmt 0 view .LVU2483
 7437 0016 FFF7FEFF 		bl	HAL_GetTick
 7438              	.LVL460:
3415:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7439              		.loc 1 3415 7 view .LVU2484
 7440 001a 0246     		mov	r2, r0
 7441 001c 6421     		movs	r1, #100
 7442 001e 2046     		mov	r0, r4
 7443 0020 FFF7FEFF 		bl	SPI_EndRxTxTransaction
 7444              	.LVL461:
3415:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7445              		.loc 1 3415 6 view .LVU2485
 7446 0024 08B1     		cbz	r0, .L506
3417:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7447              		.loc 1 3417 5 is_stmt 1 view .LVU2486
3417:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7448              		.loc 1 3417 21 is_stmt 0 view .LVU2487
 7449 0026 4023     		movs	r3, #64
 7450 0028 2366     		str	r3, [r4, #96]
 7451              	.L506:
3421:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7452              		.loc 1 3421 3 is_stmt 1 view .LVU2488
 7453 002a 2268     		ldr	r2, [r4]
 7454 002c 1368     		ldr	r3, [r2]
 7455 002e 23F04003 		bic	r3, r3, #64
 7456 0032 1360     		str	r3, [r2]
3424:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7457              		.loc 1 3424 3 view .LVU2489
3424:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7458              		.loc 1 3424 7 is_stmt 0 view .LVU2490
 7459 0034 FFF7FEFF 		bl	HAL_GetTick
 7460              	.LVL462:
 7461 0038 0090     		str	r0, [sp]
 7462 003a 6423     		movs	r3, #100
 7463 003c 0022     		movs	r2, #0
 7464 003e 4FF4C061 		mov	r1, #1536
 7465 0042 2046     		mov	r0, r4
 7466 0044 FFF7FEFF 		bl	SPI_WaitFifoStateUntilTimeout
 7467              	.LVL463:
3424:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7468              		.loc 1 3424 6 view .LVU2491
 7469 0048 08B1     		cbz	r0, .L507
3426:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7470              		.loc 1 3426 5 is_stmt 1 view .LVU2492
3426:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7471              		.loc 1 3426 21 is_stmt 0 view .LVU2493
 7472 004a 4023     		movs	r3, #64
 7473 004c 2366     		str	r3, [r4, #96]
 7474              	.L507:
3430:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7475              		.loc 1 3430 3 is_stmt 1 view .LVU2494
3430:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7476              		.loc 1 3430 11 is_stmt 0 view .LVU2495
 7477 004e A36D     		ldr	r3, [r4, #88]
3430:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
ARM GAS  /tmp/ccqUhOmw.s 			page 249


 7478              		.loc 1 3430 6 view .LVU2496
 7479 0050 0BB1     		cbz	r3, .L508
3432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7480              		.loc 1 3432 5 is_stmt 1 view .LVU2497
3432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7481              		.loc 1 3432 21 is_stmt 0 view .LVU2498
 7482 0052 5B6B     		ldr	r3, [r3, #52]
3432:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****     {
 7483              		.loc 1 3432 8 view .LVU2499
 7484 0054 D3B9     		cbnz	r3, .L505
 7485              	.L508:
3439:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 7486              		.loc 1 3439 3 is_stmt 1 view .LVU2500
3439:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   hspi->TxXferCount = 0U;
 7487              		.loc 1 3439 21 is_stmt 0 view .LVU2501
 7488 0056 0023     		movs	r3, #0
 7489 0058 A4F84630 		strh	r3, [r4, #70]	@ movhi
3440:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7490              		.loc 1 3440 3 is_stmt 1 view .LVU2502
3440:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7491              		.loc 1 3440 21 is_stmt 0 view .LVU2503
 7492 005c E387     		strh	r3, [r4, #62]	@ movhi
3443:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7493              		.loc 1 3443 3 is_stmt 1 view .LVU2504
3443:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7494              		.loc 1 3443 11 is_stmt 0 view .LVU2505
 7495 005e 236E     		ldr	r3, [r4, #96]
3443:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   {
 7496              		.loc 1 3443 6 view .LVU2506
 7497 0060 402B     		cmp	r3, #64
 7498 0062 01D0     		beq	.L510
3446:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7499              		.loc 1 3446 5 is_stmt 1 view .LVU2507
3446:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   }
 7500              		.loc 1 3446 21 is_stmt 0 view .LVU2508
 7501 0064 0023     		movs	r3, #0
 7502 0066 2366     		str	r3, [r4, #96]
 7503              	.L510:
3450:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7504              		.loc 1 3450 3 is_stmt 1 view .LVU2509
 7505              	.LBB15:
3450:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7506              		.loc 1 3450 3 view .LVU2510
 7507 0068 0022     		movs	r2, #0
 7508 006a 0292     		str	r2, [sp, #8]
3450:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7509              		.loc 1 3450 3 view .LVU2511
 7510 006c 2368     		ldr	r3, [r4]
 7511 006e D968     		ldr	r1, [r3, #12]
 7512 0070 0291     		str	r1, [sp, #8]
3450:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7513              		.loc 1 3450 3 view .LVU2512
 7514 0072 9968     		ldr	r1, [r3, #8]
 7515 0074 0291     		str	r1, [sp, #8]
3450:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7516              		.loc 1 3450 3 view .LVU2513
 7517 0076 0299     		ldr	r1, [sp, #8]
ARM GAS  /tmp/ccqUhOmw.s 			page 250


 7518              	.LBE15:
3450:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   __HAL_SPI_CLEAR_FREFLAG(hspi);
 7519              		.loc 1 3450 3 view .LVU2514
3451:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7520              		.loc 1 3451 3 view .LVU2515
 7521              	.LBB16:
3451:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7522              		.loc 1 3451 3 view .LVU2516
 7523 0078 0392     		str	r2, [sp, #12]
3451:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7524              		.loc 1 3451 3 view .LVU2517
 7525 007a 9B68     		ldr	r3, [r3, #8]
 7526 007c 0393     		str	r3, [sp, #12]
3451:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7527              		.loc 1 3451 3 view .LVU2518
 7528 007e 039B     		ldr	r3, [sp, #12]
 7529              	.LBE16:
3451:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7530              		.loc 1 3451 3 view .LVU2519
3454:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7531              		.loc 1 3454 3 view .LVU2520
3454:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7532              		.loc 1 3454 16 is_stmt 0 view .LVU2521
 7533 0080 0123     		movs	r3, #1
 7534 0082 84F85D30 		strb	r3, [r4, #93]
3460:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** #endif /* USE_HAL_SPI_REGISTER_CALLBACKS */
 7535              		.loc 1 3460 3 is_stmt 1 view .LVU2522
 7536 0086 2046     		mov	r0, r4
 7537 0088 FFF7FEFF 		bl	HAL_SPI_AbortCpltCallback
 7538              	.LVL464:
 7539              	.L505:
3462:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7540              		.loc 1 3462 1 is_stmt 0 view .LVU2523
 7541 008c 04B0     		add	sp, sp, #16
 7542              		.cfi_def_cfa_offset 8
 7543              		@ sp needed
 7544 008e 10BD     		pop	{r4, pc}
3462:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7545              		.loc 1 3462 1 view .LVU2524
 7546              		.cfi_endproc
 7547              	.LFE167:
 7549              		.section	.text.HAL_SPI_GetState,"ax",%progbits
 7550              		.align	1
 7551              		.global	HAL_SPI_GetState
 7552              		.syntax unified
 7553              		.thumb
 7554              		.thumb_func
 7556              	HAL_SPI_GetState:
 7557              	.LVL465:
 7558              	.LFB157:
2997:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Return SPI handle state */
 7559              		.loc 1 2997 1 is_stmt 1 view -0
 7560              		.cfi_startproc
 7561              		@ args = 0, pretend = 0, frame = 0
 7562              		@ frame_needed = 0, uses_anonymous_args = 0
 7563              		@ link register save eliminated.
2999:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
ARM GAS  /tmp/ccqUhOmw.s 			page 251


 7564              		.loc 1 2999 3 view .LVU2526
2999:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 7565              		.loc 1 2999 14 is_stmt 0 view .LVU2527
 7566 0000 90F85D00 		ldrb	r0, [r0, #93]	@ zero_extendqisi2
 7567              	.LVL466:
3000:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7568              		.loc 1 3000 1 view .LVU2528
 7569 0004 7047     		bx	lr
 7570              		.cfi_endproc
 7571              	.LFE157:
 7573              		.section	.text.HAL_SPI_GetError,"ax",%progbits
 7574              		.align	1
 7575              		.global	HAL_SPI_GetError
 7576              		.syntax unified
 7577              		.thumb
 7578              		.thumb_func
 7580              	HAL_SPI_GetError:
 7581              	.LVL467:
 7582              	.LFB158:
3009:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c ****   /* Return SPI ErrorCode */
 7583              		.loc 1 3009 1 is_stmt 1 view -0
 7584              		.cfi_startproc
 7585              		@ args = 0, pretend = 0, frame = 0
 7586              		@ frame_needed = 0, uses_anonymous_args = 0
 7587              		@ link register save eliminated.
3011:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 7588              		.loc 1 3011 3 view .LVU2530
3011:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** }
 7589              		.loc 1 3011 14 is_stmt 0 view .LVU2531
 7590 0000 006E     		ldr	r0, [r0, #96]
 7591              	.LVL468:
3012:Drivers/STM32F3xx_HAL_Driver/Src/stm32f3xx_hal_spi.c **** 
 7592              		.loc 1 3012 1 view .LVU2532
 7593 0002 7047     		bx	lr
 7594              		.cfi_endproc
 7595              	.LFE158:
 7597              		.text
 7598              	.Letext0:
 7599              		.file 2 "/home/david/.config/Code/User/globalStorage/bmd.stm32-for-vscode/@xpack-dev-tools/arm-non
 7600              		.file 3 "/home/david/.config/Code/User/globalStorage/bmd.stm32-for-vscode/@xpack-dev-tools/arm-non
 7601              		.file 4 "Drivers/CMSIS/Device/ST/STM32F3xx/Include/stm32f302xc.h"
 7602              		.file 5 "Drivers/CMSIS/Device/ST/STM32F3xx/Include/stm32f3xx.h"
 7603              		.file 6 "Drivers/STM32F3xx_HAL_Driver/Inc/stm32f3xx_hal_def.h"
 7604              		.file 7 "Drivers/STM32F3xx_HAL_Driver/Inc/stm32f3xx_hal_dma.h"
 7605              		.file 8 "Drivers/STM32F3xx_HAL_Driver/Inc/stm32f3xx_hal_spi.h"
 7606              		.file 9 "Drivers/CMSIS/Device/ST/STM32F3xx/Include/system_stm32f3xx.h"
 7607              		.file 10 "Drivers/STM32F3xx_HAL_Driver/Inc/stm32f3xx_hal.h"
ARM GAS  /tmp/ccqUhOmw.s 			page 252


DEFINED SYMBOLS
                            *ABS*:0000000000000000 stm32f3xx_hal_spi.c
     /tmp/ccqUhOmw.s:21     .text.SPI_WaitFlagStateUntilTimeout:0000000000000000 $t
     /tmp/ccqUhOmw.s:26     .text.SPI_WaitFlagStateUntilTimeout:0000000000000000 SPI_WaitFlagStateUntilTimeout
     /tmp/ccqUhOmw.s:200    .text.SPI_WaitFlagStateUntilTimeout:00000000000000c4 $d
     /tmp/ccqUhOmw.s:205    .text.SPI_WaitFifoStateUntilTimeout:0000000000000000 $t
     /tmp/ccqUhOmw.s:210    .text.SPI_WaitFifoStateUntilTimeout:0000000000000000 SPI_WaitFifoStateUntilTimeout
     /tmp/ccqUhOmw.s:415    .text.SPI_WaitFifoStateUntilTimeout:00000000000000ec $d
     /tmp/ccqUhOmw.s:420    .text.SPI_EndRxTxTransaction:0000000000000000 $t
     /tmp/ccqUhOmw.s:425    .text.SPI_EndRxTxTransaction:0000000000000000 SPI_EndRxTxTransaction
     /tmp/ccqUhOmw.s:518    .text.SPI_EndRxTransaction:0000000000000000 $t
     /tmp/ccqUhOmw.s:523    .text.SPI_EndRxTransaction:0000000000000000 SPI_EndRxTransaction
     /tmp/ccqUhOmw.s:642    .text.SPI_AbortRx_ISR:0000000000000000 $t
     /tmp/ccqUhOmw.s:647    .text.SPI_AbortRx_ISR:0000000000000000 SPI_AbortRx_ISR
     /tmp/ccqUhOmw.s:761    .text.SPI_AbortRx_ISR:0000000000000088 $d
     /tmp/ccqUhOmw.s:767    .text.SPI_AbortTx_ISR:0000000000000000 $t
     /tmp/ccqUhOmw.s:772    .text.SPI_AbortTx_ISR:0000000000000000 SPI_AbortTx_ISR
     /tmp/ccqUhOmw.s:956    .text.SPI_AbortTx_ISR:00000000000000e8 $d
     /tmp/ccqUhOmw.s:962    .text.HAL_SPI_MspInit:0000000000000000 $t
     /tmp/ccqUhOmw.s:968    .text.HAL_SPI_MspInit:0000000000000000 HAL_SPI_MspInit
     /tmp/ccqUhOmw.s:983    .text.HAL_SPI_Init:0000000000000000 $t
     /tmp/ccqUhOmw.s:989    .text.HAL_SPI_Init:0000000000000000 HAL_SPI_Init
     /tmp/ccqUhOmw.s:1176   .text.HAL_SPI_MspDeInit:0000000000000000 $t
     /tmp/ccqUhOmw.s:1182   .text.HAL_SPI_MspDeInit:0000000000000000 HAL_SPI_MspDeInit
     /tmp/ccqUhOmw.s:1197   .text.HAL_SPI_DeInit:0000000000000000 $t
     /tmp/ccqUhOmw.s:1203   .text.HAL_SPI_DeInit:0000000000000000 HAL_SPI_DeInit
     /tmp/ccqUhOmw.s:1260   .text.HAL_SPI_Transmit:0000000000000000 $t
     /tmp/ccqUhOmw.s:1266   .text.HAL_SPI_Transmit:0000000000000000 HAL_SPI_Transmit
     /tmp/ccqUhOmw.s:1730   .text.HAL_SPI_TransmitReceive:0000000000000000 $t
     /tmp/ccqUhOmw.s:1736   .text.HAL_SPI_TransmitReceive:0000000000000000 HAL_SPI_TransmitReceive
     /tmp/ccqUhOmw.s:2436   .text.HAL_SPI_Receive:0000000000000000 $t
     /tmp/ccqUhOmw.s:2442   .text.HAL_SPI_Receive:0000000000000000 HAL_SPI_Receive
     /tmp/ccqUhOmw.s:2804   .text.HAL_SPI_Transmit_IT:0000000000000000 $t
     /tmp/ccqUhOmw.s:2810   .text.HAL_SPI_Transmit_IT:0000000000000000 HAL_SPI_Transmit_IT
     /tmp/ccqUhOmw.s:2975   .text.HAL_SPI_Transmit_IT:00000000000000a8 $d
     /tmp/ccqUhOmw.s:5482   .text.SPI_TxISR_16BIT:0000000000000000 SPI_TxISR_16BIT
     /tmp/ccqUhOmw.s:5421   .text.SPI_TxISR_8BIT:0000000000000000 SPI_TxISR_8BIT
     /tmp/ccqUhOmw.s:2981   .text.HAL_SPI_TransmitReceive_IT:0000000000000000 $t
     /tmp/ccqUhOmw.s:2987   .text.HAL_SPI_TransmitReceive_IT:0000000000000000 HAL_SPI_TransmitReceive_IT
     /tmp/ccqUhOmw.s:3238   .text.HAL_SPI_TransmitReceive_IT:0000000000000104 $d
     /tmp/ccqUhOmw.s:6122   .text.SPI_2linesRxISR_16BIT:0000000000000000 SPI_2linesRxISR_16BIT
     /tmp/ccqUhOmw.s:6050   .text.SPI_2linesTxISR_16BIT:0000000000000000 SPI_2linesTxISR_16BIT
     /tmp/ccqUhOmw.s:5933   .text.SPI_2linesRxISR_8BIT:0000000000000000 SPI_2linesRxISR_8BIT
     /tmp/ccqUhOmw.s:5828   .text.SPI_2linesTxISR_8BIT:0000000000000000 SPI_2linesTxISR_8BIT
     /tmp/ccqUhOmw.s:3246   .text.HAL_SPI_Receive_IT:0000000000000000 $t
     /tmp/ccqUhOmw.s:3252   .text.HAL_SPI_Receive_IT:0000000000000000 HAL_SPI_Receive_IT
     /tmp/ccqUhOmw.s:3452   .text.HAL_SPI_Receive_IT:00000000000000f4 $d
     /tmp/ccqUhOmw.s:5672   .text.SPI_RxISR_16BIT:0000000000000000 SPI_RxISR_16BIT
     /tmp/ccqUhOmw.s:5611   .text.SPI_RxISR_8BIT:0000000000000000 SPI_RxISR_8BIT
     /tmp/ccqUhOmw.s:3458   .text.HAL_SPI_Transmit_DMA:0000000000000000 $t
     /tmp/ccqUhOmw.s:3464   .text.HAL_SPI_Transmit_DMA:0000000000000000 HAL_SPI_Transmit_DMA
     /tmp/ccqUhOmw.s:3724   .text.HAL_SPI_Transmit_DMA:0000000000000128 $d
     /tmp/ccqUhOmw.s:5163   .text.SPI_DMAHalfTransmitCplt:0000000000000000 SPI_DMAHalfTransmitCplt
     /tmp/ccqUhOmw.s:6237   .text.SPI_DMATransmitCplt:0000000000000000 SPI_DMATransmitCplt
     /tmp/ccqUhOmw.s:6194   .text.SPI_DMAError:0000000000000000 SPI_DMAError
     /tmp/ccqUhOmw.s:3731   .text.HAL_SPI_TransmitReceive_DMA:0000000000000000 $t
     /tmp/ccqUhOmw.s:3737   .text.HAL_SPI_TransmitReceive_DMA:0000000000000000 HAL_SPI_TransmitReceive_DMA
ARM GAS  /tmp/ccqUhOmw.s 			page 253


     /tmp/ccqUhOmw.s:4196   .text.HAL_SPI_TransmitReceive_DMA:0000000000000218 $d
     /tmp/ccqUhOmw.s:5267   .text.SPI_DMAHalfTransmitReceiveCplt:0000000000000000 SPI_DMAHalfTransmitReceiveCplt
     /tmp/ccqUhOmw.s:6476   .text.SPI_DMATransmitReceiveCplt:0000000000000000 SPI_DMATransmitReceiveCplt
     /tmp/ccqUhOmw.s:5215   .text.SPI_DMAHalfReceiveCplt:0000000000000000 SPI_DMAHalfReceiveCplt
     /tmp/ccqUhOmw.s:6360   .text.SPI_DMAReceiveCplt:0000000000000000 SPI_DMAReceiveCplt
     /tmp/ccqUhOmw.s:4205   .text.HAL_SPI_Receive_DMA:0000000000000000 $t
     /tmp/ccqUhOmw.s:4211   .text.HAL_SPI_Receive_DMA:0000000000000000 HAL_SPI_Receive_DMA
     /tmp/ccqUhOmw.s:4523   .text.HAL_SPI_Receive_DMA:0000000000000188 $d
     /tmp/ccqUhOmw.s:4530   .text.HAL_SPI_Abort:0000000000000000 $t
     /tmp/ccqUhOmw.s:4536   .text.HAL_SPI_Abort:0000000000000000 HAL_SPI_Abort
     /tmp/ccqUhOmw.s:4876   .text.HAL_SPI_Abort:0000000000000180 $d
     /tmp/ccqUhOmw.s:4884   .text.HAL_SPI_DMAPause:0000000000000000 $t
     /tmp/ccqUhOmw.s:4890   .text.HAL_SPI_DMAPause:0000000000000000 HAL_SPI_DMAPause
     /tmp/ccqUhOmw.s:4934   .text.HAL_SPI_DMAResume:0000000000000000 $t
     /tmp/ccqUhOmw.s:4940   .text.HAL_SPI_DMAResume:0000000000000000 HAL_SPI_DMAResume
     /tmp/ccqUhOmw.s:4984   .text.HAL_SPI_DMAStop:0000000000000000 $t
     /tmp/ccqUhOmw.s:4990   .text.HAL_SPI_DMAStop:0000000000000000 HAL_SPI_DMAStop
     /tmp/ccqUhOmw.s:5074   .text.HAL_SPI_TxCpltCallback:0000000000000000 $t
     /tmp/ccqUhOmw.s:5080   .text.HAL_SPI_TxCpltCallback:0000000000000000 HAL_SPI_TxCpltCallback
     /tmp/ccqUhOmw.s:5095   .text.HAL_SPI_RxCpltCallback:0000000000000000 $t
     /tmp/ccqUhOmw.s:5101   .text.HAL_SPI_RxCpltCallback:0000000000000000 HAL_SPI_RxCpltCallback
     /tmp/ccqUhOmw.s:5116   .text.HAL_SPI_TxRxCpltCallback:0000000000000000 $t
     /tmp/ccqUhOmw.s:5122   .text.HAL_SPI_TxRxCpltCallback:0000000000000000 HAL_SPI_TxRxCpltCallback
     /tmp/ccqUhOmw.s:5137   .text.HAL_SPI_TxHalfCpltCallback:0000000000000000 $t
     /tmp/ccqUhOmw.s:5143   .text.HAL_SPI_TxHalfCpltCallback:0000000000000000 HAL_SPI_TxHalfCpltCallback
     /tmp/ccqUhOmw.s:5158   .text.SPI_DMAHalfTransmitCplt:0000000000000000 $t
     /tmp/ccqUhOmw.s:5189   .text.HAL_SPI_RxHalfCpltCallback:0000000000000000 $t
     /tmp/ccqUhOmw.s:5195   .text.HAL_SPI_RxHalfCpltCallback:0000000000000000 HAL_SPI_RxHalfCpltCallback
     /tmp/ccqUhOmw.s:5210   .text.SPI_DMAHalfReceiveCplt:0000000000000000 $t
     /tmp/ccqUhOmw.s:5241   .text.HAL_SPI_TxRxHalfCpltCallback:0000000000000000 $t
     /tmp/ccqUhOmw.s:5247   .text.HAL_SPI_TxRxHalfCpltCallback:0000000000000000 HAL_SPI_TxRxHalfCpltCallback
     /tmp/ccqUhOmw.s:5262   .text.SPI_DMAHalfTransmitReceiveCplt:0000000000000000 $t
     /tmp/ccqUhOmw.s:5293   .text.HAL_SPI_ErrorCallback:0000000000000000 $t
     /tmp/ccqUhOmw.s:5299   .text.HAL_SPI_ErrorCallback:0000000000000000 HAL_SPI_ErrorCallback
     /tmp/ccqUhOmw.s:5314   .text.SPI_CloseTx_ISR:0000000000000000 $t
     /tmp/ccqUhOmw.s:5319   .text.SPI_CloseTx_ISR:0000000000000000 SPI_CloseTx_ISR
     /tmp/ccqUhOmw.s:5416   .text.SPI_TxISR_8BIT:0000000000000000 $t
     /tmp/ccqUhOmw.s:5477   .text.SPI_TxISR_16BIT:0000000000000000 $t
     /tmp/ccqUhOmw.s:5538   .text.SPI_CloseRx_ISR:0000000000000000 $t
     /tmp/ccqUhOmw.s:5543   .text.SPI_CloseRx_ISR:0000000000000000 SPI_CloseRx_ISR
     /tmp/ccqUhOmw.s:5606   .text.SPI_RxISR_8BIT:0000000000000000 $t
     /tmp/ccqUhOmw.s:5667   .text.SPI_RxISR_16BIT:0000000000000000 $t
     /tmp/ccqUhOmw.s:5728   .text.SPI_CloseRxTx_ISR:0000000000000000 $t
     /tmp/ccqUhOmw.s:5733   .text.SPI_CloseRxTx_ISR:0000000000000000 SPI_CloseRxTx_ISR
     /tmp/ccqUhOmw.s:5823   .text.SPI_2linesTxISR_8BIT:0000000000000000 $t
     /tmp/ccqUhOmw.s:5928   .text.SPI_2linesRxISR_8BIT:0000000000000000 $t
     /tmp/ccqUhOmw.s:6045   .text.SPI_2linesTxISR_16BIT:0000000000000000 $t
     /tmp/ccqUhOmw.s:6117   .text.SPI_2linesRxISR_16BIT:0000000000000000 $t
     /tmp/ccqUhOmw.s:6189   .text.SPI_DMAError:0000000000000000 $t
     /tmp/ccqUhOmw.s:6232   .text.SPI_DMATransmitCplt:0000000000000000 $t
     /tmp/ccqUhOmw.s:6355   .text.SPI_DMAReceiveCplt:0000000000000000 $t
     /tmp/ccqUhOmw.s:6471   .text.SPI_DMATransmitReceiveCplt:0000000000000000 $t
     /tmp/ccqUhOmw.s:6570   .text.HAL_SPI_IRQHandler:0000000000000000 $t
     /tmp/ccqUhOmw.s:6576   .text.HAL_SPI_IRQHandler:0000000000000000 HAL_SPI_IRQHandler
     /tmp/ccqUhOmw.s:6837   .text.HAL_SPI_IRQHandler:0000000000000114 $d
     /tmp/ccqUhOmw.s:6847   .text.SPI_DMAAbortOnError:0000000000000000 SPI_DMAAbortOnError
     /tmp/ccqUhOmw.s:6842   .text.SPI_DMAAbortOnError:0000000000000000 $t
ARM GAS  /tmp/ccqUhOmw.s 			page 254


     /tmp/ccqUhOmw.s:6879   .text.HAL_SPI_AbortCpltCallback:0000000000000000 $t
     /tmp/ccqUhOmw.s:6885   .text.HAL_SPI_AbortCpltCallback:0000000000000000 HAL_SPI_AbortCpltCallback
     /tmp/ccqUhOmw.s:6900   .text.HAL_SPI_Abort_IT:0000000000000000 $t
     /tmp/ccqUhOmw.s:6906   .text.HAL_SPI_Abort_IT:0000000000000000 HAL_SPI_Abort_IT
     /tmp/ccqUhOmw.s:7239   .text.HAL_SPI_Abort_IT:0000000000000148 $d
     /tmp/ccqUhOmw.s:7406   .text.SPI_DMATxAbortCallback:0000000000000000 SPI_DMATxAbortCallback
     /tmp/ccqUhOmw.s:7254   .text.SPI_DMARxAbortCallback:0000000000000000 SPI_DMARxAbortCallback
     /tmp/ccqUhOmw.s:7249   .text.SPI_DMARxAbortCallback:0000000000000000 $t
     /tmp/ccqUhOmw.s:7401   .text.SPI_DMATxAbortCallback:0000000000000000 $t
     /tmp/ccqUhOmw.s:7550   .text.HAL_SPI_GetState:0000000000000000 $t
     /tmp/ccqUhOmw.s:7556   .text.HAL_SPI_GetState:0000000000000000 HAL_SPI_GetState
     /tmp/ccqUhOmw.s:7574   .text.HAL_SPI_GetError:0000000000000000 $t
     /tmp/ccqUhOmw.s:7580   .text.HAL_SPI_GetError:0000000000000000 HAL_SPI_GetError

UNDEFINED SYMBOLS
HAL_GetTick
SystemCoreClock
HAL_DMA_Start_IT
HAL_DMA_Abort
HAL_DMA_Abort_IT
