(footprint "TestPoint_Harwin_S2761-46R"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -1.4 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "aa879e27-4e11-43b8-95fe-a1032e23ba69")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "TestPoint_Harwin_S2761-46R"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "567bfdb8-d05d-4cd4-b9b4-36ac107685b7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "71559dba-dafb-4194-8035-7ad7412915fb")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "4ca11883-5dcd-4ca0-8975-9bc6cac78e97")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "38af5a99-f817-4d37-b926-da0b54eff7af")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -0.9 -0.5)
		(end 0.9 0.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "12a5feb6-799e-4bdb-95cc-13f0e7a4b618")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "405e19d4-912d-4645-88a6-c590b1249e56")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at 0 0)
		(size 1.8 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
		(uuid "ff5d58c9-c45a-4b6e-ab6f-179dd45f8ea9")
	)
	(model "${KIPRJMOD}/FT_Libraries/FaSTTUBe_connectors.pretty/3d_models/s2761-46r.stp"
		(offset
			(xyz 0 0 0.2)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
)
