(footprint "DSI-M8MS_6CON_M8_L90"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "J2"
		(at 0.05 -3.4 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "07ef7268-b789-43cb-9221-215fcde6e8a4")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "M8 6 Pin"
		(at 0 3.85 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "17c8ad41-1754-4895-a54f-e734a068ee5d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Connector_Phoenix_SACC:DSI-M8MS_6CON_M8_L90"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "9e6cb4e7-f99e-4000-b1ac-46f8e38084cd")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "99738fad-f968-46c4-a5d0-6da904cab03b")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "b2026014-f91e-4969-b2bf-cfbb358cfe15")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -6.4 -8.200056)
		(end 6.4 2.7)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "cba175a3-3104-4b3a-a40f-092847f8b7f8")
	)
	(fp_line
		(start -5 -9.2)
		(end 5 -9.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "7fcad5c3-8868-44dd-8572-258ec4c0df96")
	)
	(fp_line
		(start -5 -8.2)
		(end 5 -8.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "eff3f9e9-3e94-4170-b46f-77b5ab32c2b6")
	)
	(fp_text user "${REFERENCE}"
		(at 0 5.374 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "e720d785-41c3-41d2-bae4-b280363526b0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" thru_hole circle
		(at -6.25 0)
		(size 4 4)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6e83b98e-59c9-4b41-9829-aad1c26c61bc")
	)
	(pad "" thru_hole circle
		(at 6.25 0)
		(size 4 4)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "93ece0ca-8bb4-4719-a6f3-19291cda9ade")
	)
	(pad "1" thru_hole circle
		(at 1.365 -1.31)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8077f80e-d183-404c-9e46-58b3bf06affb")
	)
	(pad "2" thru_hole circle
		(at -1.365 -1.31)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "449a16cd-7801-439b-9831-57d8ba4f8401")
	)
	(pad "3" thru_hole circle
		(at -1.75 1.16)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1df8f378-ec24-42d9-957b-dfbf38b858be")
	)
	(pad "4" thru_hole circle
		(at 0 1.9)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "705f8b92-47e3-4b9c-9161-17f24e1e9a8a")
	)
	(pad "5" thru_hole circle
		(at 1.75 1.16)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4aee250e-7c6a-4b71-b679-47cb342694cd")
	)
	(pad "6" thru_hole circle
		(at 0 0)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b5a92ed9-c070-440b-83d1-7d82c105d2a3")
	)
	(model "${KIPRJMOD}/IMU-parts/SACC-DSI-M8MS-6CON-M8-L90 SH.stp"
		(offset
			(xyz 0 0 -2.4)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 180)
		)
	)
)
