(footprint "Micro_Mate-N-Lok_3p_vertical" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 63617341)
  (attr smd)
  (fp_text reference "REF**" (at 0 3.81 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 42713045-fffd-4b2d-ae1e-7232d705fb12)
  )
  (fp_text value "Micro_Mate-N-Lok_3p_vertical" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c0515cd2-cdaa-467e-8354-0f6eadfa35c9)
  )
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1bf544e3-5940-4576-9291-2464e95c0ee2)
  )
  (fp_line (start 5.5 -2.5) (end 4 -2.5) (layer "F.SilkS") (width 0.12) (tstamp 0239a7dc-4f11-4dd5-9564-b10e3cb51ffa))
  (fp_line (start 1 -2.5) (end 2 -2.5) (layer "F.SilkS") (width 0.12) (tstamp 26b5b06d-6731-4f1d-a50f-a1a758285eac))
  (fp_line (start 5.5 2.5) (end 5.5 1.25) (layer "F.SilkS") (width 0.12) (tstamp 3836c63d-ca60-4e8e-a339-40980bdccc31))
  (fp_line (start -2 -2.5) (end -1 -2.5) (layer "F.SilkS") (width 0.12) (tstamp 466f8d1c-c448-4a97-87ec-4e94847952fc))
  (fp_line (start 1 -3) (end 1 -2.5) (layer "F.SilkS") (width 0.12) (tstamp 4925c46f-467c-40b3-95db-ef4df267cd8b))
  (fp_line (start -5.5 -1.25) (end -5.5 -2.5) (layer "F.SilkS") (width 0.12) (tstamp 68d14432-223b-47bb-bd26-18873cfb3df2))
  (fp_line (start -5.5 -1.25) (end -6.5 -1.25) (layer "F.SilkS") (width 0.12) (tstamp 721eced1-7601-448b-b032-57ae840a5bc6))
  (fp_line (start -5.5 1.25) (end -5.5 2.5) (layer "F.SilkS") (width 0.12) (tstamp 75ada5c7-eed3-466b-a900-bb7cf3da6f9e))
  (fp_line (start 5.5 1.25) (end 6.5 1.25) (layer "F.SilkS") (width 0.12) (tstamp 8e73e860-7df5-47ee-9d85-a51cffff4073))
  (fp_line (start -6.5 1.25) (end -5.5 1.25) (layer "F.SilkS") (width 0.12) (tstamp 908ce94b-b837-4c84-b759-ec4fbb006eea))
  (fp_line (start -1 -2.5) (end -1 -3) (layer "F.SilkS") (width 0.12) (tstamp 947acefe-ac33-4206-9de3-25b50b4731dd))
  (fp_line (start -5.5 2.5) (end 5.5 2.5) (layer "F.SilkS") (width 0.12) (tstamp d9b138bc-0203-4547-9bd8-5f8e532ba1ac))
  (fp_line (start 6.5 -1.25) (end 5.5 -1.25) (layer "F.SilkS") (width 0.12) (tstamp e7987f0c-e4c6-4aae-a5d6-e1cfea057719))
  (fp_line (start -5.5 -2.5) (end -4 -2.5) (layer "F.SilkS") (width 0.12) (tstamp ed2acee5-b6b0-4723-bb74-ad84b2a662e5))
  (fp_line (start 5.5 -1.25) (end 5.5 -2.5) (layer "F.SilkS") (width 0.12) (tstamp f1084b0d-b992-4d4c-9074-1c148a908ad5))
  (fp_circle (center 6.25 -3.5) (end 6.75 -3.5) (layer "F.SilkS") (width 0.12) (fill solid) (tstamp 63489ebf-0f52-43a6-a0ab-158b1a7d4988))
  (fp_rect (start -8.5 -4.5) (end 8.5 2.5) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 312474c5-a081-4cd1-b2e6-730f0718514a))
  (fp_line (start 4.318 1.27) (end 5.08 1.27) (layer "F.Fab") (width 0.1) (tstamp c6462399-f2e4-4f1a-b34a-b49a04c8bdb9))
  (fp_line (start 4.318 1.778) (end 4.318 1.27) (layer "F.Fab") (width 0.1) (tstamp f284b1e2-75a4-4a3f-a5f4-6f05f15fb4f5))
  (pad "" smd roundrect (at -6.7 0) (size 3.43 1.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1f3003e6-dce5-420f-906b-3f1e92b67249))
  (pad "" smd roundrect (at 6.7 0) (size 3.43 1.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 378af8b4-af3d-46e7-89ae-deff12ca9067))
  (pad "1" smd roundrect (at 3 -3.2) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 23e32b5c-4ca6-4614-a426-44d605a7d8fd))
  (pad "2" smd roundrect (at 0 -3.2) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8c0807a7-765b-4fa5-baaa-e09a2b610e6b))
  (pad "3" smd roundrect (at -3 -3.2) (size 1.27 2.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ebd06df3-d52b-4cff-99a2-a771df6d3733))
  (model "${KIPRJMOD}/FT_libraries/FaSTTUBe_connectors.pretty/3d_models/Micro_Mate-N-Lok_3p_vertical.stp"
    (offset (xyz 0 0 9.24))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 180))
  )
)
