(footprint "ASX202-06SN" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 636172D1)
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -4 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4c9fdea7-ba0c-45cc-8f66-240980c37d5c)
  )
  (fp_text value "ASX202-06SN" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c58960d9-4cac-4036-ad2e-1aef26946dae)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5b96c1ad-46ba-4366-8241-fbc1cd0e9bbd)
  )
  (pad "1" thru_hole circle (at 0 0) (size 1.3 1.3) (drill 0.65) (layers *.Cu *.Mask) (tstamp be645d0f-8568-47a0-a152-e3ddd33563eb))
  (pad "2" thru_hole circle (at 1.71 -0.56) (size 1.3 1.3) (drill 0.65) (layers *.Cu *.Mask) (tstamp a5e521b9-814e-4853-a5ac-f158785c6269))
  (pad "3" thru_hole circle (at 1.06 1.46) (size 1.3 1.3) (drill 0.65) (layers *.Cu *.Mask) (tstamp 935f462d-8b1e-4005-9f1e-17f537ab1756))
  (pad "4" thru_hole circle (at -1.06 1.46) (size 1.3 1.3) (drill 0.65) (layers *.Cu *.Mask) (tstamp 173f6f06-e7d0-42ac-ab03-ce6b79b9eeee))
  (pad "5" thru_hole circle (at -1.71 -0.56) (size 1.3 1.3) (drill 0.65) (layers *.Cu *.Mask) (tstamp 309b3bff-19c8-41ec-a84d-63399c649f46))
  (pad "6" thru_hole circle (at 0 -1.8) (size 1.3 1.3) (drill 0.65) (layers *.Cu *.Mask) (tstamp 81a15393-727e-448b-a777-b18773023d89))
  (model "${KIPRJMOD}/FT_libraries/FaSTTUBe_connectors.pretty/3d_models/ASX002-06SN-HE.STEP"
    (offset (xyz 0 0 8.5))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 -90 0))
  )
)
