# ros2_control_can

**Adds ROS2 Galactic and Humble support**

This node is designed to provide an interface between a `diff_drive_controller` from `ros_control` and an Arduino running firmware from `ros_arduino_bridge`.
