(footprint "SW_Wurth_WS-TOTV_472121020311" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Ø 6.35mm Panel Cut-Out Vertical Operation Toggle Switch, body 12.7x6.6x23.2mm, https://www.we-online.com/en/components/products/datasheet/472121020311?ki")
  (tags "THT")
  (attr through_hole)
  (fp_text reference "REF**" (at 4.7 -4.55 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "SW_Wurth_WS-TOTV_472121020311" (at 4.7 4.55 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "${REFERENCE}" (at 4.7 0 unlocked) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.075)))
  )
  (fp_rect (start -1.7599999999999996 -3.4099999999999997) (end 11.16 3.4099999999999997)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS"))
  (fp_rect (start -1.8999999999999995 -3.55) (end 11.3 3.55)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd"))
  (fp_rect (start -1.6499999999999995 -3.3) (end 11.05 3.3)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab"))
  (fp_line (start -1.9849999999999994 -1.375) (end -1.9849999999999994 1.375)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS"))
  (fp_line (start -1.6499999999999995 -1.375) (end 4.440892098500626e-16 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab"))
  (fp_line (start -1.6499999999999995 1.375) (end 4.440892098500626e-16 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab"))
  (pad "1" thru_hole rect (at 0 0) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask"))
  (pad "2" thru_hole circle (at 4.7 0) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask"))
  (pad "3" thru_hole circle (at 9.4 0) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask"))
  (model "${WE_3DMODEL_DIR}/Switch_THT_Wurth.3dshapes/SW_Wurth_WS-TOTV_472121020311.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)