(footprint "SW_Wurth_WS-TOTV_472131010111" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Ø 6.35mm Panel Cut-Out Vertical Operation Toggle Switch, body 12.7x11.4x29.6mm, https://www.we-online.com/en/components/products/datasheet/472131010111?ki")
  (tags "THT")
  (attr through_hole)
  (fp_text reference "REF**" (at 4.7 -4.55 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 365a85e6-47df-46b5-8292-10e4a2130000)
  )
  (fp_text value "SW_Wurth_WS-TOTV_472131010111" (at 4.7 9.35 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp dc799fa4-f846-4d69-b033-fd0bc9e7fc00)
  )
  (fp_text user "${REFERENCE}" (at 4.7 2.4 unlocked) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    (tstamp c8f3368e-f5b6-4540-a85f-e4f76ff68415)
  )
  (fp_line (start -1.985 -1.375) (end -1.985 1.375)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 47974db9-6c77-42c8-bf74-aa32a080002e))
  (fp_rect (start -1.76 -3.41) (end 11.16 8.21)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp c377b580-b627-4791-b543-a0a6c5ae5fba))
  (fp_rect (start -1.9 -3.55) (end 11.3 8.35)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp c6ee52c4-3f7c-43ce-b9b0-3e25d386550f))
  (fp_line (start -1.65 -1.375) (end 0 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b5e70b0f-61a3-4283-868d-e3ef58d897f6))
  (fp_line (start -1.65 1.375) (end 0 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ab99eefc-d275-4abc-8caf-7b99b74e3d95))
  (fp_rect (start -1.65 -3.3) (end 11.05 8.1)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 2bed62b0-cebd-42ba-99d2-728df336162e))
  (pad "1" thru_hole rect (at 0 0) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp efbb5c7e-a2a3-40f8-9e33-6f804162d8d3))
  (pad "2" thru_hole circle (at 4.7 0) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp 584ceea7-1e94-4d98-ac52-6acd021a783c))
  (pad "3" thru_hole circle (at 9.4 0) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp 6a2e2e50-dce5-48fd-aeab-fa07d2433fcc))
  (pad "4" thru_hole circle (at 0 4.8) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp 869d5f71-e620-4de4-a038-717d9d591fc1))
  (pad "5" thru_hole circle (at 4.7 4.8) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp 6f440a1c-fdfb-4431-9059-eb8678e382b7))
  (pad "6" thru_hole circle (at 9.4 4.8) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp 19450fb3-6596-4972-9334-f83125aa5da2))
  (model "${WE_3DMODEL_DIR}/Switch_THT_Wurth.3dshapes/SW_Wurth_WS-TOTV_472131010111.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
