(footprint "SW_Wurth_WS-TOTV_472131020311" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Ø 6.35mm Panel Cut-Out Vertical Operation Toggle Switch, body 12.7x11.4x24.6mm, https://www.we-online.com/en/components/products/datasheet/472131020311?ki")
  (tags "THT")
  (attr through_hole)
  (fp_text reference "REF**" (at 4.7 -4.55 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp bc632b9d-8fb9-4eb6-81bd-f2ae0818a805)
  )
  (fp_text value "SW_Wurth_WS-TOTV_472131020311" (at 4.7 9.35 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b2286577-cb57-414e-8cb6-929e04294756)
  )
  (fp_text user "${REFERENCE}" (at 4.7 2.4 unlocked) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    (tstamp 5ea08283-76e1-4d15-ad65-872c33132ceb)
  )
  (fp_line (start -1.985 -1.375) (end -1.985 1.375)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 422838ce-e18f-4c80-8a07-941228948200))
  (fp_rect (start -1.76 -3.41) (end 11.16 8.21)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp ece8aa83-3f3e-48ec-9730-87bf95422e62))
  (fp_rect (start -1.9 -3.55) (end 11.3 8.35)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp df1163c3-4d9b-43b6-9ab2-d26d8fcdf5d3))
  (fp_line (start -1.65 -1.375) (end 0 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8cdc76be-7a29-47ea-b16e-06f3b24168dc))
  (fp_line (start -1.65 1.375) (end 0 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e286d3b3-c07f-470b-9a2b-737c95ed5c07))
  (fp_rect (start -1.65 -3.3) (end 11.05 8.1)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 08c36265-1940-4e6e-aae7-ae5d58a4ef52))
  (pad "1" thru_hole rect (at 0 0) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp 944320f8-5882-4483-a027-6fa84797d8ea))
  (pad "2" thru_hole circle (at 4.7 0) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp f3ca3c19-1906-4b56-a313-ce554ed827e9))
  (pad "3" thru_hole circle (at 9.4 0) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp f6c9b991-7118-432c-817c-d5a3715e71e8))
  (pad "4" thru_hole circle (at 0 4.8) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp ea7f8607-847a-4a35-b8fa-6798ea61dc87))
  (pad "5" thru_hole circle (at 4.7 4.8) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp 07d4fd24-3716-4d4f-a5cb-71f366b98b77))
  (pad "6" thru_hole circle (at 9.4 4.8) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp e4ce029b-c8e1-4468-854c-92bfcf2fe49f))
  (model "${WE_3DMODEL_DIR}/Switch_THT_Wurth.3dshapes/SW_Wurth_WS-TOTV_472131020311.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
