(footprint "SW_Wurth_WS-TOTV_472133020311" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Ø 6.35mm Panel Cut-Out Vertical Operation Toggle Switch, body 12.7x11.4x24.8mm, https://www.we-online.com/en/components/products/datasheet/472133020311?ki")
  (tags "THT")
  (attr through_hole)
  (fp_text reference "REF**" (at 4.7 -4.55 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 34d5eb7d-a2d5-49d3-95e7-58b81c80ed0f)
  )
  (fp_text value "SW_Wurth_WS-TOTV_472133020311" (at 4.7 9.35 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 753eaf6f-4087-4c08-a76d-1f58ecde0efc)
  )
  (fp_text user "${REFERENCE}" (at 4.7 2.4 unlocked) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    (tstamp 1bad602d-1dc2-4eca-953a-c75df6b91d4b)
  )
  (fp_line (start -1.985 -1.375) (end -1.985 1.375)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 88f21deb-18d8-4790-b242-6eb53f81f6f7))
  (fp_rect (start -1.76 -3.41) (end 11.16 8.21)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 028ef514-1887-4db4-aa37-1e6211d46136))
  (fp_rect (start -1.9 -3.55) (end 11.3 8.35)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp df897f37-7afb-44ef-926b-6b65122ce642))
  (fp_line (start -1.65 -1.375) (end 0 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 38ae94b9-2c18-40d8-8d3a-3bb3682d99ab))
  (fp_line (start -1.65 1.375) (end 0 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9bfa5ace-cc2f-410b-84da-1294b06a7746))
  (fp_rect (start -1.65 -3.3) (end 11.05 8.1)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 392f5348-8599-45af-aff6-89c496b95444))
  (pad "1" thru_hole rect (at 0 0) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp 1d17b837-8174-4842-81dc-6a351822e6d1))
  (pad "2" thru_hole circle (at 4.7 0) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp b5fa7c29-fffe-4a2f-aa39-42de5a488c09))
  (pad "3" thru_hole circle (at 9.4 0) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp 8ea3cfc8-12e8-4598-b395-f4ecd7c56a02))
  (pad "4" thru_hole circle (at 0 4.8) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp 9a11f9b5-88ea-4e77-9b43-ca76529629c6))
  (pad "5" thru_hole circle (at 4.7 4.8) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp 062ba091-9c11-43ef-b4e0-f9442877da24))
  (pad "6" thru_hole circle (at 9.4 4.8) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp c66e4199-8079-4c80-a4f9-ee61d26a14cd))
  (model "${WE_3DMODEL_DIR}/Switch_THT_Wurth.3dshapes/SW_Wurth_WS-TOTV_472133020311.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
