(footprint "SW_Wurth_WS-MITV_463091691402" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Terminal with Actuator, Right Angle Operation Micro Switch, 12.8 x 5.8 mm, body 12.8x6.5x5.8mm, https://www.we-online.com/en/components/products/datasheet/463091691402?ki")
  (tags "THT")
  (attr through_hole)
  (fp_text reference "REF**" (at 5.08 -11.15 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 73fd0e49-b259-4de8-a036-c1263ca4cda0)
  )
  (fp_text value "SW_Wurth_WS-MITV_463091691402" (at 5.08 2.15 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 461960c9-fde1-4f6c-b884-d7a05c647a02)
  )
  (fp_text user "${REFERENCE}" (at 5.08 -6.05 unlocked) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    (tstamp 31ea39d2-e5c8-4765-84c8-058fa2ada324)
  )
  (fp_rect (start -1.43 -9.41) (end 11.59 -2.69)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 89435442-7d93-44a4-9d21-8912ee8469cb))
  (fp_rect (start -1.57 -10.15) (end 11.73 1.15)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 651b59e5-6656-4a07-9221-171b766187d1))
  (fp_rect (start -1.32 -9.3) (end 11.48 -2.8)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp da47c1cb-0100-4297-b3c8-f17448108ff3))
  (pad "C" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp b94954f4-550d-4aca-a52e-8af04b0eaade))
  (pad "NC" thru_hole circle (at 10.16 0) (size 1.8 1.8) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp dc613801-82b8-4068-abcc-5624f16bc073))
  (pad "NO" thru_hole circle (at 5.08 0) (size 1.8 1.8) (drill 1.2) (layers "*.Cu" "*.Mask") (tstamp f2684a5f-f83e-46e5-9f72-b0b21efc55a9))
  (model "${WE_3DMODEL_DIR}/Switch_THT_Wurth.3dshapes/SW_Wurth_WS-MITV_463091691402.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
