(footprint "SW_Wurth_WS-TOTV_472133010111" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Ø 6.35mm Panel Cut-Out Vertical Operation Toggle Switch, body 12.7x11.4x29.9mm, https://www.we-online.com/en/components/products/datasheet/472133010111?ki")
  (tags "THT")
  (attr through_hole)
  (fp_text reference "REF**" (at 4.7 -4.55 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 18b07c9b-c7ac-4605-9fb4-a870b5076017)
  )
  (fp_text value "SW_Wurth_WS-TOTV_472133010111" (at 4.7 9.35 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fae7ea71-6f76-44d8-b7ba-479cbea33177)
  )
  (fp_text user "${REFERENCE}" (at 4.7 2.4 unlocked) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    (tstamp 1100f372-4a38-4312-aece-3713b2b7b892)
  )
  (fp_line (start -1.985 -1.375) (end -1.985 1.375)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7c639d17-bfb3-44f3-aa21-52159ee9277f))
  (fp_rect (start -1.76 -3.41) (end 11.16 8.21)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 5b52957d-5299-4b50-a025-3ed3513812ef))
  (fp_rect (start -1.9 -3.55) (end 11.3 8.35)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 8d75f1de-15ff-4f37-adf5-a8f43267e1da))
  (fp_line (start -1.65 -1.375) (end 0 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 864982a8-e16d-4407-8324-4e8fe4f4baea))
  (fp_line (start -1.65 1.375) (end 0 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0f297345-039d-4983-a6da-57f1cb16861d))
  (fp_rect (start -1.65 -3.3) (end 11.05 8.1)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp a6911fb3-a2a6-4eb3-af82-77301ce743fa))
  (pad "1" thru_hole rect (at 0 0) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp 4a23f1de-4f2e-4fdf-8686-5acff61562b8))
  (pad "2" thru_hole circle (at 4.7 0) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp c5382586-eeaf-474c-9d35-309960a68a9b))
  (pad "3" thru_hole circle (at 9.4 0) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp 0d5b392b-eeda-4c54-94a3-4b060082d673))
  (pad "4" thru_hole circle (at 0 4.8) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp 5218a8f4-880e-4305-a09a-4103d871fba3))
  (pad "5" thru_hole circle (at 4.7 4.8) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp 2efb7e04-2fc8-4b81-b0dc-85aa5311842b))
  (pad "6" thru_hole circle (at 9.4 4.8) (size 2.75 2.75) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp 918e8004-a495-4cb0-a70b-a9046952a48c))
  (model "${WE_3DMODEL_DIR}/Switch_THT_Wurth.3dshapes/SW_Wurth_WS-TOTV_472133010111.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
