<?xml version="1.0" encoding="utf-8"?>
<!--/3045963/1031803/2.50/9/3/Integrated Circuit/-->
<!DOCTYPE curve SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<description>&lt;Hot Swap Voltage Controllers 2.7-V to 19-V, 85m , 0.13-2A eFuse with selectable over voltage protection clamp in leaded package 8-SO PowerPAD -40 to 125&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOIC127P600X170-9N">
<description>&lt;b&gt;DDA (PDSO-G8)&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
<symbols>
<symbol name="TPS259621DDAT">
<pin name="GND_1" direction="io"/>
<pin name="DVDT" direction="io"/>
<pin name="EN/UVLO" direction="io"/>
<pin name="IN" direction="io"/>
<pin name="GND_2" direction="io"/>
<pin name="OVLO/OVCSEL" direction="io"/>
<pin name="ILM" direction="io"/>
<pin name="!FLT" direction="io"/>
<pin name="OUT" direction="io"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TPS259621DDAT" prefix="IC">
<description>&lt;b&gt;Hot Swap Voltage Controllers 2.7-V to 19-V, 85m , 0.13-2A eFuse with selectable over voltage protection clamp in leaded package 8-SO PowerPAD -40 to 125&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="https://www.ti.com/lit/gpn/TPS2596"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="TPS259621DDAT"/>
</gates>
<devices>
<device name="" package="SOIC127P600X170-9N">
<connects>
<connect gate="G$1" pin="GND_1" pad="1"/>
<connect gate="G$1" pin="DVDT" pad="2"/>
<connect gate="G$1" pin="EN/UVLO" pad="3"/>
<connect gate="G$1" pin="IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="!FLT" pad="6"/>
<connect gate="G$1" pin="ILM" pad="7"/>
<connect gate="G$1" pin="OVLO/OVCSEL" pad="8"/>
<connect gate="G$1" pin="GND_2" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="Mouser_Part_Number" value="595-TPS259621DDAT"/>
<attribute name="Mouser_Price-Stock" value="https://www.mouser.co.uk/ProductDetail/Texas-Instruments/TPS259621DDAT?qs=XeJtXLiO41RIvFY51dY0JA%3D%3D"/>
<attribute name="Manufacturer_Name" value="Texas Instruments"/>
<attribute name="Manufacturer_Part_Number" value="TPS259621DDAT"/>
<attribute name="Description" value="Hot Swap Voltage Controllers 2.7-V to 19-V, 85m , 0.13-2A eFuse with selectable over voltage protection clamp in leaded package 8-SO PowerPAD -40 to 125"/>
<attribute name="Height" value="1.7mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
