<?xml version="1.0" encoding="utf-8"?>
<!--/1512048/1031803/2.50/8/3/Integrated Circuit/-->
<!DOCTYPE curve SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<description>&lt;Board Mount Temperature Sensors High Accuracy Upgrade to Industry Standard LM75 / TMP75 I2C Temperature Sensor 8-VSSOP -55 to 125&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOP65P490X110-8N">
<description>&lt;b&gt;DGK (S-PDSO-G8)&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
<symbols>
<symbol name="TMP1075DGKR">
<pin name="SDA" direction="io"/>
<pin name="SCL" direction="io"/>
<pin name="ALERT" direction="io"/>
<pin name="GND" direction="io"/>
<pin name="V+" direction="io"/>
<pin name="A0" direction="io"/>
<pin name="A1" direction="io"/>
<pin name="A2" direction="io"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TMP1075DGKR" prefix="IC">
<description>&lt;b&gt;Board Mount Temperature Sensors High Accuracy Upgrade to Industry Standard LM75 / TMP75 I2C Temperature Sensor 8-VSSOP -55 to 125&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="https://datasheet.datasheetarchive.com/originals/distributors/DKDS41/DSANUWW0029535.pdf"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="TMP1075DGKR"/>
</gates>
<devices>
<device name="" package="SOP65P490X110-8N">
<connects>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="ALERT" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="A1" pad="6"/>
<connect gate="G$1" pin="A0" pad="7"/>
<connect gate="G$1" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="Mouser_Part_Number" value="595-TMP1075DGKR"/>
<attribute name="Mouser_Price-Stock" value="https://www.mouser.co.uk/ProductDetail/Texas-Instruments/TMP1075DGKR?qs=F5EMLAvA7IAxhm6M9l3v6Q%3D%3D"/>
<attribute name="Manufacturer_Name" value="Texas Instruments"/>
<attribute name="Manufacturer_Part_Number" value="TMP1075DGKR"/>
<attribute name="Description" value="Board Mount Temperature Sensors High Accuracy Upgrade to Industry Standard LM75 / TMP75 I2C Temperature Sensor 8-VSSOP -55 to 125"/>
<attribute name="Height" value="1.1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
