(footprint "BatteryHolder_Keystone_3003_1x2032" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "http://www.keyelco.com/product-pdf.cfm?p=787")
  (tags "Keystone type 3009 coin cell retainer")
  (attr smd)
  (fp_text reference "REF**" (at 0 -14.5) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 7a0c729a-d060-4348-9c65-bebc5fe3b686)
  )
  (fp_text value "BatteryHolder_Keystone_3003_1x2032" (at 0 14) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2516b493-0369-45e3-aff3-028660f8a18e)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e5a545fa-eb0f-404e-922b-f375f7c0b873)
  )
  (fp_line (start -11 -5) (end -11 -2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 23cca8c6-0cb9-435a-987c-8691ea98fecb))
  (fp_line (start -11 2) (end -11 5)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cdb2f60a-b6d7-45de-8b16-334c386c15bf))
  (fp_line (start -6 10) (end 6 10)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cc610223-c065-471a-b9c9-b3e79e6cec67))
  (fp_line (start -4 -11) (end -11 -5)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp beef446d-0903-4f46-8d0c-a6f2d126fa91))
  (fp_line (start -4 -11) (end 4 -11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0b8c9e1d-0f81-4bc8-853f-a7968967f892))
  (fp_line (start 4 -11) (end 11 -5)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 49a2fa98-e8ff-4efd-a44b-9d41df240065))
  (fp_line (start 11 -5) (end 11 -2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cb9588a8-02e0-4adf-ad2a-d77abcc2e03b))
  (fp_line (start 11 2) (end 11 5)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6156fbb9-10f9-4b41-832c-022d7cdd2c7a))
  (fp_arc (start -6 10) (mid -9.535534 8.535534) (end -11 5)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a7ba1cc8-8981-449c-b2bc-34a37005bfac))
  (fp_arc (start 11 5) (mid 9.535534 8.535534) (end 6 10)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 849cd5cf-ae5b-48aa-bf29-0df4e1b44bc0))
  (fp_circle (center 0 0) (end 10.25 0)
    (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp 14bf1648-52bc-4f6b-b682-e2556c635f81))
  (fp_line (start -11.25 -5.25) (end -11.25 -2)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2f272c28-60ae-426a-a960-df433b36fb15))
  (fp_line (start -11.25 1.95) (end -11.25 10.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c0195f52-c22c-4fd9-9748-bb2e07b37c78))
  (fp_line (start -11.25 10.5) (end 11.25 10.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9800a8ff-5e22-4572-a0bd-cbff3ede2885))
  (fp_line (start -4.25 -11.25) (end -11.25 -5.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fe064c40-1906-4f27-ad03-fcdc9721af60))
  (fp_line (start -4.25 -11.25) (end 4.25 -11.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 512dfa8e-8816-4edf-9cdc-8b7b99fa1402))
  (fp_line (start 4.25 -11.25) (end 11.25 -5.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp af970bd0-e34e-4134-bd26-6eaed4114fa0))
  (fp_line (start 11.25 -5.25) (end 11.25 -1.948519)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6597c953-5b42-428b-8417-2dd30c909a86))
  (fp_line (start 11.25 2) (end 11.25 10.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 55d36568-32b0-40bd-94a1-5af7f3f59268))
  (fp_arc (start -11.25 1.95) (mid -12.569653 -0.025) (end -11.25 -2)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ced48917-0d8e-4c24-9c14-8161c5b9fbcc))
  (fp_arc (start 11.25 -1.948519) (mid 12.569158 0.02574) (end 11.25 2)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 447f4bdf-fcac-44e0-835f-a681406808d6))
  (fp_line (start -10.6 -4.7) (end -10.6 4.7)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 98add012-4e29-4318-8bfd-1e09e949192b))
  (fp_line (start -10.6 -4.7) (end -10 -4.7)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3bfe89a9-4776-43e7-8ed7-1a95a71b5922))
  (fp_line (start -10.6 4.7) (end -10 4.7)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 86948d73-e0c7-4481-a235-2aa76ca988eb))
  (fp_line (start -10 5.9) (end -10 4.7)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d0c68abf-3326-455d-902c-61beab0a9d80))
  (fp_line (start -3.8 -10.6) (end -3.8 -10)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0242305d-f479-46e6-895c-1469a34a0565))
  (fp_line (start -3.8 -10.6) (end 3.8 -10.6)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f2be96c0-89aa-4fad-b51b-3e8c5b1e10b4))
  (fp_line (start -3.8 -10) (end -10 -4.7)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 803d1240-0d8e-45f4-8c24-31c9dc71f253))
  (fp_line (start 3.8 -10.6) (end 3.8 -10)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c7066b6d-ca8f-49b9-9047-504fddce8836))
  (fp_line (start 3.8 -10) (end 10 -4.7)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2d5f0cab-1f81-4176-8e2f-d5a716775e59))
  (fp_line (start 10 -4.7) (end 10.6 -4.7)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp de0954c2-69a7-410c-82f4-5fac3fac342a))
  (fp_line (start 10 4.7) (end 10.6 4.7)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3292b755-6378-4f6f-8f61-1c0af168f49b))
  (fp_line (start 10 5.9) (end 10 4.7)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8c7226d5-3a24-4658-a30e-ecf03f89d361))
  (fp_line (start 10.6 -4.7) (end 10.6 4.7)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0289a289-3e62-42b3-a54e-08e6df3b0e8b))
  (fp_arc (start -6.6 9.3) (mid -9.004163 8.304163) (end -10 5.9)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9f2520f4-1ab3-43c6-894e-744398c9b983))
  (fp_arc (start -5.3 8.8) (mid -5.905918 9.164612) (end -6.6 9.3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp aa1cb929-b9b7-4404-9b1c-ad785c378d9e))
  (fp_arc (start -5.3 8.8) (mid 0 6.870958) (end 5.3 8.8)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c7117efe-df9d-448c-96bb-a9810f1c2458))
  (fp_arc (start 6.6 9.3) (mid 5.905918 9.164613) (end 5.3 8.8)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9af9bd4f-0e3d-4512-b489-713dc7d736c1))
  (fp_arc (start 10 5.9) (mid 9.004163 8.304163) (end 6.6 9.3)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 31bd07eb-da36-42be-bcf3-399c390abcc8))
  (pad "1" thru_hole trapezoid (at -10.6 0) (size 2.5 3.5) (rect_delta -0.5 0) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp f00068ed-1132-478f-a18f-6ec12e24647d))
  (pad "1" thru_hole trapezoid (at 10.6 0) (size 2.5 3.5) (rect_delta 0.5 0) (drill 1.85) (layers "*.Cu" "*.Mask") (tstamp 77469923-d298-4f3a-bc14-a59eca75a1b3))
  (pad "2" smd circle (at 0 0) (size 16 16) (layers "F.Cu" "F.Mask") (tstamp 65fcd214-da6d-4e22-a73b-1c0427be6d6c))
  (model "${KICAD6_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_Keystone_3009_1x2450.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
