(footprint "MagI3C-FISM_SIP-7" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 6226972D)
  (attr through_hole)
  (fp_text reference "REF**" (at -7.62 7.62 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 59ec3156-036e-4049-89db-91a9dd07095f)
  )
  (fp_text value "MagI3C-FISM_SIP-7" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d39d813e-3e64-490c-ba5c-a64bb5ad6bd0)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6a2b20ae-096c-4d9f-92f8-2087c865914f)
  )
  (fp_rect (start -10.16 -1.27) (end 10.16 5.78) (layer "F.SilkS") (width 0.12) (fill none) (tstamp b6135480-ace6-42b2-9c47-856ef57cded1))
  (fp_rect (start -10.16 -1.27) (end 10.16 5.78) (layer "Margin") (width 0.12) (fill none) (tstamp f7667b23-296e-4362-a7e3-949632c8954b))
  (pad "1" thru_hole circle (at -7.62 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask) (tstamp cf386a39-fc62-49dd-8ec5-e044f6bd67ce))
  (pad "2" thru_hole circle (at -5.08 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask) (tstamp eae0ab9f-65b2-44d3-aba7-873c3227fba7))
  (pad "5" thru_hole circle (at 2.54 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask) (tstamp 609b9e1b-4e3b-42b7-ac76-a62ec4d0e7c7))
  (pad "7" thru_hole circle (at 7.62 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask) (tstamp 25e5aa8e-2696-44a3-8d3c-c2c53f2923cf))
)
