(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "TMP1075DSGR" (in_bom yes) (on_board yes)
    (property "Reference" "IC" (at 26.67 7.62 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Value" "TMP1075DSGR" (at 26.67 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "SON50P200X200X80-9N" (at 26.67 -94.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/tmp1075.pdf" (at 26.67 -194.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "ki_description" "High-accuracy upgrade to industry standard LM75 / TMP75 I2C temperature sensor" (at 26.67 -294.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Height" "0.8" (at 26.67 -394.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Part Number" "595-TMP1075DSGR" (at 26.67 -494.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/TMP1075DSGR?qs=gZXFycFWdAOidBdJW42bRw%3D%3D" (at 26.67 -594.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Name" "Texas Instruments" (at 26.67 -694.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Part_Number" "TMP1075DSGR" (at 26.67 -794.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (rectangle
      (start 5.08 2.54)
      (end 25.4 -15.24)
      (stroke (width 0.254) (type default))
      (fill (type background))
    )
    (pin passive line (at 0 0 0) (length 5.08)
      (name "SDA" (effects (font (size 1.27 1.27))))
      (number "1" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -2.54 0) (length 5.08)
      (name "SCL" (effects (font (size 1.27 1.27))))
      (number "2" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -5.08 0) (length 5.08)
      (name "ALERT" (effects (font (size 1.27 1.27))))
      (number "3" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -7.62 0) (length 5.08)
      (name "GND" (effects (font (size 1.27 1.27))))
      (number "4" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 15.24 -20.32 90) (length 5.08)
      (name "EP" (effects (font (size 1.27 1.27))))
      (number "9" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 30.48 0 180) (length 5.08)
      (name "V+" (effects (font (size 1.27 1.27))))
      (number "8" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 30.48 -2.54 180) (length 5.08)
      (name "A0" (effects (font (size 1.27 1.27))))
      (number "7" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 30.48 -5.08 180) (length 5.08)
      (name "A1" (effects (font (size 1.27 1.27))))
      (number "6" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 30.48 -7.62 180) (length 5.08)
      (name "A2" (effects (font (size 1.27 1.27))))
      (number "5" (effects (font (size 1.27 1.27))))
    )
  )
)
