(footprint "Micro_Mate-N-Lok_3p_vertical"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 3.81 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "42713045-fffd-4b2d-ae1e-7232d705fb12")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Micro_Mate-N-Lok_3p_vertical"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "c0515cd2-cdaa-467e-8354-0f6eadfa35c9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9faea814-d577-4b6a-96f0-f26618a13cf8")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "045ca890-2c18-45a6-ad61-80ba2409b768")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "fa1475f6-69b0-42d0-a755-6e7e721f0573")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -5.588 -2.54)
		(end -4.064 -2.54)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6d26d68f-1ca7-4ff3-b058-272f1c399047")
	)
	(fp_line
		(start -5.588 -1.27)
		(end -5.588 -2.54)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "378af8b4-af3d-46e7-89ae-deff12ca9067")
	)
	(fp_line
		(start -5.588 2.54)
		(end -5.588 1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c830e3bc-dc64-4f65-8f47-3b106bae2807")
	)
	(fp_line
		(start -2.032 -2.54)
		(end -1.016 -2.54)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b7199d9b-bebb-4100-9ad3-c2bd31e21d65")
	)
	(fp_line
		(start -1.016 -2.54)
		(end -1.016 -3.048)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5114c7bf-b955-49f3-a0a8-4b954c81bde0")
	)
	(fp_line
		(start 1.016 -3.048)
		(end 1.016 -2.54)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5ca4be1c-537e-4a4a-b344-d0c8ffde8546")
	)
	(fp_line
		(start 1.016 -2.54)
		(end 2.032 -2.54)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "aa2ea573-3f20-43c1-aa99-1f9c6031a9aa")
	)
	(fp_line
		(start 4.064 -2.54)
		(end 5.588 -2.54)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "31e08896-1992-4725-96d9-9d2728bca7a3")
	)
	(fp_line
		(start 5.588 -2.54)
		(end 5.588 -1.27)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f2c93195-af12-4d3e-acdf-bdd0ff675c24")
	)
	(fp_line
		(start 5.588 1.27)
		(end 5.588 2.54)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1d9cdadc-9036-4a95-b6db-fa7b3b74c869")
	)
	(fp_line
		(start 5.588 2.54)
		(end -5.588 2.54)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "12422a89-3d0c-485c-9386-f77121fd68fd")
	)
	(fp_circle
		(center -6.35 -3.81)
		(end -5.85 -3.81)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "63489ebf-0f52-43a6-a0ab-158b1a7d4988")
	)
	(fp_rect
		(start -8.89 -5.08)
		(end 8.89 2.54)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "312474c5-a081-4cd1-b2e6-730f0718514a")
	)
	(fp_line
		(start 4.318 1.27)
		(end 5.08 1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c6462399-f2e4-4f1a-b34a-b49a04c8bdb9")
	)
	(fp_line
		(start 4.318 1.778)
		(end 4.318 1.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f284b1e2-75a4-4a3f-a5f4-6f05f15fb4f5")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "1bf544e3-5940-4576-9291-2464e95c0ee2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" smd roundrect
		(at -6.7 0)
		(size 3.43 1.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "1f3003e6-dce5-420f-906b-3f1e92b67249")
	)
	(pad "" smd roundrect
		(at 6.7 0)
		(size 3.43 1.65)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "378af8b4-af3d-46e7-89ae-deff12ca9067")
	)
	(pad "1" smd roundrect
		(at -3 -3.2)
		(size 1.27 2.54)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "ebd06df3-d52b-4cff-99a2-a771df6d3733")
	)
	(pad "2" smd roundrect
		(at 0 -3.2)
		(size 1.27 2.54)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "8c0807a7-765b-4fa5-baaa-e09a2b610e6b")
	)
	(pad "3" smd roundrect
		(at 3 -3.2)
		(size 1.27 2.54)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "23e32b5c-4ca6-4614-a426-44d605a7d8fd")
	)
	(model "${KIPRJMOD}/Symbol_Library/FaSTTUBe_connectors_3dmodels/Micro_Mate-N-Lok_3p_vertical.stp"
		(offset
			(xyz 0 0 9.24)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 180)
		)
	)
)