(footprint "Binder_M12-A_12P_Female_NoSilk" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 62083683)
  (attr through_hole)
  (fp_text reference "J2" (at 0 -10.045) (layer "F.SilkS") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp aa2b0a93-cf71-4f1a-9437-882c36d07d80)
  )
  (fp_text value "Binder-M12-12P" (at 0 10.045) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fb3d633b-8978-4288-8347-3cba8378f752)
  )
  (fp_circle (center 0 0) (end 0 9.37) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 119c80a2-9d7e-4bbc-9b8d-a9fb4eff2301))
  (fp_line (start -0.6 -3.7) (end -0.6 -4.1) (layer "F.Fab") (width 0.12) (tstamp 4ff95af7-d058-424d-aaf3-96a69c53afd3))
  (fp_line (start 0.6 -3.7) (end 0.6 -4.1) (layer "F.Fab") (width 0.12) (tstamp f1f38b2a-b0ac-44fc-acf3-eb28f9edcb70))
  (fp_arc (start 0.6 -3.7) (mid 0 -3.1) (end -0.6 -3.7) (layer "F.Fab") (width 0.12) (tstamp fc37e9b8-13d7-4762-aca2-931a3e66a3ef))
  (fp_circle (center 0 0) (end 0 9) (layer "F.Fab") (width 0.1) (fill none) (tstamp 0f691f3c-0b7a-47a3-8297-f765fc827b9b))
  (fp_circle (center 0 -0.1) (end 0 -4.2) (layer "F.Fab") (width 0.12) (fill none) (tstamp 98cf9718-dafb-47bb-b0c4-293529a8f44c))
  (pad "1" thru_hole circle (at -1.428 -2.524) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask) (tstamp 54df4804-24ea-43b3-bccc-9c4163b5f544))
  (pad "2" thru_hole circle (at 1.428 -2.524) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask) (tstamp a6949e52-d0d1-4a77-a548-57d1360f470e))
  (pad "3" thru_hole circle (at 2.672 -1.127) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask) (tstamp 26996f56-0ebb-43ad-b15d-58cde1ec17c3))
  (pad "4" thru_hole circle (at 2.804 0.738) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask) (tstamp be57b1c1-68e6-4dba-b2b5-ad0d8b683384))
  (pad "5" thru_hole circle (at 1.77 2.297) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask) (tstamp 19dfcf90-cdac-409e-9dc0-08d5a6ca3dab))
  (pad "6" thru_hole circle (at 0 2.9) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask) (tstamp a9ebf4ce-4494-47d9-b02d-a3c1d4ce80fb))
  (pad "7" thru_hole circle (at -1.77 2.297) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask) (tstamp fe2acaed-a2cd-48b4-bef0-2a5143ddeb93))
  (pad "8" thru_hole circle (at -2.804 0.738) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask) (tstamp 1a0bfc3a-02b7-43f3-9bf1-a51234353b67))
  (pad "9" thru_hole circle (at -2.672 -1.127) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask) (tstamp 9b0a9bd6-d2e6-4357-86d3-998e035ab37e))
  (pad "10" thru_hole circle (at 0 -1.1) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask) (tstamp 836e2893-8082-412e-8fb2-4a549a706c43))
  (pad "11" thru_hole circle (at 0.952627 0.549999) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask) (tstamp 1116e4d3-7a4c-47d3-a9bd-4965b0465262))
  (pad "12" thru_hole circle (at -0.952627 0.55) (size 1.1 1.1) (drill 0.8) (layers *.Cu *.Mask) (tstamp 6bb76e5f-c8e7-49ac-b154-410c47f57a43))
  (model "${KIPRJMOD}/packages3d/Binder.3dshapes/M12-12P.stp"
    (offset (xyz 12.75 0 -2.5))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 180 -45))
  )
)
