FILE_TYPE = MULTI_PHYS_TABLE;

PART 'TLV9002IDDFR'
CLASS = IC
{========================================================================================}
:"MANUFACTURER_NAME", "MANUFACTURER_PART_NUMBER"= "PART_NUMBER", "JEDEC_TYPE", "PACK_TYPE", "MOUSER_PART_NUMBER", "MOUSER_PRICE/STOCK", "DESCRIPTION", "DATASHEET", "HEIGHT";
{========================================================================================}
 "Texas Instruments", "TLV9002IDDFR" (!) = "", "SOT65P280X110-8N", "SOT23 (8-Pin)", "595-TLV9002IDDFR", "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/TLV9002IDDFR?qs=mAH9sUMRCtuVJ6NmNV%252Bgrw%3D%3D", "Operational Amplifiers - Op Amps 2-Channel, 1MHz, RRIO, 1.8V to 5.5V Operational Amplifier for Cost-Optimized Systems 8-SOT-23-THIN -40 to 125", "https://www.ti.com/lit/gpn/TLV9002", "1.1 mm"
END_PART

END.
