(part "AD623ARMZ"
    (packageRef "SOP65P490X110-8N")
    (interface
        (port "1" (symbPinId 1) (portName "–RG") (portType INOUT))
        (port "2" (symbPinId 2) (portName "–IN") (portType INOUT))
        (port "3" (symbPinId 3) (portName "+IN") (portType INOUT))
        (port "4" (symbPinId 4) (portName "–VS") (portType INOUT))
        (port "5" (symbPinId 5) (portName "REF") (portType INOUT))
        (port "6" (symbPinId 6) (portName "OUTPUT") (portType INOUT))
        (port "7" (symbPinId 7) (portName "+VS") (portType INOUT))
        (port "8" (symbPinId 8) (portName "+RG") (portType INOUT))
    )
    (partClass UNDEF)
    (useInSchema Y)
    (useInLayout Y)
    (inPartsList Y)
    (partType NORMAL)
    (placeRestriction FREE)
    (property "compKind" "101")
    (property "Mouser_Part_Number" "584-AD623ARMZ")
    (property "Mouser_Price/Stock" "https://www.mouser.co.uk/ProductDetail/Analog-Devices/AD623ARMZ?qs=NmRFExCfTkHh9YiJNpc9iA%3D%3D")
    (property "Manufacturer_Name" "Analog Devices")
    (property "Manufacturer_Part_Number" "AD623ARMZ")
    (property "Description" "AD623ARMZ, Instrumention Amplifier, 0.5mV Offset, 70dB CMRR, Rail-Rail Output, 3, 5, 9V, 8-Pin MSOP")
    (property "Datasheet_Link" "http://www.analog.com/static/imported-files/data_sheets/AD623.pdf")
    (property "symbolName1" "AD623ARMZ")
)
