(Japanese_coding: sjis)
(function "ECS_3024"
    (uver 1)
    (cuser "SamacSys")
    (uuser "SamacSys")
    (ctime 2015-04-16-09:48:08)
    (utime 2023-03-07-16:10:32)
    (interface
        (port "1" (symbPinId 1) (portType INOUT))
        (port "2" (symbPinId 2) (portType INOUT))
        (port "3" (symbPinId 3) (portType INOUT))
        (port "4" (symbPinId 4) (portType INOUT))
        (port "5" (symbPinId 8) (portType INOUT))
        (port "6" (symbPinId 7) (portType INOUT))
        (port "7" (symbPinId 6) (portType INOUT))
        (port "8" (symbPinId 5) (portType INOUT))
    )
    (property "symbolName" "AD623ARMZ")
)


(pinAssign "ECS_3024"
    (uver 1)
    (cuser "SamacSys")
    (uuser "SamacSys")
    (ctime 2015-04-16-09:48:08)
    (utime 2023-03-07-16:10:32)
    (interface
        (port "1" (symbPinId 1) (portName "–RG") (portType INOUT))
        (port "2" (symbPinId 2) (portName "–IN") (portType INOUT))
        (port "3" (symbPinId 3) (portName "+IN") (portType INOUT))
        (port "4" (symbPinId 4) (portName "–VS") (portType INOUT))
        (port "5" (symbPinId 8) (portName "REF") (portType INOUT))
        (port "6" (symbPinId 7) (portName "OUTPUT") (portType INOUT))
        (port "7" (symbPinId 6) (portName "+VS") (portType INOUT))
        (port "8" (symbPinId 5) (portName "+RG") (portType INOUT))
    )
    (internal
        (funcInst (functionRef "ECS_3024")
                (port "1" (match "1"))
                (port "2" (match "2"))
                (port "3" (match "3"))
                (port "4" (match "4"))
                (port "5" (match "5"))
                (port "6" (match "6"))
                (port "7" (match "7"))
                (port "8" (match "8"))
        )
    )
    (property "usePowerBox" "No")
    (property "symbolName" "AD623ARMZ")
)


(part "AD623ARMZ"
    (uver 1)
    (cuser "SamacSys")
    (uuser "SamacSys")
    (ctime 2015-04-16-09:48:08)
    (utime 2023-03-07-16:10:32)
    (packageRef "AD623ARMZ")
    (pinAssignRef "ECS_3024")
    (interface
        (port "1" (symbPinId 1) (portName "–RG") (portType INOUT))
        (port "2" (symbPinId 2) (portName "–IN") (portType INOUT))
        (port "3" (symbPinId 3) (portName "+IN") (portType INOUT))
        (port "4" (symbPinId 4) (portName "–VS") (portType INOUT))
        (port "5" (symbPinId 8) (portName "REF") (portType INOUT))
        (port "6" (symbPinId 7) (portName "OUTPUT") (portType INOUT))
        (port "7" (symbPinId 6) (portName "+VS") (portType INOUT))
        (port "8" (symbPinId 5) (portName "+RG") (portType INOUT))
    )
    (partClass UNDEF)
    (useInSchema Y)
    (useInLayout Y)
    (inPartsList Y)
    (partType NORMAL)
    (placeRestriction FREE)
    (property "enetNonSeries" "YES")
    (property "refDesPrefix" "IC")
    (property "description" "AD623ARMZ, Instrumention Amplifier, 0.5mV Offset, 70dB CMRR, Rail-Rail Output, 3, 5, 9V, 8-Pin MSOP")
    (property "Mouser_Part_Number" "584-AD623ARMZ")
    (property "Mouser_Price/Stock" "https://www.mouser.co.uk/ProductDetail/Analog-Devices/AD623ARMZ?qs=NmRFExCfTkHh9YiJNpc9iA%3D%3D")
    (property "Manufacturer_Name" "Analog Devices")
    (property "Manufacturer_Part_Number" "AD623ARMZ")
    (property "Datasheet_Link" "http://www.analog.com/static/imported-files/data_sheets/AD623.pdf")
    (property "compAreaTopHeight" 1.1)
)


