(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "LDL1117S33R" (in_bom yes) (on_board yes)
    (property "Reference" "IC" (at 29.21 7.62 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Value" "LDL1117S33R" (at 29.21 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "SOT230P700X180-4N" (at 29.21 -94.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Datasheet" "https://componentsearchengine.com/Datasheets/2/LDL1117S33R.pdf" (at 29.21 -194.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "ki_description" "STMICROELECTRONICS - LDL1117S33R - LDO, FIXED, 3.3V, 1.2A, SOT-223-3" (at 29.21 -294.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Height" "1.8" (at 29.21 -394.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Part Number" "511-LDL1117S33R" (at 29.21 -494.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/STMicroelectronics/LDL1117S33R?qs=AQlKX63v8Rt9Bf6AWSrbFg%3D%3D" (at 29.21 -594.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Name" "STMicroelectronics" (at 29.21 -694.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Part_Number" "LDL1117S33R" (at 29.21 -794.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (rectangle
      (start 5.08 2.54)
      (end 27.94 -7.62)
      (stroke (width 0.254) (type default))
      (fill (type background))
    )
    (pin power_in line (at 0 0 0) (length 5.08)
      (name "GND" (effects (font (size 1.27 1.27))))
      (number "1" (effects (font (size 1.27 1.27))))
    )
    (pin output line (at 0 -2.54 0) (length 5.08)
      (name "VOUT_1" (effects (font (size 1.27 1.27))))
      (number "2" (effects (font (size 1.27 1.27))))
    )
    (pin input line (at 0 -5.08 0) (length 5.08)
      (name "VIN" (effects (font (size 1.27 1.27))))
      (number "3" (effects (font (size 1.27 1.27))))
    )
    (pin output line (at 33.02 0 180) (length 5.08)
      (name "VOUT_2" (effects (font (size 1.27 1.27))))
      (number "4" (effects (font (size 1.27 1.27))))
    )
  )
)
